<?xml version="1.0" encoding="UTF-8"?>
<!-- edited with SAPE SAP Editor -->
<SAP xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="sap.xsd">
    <DocInfoSection>
        <DocName DocType="SAP">mphp</DocName>
        <DocNum Number="100" Project="8441"/>
        <Description>
            <Section>The Protocol Stacks are used to define the functionality of the GSM protocols for interfaces. The GSM specifications are normative when used to describe the functionality of interfaces, but the stacks and the subdivision of protocol layers does not imply or restrict any implementation.</Section>
            <Section>The protocol stack for GPRS consists of several entities. Each entity has one ore more service access points, over which the entity provides a service for the upper entity.</Section>
            <Section>Figure 1-1: Architecture of the GSM/GPRS protocol stack</Section>
            <Section>The information units passed via the SAPs are called primitives and consists of an operation code and several parameters. See the Users Guide for details.</Section>
            <Section>The entities of the GPRS protocol stack are:</Section>
            <Section>1.1 GRR (RLC/MAC) - Radio Link Control/Medium Access Control</Section>
            <Section>This layer contains two functions: The Radio Link Control function provides a radio-solution-dependent reliable link. The Medium Access Control function controls the access signalling (request and grant) procedures for the radio channel, and the mapping of LLC frames onto the GSM physical channel.</Section>
            <Section>1.2 LLC - Logical Link Control</Section>
            <Section>The LLC entity provides multiple highly reliable logical links for asynchronous data transfer between the MS and the network. It supports variable-length information frames, acknowledged and unacknowledged data transfer, flow and sequence control, error detection and recovery, notification of unrecoverable errors, user identity confidentiality, and ciphering of user and signaling data.</Section>
            <Section>1.3 GMM - GPRS Mobility Management</Section>
            <Section>The GMM entity provides procedures for the mobility of the MS, such as informing the network of its present location, and user identity confidentiality. It manages the GMM context (attach, detach, routing area updating), supports security functions such as authentication of user and MS, controls ciphering of data, and initiates the response to paging messages.</Section>
            <Section>1.4 SM - Session Management</Section>
            <Section>The main function of the session management (SM) is to support PDP context handling of the user terminal. Session Management activates, modifies and deletes the contexts for packet data protocols (PDP). Session Management services are provided at the SMREG-SAP and the SNSM-SAP for anonymous and non-anonymous access. The non-anonymous and anonymous access procedures for PDP context activation and PDP context deactivation are available at the SMREG-SAP. In addition there exists a PDP context modification for non-anonymous PDP contexts.</Section>
            <Section>1.5 SNDCP - Subnetwork Dependant Convergence Protocol</Section>
            <Section>SNDCP carries out all functions related to transfer of Network layer Protocol Data Units (N-PDUs) over GPRS in a transparent way. SNDCP helps to improve channel efficiency by means of compression techniques. The set of protocol entities above SNDCP consists of commonly used network protocols. They all use the same SNDCP entity, which then performs multiplexing of data coming from different sources to be sent using the service provided by the LLC layer.</Section>
            <Section>1.6 GACI - GPRS Application Control Interface</Section>
            <Section>The GACI is the GPRS extension of the ACI. It is specified in GSM 07.07 and 07.60. It is responsible for processing of the GPRS related AT Commands to setup, activate and deactivate the PDP context parameter. It also provides functionality for the interworking between GMM/SM/SNDCP and a packet oriented protocol like PPP.</Section>
            <Section>1.7 USART - Universal Synchronous Asynchronous Receiver Transmitter Driver</Section>
            <Section>The USART is a hardware component that facilitates a connection between the mobile station and terminal equipment (e.g. a PC). This interface uses some of the circuits described in V.24.</Section>
            <Section>The data exchange provided by this unit is serial and asynchronous (synchronous communication is not in the scope of this document). A driver that uses interrupts to manage a circular buffer for the sending and receiving direction is necessary in order to use this component in the GPRS. The driver has to be able to perform flow control.</Section>
            <Section>1.8 TOM - Tunnelling of Messages</Section>
            <Section>The TOM entity is present if and only if HS136 is supported (the feature flag FF_HS136 is enabled).</Section>
            <Section>The main function of TOM is to tunnel non-GSM signalling messages between the MS and the SGSN. The only non-GSM signalling which is currently supported by TOM is for the EGPRS-136 system (according to TIA/EIA-136-376). Data transfer in both uplink and downlink direction is possible. Two different priorities (high, low) of signalling data transfer are supported. TOM uses the unacknowledged mode of LLC and the acknowledged mode of GRR (RLC/MAC).</Section>
        </Description>
        <DocHistory>
            <DocVersion Number="001" Year="99"/>
            <Date Day="13" Month="4" Year="1999"/>
            <Author>Ilker</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Demirel Initial</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="002" Year="99"/>
            <Date Day="10" Month="5" Year="1999"/>
            <Author>Stefan</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Liepolt consider s921 v0.4 and s921bis v0.2</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="003" Year="99"/>
            <Date Day="11" Month="6" Year="1999"/>
            <Author>Ilker</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Demirel New document header added</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="004" Year="99"/>
            <Date Day="12" Month="7" Year="1999"/>
            <Author>Stefan</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Liepolt consider s921 v0.6 and s921bis v0.5</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="005" Year="99"/>
            <Date Day="14" Month="10" Year="1999"/>
            <Author>DB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Removed dummy parameter.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="006" Year="99"/>
            <Date Day="10" Month="1" Year="2000"/>
            <Author>SL</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>consider s921 v0.8</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="007" Year="99"/>
            <Date Day="10" Month="3" Year="2000"/>
            <Author>SL</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>update according to S2</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="008" Year="99"/>
            <Date Day="1" Month="8" Year="2000"/>
            <Author>PZ</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>update to S921 v1.3 and S921bis v1.1</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="009" Year="00"/>
            <Date Day="21" Month="11" Year="2000"/>
            <Author>SAB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Updates for interference measurements added</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="010" Year="00"/>
            <Date Day="30" Month="11" Year="2000"/>
            <Author>SAB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Change L2_PCHANNEL_PAPCH to L2_PCHANNEL_PACCH</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="011" Year="03"/>
            <Date Day="13" Month="1" Year="2003"/>
            <Author>SAB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add references</Comment>
        </DocHistory>
        <DocRef>
            <RefId>[1]</RefId>
            <RefTitle>GSM 05.02 version 8.0.0 Release 1999Digital cellular telecommunications system (Phase 2+);Multiplexing and multiple access on the radio path</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[2]</RefId>
            <RefTitle>GSM 04.60 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);General Packet Radio Service (GPRS);Mobile Station (MS) - Base Station System (BSS) interface;Radio Link Control/ Medium Access Control (RLC/MAC) protocol</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[3]</RefId>
            <RefTitle>GSM 04.08 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);Mobile radio interface layer 3 specification</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[4]</RefId>
            <RefTitle>GSM 03.64 version 6.1.0 Release 1997Digital cellular telecommunications system (Phase 2+);General Packet Radio Service (GPRS);Overall description of the GPRS radio interface; Stage 2</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[5]</RefId>
            <RefTitle>GSM 03.60 version 6.3.1 Release 1997Digital cellular telecommunications system (Phase 2+);General Packet Radio Service (GPRS);Service description; Stage 2</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[6]</RefId>
            <RefTitle>GSM 04.07 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);Mobile radio interface signalling layer 3; General aspects</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[7]</RefId>
            <RefTitle>GSM 04.64 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);General Packet Radio Service (GPRS);Mobile Station - Serving GPRS Support Node (MS-SGSN)Logical Link Control (LLC) layer specification</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[8]</RefId>
            <RefTitle>GSM 05.08 version 6.4.0 Release 1997Digital cellular telecommunications system (Phase 2+);Radio subsystem link control</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[9]</RefId>
            <RefTitle>GSM 05.10 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);Radio subsystem synchronization</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[10]</RefId>
            <RefTitle>GSM 03.20 TS 100 929: July 1998 (GSM 03.20 version 6.0.1)Security related network functions, ETSI</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[11]</RefId>
            <RefTitle>Draft GSM 03.22: August 1998 (GSM 03.22 version 6.1.0)Functions related to Mobile Station (MS) in idle mode and group receive mode, ETSI</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[12]</RefId>
            <RefTitle>GSM 04.65 V6.3.0: Subnetwork Dependant Convergence Protocol ETSI, March 1999</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[13]</RefId>
            <RefTitle>ITU-T V42bis ITU-T, Recommendation V.42 bis 1990</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[14]</RefId>
            <RefTitle>GSM 09.60 GPRS Tunneling Protocol (GTP) across the Gn and Gp Interface</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[15]</RefId>
            <RefTitle>RFC 1661 IETF STD 51 July 1994The Point-to-Point Protocol (PPP)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[16]</RefId>
            <RefTitle>RFC 1662 IETF STD 51 July 1994PPP in HDLC-like Framing</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[17]</RefId>
            <RefTitle>RFC 1570 January 1994PPP LCP Extensions</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[18]</RefId>
            <RefTitle>RFC 1989 August 1996PPP Link Quality Monitoring</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[19]</RefId>
            <RefTitle>RFC 1332 May 1992The PPP Internet Protocol Control Protocol (IPCP)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[20]</RefId>
            <RefTitle>RFC 1877 December 1995PPP IPCP Extensions for Name Server Addresses</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[21]</RefId>
            <RefTitle>RFC 2153 May 1997PPP Vendor Extensions</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[22]</RefId>
            <RefTitle>RFC 1334 October 1992PPP Authentication Protocols (for Password Authentication Protocol only)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[23]</RefId>
            <RefTitle>RFC 1994 August 1996PPP Challenge Handshake Authentication Protocol (CHAP)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[24]</RefId>
            <RefTitle>TIA/EIA-136-370Packet-Data Services - Enhanced General Packet Radio for TIA/EIA-136 (EGPRS-136) - Overview, Telecommunications Industry Association</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[25]</RefId>
            <RefTitle>TIA/EIA-136-376Packet-Data Services - EGPRS-136 Mobility Management, Telecommunications Industry Association</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[26]</RefId>
            <RefTitle>TIA/EIA-136-972Packet-Data Services - Stage 2 Description, Telecommunications Industry Association</RefTitle>
        </DocRef>
    </DocInfoSection>
    <ConstantsSection>
        <Description>
            <Section>This section contains all constants that are defined for the MPHP SAP</Section>
        </Description>
        <Constant>
            <Alias>MAX_L2_FRAME_SIZE</Alias>
            <Value ValueType="DEC">23</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_RELATIVE_POS</Alias>
            <Value ValueType="DEC">20</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MPHP_NUMC_MA</Alias>
            <Value ValueType="DEC">64</Value>
            <Comment>Maximum number of carriers in the mobile allocation list handled by L1.</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_USF_TABLE</Alias>
            <Value ValueType="DEC">8</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_ALLOC_BITMAP</Alias>
            <Value ValueType="DEC">127</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MPHP_NUMC_BA_GPRS_SC</Alias>
            <Value ValueType="DEC">33</Value>
            <Comment>Maximum number of carriers in the BA(GPRS) list plus the serving cell carrier handled by L1.</Comment>
        </Constant>
        <History>
            <Date Day="13" Month="4" Year="1999"/>
            <Author>ID</Author>
            <Comment>Maximum array value for relative position is added</Comment>
        </History>
        <History>
            <Date Day="14" Month="4" Year="1999"/>
            <Author>ID</Author>
            <Comment>Maximum entries for mobile allocation list is added</Comment>
        </History>
        <History>
            <Date Day="14" Month="4" Year="1999"/>
            <Author>ID</Author>
            <Comment>Maximum size of PSI data field is added</Comment>
        </History>
        <History>
            <Date Day="5" Month="5" Year="1999"/>
            <Author>SL</Author>
            <Comment>some defines added</Comment>
        </History>
        <History>
            <Date Day="1" Month="8" Year="2000"/>
            <Author>PZ</Author>
            <Comment>cleanup and rename</Comment>
        </History>
        <History>
            <Date Day="16" Month="1" Year="2001"/>
            <Author>LEP</Author>
            <Comment>consider S921_bis V1.4</Comment>
        </History>
        <History>
            <Date Day="2" Month="4" Year="2001"/>
            <Author>SAB</Author>
            <Comment>Constant CARRIER_LIST_MAX_INC_SC removed, constant CARRIER_LIST_MAX_INC_SC_NEW renamed by MPHP_NUMC_BA_GPRS_SC, constant CARRIER_LIST_MAX_EXC_SC renamed by MPHP_NUMC_MA</Comment>
        </History>
    </ConstantsSection>
    <PrimitivesSection PrimIDType="BIT16" SAPid="2">
        <Description>
            <Section>This section contains all primitives that are defined for the MPHP SAP</Section>
        </Description>
        <Primitive>
            <Description>
                <Section>The MPHP_SCELL_PBCCH_REQ is used to read selected blocks of packet system information broadcast on the control channel PBCCH of the serving cell.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_SCELL_PBCCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="28"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>psi_nr</Name>
                </ItemLink>
                <Comment>PSI number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>bs_pbcch_blks</Name>
                </ItemLink>
                <Comment>Number of PBCCH blocks</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>pb</Name>
                </ItemLink>
                <Comment>Power reduction value</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>psi1_rep_period</Name>
                </ItemLink>
                <Comment>Occurrence of PSI1</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>relative_pos_array</Name>
                </ItemLink>
                <Control>[MAX_RELATIVE_POS]</Control>
                <Comment>Position of other PSIs</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_ch_des</Name>
                </ItemLink>
                <Comment>Packet Channel Description</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_freq_list</Name>
                </ItemLink>
                <Comment>Mobile allocation</Comment>
            </PrimItem>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.6</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.8 (change sequence of tn,tsc)</Comment>
            </History>
            <History>
                <Date Day="26" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>change usage of structures</Comment>
            </History>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>consider S921 v1.3 (pb added)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHP_DATA_IND is used to indicate data to GPRS RR (GRR).</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_DATA_IND</Name>
                <PrimID Direction="UPLINK" Number="40"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>Radio frequency; belongs to BCCH !! not to any GPRS channel</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>l2_channel</Name>
                </ItemLink>
                <Comment>Layer2 channel</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>error_flag</Name>
                </ItemLink>
                <Comment>Error flag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>l2_frame</Name>
                </ItemLink>
                <Control>[MAX_L2_FRAME_SIZE]</Control>
                <Comment>Decoded data</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>relative_pos</Name>
                </ItemLink>
                <Comment>Relative position</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>pccch_lev</Name>
                </ItemLink>
                <Comment>PCCCH_LEV</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>fn</Name>
                </ItemLink>
                <Comment>Full frame number</Comment>
            </PrimItem>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.6</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This is a trigger which stops the serving cell PBCCH reading process.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_SCELL_PBCCH_STOP_REQ</Name>
                <PrimID Direction="UPLINK" Number="29"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This is a trigger which confirms the stop request.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_SCELL_PBCCH_STOP_CON</Name>
                <PrimID Direction="UPLINK" Number="30"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MPHP_START_PCCCH_REQ is used to start and specify the reading process of the PCCCH in intention to receive PPCH blocks.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_START_PCCCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="25"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>imsi_mod</Name>
                </ItemLink>
                <Comment>IMSImod</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>kcn</Name>
                </ItemLink>
                <Comment>KCN</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>split_pg_cycle</Name>
                </ItemLink>
                <Comment>SPLIT_PG_CYCLE</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>bs_pag_blks_res</Name>
                </ItemLink>
                <Comment>BS_PAG_BLKS_RES</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>bs_pbcch_blks</Name>
                </ItemLink>
                <Comment>BS_PBCCH_BLKS</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>pb</Name>
                </ItemLink>
                <Comment>Power reduction value</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <Comment>Page mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_ch_des</Name>
                </ItemLink>
                <Comment>Packet Channel Description</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_freq_list</Name>
                </ItemLink>
                <Comment>Mobile allocation</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.6</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.8 (change sequence of tn,tsc)</Comment>
            </History>
            <History>
                <Date Day="26" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>change usage of structures</Comment>
            </History>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>consider S921 v1.3 (pb added)</Comment>
            </History>
            <History>
                <Date Day="4" Month="7" Year="2001"/>
                <Author>ID</Author>
                <Comment>remove PC_MEAS_CHAN (S921 v1.7)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is a trigger request without parameter in intention to stop the PCCCH reading process.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_STOP_PCCCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="26"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is a trigger request without parameter. It confirms the stop request.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_STOP_PCCCH_CON</Name>
                <PrimID Direction="UPLINK" Number="27"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message configures and start (or update) power monitoring on frequency list. It's sent to L1 for a periodic measurement processing.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_CR_MEAS_REQ</Name>
                <PrimID Direction="UPLINK" Number="31"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>nb_carrier</Name>
                </ItemLink>
                <Comment>Number of neighbour cell carrier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>carrier_list</Name>
                </ItemLink>
                <Control>[MPHP_NUMC_BA_GPRS_SC]</Control>
                <Comment>List of carrier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>list_id</Name>
                </ItemLink>
                <Comment>List identifier</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHP_CR_MEAS_IND reports a specific number of measurements.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_CR_MEAS_IND</Name>
                <PrimID Direction="UPLINK" Number="41"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>nmeas</Name>
                </ItemLink>
                <Comment>Number of measurements reported</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_ncell_meas</Name>
                </ItemLink>
                <Control>[MPHP_NUMC_BA_GPRS_SC]</Control>
                <Comment>NCELL Measurements</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>list_id</Name>
                </ItemLink>
                <Comment>List identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>reporting_period</Name>
                </ItemLink>
                <Comment>Reporting period</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.6</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.8</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This is a request message to stop the measurements.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_CR_MEAS_STOP_REQ</Name>
                <PrimID Direction="UPLINK" Number="32"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is a trigger request without parameter. It confirms the stop request.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_CR_MEAS_STOP_CON</Name>
                <PrimID Direction="UPLINK" Number="33"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message starts interference signal strength measurements on at least 2 contiguous frames (search frames and PTCCH frames of MFL52) per paging. This message is sent to L1 in order to performed 2 measures of 1 carrier on a specific Time slot Number. This is a one shot process, to 1 request is associated only 1report.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_INT_MEAS_REQ</Name>
                <PrimID Direction="UPLINK" Number="34"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_frequency_par</Name>
                </ItemLink>
                <Comment>Frequency parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>carrier_id</Name>
                </ItemLink>
                <Comment>Measurement Carrier Identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>ts_mask</Name>
                </ItemLink>
                <Comment>Timeslot number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>m_class</Name>
                </ItemLink>
                <Comment>Multislot class</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.6</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.8</Comment>
            </History>
            <History>
                <Date Day="11" Month="1" Year="2000"/>
                <Author>ID</Author>
                <Comment>arfcn removed from the sixth line</Comment>
            </History>
            <History>
                <Date Day="26" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>change usage of structures</Comment>
            </History>
            <History>
                <Date Day="2" Month="5" Year="2000"/>
                <Author>SL</Author>
                <Comment>update to PL 0.5 (ms_class added; freq_struct changed)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MPHP_IDLE_INT_MEAS_IND reports the result of co-channel interference measurement.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_INT_MEAS_IND</Name>
                <PrimID Direction="UPLINK" Number="42"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>int_meas_rxlev</Name>
                </ItemLink>
                <Control>[8]</Control>
                <Comment>Idle Int. Meas. Level</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>carrier_id</Name>
                </ItemLink>
                <Comment>Measurement carrier identifier</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is a trigger to stop co-channel interference measurement.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_INT_MEAS_STOP_REQ</Name>
                <PrimID Direction="UPLINK" Number="35"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is a trigger request without parameter. It confirms the stop request.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_INT_MEAS_STOP_CON</Name>
                <PrimID Direction="UPLINK" Number="36"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MPHP_NCELL_PBCCH_REQ starts a one shot process to read neighbour cells PBCCH.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_NCELL_PBCCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="37"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>bs_pbcch_blks</Name>
                </ItemLink>
                <Comment>Number of PBCCH blocks</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>pb</Name>
                </ItemLink>
                <Comment>PB</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>psi1_rep_period</Name>
                </ItemLink>
                <Comment>Occurrence of PSI1</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>relative_pos</Name>
                </ItemLink>
                <Comment>Relative position</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_ch_des</Name>
                </ItemLink>
                <Comment>Packet Channel Description</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_freq_list</Name>
                </ItemLink>
                <Comment>Mobile allocation list</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>bcch_carrier</Name>
                </ItemLink>
                <Comment>BCCH Carrier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>Frame number offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>time_alignment</Name>
                </ItemLink>
                <Comment>Time alignment</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.6</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.8</Comment>
            </History>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>consider S921 V1.3 (bcch_carrier added, ma_list changed)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This messages reports the requested PBCCH blocks.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_NCELL_PBCCH_IND</Name>
                <PrimID Direction="UPLINK" Number="44"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>Radio frequency</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>l2_channel</Name>
                </ItemLink>
                <Comment>Layer2 channel</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>error_flag</Name>
                </ItemLink>
                <Comment>Error flag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>l2_frame</Name>
                </ItemLink>
                <Control>[MAX_L2_FRAME_SIZE]</Control>
                <Comment>Decoded data</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>relative_pos</Name>
                </ItemLink>
                <Comment>Relative position</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>pccch_lev</Name>
                </ItemLink>
                <Comment>PCCCH_LEV</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>fn</Name>
                </ItemLink>
                <Comment>Full frame number</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.6</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_NCELL_PBCCH_STOP_REQ</Name>
                <PrimID Direction="UPLINK" Number="38"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is a trigger request without parameter. It confirms the stop request. todo_opc</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_NCELL_PBCCH_STOP_CON</Name>
                <PrimID Direction="UPLINK" Number="39"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is used to send a PRACH block.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_RA_REQ</Name>
                <PrimID Direction="UPLINK" Number="18"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>txpwr</Name>
                </ItemLink>
                <Comment>Transmit power</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>rand</Name>
                </ItemLink>
                <Comment>Delay</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>channel_request_data</Name>
                </ItemLink>
                <Comment>Channel request data</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>bs_prach_blks</Name>
                </ItemLink>
                <Comment>BS_PRACH_BLKS</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>burst_type</Name>
                </ItemLink>
                <Comment>Access burst type</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider s921 v0.6</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is generated by the PL every time it transmits the requested PRACH block.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_RA_CON</Name>
                <PrimID Direction="UPLINK" Number="19"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>fn</Name>
                </ItemLink>
                <Comment>Full frame number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>channel_request_data</Name>
                </ItemLink>
                <Comment>Channel request data</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is used to stop sending PRACH.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_RA_STOP_REQ</Name>
                <PrimID Direction="UPLINK" Number="20"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message confirms MPHP_RA_STOP_REQ.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_RA_STOP_CON</Name>
                <PrimID Direction="UPLINK" Number="21"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is send to send the polling response.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_POLLING_RESPONSE_REQ</Name>
                <PrimID Direction="UPLINK" Number="22"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>poll_resp_type</Name>
                </ItemLink>
                <Comment>Polling Response Type</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>poll_data</Name>
                </ItemLink>
                <Control>[MAX_L2_FRAME_SIZE+1]</Control>
                <Comment>polling request data</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>fn</Name>
                </ItemLink>
                <Comment>Full frame number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>ta_index</Name>
                </ItemLink>
                <Comment>timing advance index</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>txpwr</Name>
                </ItemLink>
                <Comment>Transmit power</Comment>
            </PrimItem>
            <History>
                <Date Day="13" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>Consider s921_0v9 (0v8 is not sufficient)</Comment>
            </History>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>type and name of channel request data changed</Comment>
            </History>
            <History>
                <Date Day="2" Month="5" Year="2000"/>
                <Author>SL</Author>
                <Comment>update to PL 0.5 (ta_index and txpwr added)</Comment>
            </History>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>consider S921 v1.3 (poll data length with constant)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This is the reporting message reporting refer to MPHP_POLLING_REQ.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_POLLING_IND</Name>
                <PrimID Direction="UPLINK" Number="23"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>fn</Name>
                </ItemLink>
                <Comment>Frame number</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MPHP_ASSIGNMENT_REQ is used to set a TBF in the PL.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_ASSIGNMENT_REQ</Name>
                <PrimID Direction="UPLINK" Number="6"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>assign_id</Name>
                </ItemLink>
                <Comment>Assignment ID</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>assign_cmd</Name>
                </ItemLink>
                <Comment>Assignment command</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>m_class</Name>
                </ItemLink>
                <Comment>Multislot class</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>if_meas_enable</Name>
                </ItemLink>
                <Comment>INTERF_MEAS_ENABLE</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>pc_meas_chan</Name>
                </ItemLink>
                <Comment>PC_MEAS_CHAN</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>burst_type</Name>
                </ItemLink>
                <Comment>Access burst type</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_timing_advance</Name>
                </ItemLink>
                <Comment>Packet timing advance</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_dl_power</Name>
                </ItemLink>
                <Comment>Downlink Power Control</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <Comment>Training sequence code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_frequency_par</Name>
                </ItemLink>
                <Comment>Frequency parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_tbf_start</Name>
                </ItemLink>
                <Comment>TBF starting time</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>mac_mode</Name>
                </ItemLink>
                <Comment>MAC Mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_dl_alloc</Name>
                </ItemLink>
                <Comment>Downlink resource allocation</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_ul_alloc</Name>
                </ItemLink>
                <Comment>Uplink resource allocation</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="2" Month="5" Year="2000"/>
                <Author>SL</Author>
                <Comment>update to PL 0.5 (assign_id and if_meas_enable  added)</Comment>
            </History>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>consider S921 v1.3 (p_dl_power added)</Comment>
            </History>
            <History>
                <Date Day="4" Month="7" Year="2001"/>
                <Author>ID</Author>
                <Comment>Add pc_meas_chan, access_burst_type (S921bis 1.6)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This is the trigger according to MPHP_ASSIGNMENT_REQ.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_ASSIGNMENT_CON</Name>
                <PrimID Direction="UPLINK" Number="7"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>assign_id</Name>
                </ItemLink>
                <Comment>Assignment ID</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
            <History>
                <Date Day="2" Month="5" Year="2000"/>
                <Author>SL</Author>
                <Comment>update to PL 0.5 (assign_id added)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The message is used to repeat a uplink fixed allocation.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_REPEAT_UL_FIXED_ALLOC_REQ</Name>
                <PrimID Direction="UPLINK" Number="10"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>repeat_alloc</Name>
                </ItemLink>
                <Comment>Repeat allocation</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>ts_override</Name>
                </ItemLink>
                <Comment>Timeslot override</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_tbf_start</Name>
                </ItemLink>
                <Comment>TBF starting time</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This is the confirm to MPHP_REPEAT_UL_FIXED_ALLOC_REQ.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_REPEAT_UL_FIXED_ALLOC_CON</Name>
                <PrimID Direction="UPLINK" Number="11"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is used to send a single block.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_SINGLE_BLOCK_REQ</Name>
                <PrimID Direction="UPLINK" Number="1"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>assign_id</Name>
                </ItemLink>
                <Comment>Assignment ID</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>purpose</Name>
                </ItemLink>
                <Comment>Single Block Purpose</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>pc_meas_chan</Name>
                </ItemLink>
                <Comment>PC_MEAS_CHAN</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>burst_type</Name>
                </ItemLink>
                <Comment>Access burst type</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_timing_advance</Name>
                </ItemLink>
                <Comment>Packet timing advance</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_dl_power</Name>
                </ItemLink>
                <Comment>Downlink Power Control</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <Comment>Training sequence code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_frequency_par</Name>
                </ItemLink>
                <Comment>Frequency parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_tbf_start</Name>
                </ItemLink>
                <Comment>TBF starting time</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <Comment>Timeslot number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>l2_frame</Name>
                </ItemLink>
                <Control>[MAX_L2_FRAME_SIZE]</Control>
                <Comment>Decoded data</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>consider S921 v1.3 (p_dl_power added)</Comment>
            </History>
            <History>
                <Date Day="4" Month="7" Year="2001"/>
                <Author>ID</Author>
                <Comment>add pc_meas_chan, burst_type (S921bis V1.6)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is a trigger request without parameter. It confirms the MPHP_SINGLE_BLOCK_REQ after sending the single block.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_SINGLE_BLOCK_CON</Name>
                <PrimID Direction="UPLINK" Number="2"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>assign_id</Name>
                </ItemLink>
                <Comment>Assignment ID</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>purpose</Name>
                </ItemLink>
                <Comment>Single Block Purpose</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>sb_status</Name>
                </ItemLink>
                <Comment>Single Block Status</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>dl_error</Name>
                </ItemLink>
                <Comment>Downlink Error Flag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>l2_frame</Name>
                </ItemLink>
                <Control>[MAX_L2_FRAME_SIZE]</Control>
                <Comment>Decoded data</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>removed dummy parameter.</Comment>
            </History>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>parameters added</Comment>
            </History>
            <History>
                <Date Day="2" Month="5" Year="2000"/>
                <Author>SL</Author>
                <Comment>update to PL 0.5(assign_id and dl_error added)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>Stop single block transfer</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_STOP_SINGLE_BLOCK_REQ</Name>
                <PrimID Direction="UPLINK" Number="3"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>Confirmation to stopping of single block transfer</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_STOP_SINGLE_BLOCK_CON</Name>
                <PrimID Direction="UPLINK" Number="4"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="23" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message releases an TBF. It is possible to release uplink TBF, downlink TBF or up- and downlink TBF.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_TBF_RELEASE_REQ</Name>
                <PrimID Direction="UPLINK" Number="8"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>tbf_type</Name>
                </ItemLink>
                <Comment>TBF Type</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>It confirms the MPHP_TBF_RELEASE_REQ.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_TBF_RELEASE_CON</Name>
                <PrimID Direction="UPLINK" Number="9"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>tbf_type</Name>
                </ItemLink>
                <Comment>TBF Type</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
            <History>
                <Date Day="6" Month="3" Year="2002"/>
                <Author>CAN</Author>
                <Comment>add tbf type  parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message informs the PL about the partly release(one or more slot) of the PDCH.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_PDCH_RELEASE_REQ</Name>
                <PrimID Direction="UPLINK" Number="12"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>assign_id</Name>
                </ItemLink>
                <Comment>Assignment ID</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>ts_mask</Name>
                </ItemLink>
                <Comment>Timeslots available</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="2" Month="5" Year="2000"/>
                <Author>SL</Author>
                <Comment>update to PL 0.5</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This is the trigger according to MPHP_PDCH_RELEASE_REQ.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_PDCH_RELEASE_CON</Name>
                <PrimID Direction="UPLINK" Number="13"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>assign_id</Name>
                </ItemLink>
                <Comment>Assignment ID</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
            <History>
                <Date Day="2" Month="5" Year="2000"/>
                <Author>SL</Author>
                <Comment>update to PL 0.5 (assign_id added)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message informs the PL about changing of timing advance parameter.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_TIMING_ADVANCE_REQ</Name>
                <PrimID Direction="UPLINK" Number="14"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>assign_id</Name>
                </ItemLink>
                <Comment>Assignment ID</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_timing_advance</Name>
                </ItemLink>
                <Comment>Packet timing advance</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>Consider S921_bis V1.1 (assign_id added)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is used to confirm MPHP_TIMING_ADVANCE_REQ.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_TIMING_ADVANCE_CON</Name>
                <PrimID Direction="UPLINK" Number="15"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>assign_id</Name>
                </ItemLink>
                <Comment>Assignment ID</Comment>
            </PrimItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
            <History>
                <Date Day="2" Month="5" Year="2000"/>
                <Author>SL</Author>
                <Comment>update to PL 0.5 (assign_id added)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message informs the PL about changing of power parameter for PSI-reading.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_UPDATE_PSI_PARAM_REQ</Name>
                <PrimID Direction="UPLINK" Number="16"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>pb</Name>
                </ItemLink>
                <Comment>Pb</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>burst_type</Name>
                </ItemLink>
                <Comment>Access burst type</Comment>
            </PrimItem>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="7" Year="2001"/>
                <Author>ID</Author>
                <Comment>Remove PC_MEAS_CHAN, add burst_type (S921bis Ver 1.6)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>This message is used to confirm MPHP_UPDATE_PSI_PARAM_REQ.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_UPDATE_PSI_PARAM_CON</Name>
                <PrimID Direction="UPLINK" Number="17"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>DB</Author>
                <Comment>Removed dummy parameter.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>In case of packet transfer mode this message is used to trigger the measurement for the cell reselection procedure.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_TCR_MEAS_REQ</Name>
                <PrimID Direction="UPLINK" Number="45"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>nb_carrier</Name>
                </ItemLink>
                <Comment>Number of neighbour cell carrier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>carrier_list</Name>
                </ItemLink>
                <Control>[MPHP_NUMC_BA_GPRS_SC]</Control>
                <Comment>List of carrier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>list_id</Name>
                </ItemLink>
                <Comment>List identifier</Comment>
            </PrimItem>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="3" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>Consider S921_bis V1.5 and MPHC.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>In case of packet transfer mode this message is used to send the result of MPHP_TCR_MEAS_REQ.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_TCR_MEAS_IND</Name>
                <PrimID Direction="UPLINK" Number="46"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>acc_level</Name>
                </ItemLink>
                <Control>[MPHP_NUMC_BA_GPRS_SC]</Control>
                <Comment>Power strength level N-Cell</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>acc_nbr</Name>
                </ItemLink>
                <Control>[MPHP_NUMC_BA_GPRS_SC]</Control>
                <Comment>Frequency Channel Number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>list_id</Name>
                </ItemLink>
                <Comment>List identifier</Comment>
            </PrimItem>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MPHP_TINT_MEAS_IND reports the result of co-channel interference measurement while in transfer mode.</Section>
            </Description>
            <PrimDef>
                <Name>MPHP_TINT_MEAS_IND</Name>
                <PrimID Direction="UPLINK" Number="43"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>int_meas_rxlev</Name>
                </ItemLink>
                <Control>[8]</Control>
                <Comment>Idle Int. Meas. Level</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>carrier_id</Name>
                </ItemLink>
                <Comment>Measurement carrier identifier</Comment>
            </PrimItem>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
    </PrimitivesSection>
    <PrimStructElementsSection>
        <Description>
            <Section>Parameters shall be part of the primitives described below and if applied the parameters shall contain the values specified here. These values are selected to correspond element values used in the air interface protocol.</Section>
        </Description>
        <PrimStructElem>
            <Description>
                <Section>This parameter specifies the arfcn list for mobile allocation (MA). This parameter is used in MPHP_SCELL_PBCCH_REQ, MPHP_DATA_IND, MPHP_START_PCCCH_REQ, MPHP_CR_MEAS_IND, MPHP_INT_MEAS_REQ, MPHP_NCELL_PBCCH_REQ, MPHP_NCELL_PBCCH_IND and also in the structure 'Frequency parameter'.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_freq_list</Name>
                <Comment>list of frequencies</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_rf_chan_cnt</Name>
                </ItemLink>
                <Comment>Number of channels</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_rf_chan_no</Name>
                </ItemLink>
                <Comment>Radio Frequency List</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>consider S921 V1.3 (converted this element to structure)</Comment>
            </History>
            <History>
                <Date Day="17" Month="1" Year="2001"/>
                <Author>LEP</Author>
                <Comment>consider S921 V1.5</Comment>
            </History>
            <History>
                <Date Day="3" Month="3" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>Consider S921_bis V1.5 and MPHC.</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>This parameter is used in MPHP_INT_MEAS_IND.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>int_meas_rxlev</Name>
                <Comment>Idle Int. Meas. Level</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>rx_lev</Name>
                </ItemLink>
                <Control>[2]</Control>
                <Comment>Downlink Control Timeslot</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>consider S921 V1.3 (changed to struct)</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The structure describes the timing advance and is used in MPHP_ASSIGNMENT_REQ, MPHP_REPEAT_UL_FIXED_ALLOC_REQ, MPHP_SINGLE_BLOCK_REQ and MPHP_TIMING_ADVANCE_REQ.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_timing_advance</Name>
                <Comment/>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>ta_value</Name>
                </ItemLink>
                <Comment>timing advance value</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>ta_index</Name>
                </ItemLink>
                <Comment>timing advance index</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <Comment>timing advance timeslot number</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>This structure describes frequency related values. This parameter is used in MPHP_ASSIGNMENT_REQ and MPHP_SINGLE_BLOCK_REQ.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_frequency_par</Name>
                <Comment/>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_chan_sel</Name>
                </ItemLink>
                <Comment>Channel Selection</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_freq_list</Name>
                </ItemLink>
                <Comment>Mobile Allocation</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="27" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>change usage of structure</Comment>
            </History>
            <History>
                <Date Day="3" Month="3" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>Consider S921_bis V1.5.</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>This parameter identifies the downlink TFI and the assigned slots. This parameter is used in MPHP_ASSIGNMENT_REQ.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_dl_alloc</Name>
                <Comment/>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>dl_tfi</Name>
                </ItemLink>
                <Comment>Downlink TFI</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>ts_mask</Name>
                </ItemLink>
                <Comment>Downlink Timeslot Allocation</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>This parameter is used in MPHP_ASSIGNMENT_REQ.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_ul_alloc</Name>
                <Comment/>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>ul_tfi</Name>
                </ItemLink>
                <Comment>Uplink TFI</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>ts_mask</Name>
                </ItemLink>
                <Comment>Uplink Timeslot Allocation</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_dynamic_alloc</Name>
                </ItemLink>
                <Comment>Dynamic Allocation</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_fixed_alloc</Name>
                </ItemLink>
                <Comment>Fixed Allocation</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>This parameter is used in MPHP_ASSIGNMENT_REQ.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_dynamic_alloc</Name>
                <Comment/>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>usf_table</Name>
                </ItemLink>
                <Control>[MAX_USF_TABLE]</Control>
                <Comment>USF Index Table</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>usf_gran</Name>
                </ItemLink>
                <Comment>USF granularity</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>This parameter is used in MPHP_ASSIGNMENT_REQ.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_fixed_alloc</Name>
                <Comment/>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>dl_ctrl_ts</Name>
                </ItemLink>
                <Comment>Downlink Control Timeslot</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>size_bitmap</Name>
                </ItemLink>
                <Comment>Allocation Bitmap Length</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>bitmap</Name>
                </ItemLink>
                <Control>[MAX_ALLOC_BITMAP]</Control>
                <Comment>Allocation Bitmap</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="1" Year="2003"/>
                <Author>SAB</Author>
                <Comment>Add references</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>This parameter is used in MPHP_ASSIGNMENT_REQ and MPHP_SINGLE_BLOCK_REQ.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_tbf_start</Name>
                <Comment/>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>tbf_start_present</Name>
                </ItemLink>
                <Comment>Starting time present</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>fn</Name>
                </ItemLink>
                <Comment>Full frame number</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_ncell_meas</Name>
                <Comment/>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>rxlev</Name>
                </ItemLink>
                <Comment>RX-Level</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="10" Month="1" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>consider S921 v1.3 (arfcn removed)</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_ch_des</Name>
                <Comment/>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_chan_sel</Name>
                </ItemLink>
                <Comment>Channel Selection</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <Comment>Timeslot number</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <Comment>Training sequence code</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="26" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_chan_sel</Name>
                <Comment/>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>hopping</Name>
                </ItemLink>
                <Comment>Hopping flag</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_rf_ch</Name>
                </ItemLink>
                <Comment>Channel Selection Choice</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="26" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>This definition is in TI-Documents an union. The 2 byte of this element are either arfcn or mobile allocation offset(maio) and and hopping sequence nummer(hsn). This struct is used in .Frequency parameter and Channel Selection.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_rf_ch</Name>
                <Comment/>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>Absolute RF</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="26" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_dl_power</Name>
                <Comment/>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p0</Name>
                </ItemLink>
                <Comment>P0</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>bts_pwr_ctl_mode</Name>
                </ItemLink>
                <Comment>BTS_PWR_CTL_MODE</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>pr_mode</Name>
                </ItemLink>
                <Comment>PR_MODE</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>p_rf_chan_no</Name>
                <Comment>Frequency list</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphp</DocName>
                    <Name>p_radio_freq</Name>
                </ItemLink>
                <Control>[MPHP_NUMC_MA]</Control>
                <Comment>Radio Frequency List</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="16" Month="1" Year="2001"/>
                <Author>LEP</Author>
                <Comment>Consider S921_bis V1.5.</Comment>
            </History>
            <History>
                <Date Day="3" Month="3" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>Resolve naming conflict with MPHC.</Comment>
            </History>
        </PrimStructElem>
    </PrimStructElementsSection>
    <PrimBasicElementsSection>
        <Description>
            <Section>Parameters shall be part of the primitives described below and if applied the parameters shall contain the values specified here. These values are selected to correspond element values used in the air interface protocol.</Section>
        </Description>
        <PrimBasicElem>
            <Description>
                <Section>The parameter specifies the number of PSI to read. This parameter is used in MPHP_SCELL_PBCCH_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>psi_nr</Name>
                <Type>U8</Type>
                <Comment>Specifies the number of PSI to read</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_psi_nr</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines the number of PBCCH blocks per multiframe. This parameter is used in MPHP_SCELL_PBCCH_REQ, MPHP_START_PCCCH_REQ and MPHP_NCELL_PBCCH_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bs_pbcch_blks</Name>
                <Type>U8</Type>
                <Comment>Number of PBCCH per multiframe</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_bs_pbcch_blks</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines the occurrence of PSI1 message. This parameter is used in MPHP_SCELL_PBCCH_REQ and MPHP_NCELL_PBCCH_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>psi1_rep_period</Name>
                <Type>U8</Type>
                <Comment>psi1 repeat period</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_psi1_rep_period</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter specifies the position of the PSI messages other than the PSI1. The position is relative to the B0 when TC=0. This parameter is used in MPHP_SCELL_PBCCH_REQ and MPHP_NCELL_PBCCH_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>relative_pos_array</Name>
                <Type>U8</Type>
                <Comment>relative position to B0</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_relative_pos_array</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter indicates whether the hopping procedure is used or not. This parameter is used in MPHP_SCELL_PBCCH_REQ, MPHP_START_PCCCH_REQ, MPHP_INT_MEAS_REQ, MPHP_NCELL_PBCCH_REQ and also in the structure 'Frequency parameter'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>hopping</Name>
                <Type>U8</Type>
                <Comment>hopping indicator</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_hopping</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="31" Month="10" Year="2000"/>
                <Author>SAB</Author>
                <Comment>Updated for interference measurements</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter specifies absolute radio frequency channel number. This parameter is used in the signals MPHP_SCELL_PBCCH_REQ, MPHP_DATA_IND, MPHP_START_PCCCH_REQ, MPHP_CR_MEAS_IND, MPHP_INT_MEAS_IND, MPHP_NCELL_PBCCH_REQ, MPHP_NCELL_PBCCH_IND and also in the structure 'Frequency parameter'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>arfcn</Name>
                <Type>U16</Type>
                <Comment>channel number</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines the training sequence number. This parameter is used in MPHP_SCELL_PBCCH_REQ, MPHP_START_PCCCH_REQ, MPHP_NCELL_PBCCH_REQ, MPHP_ASSIGNMENT_REQ and MPHP_SINGLE_BLOCK_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tsc</Name>
                <Type>U8</Type>
                <Comment>training sequence number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_tsc</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Value added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter specifies the timeslot number. This parameter is used in MPHP_SCELL_PBCCH_REQ, MPHP_START_PCCCH_REQ and MPHP_SINGLE_BLOCK_REQ and also in the structure 'Packet timing advance'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tn</Name>
                <Type>U8</Type>
                <Comment>timeslot number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_tn</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines the layer 2 channel type. This parameter is used in MPHP_DATA_IND and MPHP_NCELL_PBCCH_IND.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>l2_channel</Name>
                <Type>U8</Type>
                <Comment>layer 2 channel type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_l2_channel</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>L2_PCHANNEL_NPBCCH  removed</Comment>
            </History>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>L2_PCHANNEL_PAPCH added</Comment>
            </History>
            <History>
                <Date Day="30" Month="11" Year="2000"/>
                <Author>SAB</Author>
                <Comment>Change L2_PCHANNEL_PAPCH to L2_PCHANNEL_PACCH</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines whether the data block is valid or not. This parameter is used in MPHP_DATA_IND and MPHP_NCELL_PBCCH_IND.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>error_flag</Name>
                <Type>U8</Type>
                <Comment>validity of the data block</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_error_flag</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter contains the decoded data. This parameter is used in MPHP_DATA_IND, MPHP_NCELL_PBCCH_IND and MPHP_SINGLE_BLOCK_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>l2_frame</Name>
                <Type>U8</Type>
                <Comment>decoded data</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter specifies the relative position where the PBCCH has been read. This parameter is used in MPHP_DATA_IND and MPHP_NCELL_PBCCH_IND.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>relative_pos</Name>
                <Type>U8</Type>
                <Comment>relative position</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter contains the full frame number of the read block. This parameter is used only for debug reasons. This parameter is used in MPHP_DATA_IND, MPHP_NCELL_PBCCH_IND, MPHP_RA_CO and MPHP_POLLING_IND.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>fn</Name>
                <Type>U32</Type>
                <Comment>full frame number</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter contains the IMSI number modulo1000 modulo (KC * N) = ((IMSI mod 1000) and is used for PAGING_GROUP computation. This parameter is used in MPHP_START_PCCCH_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>imsi_mod</Name>
                <Type>U16</Type>
                <Comment>see description</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is used to compute the PAGING_GROUP and is content of the signal MPHP_START_PCCCH_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>split_pg_cycle</Name>
                <Type>U16</Type>
                <Comment>SPLIT_PG_CYCLE</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This elements contains the number blocks that are reserved to the PAGCH, PDTCH and PACCH. This parameter is used in MPHP_START_PCCCH_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bs_pag_blks_res</Name>
                <Type>U8</Type>
                <Comment>BS_PAG_BLKS_RES</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_bs_pag_blks_res</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>In this parameter defines the type of paging. This parameter is used in 3.5 .</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>page_mode</Name>
                <Type>U8</Type>
                <Comment>PAGE_MODE</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_page_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field specifies the number of carrier to measure. This parameter is used in MPHP_CR_MEAS_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>nb_carrier</Name>
                <Type>U8</Type>
                <Comment>neighbour cell carrier</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_nb_carrier</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The list of carrier that are to measure. This parameter is used in MPHP_CR_MEAS_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>carrier_list</Name>
                <Type>U16</Type>
                <Comment>List of carrier</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field allows to identify the list. This parameter is used in MPHP_CR_MEAS_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>list_id</Name>
                <Type>U8</Type>
                <Comment>List identifier</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter specifies the number of measurements reported. This parameter is used in the signal MPHP_CR_MEAS_IND.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>nmeas</Name>
                <Type>U8</Type>
                <Comment>Number of measurements</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_nmeas</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Reporting period defines the time between two measurements which are reported to GRR. This parameter is used in MPHP_CR_MEAS_IND.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>reporting_period</Name>
                <Type>U16</Type>
                <Comment>Reporting period</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This is a number to identify a carrier and is used in MPHP_INT_MEAS_REQ, MPHP_INT_MEAS_IND.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>carrier_id</Name>
                <Type>U8</Type>
                <Comment>Measurement Carrier Identifier</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Difference in frames between the serving cell and the non serving cell. This parameter is used in MPHP_NCELL_PBCCH_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>fn_offset</Name>
                <Type>U32</Type>
                <Comment>Frame number offset</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_fn_offset</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines the difference in quarter of bits between the beginning of the serving cell frame and the non serving cell frame. This parameter is used in MPHP_NCELL_PBCCH_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>time_alignment</Name>
                <Type>U32</Type>
                <Comment>Time alignment</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_time_alignment</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>txpwr corresponds to the maximum TX power level that may used when accessing on a PCCCH. This parameter is used in MPHP_RA_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>txpwr</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This is the delay in RACH slots from previous, in the range [S, ...., S+T-1]. This parameter is used in MPHP_RA_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rand</Name>
                <Type>U16</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter contains the decoded data that will be transmitted. This parameter is used in MPHP_RA_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>channel_request_data</Name>
                <Type>U16</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter contains the decoded data that will be transmitted.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>poll_data</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The field BS_PRACH_BLKS indicates the number of blocks reserved in a fixed way to the PRACH. This parameter is used in MPHP_RA_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bs_prach_blks</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_bs_prach_blks</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Access burst type defines the length of data in the access burst, 8 Bit or 11 Bit. This parameter is used in MPHP_RA_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>burst_type</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_burst_type</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field specifies the command is contained in the message. This parameter is used in MPHP_ASSIGNMENT_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>assign_cmd</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_assign_cmd</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Here is the multislot class described, see also 05.02, annex B. This parameter is used in MPHP_ASSIGNMENT_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>m_class</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_m_class</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is used in MPHP_REPEAT_UL_FIXED_ALLOC_REQ .</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>repeat_alloc</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_repeat_alloc</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field indicates a timeslot allocation, where Bit 8 (MSB) indicates the status of slot 0, Bit 7 indicates the status of slot 1, etc. The value 1 means times slot is assigned, 0 is not assigned. This parameter is used in the signals MPHP_REPEAT_UL_FIXED_ALLOC_REQ, MPHP_INT_MEAS_REQ, MPHP_PDCH_RELEASE_REQ and the structures 'Downlink resource allocation', 'Uplink resource allocation'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ts_mask</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This information field indicates which the timeslots whose allocation should be overridden. The override applies for one repeated allocation. Bit 8 indicates the status of timeslot 0, bit 7 indicates the status of timeslot 1, etc. At least one timeslot must be assigned.</Section>
                <Section>0 The mobile shall use the ALLOCATION_BITMAP during the allocation to determine during</Section>
                <Section>which radio blocks it shall transmit.</Section>
                <Section>1 The mobile shall transmit on all uplink radio blocks during the allocation.</Section>
                <Section>This parameter is used in MPHP_REPEAT_UL_FIXED_ALLOC_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ts_override</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This message defines the purpose for a single block request. The purpose can be 'Single block transfer without TBF establishment (measurement report)' or 'Two phases access'. This parameter is used in MPHP_SINGLE_BLOCK_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>purpose</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_purpose</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>Values modified</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is used in the structure 'Packet timing advance' .</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ta_value</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_ta_value</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is used in the structure 'Packet timing advance'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ta_index</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_ta_index</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is used in the structure 'Uplink resource allocation'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ul_tfi</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_ul_tfi</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is used in the structure 'Downlink resource allocation'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dl_tfi</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_dl_tfi</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field specifies the which allocation type must be used. This parameter is used in the structure 'Uplink resource allocation'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>mac_mode</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_mac_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is used in the structure 'Dynamic allocation'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>usf_table</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is used in the structure 'Dynamic allocation'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>usf_gran</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_usf_gran</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is used in the structure 'Fixed allocation'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dl_ctrl_ts</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_dl_ctrl_ts</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field specifies the number of elements in the Allocation Bitmap. This parameter is used in the structure 'Fixed allocation'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>size_bitmap</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_size_bitmap</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This table contains the uplink allocation on a block period basis (for instance, ALLOCATION_BITMAP[10] is the allocation for the 10th block relative to the TBF Starting time), each byte corresponds to a bitmap timeslot allocation (MSB=TS0,..., LSB=TS7). When a bit is set to 1 the PDCH corresponding to that timeslot is allocated for the considered block. These timeslot allocations must be in line with the general TIMESLOT_ALLOCATION field content. This parameter is used in the structure 'Fixed allocation'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmap</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is used in the structure 'TBF starting time'.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tbf_start_present</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_tbf_start_present</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The Pb parameter is a power reduction value used by the BTS on PBCCH/PCCCH blocks (PBCCH and PCCH are considered transmitted with the same output power), relative to the output power used on BCCH. The value is pb*-2db i.e. pb = 7 means -14dB</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>pb</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The PC_MEAS_CHAN parameter indicates where the mobile station shall measure the received power level on the downlink for the purpose of the uplink power control.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>pc_meas_chan</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_pc_meas_chan</Name>
            </ValuesLink>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter indicates which TBF must be released.</Section>
                <Section>Release only the downlink TBF</Section>
                <Section>Release only the uplink TBF</Section>
                <Section>Release both uplink and downlink TBFs</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tbf_type</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_tbf_type</Name>
            </ValuesLink>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The pccch_lev encodes the power strength level measured on PCCCH.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>pccch_lev</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field encodes the parameter KC multiply by N as defined in GSM05.02</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>kcn</Name>
                <Type>U16</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="11" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Measure is performed on this Frequency Channel Number.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>acc_nbr</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>poll_resp_type</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_poll_resp_type</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is used in MPHP_INT_MEAS_IND.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>acc_level</Name>
                <Type>U16</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is for identifiy a MPHP_ASSIGNMENT_REQ or MPHP_SINGLE_BLOCK_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>assign_id</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is for identifiy a MPHP_ASSIGNMENT_REQ or MPHP_SINGLE_BLOCK_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>p0</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bts_pwr_ctl_mode</Name>
                <Type>U8</Type>
                <Comment>should be BOOL, but BOOL is not valid in SAP</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>pr_mode</Name>
                <Type>U8</Type>
                <Comment>should be BOOL, but BOOL is not valid in SAP</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>sb_status</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_sb_status</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="2" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="16" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add c-macro values</Comment>
            </History>
            <History>
                <Date Day="25" Month="7" Year="2003"/>
                <Author>ROZ</Author>
                <Comment>S921BIS has been changed</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>if_meas_enable</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphp</DocName>
                <Name>VAL_if_meas_enable</Name>
            </ValuesLink>
            <History>
                <Date Day="2" Month="5" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="1" Month="11" Year="2000"/>
                <Author>SAB</Author>
                <Comment>Updated for interference measurements</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dl_error</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="2" Month="5" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rx_lev</Name>
                <Type>U8</Type>
                <Comment/>
            </PrimBasicElemDef>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>p_rf_chan_cnt</Name>
                <Type>U16</Type>
                <Comment>Number of channels</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bcch_carrier</Name>
                <Type>U16</Type>
                <Comment>BCCH Carrier</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>_</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>p_radio_freq</Name>
                <Type>U16</Type>
                <Comment>Absolute Radio Frequency Number</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="1" Month="8" Year="2000"/>
                <Author>PZ</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
    </PrimBasicElementsSection>
    <ValuesSection>
        <Description>
            <Section>This section contains all sets of values that are defined for the MPHP SAP</Section>
        </Description>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_psi_nr</Name>
                <Comment>values for psi_nr</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>read all PSI</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>20</MaxValue>
                <Comment>specifies the relative position array</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bs_pbcch_blks</Name>
                <Comment>values for bs_pbcch_blks</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias/>
                <Comment>B0 is used for PBCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias/>
                <Comment>B0, B6 is used for PBCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10</Value>
                <Alias/>
                <Comment>B0, B6, B3 is used for PBCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9 is used for PBCCH</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_psi1_rep_period</Name>
                <Comment>values for psi1_rep_period</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>16</MaxValue>
                <Comment>PSI is repeated every 'value' multiframes</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_relative_pos_array</Name>
                <Comment>values for relative_pos_array</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>64</MaxValue>
                <Comment>index</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_hopping</Name>
                <Comment>values for hopping</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>static</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>hopping</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MPHP_INT_MEAS_STATIC</Alias>
                <Comment>static</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MPHP_INT_MEAS_HOPPING</Alias>
                <Comment>hopping</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias/>
                <Comment>static</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias/>
                <Comment>hopping</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tsc</Name>
                <Comment>values for tsc</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>see 05.02, Annex A</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tn</Name>
                <Comment>values for tn</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias/>
                <Comment>Value not present</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>timeslot number</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_l2_channel</Name>
                <Comment>values for l2_channel</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>L2_PCHANNEL_PCCCH</Alias>
                <Comment>PCCCH block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>L2_PCHANNEL_PBCCH</Alias>
                <Comment>PBCCH block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>L2_PCHANNEL_PPCH</Alias>
                <Comment>PPCH block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>L2_PCHANNEL_PEPCH</Alias>
                <Comment>PEPCH block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>L2_PCHANNEL_PACCH</Alias>
                <Comment>PACCH block</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_error_flag</Name>
                <Comment>values for error_flag</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>valid block info</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>invalid block info</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bs_pag_blks_res</Name>
                <Comment>values for bs_pag_blks_res</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>12</MaxValue>
                <Comment>number blocks for PAGCH, PDTCH and PACCH</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_page_mode</Name>
                <Comment>values for page_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PAGE_NORMAL</Alias>
                <Comment>normal paging</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PAGE_EXT</Alias>
                <Comment>extended paging</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PAGE_REORG</Alias>
                <Comment>paging reorganisation</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_nb_carrier</Name>
                <Comment>values for nb_carrier</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>65</MaxValue>
                <Comment>_</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_nmeas</Name>
                <Comment>values for nmeas</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>65</MaxValue>
                <Comment>_</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_fn_offset</Name>
                <Comment>values for fn_offset</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>2715647</MaxValue>
                <Comment>max. GSM frames -1</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_time_alignment</Name>
                <Comment>values for time_alignment</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>4999</MaxValue>
                <Comment>_</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bs_prach_blks</Name>
                <Comment>values for bs_prach_blks</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">0000</Value>
                <Alias/>
                <Comment>No block is reserved for PRACH (default)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0001</Value>
                <Alias/>
                <Comment>B0 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0010</Value>
                <Alias/>
                <Comment>B0, B6 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0011</Value>
                <Alias/>
                <Comment>B0, B6, B3 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0101</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0110</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0111</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7, B4 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1000</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7, B4, B10 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1001</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7, B4, B10, B2 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1010</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7, B4, B10, B2, B8 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1011</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7, B4, B10, B2, B8, B5 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7, B4, B10, B2, B8, B5, B11 is used for PRACH</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_burst_type</Name>
                <Comment>values for burst_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ACCESS_8_BIT</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ACCESS_11_BIT</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_assign_cmd</Name>
                <Comment>values for assign_cmd</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DL_ASSIGNMENT</Alias>
                <Comment>Downlink assignment</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>UL_ASSIGNMENT</Alias>
                <Comment>Uplink assignment</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>UL_DL_ASSIGNMENT</Alias>
                <Comment>Uplink and downlink assignment</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>UL_TP_ACCESS</Alias>
                <Comment>Uplink Two Phase Access</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_m_class</Name>
                <Comment>values for m_class</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>12</MaxValue>
                <Comment>Speech mode</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_repeat_alloc</Name>
                <Comment>values for repeat_alloc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>cancel any pending repeat allocation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>repeat the current fixed allocation when it ends</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_purpose</Name>
                <Comment>values for purpose</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SINGLE_BLOCK_TRANSFER_DL</Alias>
                <Comment>todo ??? reception?</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SINGLE_BLOCK_TRANSFER_UL</Alias>
                <Comment>i.e. measurement report</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>TWO_PHASE_ACESS</Alias>
                <Comment>two phases access</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ta_value</Name>
                <Comment>values for ta_value</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias/>
                <Comment>value not present</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>Speech mode</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ta_index</Name>
                <Comment>values for ta_index</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias/>
                <Comment>value not present</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>15</MaxValue>
                <Comment>_</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ul_tfi</Name>
                <Comment>values for ul_tfi</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>127</MaxValue>
                <Comment>_</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_dl_tfi</Name>
                <Comment>values for dl_tfi</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>31</MaxValue>
                <Comment>_</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_mac_mode</Name>
                <Comment>values for mac_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DA</Alias>
                <Comment>Dynamic allocation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EDA</Alias>
                <Comment>Extended Dynamic allocation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>FA</Alias>
                <Comment>Fixed allocation, not half duplex mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>FA_HD</Alias>
                <Comment>Fixed allocation, half duplex mode</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_usf_gran</Name>
                <Comment>values for usf_gran</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>the ms shall transmit one RLC/MAC-Block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>the ms shall transmit four consecutive RLC/MAC-Block</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_dl_ctrl_ts</Name>
                <Comment>values for dl_ctrl_ts</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>_</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_size_bitmap</Name>
                <Comment>values for size_bitmap</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>127</MaxValue>
                <Comment>_</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tbf_start_present</Name>
                <Comment>values for tbf_start_present</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>not present</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>present</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pc_meas_chan</Name>
                <Comment>values for pc_meas_chan</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MEAS_BCCH</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MEAS_PDCH</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tbf_type</Name>
                <Comment>values for tbf_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>REL_DL_TBF</Alias>
                <Comment>Release only the downlink TBF</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>REL_UL_TBF</Alias>
                <Comment>Release only the uplink TBF</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>REL_ALL_TBF</Alias>
                <Comment>Release both uplink and downlink TBFs</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_poll_resp_type</Name>
                <Comment>values for poll_resp_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>POLL_RESP_NB_CS1</Alias>
                <Comment>normal burst</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>POLL_RESP_AB_8_BIT</Alias>
                <Comment>access burst</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>POLL_RESP_AB_11_BIT</Alias>
                <Comment>access burst</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_sb_status</Name>
                <Comment>values for sb_status</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SB_STAT_OK</Alias>
                <Comment>In uplink, indicates that the single block was sent.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SB_STAT_DL_CRC_ERROR</Alias>
                <Comment>In downlink, indicates that the downlink single block was received with no CRC_ERROR.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SB_STAT_STIME_PASSED</Alias>
                <Comment>Starting time is passed. Single block uplink/downlink was not sent/received.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SB_STAT_TA_INVALID</Alias>
                <Comment>No valid timing advance. Single block was not sent.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SB_STAT_DL_OK</Alias>
                <Comment>Valid downlink single block received ( NO CRC_ERROR).</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_if_meas_enable</Name>
                <Comment>values for if_meas_enable</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MPHP_IM_DISABLED</Alias>
                <Comment>interference measurement processing disabled</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MPHP_IM_ENABLED</Alias>
                <Comment>interference measurement processing enabled</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
    </ValuesSection>
</SAP>
