<?xml version="1.0" encoding="UTF-8"?>
<!-- edited with SAPE SAP Editor -->
<AIM xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="aim.xsd">
    <DocInfoSection>
        <DocName DocType="AIM">rr</DocName>
        <DocNum Number="604" Project="6147"/>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">The Protocol Stacks are used to define the functionality of the GSM protocols for interfaces. The GSM specifications are normative when used to describe the functionality of interfaces, but the stacks and the subdivision of protocol layers does not imply or restrict any implementation.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">The protocol stack for GPRS consists of several entities. Each entity has one ore more service access points, over which the entity provides a service for the upper entity.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">The information units passed via the SAPs are called primitives and consists of an operation code and several parameters. See the Users Guide for details.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">The present Air-interface document (MSG) defines the radio interface between Mobile Station (MS) and network. It gives the general description of messages format of layer 3 for the Radio Resource (RR) management.</XHTMLElement>
            </DocElement>
        </Description>
        <DocHistory>
            <DocVersion Number="100" Year="97"/>
            <Date Day="7" Month="5" Year="1997"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Initial version.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="101" Year="97"/>
            <Date Day="29" Month="10" Year="1997"/>
            <Author>LE</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>rest octets</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="102" Year="97"/>
            <Date Day="3" Month="2" Year="1998"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>ARFCN in cell_desc</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="103" Year="97"/>
            <Date Day="11" Month="8" Year="1998"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Values for Screening Indicator added</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="104" Year="97"/>
            <Date Day="22" Month="6" Year="2001"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Corrected value description for CBCH, sect. 6.47</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="105" Year="97"/>
            <Date Day="17" Month="7" Year="2001"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Use Condat AG, PDCH Assignment</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="106" Year="97"/>
            <Date Day="13" Month="8" Year="2001"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>3-digit-MNC</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="107" Year="97"/>
            <Date Day="2" Month="11" Year="2001"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Correct ext_meas_cap in Classmark 3</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="108" Year="97"/>
            <Date Day="25" Month="3" Year="2002"/>
            <Author>MSB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Use of the new document format; Supplement the RF access capabilities for GSM 850 and PCS 1900 (R99)</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="109" Year="97"/>
            <Date Day="15" Month="4" Year="2002"/>
            <Author>MSB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>remove all definitions for classmark 2 and 3; use linked document rr_com.doc instead</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="110" Year="97"/>
            <Date Day="1" Month="8" Year="2002"/>
            <Author>OTH</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>NO_CODE reinsert - AMR functionality enabled.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="111" Year="97"/>
            <Date Day="11" Month="7" Year="2002"/>
            <Author>MPA</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Fix problems on Nortel BSS when hopping enabled. Add Spare if "Change Mark" is not present on "Packet Channel Description"</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="112" Year="97"/>
            <Date Day="20" Month="8" Year="2002"/>
            <Author>OTH</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Length description of APDU Data element updated.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="113" Year="97"/>
            <Date Day="11" Month="12" Year="2002"/>
            <Author>MSB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Manual merge from 133 to G23M. Update references, version numbers and content table.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="114" Year="97"/>
            <Date Day="19" Month="12" Year="2002"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>U_EXT_MEAS_REPORT is 'uplink'.</Comment>
        </DocHistory>
        <DocRef>
            <RefId>[1]</RefId>
            <RefTitle>Digital cellular telecommunications system (Phase 2+);Mobile radio interface layer 3 specification,  (GSM 4.08, December 1995, version 5.0.0)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[1a]</RefId>
            <RefTitle>GSM 2.81, Line Identification Supplementary Services - Stage 1ETS 300 514, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[2]</RefId>
            <RefTitle>GSM 2.82, Call Forwarding Supplementary Services - Stage 1ETS 300 515, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[3]</RefId>
            <RefTitle>GSM 2.83, Call Waiting and Call Hold Supplementary Services - Stage 1ETS 300 516, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[4]</RefId>
            <RefTitle>GSM 2.84, Multi Party Supplementary Services - Stage 1ETS 300 517, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[5]</RefId>
            <RefTitle>GSM 2.85, Closed User Group Supplementary Services - Stage 1ETS 300 518, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[6]</RefId>
            <RefTitle>GSM 2.86, Advice of Charge Supplementary Services - Stage 1ETS 300 519, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[7]</RefId>
            <RefTitle>GSM 2.88, Call Barring Supplementary Services - Stage 1ETS 300 520, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[8]</RefId>
            <RefTitle>GSM 3.14, Support of Dual Tone Multi Frequency Signalling via the GSM SystemETS 300 532, ETSI, April 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[9]</RefId>
            <RefTitle>GSM 3.40, Technical Realization of the Short Message Service Point-to-PointETS 300 536, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[10]</RefId>
            <RefTitle>GSM 3.41, Technical Realization of Short Message Service Cell BroadcastETS 300 537, ETSI, June 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[11]</RefId>
            <RefTitle>GSM 3.81, Line Identification Supplementary Services - Stage 2ETS 300 542, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[12]</RefId>
            <RefTitle>GSM 3.82, Call Forwarding Supplementary Services - Stage 2ETS 300 543, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[13]</RefId>
            <RefTitle>GSM 3.83, Call Waiting and Call Hold Supplementary Services - Stage 2ETS 300 544, ETSI, November 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[14]</RefId>
            <RefTitle>GSM 3.84, Multi Party Supplementary Services - Stage 2ETS 300 545, ETSI, November 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[15]</RefId>
            <RefTitle>GSM 3.85, Closed User Group Supplementary Services - Stage 2ETS 300 546, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[16]</RefId>
            <RefTitle>GSM 3.86, Advice of Charge Supplementary Services - Stage 2ETS 300 547, ETSI, March 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[17]</RefId>
            <RefTitle>GSM 3.88, Call Barring Supplementary Services - Stage 2ETS 300 548, ETSI, November 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[18]</RefId>
            <RefTitle>GSM 4.01, MS-BSS Interface General Aspects and PrinciplesETS 300 550, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[18a]</RefId>
            <RefTitle>GSM 4.03, MS-BSS Interface Channel Structures and Access CapabilitiesETS 300 552, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[19]</RefId>
            <RefTitle>GSM 4.05, Data Link Layer General AspectsETS 300 554, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[20]</RefId>
            <RefTitle>GSM 4.06, MS-BSS Interface Data Link Layer SpecificationETS 300 555, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[21]</RefId>
            <RefTitle>GSM 4.07, Mobile Radio Interface Signalling Layer 3 General AspectsETS 300 556, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[22]</RefId>
            <RefTitle>GSM 4.08, Mobile Radio Interface Layer 3 SpecificationETS 300 557, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[23]</RefId>
            <RefTitle>GSM 4.10, Mobile Radio Interface Layer 3 Supplementary Services Specification General AspectsETS 300 558, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[24]</RefId>
            <RefTitle>GSM 4.11, Point-to-Point Short Message Service Support on Mobile Radio InterfaceETS 300 559, ETSI, October 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[25]</RefId>
            <RefTitle>GSM 4.12, Short Message Service Cell Broadcast Support on Mobile Radio InterfaceETS 300 560, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[26]</RefId>
            <RefTitle>GSM 4.80, Mobile Radio Interface Supplementary Services Specification Formats and CodingETS 300 564, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[27]</RefId>
            <RefTitle>GSM 4.81, Line Identification Supplementary Services - Stage 3ETS 300 565, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[28]</RefId>
            <RefTitle>GSM 4.82, Call Forwarding Supplementary Services - Stage 3ETS 300 566, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[29]</RefId>
            <RefTitle>GSM 4.83, Call Waiting and Call Hold Supplementary Services - Stage 3ETS 300 567, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[30]</RefId>
            <RefTitle>GSM 4.84, Multi Party Supplementary Services - Stage 3ETS 300 568, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[31]</RefId>
            <RefTitle>GSM 4.85, Closed User Group Supplementary Services - Stage 3ETS 300 569, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[32]</RefId>
            <RefTitle>GSM 4.86, Advice of Charge Supplementary Services - Stage 3ETS 300 570, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[33]</RefId>
            <RefTitle>GSM 4.88, Call Barring Supplementary Services - Stage 3ETS 300 571, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[34]</RefId>
            <RefTitle>GSM 5.01, Physical Layer on the Radio Path General DescriptionETS 300 573, ETSI, October 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[35]</RefId>
            <RefTitle>GSM 5.02, Multiplexing and Multiple Access on the Radio PathETS 300 574, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[36]</RefId>
            <RefTitle>GSM 5.08, Radio Sub-system Link ControlETS 300 578, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[37]</RefId>
            <RefTitle>GSM 5.10, Radio Sub-system SynchronisationETS 300 579, ETSI, October 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[38]</RefId>
            <RefTitle>Service Access Point MMREG,  6147.100.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[39]</RefId>
            <RefTitle>Service Access Point MNCC,  6147.101.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[40]</RefId>
            <RefTitle>Service Access Point MNSS,  6147.102.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[41]</RefId>
            <RefTitle>Service Access Point MNSMS,  6147.103.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[42]</RefId>
            <RefTitle>Service Access Point MMCC,  6147.104.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[43]</RefId>
            <RefTitle>Service Access Point MMSS,  6147.105.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[44]</RefId>
            <RefTitle>Service Access Point MMSMS,  6147.106.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[45]</RefId>
            <RefTitle>Service Access Point RR,  6147.107.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[46]</RefId>
            <RefTitle>Service Access Point SIM,  6147.108.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[47]</RefId>
            <RefTitle>Service Access Point MPH,  6147.109.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[48]</RefId>
            <RefTitle>Service Access Point DL,  6147.110.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[49]</RefId>
            <RefTitle>Service Access Point MDL,  6147.111.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[50]</RefId>
            <RefTitle>Service Access Point PH,  6147.112.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[51]</RefId>
            <RefTitle>Service Access Point MMI,  6147.113.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[52]</RefId>
            <RefTitle>Message Sequence Charts CC,  6147.200.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[53]</RefId>
            <RefTitle>Message Sequence Charts SS,  6147.201.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[54]</RefId>
            <RefTitle>Message Sequence Charts SMS,  6147.202.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[55]</RefId>
            <RefTitle>Message Sequence Charts MM,  6147.203.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[56]</RefId>
            <RefTitle>Message Sequence Charts RR,  6147.204.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[57]</RefId>
            <RefTitle>Message Sequence Charts DL,  6147.205.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[58]</RefId>
            <RefTitle>Users Guide,    6147.300.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[59]</RefId>
            <RefTitle>Test Specification CC,   6147.400.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[60]</RefId>
            <RefTitle>Test Specification SS,   6147.401.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[61]</RefId>
            <RefTitle>Test Specification SMS,  6147.402.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[62]</RefId>
            <RefTitle>Test Specification MM,  6147.403.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[63]</RefId>
            <RefTitle>Test Specification RR,   6147.404.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[64]</RefId>
            <RefTitle>Test Specification DL,   6147.405.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[65]</RefId>
            <RefTitle>Test Specification CCD,  6147.406.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[66]</RefId>
            <RefTitle>SDL Specification CC,   6147.500.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[67]</RefId>
            <RefTitle>SDL Specification SS,   6147.501.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[68]</RefId>
            <RefTitle>SDL Specification SMS,  6147.502.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[69]</RefId>
            <RefTitle>SDL Specification MM,  6147.503.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[70]</RefId>
            <RefTitle>SDL Specification RR,   6147.504.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[71]</RefId>
            <RefTitle>SDL Specification DL,   6147.505.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[72]</RefId>
            <RefTitle>Message Specification CC,  6147.600.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[73]</RefId>
            <RefTitle>Message Specification SS,  6147.601.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[74]</RefId>
            <RefTitle>Message Specification SMS,  6147.602.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[75]</RefId>
            <RefTitle>Message Specification MM,  6147.603.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[76]</RefId>
            <RefTitle>Message Specification RR,  6147.604.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[77]</RefId>
            <RefTitle>Message Specification DL,  6147.605.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[78]</RefId>
            <RefTitle>Technical Documentation CC,  6147.700.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[79]</RefId>
            <RefTitle>Technical Documentation SS,  6147.701.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[80]</RefId>
            <RefTitle>Technical Documentation SMS,  6147.702.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[81]</RefId>
            <RefTitle>Technical Documentation MM,  6147.703.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[82]</RefId>
            <RefTitle>Technical Documentation RR,  6147.704.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[83]</RefId>
            <RefTitle>Technical Documentation DL,  6147.705.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[84]</RefId>
            <RefTitle>Technical Documentation CCD,  6147.706.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[3GPP_TS04.18]</RefId>
            <RefTitle>3GPP TS 04.18 V8.12.0 (2001-12)3rd Generation Partnership Project; Technical Specification Group GSM EDGE Radio Access Network; Mobile radio interface layer 3 specification, Radio Resource Control Protocol (Release 1999)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[MSG_RR_COM]</RefId>
            <RefTitle>RR_COM, Common Air Interface Message Specification, 6147.604.97.001, Condat AG</RefTitle>
        </DocRef>
    </DocInfoSection>
    <ConstantsSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">2 Constants</XHTMLElement>
            </DocElement>
        </Description>
        <Constant>
            <Alias>L3MAX_ACK</Alias>
            <Value ValueType="DEC">251</Value>
            <Comment>GSM 4.06, section 5.8.5</Comment>
        </Constant>
        <Constant>
            <Alias>L3MAX</Alias>
            <Value ValueType="DEC">251</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_APDU_DATA</Alias>
            <Value ValueType="DEC">248</Value>
            <Comment>(L3MAX - (4*1/2 +1)) 3GPP 04.18 9.1.53</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_ARFCN</Alias>
            <Value ValueType="DEC">20</Value>
            <Comment>(L3MAX_ACK-3-3) * 8 / (10 + 1) =178</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_ARFCNI</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_GR_C_INFO</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_ITP</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_LSA_ID</Alias>
            <Value ValueType="DEC">2</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_POS</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_RANGE</Alias>
            <Value ValueType="DEC">10</Value>
            <Comment>(L3MAX_ACK-3-3) * 8 / (2 * 10 + 1)=93</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_RFL</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>N_MAX_RANGE</Alias>
            <Value ValueType="DEC">30</Value>
            <Comment>(L3MAX_ACK-3-3) * 8 / (2 * 10) = 98</Comment>
        </Constant>
        <Constant>
            <Alias>N_CELL_MRES</Alias>
            <Value ValueType="DEC">6</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>N_FREQ_SHORT_LIST</Alias>
            <Value ValueType="DEC">9</Value>
            <Comment>sizeof(IE) - sizeof(IEI)</Comment>
        </Constant>
        <Constant>
            <Alias>N_FREQ_SKIP</Alias>
            <Value ValueType="DEC">16</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>N_MAX_FREQ_LIST</Alias>
            <Value ValueType="DEC">250</Value>
            <Comment>L3MAX - sizeof(IEI)</Comment>
        </Constant>
        <Constant>
            <Alias>N_MOB_ALLOC</Alias>
            <Value ValueType="DEC">8</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>NCELL_DESC_BIT_LEN</Alias>
            <Value ValueType="DEC">128</Value>
            <Comment>16 bytes BA list</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_ACCESS_TT</Alias>
            <Value ValueType="DEC">4</Value>
            <Comment>Assumed max number of access type technologies</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_FDD</Alias>
            <Value ValueType="DEC">131</Value>
            <Comment>(L3MAX_ACK-3-1-1)*8/(14+1) = 131,2</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_TDD</Alias>
            <Value ValueType="DEC">131</Value>
            <Comment>(L3MAX_ACK-3-1-1)*8/(14+1) = 131,2</Comment>
        </Constant>
        <History>
            <Date Day="7" Month="5" Year="1997"/>
            <Author>VK</Author>
            <Comment>Initial</Comment>
        </History>
        <History>
            <Date Day="5" Month="4" Year="2000"/>
            <Author>LG</Author>
            <Comment>added MAX_ARFCN, MAX_ARFCNI, MAX_CR_C_INFO, MAXITP, MAX_LSA_ID, MAX_POS, MAX_RANGE, MAX_RFL, changed value for N_MAX_RANGE</Comment>
        </History>
        <History>
            <Date Day="19" Month="7" Year="2002"/>
            <Author>OTH</Author>
            <Comment>MAX_APDU_DATA - max length of the APDU data field.</Comment>
        </History>
        <History>
            <Date Day="28" Month="03" Year="2006"/>
            <Author>xparapgu</Author>
            <Comment>Added MAX_ACCESS_TT</Comment>
        </History>
    </ConstantsSection>
    <MessagesSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all messages that are defined for the RR AIM</XHTMLElement>
            </DocElement>
        </Description>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH from the mobile station to the network to indicate that the mobile station has established the main signaling link successfully.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.3</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>b_applic_info</Name>
                <MsgID Direction="BOTH" IDType="BIN">00111000</MsgID>
                <Comment>Application Information</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>apdu_id</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.48</SpecRef>
                <Comment>APDU ID</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>apdu_flags</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.49</SpecRef>
                <Comment>APDU Flags</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>apdu_data</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.2.50</SpecRef>
                <Comment>APDU Data</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="7" Year="2002"/>
                <Author>OTH</Author>
                <Comment>Initial - add Application Information APDU for LCS</Comment>
            </History>
            <History>
                <Date Day="16" Month="10" Year="2002"/>
                <Author>VK</Author>
                <Comment>rename d_applic_info to b_applic_info</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the network to the mobile station to allocate an additional dedicated channel while keeping the previously allocated channels.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.1</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_add_assign</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00111011</MsgID>
                <Comment>Additional assignment</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_alloc</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">72</ItemTag>
                <SpecRef>10.5.2.21</SpecRef>
                <Comment>Mobile Allocation</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>start_time</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.2.38</SpecRef>
                <Comment>Starting Time</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the network to the mobile station to change the channel configuration to another independent dedicated channel configuration, when no timing adjustment is needed.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.2</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_assign_cmd</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00101110</MsgID>
                <Comment>Assignment command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Description of the First Channel, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pow_cmd</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.28</SpecRef>
                <Comment>Power Command</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_list_after</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <SpecRef>10.5.2.13</SpecRef>
                <Comment>Frequency List, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_chan_desc</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">62</ItemTag>
                <SpecRef>10.5.2.1b</SpecRef>
                <Comment>Cell Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>multislot_alloc</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">10</ItemTag>
                <SpecRef>10.5.2.21b</SpecRef>
                <Comment>Multislot Configuration</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">63</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 1st  Channel</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode2</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">11</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 2nd  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode3</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">13</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 3rd  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode4</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">14</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 4th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode5</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">15</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 5th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode6</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">16</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 6th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode7</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">17</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 7th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode8</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">18</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 8th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc_after_2</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">64</ItemTag>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Description of the 2nd Channel, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode_2</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">66</ItemTag>
                <SpecRef>10.5.2.7</SpecRef>
                <Comment>Mode of the 2nd  Channel</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_alloc_after</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">72</ItemTag>
                <SpecRef>10.5.2.21</SpecRef>
                <Comment>Mobile Allocation, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>start_time</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.2.38</SpecRef>
                <Comment>Starting Time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_list_before</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">19</ItemTag>
                <SpecRef>10.5.2.13</SpecRef>
                <Comment>Frequency List, before time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc_before</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Description of the 1st Channel, before time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc_before_2</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">1D</ItemTag>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Description of the 2nd Channel, before time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_chan_seq</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>10.5.2.12</SpecRef>
                <Comment>Frequency channel sequence before time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_alloc_before</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">21</ItemTag>
                <SpecRef>10.5.2.21</SpecRef>
                <Comment>Mobile Allocation, before time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ciph_mode_set</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">09</ItemTag>
                <SpecRef>10.5.2.9</SpecRef>
                <Comment>Cipher Mode Setting</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>vgcs_tmi</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">01</ItemTag>
                <SpecRef>10.5.2.42a</SpecRef>
                <Comment>VGCS Target Mode Indication</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>multirate_conf</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">03</ItemTag>
                <SpecRef>10.5.2.21aa</SpecRef>
                <Comment>Multi Rate Configuration</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>conform to V7.1.2</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH from the mobile station to the network to indicate that the mobile station has established the main signaling link successfully.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.3</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>u_assign_comp</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00101001</MsgID>
                <Comment>Assignment complete</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rr_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.31</SpecRef>
                <Comment>RR Cause</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>short name is u_assign_comp instead of d_assign_comp</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH on the old channel from the mobile station to the network to indicate that the mobile station has failed to seize the new channel.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.4</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>u_assign_fail</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00101111</MsgID>
                <Comment>Assignment failure</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rr_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.31</SpecRef>
                <Comment>RR cause</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>short name is u_assign_fail instead of d_assign_fail</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the network to the mobile station to request the setting of the mode for the indicated channel.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.5</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_chan_mod</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00010000</MsgID>
                <Comment>Channel mode modify</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Channel Mode</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>vgcs_tmi</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">01</ItemTag>
                <SpecRef>10.5.2.42a</SpecRef>
                <Comment>VGCS Target Mode Indication</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>multirate_conf</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">03</ItemTag>
                <SpecRef>10.5.2.21aa</SpecRef>
                <Comment>Multi-Rate Configuration</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>conform to V7.1.2</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the mobile station to the network to indicate the successful or unsuccessful execution of a channel mode modify request.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.6</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>u_chan_mod_ack</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00010111</MsgID>
                <Comment>Channel mode modify acknowledge</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Channel Mode</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH from the network to the mobile station to initiate deactivation of the dedicated channel used.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_chan_rel</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00001101</MsgID>
                <Comment>Channel release</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rr_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.31</SpecRef>
                <Comment>RR Cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ba_range</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">73</ItemTag>
                <SpecRef>10.5.2.1</SpecRef>
                <Comment>BA Range</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>group_chan_desc</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">74</ItemTag>
                <SpecRef>10.5.2.14b</SpecRef>
                <Comment>Group Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>group_ckn</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>10.5.1.10</SpecRef>
                <Comment>Group Cipher Key Number</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gprs_resum</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">0C</ItemTag>
                <SpecRef>10.5.2.14c</SpecRef>
                <Comment>GPRS Resumption</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ba_list_pref</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">75</ItemTag>
                <SpecRef>10.5.2.1c</SpecRef>
                <Comment>BA List Pref</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>utran_freq_list</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">76</ItemTag>
                <Version>REL99</Version>
                <SpecRef>10.5.2.1d</SpecRef>
                <Comment>UTRAN Freq List</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_chan_desc</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">62</ItemTag>
                <Version>REL99</Version>
                <SpecRef>10.5.2.1b</SpecRef>
                <Comment>Cell Channel Description</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>conform to V7.1.2</Comment>
            </History>
            <History>
                <Date Day="02" Month="05" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Conform to R99 standards</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH from the network to the mobile station to indicate that the network has started deciphering and that enciphering and deciphering shall be started in the mobile station, or to indicate that ciphering will not be performed.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.9</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_ciph_cmd</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00110101</MsgID>
                <Comment>Ciphering mode command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ciph_mode_set</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.9</SpecRef>
                <Comment>Ciphering Mode Setting</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ciph_res</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.10</SpecRef>
                <Comment>Cipher Response</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH from the mobile station to the network to indicate that enciphering and deciphering has been started in the mobile station.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.10</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>u_ciph_comp</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00110010</MsgID>
                <Comment>Ciphering mode complete</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_ident</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">17</ItemTag>
                <SpecRef>10.5.1.4</SpecRef>
                <Comment>Mobile Equipment Identity</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the mobile station to the network to indicate a classmark change or as a response to a classmark enquiry.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP_TS04.18] section 9.1.11</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>u_class_chng</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00010110</MsgID>
                <Comment>Classmark change</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mob_class_2</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.1.6</SpecRef>
                <Comment>Mobile Station Classmark</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mob_class_3</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">20</ItemTag>
                <SpecRef>10.5.1.7</SpecRef>
                <Comment>Additional Mobile Station Classmark Information</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>conform to V7.1.2</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the network to the mobile station to request classmark information.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.18] section 9.1.12</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_class_enq</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00010011</MsgID>
                <Comment>Classmark enquiry</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>class_enq_mask</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">10</ItemTag>
                <Version>REL99</Version>
                <SpecRef>10.5.2.7c</SpecRef>
                <Comment>Classmark enquiry mask</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="16" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Added class_enq_mask</Comment>
            </History>
            <History>
                <Date Day="25" Month="04" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Removed REL99 feature flag</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the network to the mobile station to change the channel configuration of a multi slot configuration.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.12b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_conf_change_cmd</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00110000</MsgID>
                <Comment>Configuration Change Command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>multislot_alloc</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.2.21b</SpecRef>
                <Comment>Multislot Configuration</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">63</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 1st  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode2</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">11</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 2nd  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode3</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">13</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 3rd  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode4</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">14</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 4th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode5</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">15</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 5th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode6</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">16</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 6th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode7</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">17</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 7th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode8</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">18</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 8th  Channel Set</Comment>
            </MsgItem>
            <History>
                <Date Day="17" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH from the mobile station to the network to indicate that the mobile station has changed to the ordered channel configuration successfully.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.12c</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_conf_change_ack</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00110001</MsgID>
                <Comment>Configuration Change Acknowledge</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <History>
                <Date Day="17" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH from the mobile station to the network to indicate that the mobile station has not managed to switch to the channel configuration ordered by the configuration change command and is still using the previous configuration.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.12d</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_config_change_rej</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00110011</MsgID>
                <Comment>Configuration Change Reject</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rr_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.31</SpecRef>
                <Comment>RR Cause</Comment>
            </MsgItem>
            <History>
                <Date Day="17" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the SACCH by the network to order the mobile station to send one extended measurement report.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.51</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_ext_meas_order</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00110111</MsgID>
                <Comment>Extended Measurement Order</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ext_meas_freq</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.46</SpecRef>
                <Comment>Extended Measurement Frequency List</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="19" Month="12" Year="2002"/>
                <Author>VK</Author>
                <Comment>u_ext_meas_report is 'uplink'</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the SACCH by the mobile station to the network to report extended measurement results.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.5</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>u_ext_meas_report</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00110110</MsgID>
                <Comment>Extended Measurement Report</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ext_meas_res</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.45</SpecRef>
                <Comment>Extended Measurement Results</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH from the network to the mobile station to indicate that the frequencies and the hopping sequence of the allocated channels shall be changed.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.13</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_freq_redef</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00010100</MsgID>
                <Comment>Frequency redefinition</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_alloc</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.2.21</SpecRef>
                <Comment>Mobile Allocation</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>start_time</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.38</SpecRef>
                <Comment>Starting Time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_chan_desc</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">62</ItemTag>
                <SpecRef>10.5.2.1b</SpecRef>
                <Comment>Cell Channel Description</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the mobile station to request a suspension of the GPRS services.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.13b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>u_gprs_susp_req</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00110100</MsgID>
                <Comment>GPRS suspension request</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ded_tlli</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.41a</SpecRef>
                <Comment>Temporary Logical Link Identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rout_area_id</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.5.15</SpecRef>
                <Comment>Routing Area Identification</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>susp_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.47</SpecRef>
                <Comment>Suspension Cause</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the network to the mobile station to change the dedicated channel configuration, timing adjustment needed.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.15</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_handov_cmd</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00101011</MsgID>
                <Comment>Handover command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.2</SpecRef>
                <Comment>Cell Description</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc_after</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Description of 1st channel, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>handov_ref</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.15</SpecRef>
                <Comment>Handover Reference</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pow_cmd_access</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.28a</SpecRef>
                <Comment>Power Command and Access type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>synch_ind</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>10.5.2.39</SpecRef>
                <Comment>Synchronization Indication</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_short_list_after</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">02</ItemTag>
                <SpecRef>10.5.2.14</SpecRef>
                <Comment>Frequency Short List, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_list_after</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <SpecRef>10.5.2.13</SpecRef>
                <Comment>Frequency List, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_chan_desc</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">62</ItemTag>
                <SpecRef>10.5.2.1b</SpecRef>
                <Comment>Cell Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>multislot_alloc</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">10</ItemTag>
                <Version>REL99</Version>
                <SpecRef>10.5.2.21b</SpecRef>
                <Comment>Multislot Configuration</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">63</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the First Channel</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode2</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">11</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 2nd  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode3</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">13</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 3rd  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode4</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">14</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 4th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode5</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">15</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 5th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode6</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">16</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 6th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode7</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">17</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 7th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode8</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">18</ItemTag>
                <SpecRef>10.5.2.6</SpecRef>
                <Comment>Mode of the 8th  Channel Set</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc_after_2</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">64</ItemTag>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Description of 2nd Channel, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_mode_2</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">66</ItemTag>
                <SpecRef>10.5.2.7</SpecRef>
                <Comment>Mode of the 2nd Channel</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_chan_seq_after</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">69</ItemTag>
                <SpecRef>10.5.2.12</SpecRef>
                <Comment>Freq. Channel Sequence, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_alloc_after</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">72</ItemTag>
                <SpecRef>10.5.2.21</SpecRef>
                <Comment>Mobile Allocation, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>start_time</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.2.38</SpecRef>
                <Comment>Starting Time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>time_diff</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7B</ItemTag>
                <SpecRef>10.5.2.41</SpecRef>
                <Comment>Real Time Difference</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>time_advance</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">7D</ItemTag>
                <SpecRef>10.5.2.40</SpecRef>
                <Comment>Timing Advance</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_short_list_before</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">12</ItemTag>
                <SpecRef>10.5.2.14</SpecRef>
                <Comment>Frequency Short List, before time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_list_before</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">19</ItemTag>
                <SpecRef>10.5.2.13</SpecRef>
                <Comment>Frequency List, before time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc_before</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Description of 1st Channel, before time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc_before_2</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">1D</ItemTag>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Description of 2nd Channel, before time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_chan_seq_before</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>10.5.2.12</SpecRef>
                <Comment>Freq. channel sequence before time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_alloc_before</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">21</ItemTag>
                <SpecRef>10.5.2.21</SpecRef>
                <Comment>Mobile Allocation, before time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ciph_mode_set</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">09</ItemTag>
                <SpecRef>10.5.2.9</SpecRef>
                <Comment>Cipher Mode Setting</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>vgcs_tmi</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">01</ItemTag>
                <SpecRef>10.5.2.42a</SpecRef>
                <Comment>VGCS Target Mode Indication</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>multirate_conf</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">03</ItemTag>
                <SpecRef>10.5.2.21aa</SpecRef>
                <Comment>Multi Rate Configuration</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>conform to V7.1.2</Comment>
            </History>
            <History>
                <Date Day="16" Month="03" Year="2006"/>
                <Author>GP</Author>
                <Comment>conform to REL99</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH from the mobile station to the network to indicate that the mobile station has established the main signalling link successfully.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.16</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>u_handov_comp</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00101100</MsgID>
                <Comment>Handover complete</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rr_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.31</SpecRef>
                <Comment>RR Cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_time_diff</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">77</ItemTag>
                <SpecRef>10.5.2.21a</SpecRef>
                <Comment>Mobile Observed Time Difference</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH on the old channel from the mobile station to the network to indicate that the mobile station has failed to seize the new channel.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.17</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>u_handov_fail</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00101000</MsgID>
                <Comment>Handover failure</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rr_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.31</SpecRef>
                <Comment>RR Cause</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the CCCH by the network to the mobile station in idle mode to change the channel configuration to a dedicated configuration while staying in the same cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.18</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_imm_assign</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00111111</MsgID>
                <Comment>Immediate assignment</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>10.5.2.25b</SpecRef>
                <Comment>Dedicated Mode Or TBF Spare</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tma</Name>
                </ItemLink>
                <SpecRef>10.5.2.25b</SpecRef>
                <Comment>Two-message Assignment</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>dl</Name>
                </ItemLink>
                <SpecRef>10.5.2.25b</SpecRef>
                <Comment>Downlink Assignment</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>d_t</Name>
                </ItemLink>
                <SpecRef>10.5.2.25b</SpecRef>
                <Comment>Dedicated Mode or TBF</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.26</SpecRef>
                <Comment>Page Mode</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <Control>
                    <Condition>d_t=0</Condition>
                </Control>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pck_chan_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <Control>
                    <Condition>d_t=1</Condition>
                </Control>
                <SpecRef>10.5.2.25a</SpecRef>
                <Comment>Packet Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>req_ref</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.30</SpecRef>
                <Comment>Request Reference</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>time_advance</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.40</SpecRef>
                <Comment>Timing Advance</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_alloc</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.2.21</SpecRef>
                <Comment>Mobile Allocation</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>start_time</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.2.38</SpecRef>
                <Comment>Starting Time</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ia_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.16</SpecRef>
                <Comment>IA Rest Octets (freq. parameters, before time)</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>conform to V7.1.2</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the CCCH by the network to two mobile stations in idle mode to change their channel configurations to different dedicated configurations while they stay in the same cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.19</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_imm_assign_ext</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00111001</MsgID>
                <Comment>Immediate assignment extended</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.26</SpecRef>
                <Comment>Page Mode</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <SpecRef>10.5.1.8</SpecRef>
                <Comment>Spare Half Octet</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Channel Description 1</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>req_ref</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.30</SpecRef>
                <Comment>Request Reference 1</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>time_advance</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.40</SpecRef>
                <Comment>Timing Advance 1</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc_2</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Channel Description 2</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>req_ref_2</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.30</SpecRef>
                <Comment>Request Reference 2</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>time_advance_2</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.40</SpecRef>
                <Comment>Timing Advance 2</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_alloc</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.2.21</SpecRef>
                <Comment>Mobile Allocation</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>start_time</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.2.38</SpecRef>
                <Comment>Starting Time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>10.5.2.18</SpecRef>
                <Comment>IAX Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>Rest Octet removed</Comment>
            </History>
            <History>
                <Date Day="26" Month="10" Year="1999"/>
                <Author>VK</Author>
                <Comment>Introduce rest octets</Comment>
            </History>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>IAX Rest Octets as spare padding</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the CCCH by the network to up to four mobile stations to indicate that no channel is available for assignment.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.20</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_imm_assign_rej</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00111010</MsgID>
                <Comment>Immediate assignment reject</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.26</SpecRef>
                <Comment>Page Mode</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <SpecRef>10.5.1.8</SpecRef>
                <Comment>Spare Half Octet</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>req_ref</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.30</SpecRef>
                <Comment>Request Reference 1</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t3122</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.43</SpecRef>
                <Comment>T3122 Wait Indication 1</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>req_ref_2</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.30</SpecRef>
                <Comment>Request Reference 2</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t3122_2</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.43</SpecRef>
                <Comment>T3122 Wait Indication 2</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>req_ref_3</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.30</SpecRef>
                <Comment>Request Reference 3</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t3122_3</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.43</SpecRef>
                <Comment>T3122 Wait Indication 3</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>req_ref_4</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.30</SpecRef>
                <Comment>Request Reference 4</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t3122_4</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.43</SpecRef>
                <Comment>T3122 Wait Indication 4</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>iar_rest_oct</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <Version>REL99</Version>
                <SpecRef>10.5.2.17</SpecRef>
                <Comment>IAR Rest Octets</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <Version>!REL99</Version>
                <SpecRef>10.5.2.17</SpecRef>
                <Comment>IAR Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>Rest octet removed</Comment>
            </History>
            <History>
                <Date Day="26" Month="10" Year="1999"/>
                <Author>VK</Author>
                <Comment>Introduce rest octets</Comment>
            </History>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>rest octets as spare padding</Comment>
            </History>
            <History>
                <Date Day="27" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>made iar_rest_octet to a real IE</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the SACCH by the mobile station to the network to report measurement results about the dedicated channel and about neighbor cells.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.21</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>u_meas_rep</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00010101</MsgID>
                <Comment>Measurement report</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>meas_result</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.20</SpecRef>
                <Comment>Measurement Results</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the NCH by the network to notify the mobile stations of VBS or VGCS calls in the current cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.21b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_notify_nch</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00100000</MsgID>
                <Comment>Notification/NCH</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nt_rest_oct</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.22c</SpecRef>
                <Comment>NT/N Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the CCCH by the network to up to two mobile stations to trigger channel access by these. The mobile stations are identified by their TMSI or IMSI.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.22</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_pag_req_1</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00100001</MsgID>
                <Comment>Paging request type 1</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.26</SpecRef>
                <Comment>Page Mode</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_needed</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.8</SpecRef>
                <Comment>Channels Needed for Mobiles 1 and 2</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_ident</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.1.4</SpecRef>
                <Comment>Mobile Identity 1</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_ident_2</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">17</ItemTag>
                <SpecRef>10.5.1.4</SpecRef>
                <Comment>Mobile Identity 2</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p1_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.23</SpecRef>
                <Comment>P1 Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>Rest Octet removed</Comment>
            </History>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Rest Octet inserted</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the CCCH by the network to two or three mobile stations to trigger channel access by these. Two of the mobile stations are identified by their TMSI while the third is identified by its TMSI or IMSI.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.23</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_pag_req_2</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00100010</MsgID>
                <Comment>Paging request type 2</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.26</SpecRef>
                <Comment>Page Mode</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_needed</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.8</SpecRef>
                <Comment>Channels Needed for Mobiles 1 and 2</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tmsi_1</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.42</SpecRef>
                <Comment>Mobile Identity 1</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tmsi_2</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.42</SpecRef>
                <Comment>Mobile Identity 2</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_ident</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">17</ItemTag>
                <SpecRef>10.5.1.4</SpecRef>
                <Comment>Mobile Identity 3</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p2_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.24</SpecRef>
                <Comment>P2 Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>P2 Rest Octets as a structured IE</Comment>
            </History>
            <History>
                <Date Day="16" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change name of "imsi" to "imsi_1" to avoid confusion</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the CCCH by the network to four mobile stations to trigger channel access by these. The mobile stations are identified by their TMSIs.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.24</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_pag_req_3</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00100100</MsgID>
                <Comment>Paging request type 3</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.26</SpecRef>
                <Comment>Page Mode</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_needed</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.8</SpecRef>
                <Comment>Channels Needed for Mobiles 1 and 2</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tmsi_1</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.42</SpecRef>
                <Comment>Mobile Identity 1</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tmsi_2</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.42</SpecRef>
                <Comment>Mobile Identity 2</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tmsi_3</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.42</SpecRef>
                <Comment>Mobile Identity 3</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tmsi_4</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.42</SpecRef>
                <Comment>Mobile Identity 4</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p3_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.25</SpecRef>
                <Comment>P3 Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>P3 Rest Octets as a structured IE</Comment>
            </History>
            <History>
                <Date Day="16" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change name of "imsi" to "imsi_1" to avoid confusion</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the mobile station to the network in connection with establishment of the main signaling link as a response to the paging request message.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.25</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>u_pag_res</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00100111</MsgID>
                <Comment>Paging response</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ciph_key_num</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.1.2</SpecRef>
                <Comment>Ciphering Key Sequence Number</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <SpecRef>10.5.1.8</SpecRef>
                <Comment>Spare Half Octet</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mob_class_2</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.1.6</SpecRef>
                <Comment>Mobile Station Classmark</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_ident</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.1.4</SpecRef>
                <Comment>Mobile Identity</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the network to the mobile station to deactivate part of the dedicated channels in use.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.26</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_part_rel</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00001010</MsgID>
                <Comment>Partial release</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Channel Description</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the mobile station to the network to indicate that a part of the dedicated channels has been deactivated.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.27</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>u_part_rel_comp</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00001111</MsgID>
                <Comment>Partial release complete</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the network to the mobile station to change to a PDCH, when no timing adjustment is needed.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.13a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_pdch_ass_cmd</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00100011</MsgID>
                <Comment>PDCH Assignment Command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Description of the Channel, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_chan_desc</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">62</ItemTag>
                <SpecRef>10.5.2.1b</SpecRef>
                <Comment>Cell Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_list_after</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <SpecRef>10.5.2.13</SpecRef>
                <Comment>Frequency List, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_alloc_after</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">72</ItemTag>
                <SpecRef>10.5.2.21</SpecRef>
                <Comment>Mobile Allocation, after time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>start_time</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.2.38</SpecRef>
                <Comment>Starting Time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_list_before</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">19</ItemTag>
                <SpecRef>10.5.2.13</SpecRef>
                <Comment>Frequency List, before time</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc_before</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>Description of the Channel, before time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_chan_seq</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>10.5.2.12</SpecRef>
                <Comment>Frequency channel sequence before time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_alloc_before</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">21</ItemTag>
                <SpecRef>10.5.2.21</SpecRef>
                <Comment>Mobile Allocation, before time</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pck_ul_ass</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">22</ItemTag>
                <SpecRef>10.5.2.25c</SpecRef>
                <Comment>RR Packet Uplink Assignment</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pck_dl_ass</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">23</ItemTag>
                <SpecRef>10.5.2.25d</SpecRef>
                <Comment>RR Packet Downlink Assignment</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="2001"/>
                <Author>VK</Author>
                <Comment>Add freq_list_before (Frequency List, before time)</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the network to the mobile station to stop the sending of access bursts from the mobile station.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.28</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_phys_info</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00101101</MsgID>
                <Comment>Physical information</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>time_advance</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.40</SpecRef>
                <Comment>Timing Advance</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the network to the mobile station to order it to reselect a cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.21e</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_change_order</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00001000</MsgID>
                <Comment>RR-Cell Change Order</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.2</SpecRef>
                <Comment>Cell Description</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nc_mode</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.21c</SpecRef>
                <Comment>NC Mode For Target Cell</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DCCH by the mobile station to request the establishment of dedicated mode.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.28a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_rr_init_req</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00111100</MsgID>
                <Comment>RR Initialisation Request</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ciph_key_num</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.1.2</SpecRef>
                <Comment>Ciphering Key Sequence Number</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_coding</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.2.4a</SpecRef>
                <Comment>MAC Mode And Channel Coding</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mob_class_2</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <ItemTag TagType="ALPHA"/>
                <SpecRef>10.5.1.6</SpecRef>
                <Comment>Mobile Station Classmark</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ded_tlli</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.41a</SpecRef>
                <Comment>Temporary Logical Link Identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_req_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.8a</SpecRef>
                <Comment>Channel Request Description</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gprs_meas_res</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.20a</SpecRef>
                <Comment>GPRS Measurement Results</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent by the mobile station or the network at any time to report certain error conditions as described in section 8.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.29</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>b_rr_status</Name>
                <MsgID Direction="BOTH" IDType="BIN">00010010</MsgID>
                <Comment>RR Status</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rr_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.31</SpecRef>
                <Comment>RR Cause</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the BCCH by the network to all mobile stations within the cell giving information of control of the RACH and of the cell allocation.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.31</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_1</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00011001</MsgID>
                <Comment>System information Type 1</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_chan_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.1b</SpecRef>
                <Comment>Cell Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rach_ctrl</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.29</SpecRef>
                <Comment>RACH Control Parameter</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si1_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.32</SpecRef>
                <Comment>SI 1 Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>rest octet removed, no content</Comment>
            </History>
            <History>
                <Date Day="26" Month="10" Year="1999"/>
                <Author>VK</Author>
                <Comment>Introduce rest octets</Comment>
            </History>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>si1_rest_octet now a structured IE</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the BCCH by the network to all mobile stations within the cell giving information of control of the RACH and of the BCCH allocation in the neighbor cells.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.32</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_2</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00011010</MsgID>
                <Comment>System information Type 2</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>neigh_cell_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.22</SpecRef>
                <Comment>BCCH Frequency List</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ncc_permit</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.27</SpecRef>
                <Comment>NCC Permitted</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rach_ctrl</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.29</SpecRef>
                <Comment>RACH Control Parameter</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent optionally on the BCCH by the network to all mobile stations within the cell giving information on control of the RACH and of the extension of the BCCH allocation in the neighbour cells.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.33</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_2bis</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000010</MsgID>
                <Comment>System information Type 2bis</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>neigh_cell_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.22</SpecRef>
                <Comment>Extended BCCH Frequency List</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rach_ctrl</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.29</SpecRef>
                <Comment>RACH Control Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>10.5.2.33</SpecRef>
                <Comment>SI 2bis Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>rest octet removed, no content</Comment>
            </History>
            <History>
                <Date Day="26" Month="10" Year="1999"/>
                <Author>VK</Author>
                <Comment>Introduce rest octets</Comment>
            </History>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>si2bis_rest_oct as spare padding</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent optionally on the BCCH by the network to all mobile stations within the cell giving information on additional measurement and reporting parameters and/or UTRAN neighbour cells. A mobile station with no UTRAN capability should ignore the 3G Neighbour Cell, 3G MEASUREMENT parameter and GPRS_3G MEASUREMENT parameter descriptions in this message. The message may contain more than one instance. Special requirements for the transmission of this message apply on BCCH.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_2quater</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000111</MsgID>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>System information Type 2quater</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si_2qua_octets</Name>
                </ItemLink>
                <SpecRef>10.5.2.33b</SpecRef>
                <Comment>SI 2quater Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent optionally on the BCCH by the network to all mobile stations within the cell giving information on the extension of the BCCH allocation in the neighbour cells.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.34</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_2ter</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000011</MsgID>
                <Comment>System information Type 2ter</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>neigh_cell_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.22</SpecRef>
                <Comment>Extended BCCH Frequency List</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>10.5.2.33a</SpecRef>
                <Comment>SI 2ter Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>rest octet removed, no content</Comment>
            </History>
            <History>
                <Date Day="26" Month="10" Year="1999"/>
                <Author>VK</Author>
                <Comment>Introduce rest octets</Comment>
            </History>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>si2bis_rest_oct as spare padding</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the BCCH by the network giving information of control on the RACH, the location area identification, the cell identity and various other information about the cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.35</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_3</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00011011</MsgID>
                <Comment>System information Type 3</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_ident</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.1.1</SpecRef>
                <Comment>Cell Identity</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>loc_area_ident</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.1.3</SpecRef>
                <Comment>Location Area Identification</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ctrl_chan_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.11</SpecRef>
                <Comment>Control Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_opt_bcch</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.3</SpecRef>
                <Comment>Cell Options</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_select</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.4</SpecRef>
                <Comment>Cell Selection Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rach_ctrl</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.29</SpecRef>
                <Comment>RACH Control Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si3_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.34</SpecRef>
                <Comment>SI 3 Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>si3_rest_octet now a structured IE</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the BCCH by the network giving information on control of the RACH, the location area identification, the cell identity and various other information about the cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.36</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_4</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00011100</MsgID>
                <Comment>System information Type 4</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>loc_area_ident</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.1.3</SpecRef>
                <Comment>Location Area Identification</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_select</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.4</SpecRef>
                <Comment>Cell Selection Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rach_ctrl</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.29</SpecRef>
                <Comment>RACH Control Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_desc</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">64</ItemTag>
                <SpecRef>10.5.2.5</SpecRef>
                <Comment>CBCH Channel Description</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_alloc</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">72</ItemTag>
                <SpecRef>10.5.2.21</SpecRef>
                <Comment>CBCH Mobile Allocation</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si4_rest_oct</Name>
                </ItemLink>
                <Type>CSN1_CONCAT</Type>
                <SpecRef>10.5.2.35</SpecRef>
                <Comment>SI 4 Rest Octets</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>si4_rest_octet now a structured IE</Comment>
            </History>
            <History>
                <Date Day="20" Month="9" Year="2000"/>
                <Author>PZ</Author>
                <Comment>added V5 type to si4_rest_oct</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the SACCH by the network to mobile stations within the cell giving information on the BCCH allocation in the neighbour cells.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.37</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_5</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00011101</MsgID>
                <Comment>System information Type 5</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>neigh_cell_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.22</SpecRef>
                <Comment>BCCH Frequency List</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent optionally on the SACCH by the network to mobile stations within the cell giving information on the extension of the BCCH allocation in the neighbour cells.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.38</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_5bis</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000101</MsgID>
                <Comment>System information Type 5bis</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>neigh_cell_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.22</SpecRef>
                <Comment>Extension of the BCCH Frequency List Description</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent optionally on the SACCH by the network to mobile stations within the cell giving information on the extension of the BCCH allocation in the neighbour cells.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.39</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_5ter</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000110</MsgID>
                <Comment>System information Type 5ter</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>neigh_cell_desc</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.22</SpecRef>
                <Comment>Extended BCCH Frequency List</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the SACCH by the network to mobile stations within the cell giving information of location area identification, of cell identity and various other information.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.40</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_6</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00011110</MsgID>
                <Comment>System information Type 6</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_ident</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.1.1</SpecRef>
                <Comment>Cell Identity</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>loc_area_ident</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.1.3</SpecRef>
                <Comment>Location Area Identification</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_opt_sacch</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.3</SpecRef>
                <Comment>Cell Options</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ncc_permit</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.27</SpecRef>
                <Comment>NCC Permitted</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si6_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.35a</SpecRef>
                <Comment>SI 6 Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>added si6_rest_oct</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the BCCH by the network giving information about cell reselection parameters to be used in that cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.41</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_7</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00011111</MsgID>
                <Comment>System information Type 7</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si7_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.36</SpecRef>
                <Comment>SI 7 Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>si7_rest_octet now a structured IE</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the BCCH by the network giving information about cell reselection parameters to be used in that cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.42</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_8</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00011000</MsgID>
                <Comment>System information Type 8</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si8_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.37</SpecRef>
                <Comment>SI 8 Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>si8_rest_octet now a structured IE</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the BCCH by the network giving information on the scheduling of information on the BBCH.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.43</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_9</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000100</MsgID>
                <Comment>System information Type 9</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rach_ctrl</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.29</SpecRef>
                <Comment>RACH Control Parameter</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si9_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.37a</SpecRef>
                <Comment>SI 9 Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the BCCH by the network giving information related to GPRS in the cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.43a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_13</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000000</MsgID>
                <Comment>System information Type 13</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si13_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.37b</SpecRef>
                <Comment>SI 13 Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the BCCH by the network giving information about cell selection and reselection parameters to be used in that cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.43d</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_16</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00111101</MsgID>
                <Comment>System information Type 16</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si16_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.37e</SpecRef>
                <Comment>SI 16 Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the BCCH by the network giving information about cell selection and reselection parameters to be used in that cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.42</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_sys_info_17</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00111110</MsgID>
                <Comment>System information Type 17</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si17_rest_oct</Name>
                </ItemLink>
                <SpecRef>10.5.2.37f</SpecRef>
                <Comment>SI 17 Rest Octets</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main DDCH by the mobile station to the network to give the talker information when a new layer 2 connection is established on a VGCS channel after an uplink access.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.44</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>talker_ind</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00010001</MsgID>
                <Comment>Talker Indication</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mob_class_2</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.1.6</SpecRef>
                <Comment>Mobile Station Classmark</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mob_ident</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.1.4</SpecRef>
                <Comment>Mobile Identity</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is broadcasted on the voice group call channel on the main DCCH, SAPI 0, by the network to inform of the uplink status of the voice group call channel.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.46</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_uplink_busy</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00101010</MsgID>
                <Comment>Uplink Busy</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the uplink of the voice group call channel to initiate a deactivation of the group transmit mode or on the downlink to reject an uplink access which was already granted by the network.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.48</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>b_uplink_rel</Name>
                <MsgID Direction="BOTH" IDType="BIN">00001110</MsgID>
                <Comment>Uplink release</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rr_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.31</SpecRef>
                <Comment>RR Cause</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This message is sent on the main signaling channel by the network to stop the sending of access bursts from the mobile station and to change the channel configuration to a dedicated configuration.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.49</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>d_vgcs_uplink_grant</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00001001</MsgID>
                <Comment>VGCS uplink grant</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>req_ref</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.30</SpecRef>
                <Comment>Request Reference</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>time_advance</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.2.40</SpecRef>
                <Comment>Timing Advance</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
    </MessagesSection>
    <MsgStructElementsSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all structured elements that are defined for the RR AIM</XHTMLElement>
            </DocElement>
        </Description>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The GAMMA_TN field is the binary representation of the parameter CH for MS output power control in units of 2 dB, see 3GPP TS 05.08.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.60] section 12.9</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">ALPHA is the binary representation of the parameter ( for MS output power control in units of 0.1, see 3GPP TS 05.08. Range: 0 to 10.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.18] section 10.5.2.25c</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>alpha_gamma</Name>
                <Comment>Alpha Gamma</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Alpha</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gamma</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Gamma</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="23" Month="10" Year="2000"/>
                <Author>FRI</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="2001"/>
                <Author>VK</Author>
                <Comment>Add Description</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the information element is to provide an APDU or APDU segment.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.18] section 10.5.2.50</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>apdu_data</Name>
                <Comment>APDU Data</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>apdu_info</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[2..MAX_APDU_DATA]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>APDU Information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="19" Month="7" Year="2002"/>
                <Author>OTH</Author>
                <Comment>Initial - add APDU Data</Comment>
            </History>
            <History>
                <Date Day="20" Month="8" Year="2002"/>
                <Author>OTH</Author>
                <Comment>MAX_APDU_DATA in len field added.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The APDU Flags infrmation element provides segmentation and control information for an associated APDU.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.18] section 10.5.2.49</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>apdu_flags</Name>
                <Comment>APDU Flags</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare bit</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>c_r</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Command/Final Response</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>f_seg</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>First Segment</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>l_seg</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Last Segment</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="19" Month="7" Year="2002"/>
                <Author>OTH</Author>
                <Comment>Initial - add APDU Flags</Comment>
            </History>
            <History>
                <Date Day="9" Month="9" Year="2002"/>
                <Author>VK</Author>
                <Comment>Add spare bit</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The APDU ID information element identifies the particular protocaol and associated application for an APDU.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.18] section 10.5.2.48</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>apdu_id</Name>
                <Comment>APDU ID</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>protoc_ident</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Protocol Identifier</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="19" Month="7" Year="2002"/>
                <Author>OTH</Author>
                <Comment>Initial - add APDU ID</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the BA Range information element is to provide the mobile station with ARFCN range information which can be used in the cell selection procedure.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.1a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ba_range</Name>
                <Comment>BA Range</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>num_range</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Number of Ranges</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_range</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[2..N_MAX_RANGE]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Frequency Range</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the BA List Pref information element is to provide the mobile station with ARFCN information which can be used in the cell selection/reselection procedure.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.1c</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ba_list_pref</Name>
                <Comment>BA List Pref</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_range</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_RANGE]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Range Limits</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_ARFCN]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>BA Frequency</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>0</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Cell Description information element is to provide a minimum description of a cell, e.g. to allow the mobile station to use its preknowledge about synchronization.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.2</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cell_desc</Name>
                <Comment>Cell Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>bcch_arfcn_hi</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BCCH ARFCN (hi part)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ncc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PLMN Colour Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>bcc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BS Colour Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>bcch_arfcn_lo</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BCCH ARFCN (lo part)</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Cell Options (BCCH) information element is to provide a variety of information about a cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.3</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cell_opt_bcch</Name>
                <Comment>Cell Options (BCCH)</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pow_ctrl</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Power Control</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>dtx_b</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Discontinuous Transmission (BCCH)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rlt</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Radio Link Timeout</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Cell Options (SACCH) information element is to provide a variety of information about a cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note that this IE has a split field : dtx. The values for 'dtx' span 'dtx_s' and 'dtx2_s'.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.3a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cell_opt_sacch</Name>
                <Comment>Cell Options (SACCH)</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>dtx2_s</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Discontinuous Transmission (SACCH) high</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pow_ctrl</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Power Control</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>dtx_s</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Discontinuous Transmission (SACCH) low</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rlt</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Radio Link Timeout</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Cell Selection Parameters information element is to provide a variety of information about a cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.4</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cell_select</Name>
                <Comment>Cell Selection Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_resel_hyst</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Cell Reselect Hysteresis</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ms_txpwr_max_cch</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS-TXPWR-MAX-CCH</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>acs</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ACS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>neci</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NECI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rxlev_access_min</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RX Level Access Minimum</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Channel Description information element is to provide a description of an allocatable channel together with its SACCH.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.5</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_desc</Name>
                <Comment>Channel Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_desc_2</Name>
                <Comment>Channel Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_desc_before</Name>
                <Comment>Channel Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_desc_before_2</Name>
                <Comment>Channel Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_desc_after</Name>
                <Comment>Channel Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_desc_after_2</Name>
                <Comment>Channel Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Channel type and TDMA offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Time Slot</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Training Sequence Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>hop</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Hopping</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <Control>
                    <Condition>hop=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Absolute RF Channel Number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Allocation Index Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>hsn</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Hopping Sequence Number</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Channel Needed information element is to indicate to up to two mobile stations which type of channel is needed (for each mobile station) for the transaction linked to the paging procedure.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.8</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_needed</Name>
                <Comment>Channel Needed</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cn2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CHANNEL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cn1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CHANNEL</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Channel Needed for Mobile ID 3 and 4 field is to indicate to up to two mobile stations which type of channel is needed (for each mobile station) for the transaction linked to the paging procedure.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25 (P3 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_needed3_4</Name>
                <Comment>Channel Needed for Mobile ID 3 and 4</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cn3</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CHANNEL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cn4</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CHANNEL</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Channel Request Description information element is to indicate to the network the type of requested uplink resources or to indicate the type of paging that is being responded to.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.8a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_req_desc</Name>
                <Comment>Channel Request Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>or_ty</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MT/MO Origination type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <Control>
                    <Condition>or_ty=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00000000</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Control>
                    <TypeModifier>[3]</TypeModifier>
                    <Condition>or_ty=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>crd_prio</Name>
                </ItemLink>
                <Control>
                    <Condition>or_ty=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Channel Request Description Priority</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rlc_mode</Name>
                </ItemLink>
                <Control>
                    <Condition>or_ty=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>RLC Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>llc_fr_type</Name>
                </ItemLink>
                <Control>
                    <Condition>or_ty=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>LLC Frame Type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rbw</Name>
                </ItemLink>
                <Control>
                    <Condition>or_ty=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Requested Bandwidth</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rlc_c_oct</Name>
                </ItemLink>
                <Control>
                    <Condition>or_ty=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>RLC Octet Count</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Ciphering Key Sequence Number information element is to make it possible for the network to identify the ciphering key Kc which is stored in the mobile station without invoking the authentication procedure. The ciphering key sequence number is allocated by the network and sent with the AUTHENTICATION REQUEST message to the mobile station where it is stored together with the calculated ciphering key Kc.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.1.2</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ciph_key_num</Name>
                <Comment>Ciphering Key Sequence Number</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>key_seq</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Key Sequence</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Cipher Mode Setting information element is to indicate whether stream ciphering shall be started or not and if it is to be started, which algorithm to use.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.9</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ciph_mode_set</Name>
                <Comment>Cipher Mode Setting</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>algo_ident</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Algorithm Identifier</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>sc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Start Ciphering</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Cipher Response information element is used by the network to indicate to the mobile station which information the mobile station has to include in the CIPHERING MODE COMPLETE message.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.10</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ciph_res</Name>
                <Comment>Cipher Response</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cr</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Cipher Response</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to indicate the properties of a codec in a Multi-Rate Configuration.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21aa</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cod_prop</Name>
                <Comment>Codec Properties</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>codec_thr</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Codec Threshold</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>codec_hyst</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Codec Hysteresis</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Control Channel Description information element is to provide a variety of information about a cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.11</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ctrl_chan_desc</Name>
                <Comment>Control Channel Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mscr</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MSC Release</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>att</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Attach / detach allowed</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>bs_ag_blks_res</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BS Access Grant Blocks reserved</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ccch_conf</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Common Control Channel Configuration</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00000</Pattern>
                    <BitLen>5</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>bs_pa_mfrms</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BS Paging Multiframes</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t3212</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T 3212 time-out value</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="27" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Added mscr</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Descriptive Group Or Broadcast Call Reference information element is to provide information describing a voice group or broadcast call.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.1.9</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>dgcr</Name>
                <Comment>Descriptive Group Call Reference</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gcr</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Group Call Reference</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>sf</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Service Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>af</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Acknowledge Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>call_prio</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Call Priority</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>group_ckn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Ciphering information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Dynamic Allocation information element contains parameters necessary to define the radio resources of a dynamic allocation or an extended dynamic allocation.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>dyn_alloc</Name>
                <Comment>Dynamic Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ext_dyn_all</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Extended Dynamic Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>P0</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>usf_gran</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>USF Granularity</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tfi</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Uplink TFI Assignment</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rlc_blks</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>RLC Data Blocks Granted</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag_pp</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag Parameters Present</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tagged_usf_tn</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[8]</TypeModifier>
                    <Condition>flag_pp=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Tagged USF For Timeslot</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <Control>
                    <Condition>flag_pp=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Alpha</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>usf_gamma_csn1</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[8]</TypeModifier>
                    <Condition>flag_pp=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>USF For Timeslot And Gamma (CSN1)</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="10" Year="2000"/>
                <Author>FRI</Author>
                <Comment>added P0 &amp; USF Granularity; changed usf_gamma to usf_gamma_csn1</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Dynamic or Fixed Allocation IE contains parameters for an EGPRS  uplink packet data transfer.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.16</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>d_f_alloc</Name>
                <Version>REL99</Version>
                <Comment>Dynamic or Fixed Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tfi</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>TFI Assignment</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>poll</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Polling</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>allo_flag</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Allocation flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>d_alloc</Name>
                </ItemLink>
                <Control>
                    <Condition>allo_flag=0</Condition>
                </Control>
                <SpecRef/>
                <Comment>Dynamic Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>f_alloc</Name>
                </ItemLink>
                <Control>
                    <Condition>allo_flag=1</Condition>
                </Control>
                <SpecRef/>
                <Comment>Fixed Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mcs</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>EGPRS Modulation and coding Scheme</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tlli_bcc</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>TLLI Block Channel Coding</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>bep_period</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>BEP Period 2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>resegm</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Resegment</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>e_window</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>EGPRS Window Size</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>Alpha</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gamma</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Gamma</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ta_idx</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>Timing Advance Index</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tbf_start_time</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>TBF Starting Time</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to indicate the support of early classmark sending inside the SI 3 rest octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>es_ind_tag</Name>
                <Comment>Early Classmark Sending Tag</Comment>
            </MsgStructElemDef>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The EGPRS Packet Uplink Assignment contains parameters for an EGPRS  uplink packet data transfer.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.16</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>egprs_pua</Name>
                <Version>REL99</Version>
                <Comment>EGPRS Packet Uplink Assignment</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ext_ra</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Extended RA</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>acc_tt</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_ACCESS_TT]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>Access technology type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>d_f_alloc</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef/>
                <Comment>Dynamic or Fixed Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mb_alloc</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef/>
                <Comment>Multi Block Allocation</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of Extended Measurement Results information element is to provide the results of the measurement made by the mobile station on the carriers specified in the Extended Measurement Order.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.45</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ext_meas_res</Name>
                <Comment>Extended Measurement Results</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>sc_used</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Sequence Code Used</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>dtx_used</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DTX Used</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rx_lev_ncell</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[21]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>RX Level Ncell</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="28" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Fixed Allocation information element contains parameters necessary to define the radio resources of a fixed allocation.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>fix_alloc</Name>
                <Comment>Fixed Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tfi</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Uplink TFI Assignment</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>final</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Final Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>dl_ctrl_tn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Downlink Control Timeslot</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0_pwr_ctrl_mode</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>P0 and BTS Power Control Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ts_all</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Timeslot Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pwr_ctrl</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Power Control Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>hdm</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Half Duplex Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>fa_blk_ia</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Fixed Allocation Block Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>allo_var</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[allo_len7..127]</TypeModifier>
                    <Condition>flag1=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Allocation Bitmap Var</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="10" Year="2000"/>
                <Author>FRI</Author>
                <Comment>changed parameter sequence for Uplink TFI Assign, inserted P0 and BTS Power Control Mode, inserted spare and flag1, changed flaggingfor Blocks &amp; Alloc</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>CAN</Author>
                <Comment>Fixed Allocation Block Structure changed</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Frequency Channel Sequence information element is to provide the absolute radio frequency channel numbers used in the mobile hopping sequence. This information element shall only be used for radio frequency channels in the primary GSM band (see TS GSM 05.05).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.12</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>freq_chan_seq</Name>
                <Comment>Frequency Channel Sequence</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>freq_chan_seq_before</Name>
                <Comment>Frequency Channel Sequence</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>freq_chan_seq_after</Name>
                <Comment>Frequency Channel Sequence</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>low_arfcn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Lowest ARFCN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>inc_skip</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[N_FREQ_SKIP]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>inc skip of ARFCNn</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Frequency List information element is to provide the list of the absolute radio frequency channel numbers used in a frequency hopping sequence. There are several formats for the Frequency List information element, distinguished by the "format indicator" sub field. Some formats are frequency bit maps, the others use a special encoding scheme.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.13</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>freq_list</Name>
                <Comment>Frequency List</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>freq_list_after</Name>
                <Comment>Frequency List</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>freq_list_before</Name>
                <Comment>Frequency List</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flist</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[1..32]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Frequency List Contents</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="2" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Frequency Range is coded as the binary representation of the ARFCNs used as the limits of a range of frequencies to be used by the mobile station in cell selection (see TS GSM 05.08 and TS GSM 03.22)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.1a (BA Range)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>freq_range</Name>
                <Comment>Frequency Range</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_lower</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Frequency RANGE LOWER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_higher</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Frequency RANGE HIGHER</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The GPRS indicator is part of SI3 and SI4 rest octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34, section 10.5.2.35</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_indic</Name>
                <Comment>GPRS Indicator</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ra_color</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RA Color</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si13_pos</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SI13 Position</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the GPRS Measurement Result information element is to provide the results of GPRS measurements made by the GPRS mobile station an the serving cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.20a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_meas_res</Name>
                <Comment>GPRS Measurement Results</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>c_val</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>C Value</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rxqual</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RX Quality</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>sign_var</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Signal Variance</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="19" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The GPRS Mobile Allocation information element defines a set of radio frequency channels and a hopping sequence number, which may be allocated to a mobile station to define its channel configuration.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets) GSM_04.60 section 12.10a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_ma</Name>
                <Comment>GPRS Mobile Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>hsn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Hopping Sequence Number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rfln</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_RFL]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>RFL Number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>hop</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>allo_len6</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Allocation Bitmap Length</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>allo_bmp6</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[allo_len6+1..64]</TypeModifier>
                    <Condition>hop=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Allocation Bitmap</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>arfcn_idx</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_ARFCNI]</TypeModifier>
                    <Condition>hop=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>ARFCN Index</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="9" Month="2" Year="2001"/>
                <Author>PZ</Author>
                <Comment>Allocation Bitmap fixed</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>CAN</Author>
                <Comment>Allocation Bitmap len set to 1</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the GPRS Resumption information element is to indicate whether the network has successfully resumed GPRS services or not.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.14c</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_resum</Name>
                <Comment>GPRS Resumption</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>res_ack</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Resumption ACK</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.22c, 9.1.21a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gr_call_info</Name>
                <Comment>Group Call Information</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>dgcr</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Descriptive Group Call Reference</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gr_ch_desc</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Group Channel Description 2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Group Channel Description information element is to provide a description of an allocable voice group call or voice broadcast call channel together with its SACCH and part of the RF channels belonging to the cell allocation which is used in the mobile hopping sequence if applicable.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.14b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>group_chan_desc</Name>
                <Comment>Group Channel Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Channel type and TDMA offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Time Slot</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Training Sequence Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>hop</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Hopping</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <Control>
                    <Condition>hop=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Absolute RF Channel Number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Allocation Index Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>hsn</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Hopping Sequence Number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mac</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[1..N_MOB_ALLOC]</TypeModifier>
                    <Condition>hop=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Allocation RF Channels</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.21a (Notification/FACCH), 10.2.22c (NT/N Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gr_ch_desc</Name>
                <Comment>Group Channel Description 2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Channel type and TDMA offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Time Slot</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Training Sequence Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>hop</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Hopping</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <Control>
                    <Condition>hop=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Absolute RF Channel Number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Allocation Index Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>hsn</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Hopping Sequence Number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>hop_freq</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Hopping Frequencies</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.21a (Notification/FACCH), 10.2.22c (NT/N Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>hop_freq</Name>
                <Comment>Hopping Frequencies</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ma_len</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Allocation Length</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mac</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[ma_len..N_MOB_ALLOC]</TypeModifier>
                    <Condition>flag = 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Allocation Content</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>freq_short_list2</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Frequency Short List 2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The IA Assignment parameters contains either a packet uplink assignment construction and a packet downlink assignment construction or a second part packet assignment construction.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ia_assign_par</Name>
                <Comment>IA Assignment Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag1</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pck_upl_ass_ia</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 0 AND flag1 = 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Packet Uplink Assignment (IA)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pck_downl_ass_ia</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 0 AND flag1 # 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Packet Downlink Assignment (IA)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ia_2nd_part</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>IA Second Part Packet Assignment</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The IA EGPRS Parameters contain an EGPRS  packet uplink assignment construction or possibly future extensions of the protocol (associated with the remaining values of flag and/or flag1).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.16</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ia_egprs_par</Name>
                <Version>REL99</Version>
                <Comment>IA EGPRS Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag1</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef/>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>egprs_pua</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0 AND flag1=0</Condition>
                </Control>
                <SpecRef/>
                <Comment>EGPRS Packet Uplink Assignment</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The IA Frequency Parameters contains a frequency parameters, before time field.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ia_freq_par</Name>
                <Comment>IA Frequency Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>fp_len</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Length Of Frequency Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <Control>
                    <Condition>fp_len#0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <Control>
                    <Condition>fp_len#0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Allocation Index Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mac</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[fp_len-1..11]</TypeModifier>
                    <Condition>fp_len#0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Allocation Contents</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The IA Rest Octets information element contains spare bits and possibly either an EGPRS  packet uplink assignment construction, a packet uplink assignment construction, a packet downlink assignment construction, a second part packet assignment construction or a frequency parameters, before time field, which combines a mobile allocation and a MAIO (see the channel description information element).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.18] section 10.5.2.16</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ia_rest_oct</Name>
                <Comment>IA Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag_2bit</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag twobit</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ia_egprs_par</Name>
                </ItemLink>
                <Control>
                    <Condition>flag_2bit=0b01</Condition>
                </Control>
                <Version>REL99</Version>
                <SpecRef/>
                <Comment>IA EGPRS Packet Uplink Assignment</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ia_freq_par</Name>
                </ItemLink>
                <Control>
                    <Condition>flag_2bit=0b10</Condition>
                </Control>
                <SpecRef/>
                <Comment>IA Frequency Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ia_assign_par</Name>
                </ItemLink>
                <Control>
                    <Condition>flag_2bit=0b11</Condition>
                </Control>
                <SpecRef/>
                <Comment>IA Assignment Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="10" Year="1999"/>
                <Author>VK</Author>
                <Comment>change bit len to 88 (was 96)</Comment>
            </History>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>now a structured IE</Comment>
            </History>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Inserted flag and ia_egprs_par</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The IA Second Part Packet Assignment is empty in the current version. The presence of the Second Part Packet Assignment is the indication , that this message is the second message of two Immediate Assignment messages in an assignment of an uplink or downlink Temporary Block Flow (TBF).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ia_2nd_part</Name>
                <Comment>IA Second Part Packet Assignment</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ext_ra</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>Extended RA</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>added ext_ra</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The IAR Rest Octets information element contains spare bits or possibly Extended RA informations.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.17</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>iar_rest_oct</Name>
                <Version>REL99</Version>
                <Comment>IAR Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ext_ra</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[4]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>Extended RA</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef/>
                <Comment>Spare padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [1] section 10.5.2.37a (SI 9 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>itp</Name>
                <Comment>Info Type and Positions</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>itpo</Name>
                <Comment>Info Type and Positions Optional</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>it4</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Info Type 4</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag1</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Flag1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>it5</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Info Type 5</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>it6</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND flag1=6</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Info Type 6</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>poss</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Positions</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Location Area Identification information element is to provide an unambiguous identification of location areas within the area covered by the GSM system.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.1.3</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>loc_area_ident</Name>
                <Comment>Location Area Identification</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mcc</Name>
                </ItemLink>
                <Type>BCD_NOFILL</Type>
                <Control>
                    <TypeModifier>[3]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Country Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mnc</Name>
                </ItemLink>
                <Type>BCD_MNC</Type>
                <Control>
                    <TypeModifier>[2..3]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Network Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>lac</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Location Area Code</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="8" Year="2001"/>
                <Author>HM</Author>
                <Comment>3-digit-MNC</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The LSA ID Information is part of SI4 rest octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>lsa_id_info</Name>
                <Comment>LSA ID Information</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>lsa_id</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>LSA ID</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>lsa_id_add</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_LSA_ID]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Additional LSA IDs</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The LSA parameters are part of SI4 Rest Octets and SI16 Rest Octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35, section 10.5.2.37e</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>lsa_param</Name>
                <Comment>LSA parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>prio_thr</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Priority Threshold</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>lsa_offs</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>LSA Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>opt_mcc</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Optional MCC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mnc</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[3]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>MNC</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The LSA parameters and ID are part of SI16 Rest Octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37e</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>lsa_par_id</Name>
                <Comment>LSA Parameters and LSA ID</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>lsa_param</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>LSA parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>lsa_id_info</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>LSA ID Information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="28" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the MAC Mode and Channel Coding Requested information element is for the mobile station to indicate which channel coding rate is desired.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.4a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_coding</Name>
                <Comment>MAC Mode And Channel Coding</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mac_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MAC Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cod_scheme</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Coding Scheme</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Measurement Results information element is to provide the results of the measurements made by the mobile station on the serving cell and the neighbour cells.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.20</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>meas_result</Name>
                <Comment>Measurement Results</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ba_used</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BA used</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>dtx_used</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DTX used</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rxlev_full</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RX Level Full Serving Cell</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>meas_valid</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Measurement valid</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rxlev_sub</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RX Level Sub Serving Cell</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rxqual_full</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RX Quality Full Serving Cell</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rxqual_sub</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RX Quality Sub Serving Cell</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>num_ncell</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Number of Cells</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ncell</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[N_CELL_MRES]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Ncell</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Mobile Allocation information element is to provide that part of the RF channels belonging to the cell allocation (coded with a "1" in the cell channel description information element) which is used in the mobile hopping sequence.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>mob_alloc</Name>
                <Comment>Mobile Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>mob_alloc_before</Name>
                <Comment>Mobile Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>mob_alloc_after</Name>
                <Comment>Mobile Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mac</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[1..N_MOB_ALLOC]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Allocation Contents</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Mobile Identity information element is to provide either the international mobile subscriber identity, IMSI, the temporary mobile subscriber identity, TMSI, the international mobile equipment identity, IMEI or the international mobile equipment identity together with the software version number, IMEISV.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.1.4</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>mob_ident</Name>
                <Comment>Mobile Identity</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>mob_ident_2</Name>
                <Comment>Mobile Identity</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ident_type</Name>
                </ItemLink>
                <Control>
                    <CmdSequence>GETPOS,:,4,+,:,1,+,SETPOS</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Type of identity</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>odd_even</Name>
                </ItemLink>
                <Control>
                    <CmdSequence>SETPOS</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Odd/ Even indication</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ident_dig</Name>
                </ItemLink>
                <Type>BCDODD</Type>
                <Control>
                    <TypeModifier>[0..16]</TypeModifier>
                    <Condition>ident_type # ID_TYPE_NO_IDENT AND ident_type # ID_TYPE_TMSI</Condition>
                    <CmdSequence>SETPOS</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Identity digit</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>1111</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <Control>
                    <Condition>ident_type = ID_TYPE_TMSI</Condition>
                    <CmdSequence>:,SETPOS,8,+</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tmsi_1</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[.32]</TypeModifier>
                    <Condition>ident_type = ID_TYPE_TMSI</Condition>
                    <CmdSequence>SETPOS</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TMSI</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>tmsi added</Comment>
            </History>
            <History>
                <Date Day="16" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change name of "imsi" to "imsi_1" to avoid confusion</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">A Mobile Time Difference information element encodes a time related to the synchronization difference between the time bases of two base stations. This type of information is used in conjunction with the HANDOVER COMPLETE message.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>mob_time_diff</Name>
                <Comment>Mobile Time Difference</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>diff</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>time difference</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="2" Month="6" Year="1998"/>
                <Author>LE</Author>
                <Comment>Structure changed</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Multi Block Allocation information element gives parameters related to an EGPRS Packet Uplink Assignment.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.16 (Immediate Asignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>mb_alloc</Name>
                <Version>REL99</Version>
                <Comment>Multi Block Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>Alpha</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gamma</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Gamma</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tbf_start_time</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>TBF Starting Time</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nr_rb</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Number Of Radio Blocks Allocated</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0_bts_prmode</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>P0 BTS PR Mode</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Multi Rate Configuration information element gives all parameters related to a multi-rate speech codec.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21aa</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>multirate_conf</Name>
                <Comment>Multi Rate Configuration</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tlv_len</Name>
                </ItemLink>
                <Type>NO_CODE</Type>
                <SpecRef>-</SpecRef>
                <Comment>Length Information of TLV</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mr_vers</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Multi Rate Speech Version</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nscb</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Noise Suppression Control Bit</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>icmi</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Initial Codec Mode Indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>st_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Start Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>set_amr</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Set of AMR Codec Modes</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <Control>
                    <Condition>tlv_len&gt;2</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cod_prop</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[tlv_len-3..3]</TypeModifier>
                    <Condition>tlv_len&gt;2</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Codec Properties</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <Control>
                    <Condition>tlv_len=4</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <Control>
                    <Condition>tlv_len=5</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>NSCB added</Comment>
            </History>
            <History>
                <Date Day="27" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>revised to support (enable) decoding</Comment>
            </History>
            <History>
                <Date Day="1" Month="8" Year="2002"/>
                <Author>OT</Author>
                <Comment>NO_CODE reinsert - AMR functionality enabled.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Multislot Allocation information element is to provide a description of which channels are used in downlink and uplink respectively, in a multislot configuration.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>multislot_alloc</Name>
                <Comment>Multislot Configuration</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>dab</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Downlink Assignment Bitmap</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>uab</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Uplink Assignment Bitmap</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_set</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..8]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Channel Set Bitmap</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the NC mode information element is to inform the mobile station of the NC mode to be implemented on the target cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21c</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nc_mode</Name>
                <Comment>NC Mode For Target Cell</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ncm</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NC Mode</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.20 (Measurement Results)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ncell</Name>
                <Comment>Ncell</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rx_lev_ncell</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RX Level Ncell</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>bcch_ncell</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BCCH Frequency Ncell</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BSIC Ncell</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nc_meas_para</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>NC Measurement Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nco</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Network control order</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nc_meas_struct</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>NC Measurement struct</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nc_meas_struct</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>NC Measurement struct</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nc_non_drx</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>NC Non DRX period</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nc_rep_i</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>NC reporting period I</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nc_rep_t</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>NC reporting period T</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.23 (P1 Rest Octets), section 10.5.2.24 (P2 Rest Octets),section 10.5.2.25 (P3 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nln_stat</Name>
                <Comment>NLN(PCH) and Status</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nln_pch</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Notification List Number PCH</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nln_status</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Notification List Number Status</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.22c</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nt_rest_oct</Name>
                <Comment>NT/N Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nln_pch</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>NLN(PCH)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gr_call_info</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_GR_C_INFO]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Group Call Information</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>0</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The optional mobile country code is part of LSA parameters in SI4 rest octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>opt_mcc</Name>
                <Comment>Optional MCC</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mcc</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[3]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Country Code</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Optional selection parameters are part of SI3 and SI4 rest octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34, section 10.5.2.35</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>opt_sel_par</Name>
                <Comment>Optional Selection Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_bar_qual</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Cell Bar Qualify</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_resel_offs</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Cell Reselect Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>temp_offs</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Temporary Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>penalty_time</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Penalty Time</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The P0 and BTS Power Control Mode field is part of the packet downlink assignment of IA rest octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>p0_pwr_ctrl_mode</Name>
                <Comment>P0 and BTS Power Control Mode</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>P0</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pwr_ctrl_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BTS Power Control Mode</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.60] section 11.2.29 (Packet Uplink Assignment) 0460-670</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>p0_prmode</Name>
                <Comment>P0 PR Mode</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>P0</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pr_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PR_Mode</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="22" Month="9" Year="2000"/>
                <Author>FRI</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.60] section 11.2.29 (Packet Uplink Assignment) 0460-670</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>p0_bts_prmode</Name>
                <Comment>P0 BTS Power Control PR Mode</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>P0</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pwr_ctrl_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BTS Power Control Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pr_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PR_Mode</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="22" Month="9" Year="2000"/>
                <Author>FRI</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Packet Page Indication field indicates the kind of paging procedure associated with the mobile station identity. The field is implemented as an optional empty composition. Absence of the composition means "paging procedure for RR connection establishment", presence means "packet paging procedure".</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.23 (P1 Rest Octets), section 10.5.2.24 (P2 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pck_page1</Name>
                <Comment>Packet Page Indication 1</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>pck_page2</Name>
                <Comment>Packet Page Indication 2</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>pck_page3</Name>
                <Comment>Packet Page Indication 3</Comment>
            </MsgStructElemDef>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The P1 Rest Octets information element contains information about the status of an existing NCH, priority levels and packet page indications applied for mobile station identities.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.23</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>p1_rest_oct</Name>
                <Comment>P1 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nln_stat</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>NLN(PCH) and Status</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tagged_call_prio</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[2]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Priority 1 and 2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gr_call_info</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Group Call Information</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pck_page1</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Packet Page Indication 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pck_page2</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Packet Page Indication 2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>23</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The P2 Rest Octets information element contains information on the channel needed by the network and information about the status of an existing NCH, priority levels and packet page indications applied for mobile station identities.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.24</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>p2_rest_oct</Name>
                <Comment>P2 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cn3</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Channel Needed for Mobile ID 3</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nln_stat</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>NLN(PCH) and Status</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tagged_call_prio</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[3]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Priority 1 until 3</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pck_page3</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Packet Page Indication 3</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>23</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The P3 Rest Octets information element contains information on the channel needed by the network and information about the status of an existing NCH, priority levels and packet page indications applied for mobile station identities.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.24</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>p3_rest_oct</Name>
                <Comment>P3 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>chan_needed3_4</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Channel Needed for Mobile ID 3 and 4</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nln_stat</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>NLN(PCH) and Status</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tagged_call_prio</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[4]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Priority 1 until 4</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>23</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Packet Channel Description information element is to provide a description of a packet data physical channel (PDCH).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pck_chan_desc</Name>
                <Comment>Packet Channel Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pck_chan_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Packet Channel type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Time Slot</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Training Sequence Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>hop</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Hopping</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>indir</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Indirect</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <Control>
                    <Condition>hop=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=0 AND indir=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Absolute RF Channel Number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=1 OR hop=0 AND indir=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Allocation Index Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ma_num</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=0 AND indir=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>MA Number Indication</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=0 AND indir=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <Control>
                    <Condition>hop=0 AND indir=1 AND flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ch_mark1</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=0 AND indir=1 AND flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Change Mark 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>hsn</Name>
                </ItemLink>
                <Control>
                    <Condition>hop=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Hopping Sequence Number</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="7" Year="2002"/>
                <Author>MPA</Author>
                <Comment>add Spare if Change Mark is not present.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Packet Downlink Assignment IA is part of IA rest octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pck_downl_ass_ia</Name>
                <Comment>Packet Downlink Assignment (IA)</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ded_tlli</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Temporary Logical Link Identifier</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tfi_ass_rlc</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>TFI Assignment and RLC Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ta_idx</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Timing Advance Index</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tbf_start_time</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>TBF Starting Time</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0_bts_prmode</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>P0 BTS PR Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pda_egprs_par</Name>
                </ItemLink>
                <Type>CSN1_SHL_OPT</Type>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>PDA EGPRS Parameters</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="02" Month="05" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>added pda_egprs_par</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The RR Packet Downlink Assignment is sent by the network to the mobile station to indicate the assigned  downlink resources.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25d</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pck_dl_ass</Name>
                <Comment>RR Packet Downlink Assignment</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mac_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MAC Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rlc_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RLC Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ts_all</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Timeslot Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pck_ta</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Packet Timing Advance</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pwr_ctrl</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Power Control Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tfi</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Downlink TFI Assignment</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pck_meas_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Packet Measurement Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00000000</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>0</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>N Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Packet Downlink Assignment EGPRS Parameters are part of IA rest octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.16</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pda_egprs_par</Name>
                <Version>REL99</Version>
                <Comment>PDA EGPRS Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>e_window</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EGPRS Window Size</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>lqm_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>bep_period</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>BEP Period 2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="02" Month="05" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25d (RR Packet Downlink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pck_meas_par</Name>
                <Comment>Packet Measurement Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>meas_start</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Measurement Starting Time</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>meas_int</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Measurement Interval</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>meas_bmp</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Measurement Bitmap</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Packet Timing Advance field describes the timing advance mode and the timing advance value assigned to the mobile station.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.26</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pck_ta</Name>
                <Comment>Packet Timing Advance</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ta</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Timing Advance value</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ta_idx_nm</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Timing Advance Index and Number</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Packet Uplink Assignment IA is part of IA rest octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pck_upl_ass_ia</Name>
                <Comment>Packet Uplink Assignment (IA)</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tfi_ass_alloc</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TFI Assignment and Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>sngl_block_alloc</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Single Block Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t_ext_ra</Name>
                </ItemLink>
                <Type>CSN1_SHL_OPT</Type>
                <SpecRef>-</SpecRef>
                <Comment>Tagged Extended RA</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="2" Year="2002"/>
                <Author>MPA</Author>
                <Comment>add single block assignment</Comment>
            </History>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Add Tagged extended RA</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The RR Packet Uplink Assignment is sent by the network to the mobile station to indicate the assigned  uplink resources.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note: The recommendation is ambiguous: In the definition of IE by CSN1 Timeslot Allocation is omitted, in the description of details it occurs.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pck_ul_ass</Name>
                <Comment>RR Packet Uplink Assignment</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ccm</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Channel Coding Command</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tlli_bcc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TLLI Block Channel Coding</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pck_ta</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Packet Timing Advance</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>dyn_alloc</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0 AND flag1=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Dynamic Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>single_alloc</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Single Block Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>fix_alloc</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND flag1=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Fixed Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00000000</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>0</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>N Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="10" Year="2000"/>
                <Author>FRI</Author>
                <Comment>corrected flag values according to GSM04.08v6.7.0</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Page Mode information element is to control the action of the mobile station belonging to the paging subgroup corresponding to the paging subchannel.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.26</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>page_mode</Name>
                <Comment>Page Mode</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pm</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Page Mode</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b, GSM_04.60 section 11.2.25</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pbcch_des</Name>
                <Comment>PBCCH Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pb</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Pb</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Training Sequence Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Time Slot Number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Flag2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0 AND flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>ARFCN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Allocation Index Offset</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="22" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="7" Month="6" Year="2000"/>
                <Author>CAN</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The PCH and NCH Info is part SI 6 Rest Octets information element.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pch_nch_info</Name>
                <Comment>PCH and NCH Info</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pch_restruct</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Paging Channel Restructuring</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nln_sacch</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Notification List Number SACCH</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>call_prio</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Call Priority</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nln_status</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Notification List Number Status</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [1] section 10.5.2.37a (SI 9 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pos</Name>
                <Comment>Position</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>poso</Name>
                <Comment>Optional Position</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mod</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Modulus</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rel_pos</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[.mod+1..16]</TypeModifier>
                    <Condition>mod#0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Relative Position</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>bcch_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BCCH Type</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [1] section 10.5.2.37a (SI 9 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>poss</Name>
                <Comment>Positions</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pos</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Position</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>poso</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_POS]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Optional Position</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Power Command information element is to provide the power level to be used by the mobile station.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.28</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pow_cmd</Name>
                <Comment>Power Command</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pow</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Power Level</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Power Command and access type information element is to provide the power level to be used by the mobile station and the indication that the mobile station can avoid the transmission of handover access.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.28a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pow_cmd_access</Name>
                <Comment>Power Command &amp; access type</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>atc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Access Type Control</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pow</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Power Level</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Power Control Parameters information element contains parameters the mobile station shall use to determine its TX power level.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment), GSM_04.60 section 12.13</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pwr_ctrl</Name>
                <Comment>Power Control Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Alpha</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tagged_gamma</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[8]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Tagged Gamma</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the RACH Control Parameters information element is to provide parameters used to control the RACH utilization. This information element is broadcast to mobile stations in SYSTEM INFORMATION TYPE 1, 2, 2bis, 3, and 4 messages.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.29</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rach_ctrl</Name>
                <Comment>RACH Control Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>max_retrans</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Maximum Number of Retransmissions</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tx_integer</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Tx-integer</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_bar_access</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Cell Barred for Access</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>re</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Call Reestablishment allowed</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ac</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Access Control Class</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Request Reference information element is to provide the random access information used in the channel request and the frame number, FN modulo 42432 in which the channel request was received.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.30</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>req_ref</Name>
                <Comment>Request Reference</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>req_ref_2</Name>
                <Comment>Request Reference</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>req_ref_3</Name>
                <Comment>Request Reference</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>req_ref_4</Name>
                <Comment>Request Reference</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ra</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Random Access Information</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T1'</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t3</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T3</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Routing Area Identification information element is to provide an unambiguous identification of routing areas within the areas covered by the GSM system.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [1] section 10.5.5.15</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rout_area_id</Name>
                <Comment>Routing Area Identification</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mcc</Name>
                </ItemLink>
                <Type>BCD_NOFILL</Type>
                <Control>
                    <TypeModifier>[3]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Country Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mnc</Name>
                </ItemLink>
                <Type>BCD_MNC</Type>
                <Control>
                    <TypeModifier>[2..3]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Network Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>lac</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Location Area Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rac</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Routing Area Code</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="8" Year="2001"/>
                <Author>HM</Author>
                <Comment>3-digit-MNC</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [1] section 10.5.2.37a (SI 9 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>sched</Name>
                <Comment>Scheduling Info</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>itp</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Info Type and Positions</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>itpo</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_ITP]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Info Type and Positions Optional</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SI 1 Rest Octets information element is coded as followed:</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{SI1 rest octet} ::={ H{NCH Position} | L}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Spare padding}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [1] section 10.5.2.32</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si1_rest_oct</Name>
                <Comment>SI 1 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nch_position</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>NCH Position</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>band_indicator</Name>
                </ItemLink>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <SpecRef>10.5.2.32</SpecRef>
                <Comment>Band Indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="10" Year="1999"/>
                <Author>VK</Author>
                <Comment>Re-introduce rest octets</Comment>
            </History>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>defined as a structure</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SI 2quater Rest Octets information element contains neighbour cell lists for UTRAN cells. For cell reselection, it is used with the SI 2ter Rest Octets information to build the 3G Cell Reselection list, see clause 3.4.1.2.1.7.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : 10.5.2.33b (SI 2quater Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si_2qua_octets</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>SI 2quater Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ba_ind</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BA_ind</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>threeg_ba_ind</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ThreeG BA ind</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mp_change_mark</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MP change mark</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si2qua_index</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SI2quater_index</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si2qua_count</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SI2quater_count</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>meas_para</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Measurement parameter description</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rtdd</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Real Time Difference Description</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gprs_bsic</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS BSIC Description</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gprs_rep_prio</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS REPORT PRIORITY Description</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gprs_meas_para</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>GPRS MEASUREMENT Parameters Description</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nc_meas_para</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>NC Measurement Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si2q_extn_bits</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>SI2 Quater Extension Info</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>meas_para</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Measurement_parameter description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>report_type</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Report type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>serv_band_rep</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Serving band reporting</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_meas_para</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>GPRS MEASUREMENT Parameters Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>report_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Report type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>reporting_rate</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Reporting rate</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>inv_bsic_rep</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Invalid BSIC reporting</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>mr</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>Multiband Reporting</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>serv_band_rep</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>Serving band reporting</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>scale_ord</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Scale ord</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>report_900</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>reporting 900</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>report_1800</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>reporting 1800</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>report_400</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>reporting 400</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>report_1900</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>reporting 1900</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>report_850</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>reporting 850</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>GP</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SI 3 Rest Octets information element is coded as followed:</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{SI3 rest octet} ::={Optional selection parameter}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Optional Power offset}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{System Information 2ter Indicator}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Early Classmark Sending Control}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Scheduling if and where}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{H {GPRS Indicator} | L}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Spare padding}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Optional Selection Parameter} ::= H {Selection Parameter} | L</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Selection Parameter} ::= {CBQ} {CELL_RESELECT_OFFSET}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{TEMPORARY_OFFSET} {PENALTY_TIME}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Optional Power Offset} ::= H {Power Offset} | L</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{System Information 2ter Indicator} ::= H | L</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Early Classmark Sending Control} ::= H | L</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Scheduling if and where ::= {H {where} | L}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">GPRS Indicator ::= {RA color}{SI13 position}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si3_rest_oct</Name>
                <Comment>SI 3 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>opt_sel_par</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Optional Selection Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pow_offs</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Power Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si2ter_ind</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>System Information 2ter Indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>es_ind_tag</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Early Classmark Sending Tag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>if_and_where</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>If And Where</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gprs_indic</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>threeg_es_tag_ind</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>3G Early Classmark Sending Restriction (1 bit field)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si2quater_ind</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>SI2quater Indicator struct</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="27" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Added R99 fields</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SI 4 Rest Octets information element includes parameters which are used by the mobile station for cell reselection purposes. It may also include the POWER OFFSET parameter used by DCS1800 Class 3 MS.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SI 4 Rest Octets information element is coded as followed:</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{SI4 rest octet} ::={Optional selection parameter}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Optional Power offset}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{H {GPRS Indicator} | L}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{SI4 Rest Octets_BS} } ; -- truncation allowed, bits 'L' assumed;</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{SI4 Rest Octets_BS} ::={ </XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{L &lt;Break indicator&gt; | H &lt;SI4 Rest Octets_S&gt;}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">};</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">&lt;SI4 Rest Octets_S&gt; ::= {H {LSA Parameters} | L}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{H {Cell Identity} | L}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{H {LSA ID information} | L} ;</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Optional Selection Parameter} ::= H {Selection Parameter} | L</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Selection Parameter} ::= {CBQ} {CELL_RESELECT_OFFSET}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{TEMPORARY_OFFSET} {PENALTY_TIME}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Optional Power Offset} ::= H {Power Offset} | L</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">GPRS Indicator ::= {RA color}{SI13 position}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{LSA Parameters} ::= {Priority Threshold}{LSA Offset}{EXC_ACC}{Optional MCC}{MNC}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{LSA ID Information} ::= {LSA ID} {0 | 1 {LSA ID Information}}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.18] section 10.5.2.35, 10.5.2.36, 10.5.2.37</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si4_rest_oct</Name>
                <Comment>SI 4 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>opt_sel_par</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Optional selection Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pow_offs</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Power Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gprs_indic</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si4_rest_octets_bs</Name>
                </ItemLink>
                <Type>HL_FLAG</Type>
                <SpecRef>-</SpecRef>
                <Comment>Structure contains Break Indicator &amp; SI4 Rest Octets_S</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef/>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>add spare padding bits</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The HL_FLAG Coding type is associated with the special notations L and H. It is used to denote respectively the bit value corresponding to the padding spare bit for that position, and the other value. HL_FLAG element consists of a single bit only. The decoded value will be 0 if the encoded value is L respectively 1 if the encoded value is H.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si4_rest_octets_bs</Name>
                <Comment>Structured Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <Type>HL_FLAG</Type>
                <SpecRef>-</SpecRef>
                <Comment>HL Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>break_ind</Name>
                </ItemLink>
                <Type>HL_FLAG</Type>
                <Control>
                    <Condition>flag = 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Break Indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si4_rest_octets_s</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>SI4 Rest Octets_S</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="08" Year="2005"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SI 4 Rest Octets_S is coded as followed: &lt;SI4 Rest Octets_S&gt; ::= {L | H &lt;LSA Parameters&gt;} {L | H &lt;Cell Identity : bit(16)&gt;} {L | H &lt;LSA ID information&gt;} ;</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.35</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si4_rest_octets_s</Name>
                <Comment>SI4 Rest Octets_S</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>lsa_param</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>LSA Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cell_ident</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Cell identity</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>lsa_id_info</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>LSA ID Information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="08" Year="2005"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SI 6 Rest Octets information element contains information about the paging, notification channels, VBS and VCGS services of the cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SI 6 Rest Octets information element is coded as followed:</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{SI6 rest octet} ::={H {PCH and NCH info} | L}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{H {VBS/VCGS options} | L}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Spare padding}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{PCH and NCH info} ::= {Paging channel restructuring}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{NLN(SACCH)}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Call priority}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{NLN status}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{VBS/VCGS options} ::= {inband notifications} {inband paging}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si6_rest_oct</Name>
                <Comment>SI 6 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pch_nch_info</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>PCH and NCH Info</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>vbs_vgcs_opt</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>VBS/VGCS Options</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si6_rest_oct_dtm</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <SpecRef>-</SpecRef>
                <Comment>DTM Support Info</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>band_indicator</Name>
                </ItemLink>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <SpecRef>-</SpecRef>
                <Comment>Band Indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>18</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="04" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Added DTM Support and Band Indicator</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SI 7 Rest Octets information element includes parameters which are used by the mobile station for cell selection and reselection purposes. It may also include the POWER OFFSET parameter used by a DCS 1800 Class 3 MS.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si7_rest_oct</Name>
                <Comment>SI 7 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>si8_rest_oct</Name>
                <Comment>SI 8 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>opt_sel_par</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Optional Selection Prameter</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pow_offs</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Power Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gprs_indic</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si4_rest_octets_s</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SI Rest octets S</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="08" Year="2005"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>add spare padding bits</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SI 9 Rest Octets information element contains information about scheduling of some or all of the information on the BCCH.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SI 9 Rest Octets information element is coded as followed:</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{SI9 Rest Octet} ::={H {Scheduling Info} | L}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Spare padding}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Scheduling Info} ::= {Info Type}{Positions}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{0 | 1 {Scheduling Info}}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Info Type} ::=  0{Info Type 4}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">| 10{Info Type 5}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">| 11{Info Type 6}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Positions}  ::=  {Position}{0 | 1 {Positions}}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">{Position}  ::=  {Modulus}{Relative Position}{BCCH Type}</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si9_rest_oct</Name>
                <Comment>SI 9 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>sched</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Scheduling Info</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si13_info</Name>
                <Comment>SI 13 Info</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>bcch_cm</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BCCH Change Mark</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si_cf</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SI Change Field</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si13_cm</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>SI 13 Change Mark</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gprs_ma</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Mobile Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>flag1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rac</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Routing Area Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>spgc</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Split PG Cycle Support</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>prio_acc_thr</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Priority Access Threshold</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nco</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Network Control Order</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gprs_cell_opt</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Cell Options</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Alpha</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t_avg_w</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>T_AVG_W Value</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t_avg_t</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>T_AVG_T Value</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pc_meas_chan</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Power Control Measurement Channel</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>n_avg_i</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>N_AVG_I Value</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>psi1_period</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>PSI1 Repeat Period</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>pbcch_des</Name>
                </ItemLink>
                <Control>
                    <Condition>flag1=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>PBCCH Description</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>sgsnr</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>SGSNR bit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>changed the name to gprs_cell_opt from gprs_opt</Comment>
            </History>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>sgsnr added</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si13_rest_oct</Name>
                <Comment>SI 13 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si13_info</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>SI 13 Info</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SI 16 Rest Octets information element includes parameters which are used by the mobile station for cell selection and reselection purposes.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37d</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si16_rest_oct</Name>
                <Comment>SI 16 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>si17_rest_oct</Name>
                <Comment>SI 17 Rest Octets</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>lsa_par_id</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>LSA Parameters and LSA ID</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="28" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Single Block Allocation information element contains parameter necessary to define the radio resources of a Single Block Allocation. For example for sending of a Packet Resource Request message in a two phase access or a Measurement Report.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>single_alloc</Name>
                <Comment>Single Block Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Timeslot Number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>alpha_gamma</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Alpha Gamma</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0_pwr_ctrl_mode</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>P0 and BTS Power Control Mode</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="10" Year="2000"/>
                <Author>FRI</Author>
                <Comment>Inserted P0andBTS, changed alpha&amp; gamma to alpha_gamma</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Starting Time information element is to provide the start TDMA frame number, FN modulo 42432.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.38</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>start_time</Name>
                <Comment>Starting Time</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>tbf_start_time</Name>
                <Comment>TBF Starting Time</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>meas_start</Name>
                <Comment>Measurement Starting Time</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T1'</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t3</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T3</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>t2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>tbf_start_time and meas_start added</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to indicate inside the SI 3 rest octets the presence of a SYTEM INFORMATION TYPE 2ter message.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si2ter_ind</Name>
                <Comment>system information 2ter indicator</Comment>
            </MsgStructElemDef>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of Synchronization Indication information element is to indicate which type of handover is to be performed.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.39</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>synch_ind</Name>
                <Comment>Synchronization Indication</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>nci</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Normal cell indication</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rot</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Report Observed Time Difference</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Synchronisation indication</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.16 (IA Rest Octets, Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>t_ext_ra</Name>
                <Version>REL99</Version>
                <Comment>Tagged Extended RA</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ext_ra</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>Extended RA</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>tagged_gamma</Name>
                <Comment>Tagged Gamma</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gamma</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Gamma</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.23, section 10.5.2.24, section 10.5.2.25</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>tagged_call_prio</Name>
                <Comment>Tagged Priority</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>call_prio</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>Call Priority</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>tagged_usf_tn</Name>
                <Comment>Tagged USF For Timeslot</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>usf</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Uplink State Flag</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="10" Year="2000"/>
                <Author>FRI</Author>
                <Comment>corrected CSN1 flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Timing Advance information element is to provide the timing advance value.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.40</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>time_advance</Name>
                <Comment>Timing Advance</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>time_advance_2</Name>
                <Comment>Timing Advance</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ta</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Timing advance value</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Timing Advance Index and Number field describes the timing advance mode assigned to the mobile station.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.26 , GSM_08.60 section 12.12 (Packet Timing Advance)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ta_idx_nm</Name>
                <Comment>Timing Advance Index and Number</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ta_idx</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Timing Advance Index</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ta_nm</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Timing Advance Timeslot Number</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The TFI Assignment and Allocation field is part of the packet uplink assignment of IA rest octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>tfi_ass_alloc</Name>
                <Comment>TFI Assignment and Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tfi</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TFI Assignment</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>poll</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Polling</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>allo_flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Allocation flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>usf</Name>
                </ItemLink>
                <Control>
                    <Condition>allo_flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Uplink State Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>usf_gran</Name>
                </ItemLink>
                <Control>
                    <Condition>allo_flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>USF Granularity</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0_prmode</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <Condition>allo_flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>P0 and PR Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>allo_len5</Name>
                </ItemLink>
                <Control>
                    <Condition>allo_flag#0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Allocation Bitmap Length</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>allo_bmp5</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[allo_len5..31]</TypeModifier>
                    <Condition>allo_flag#0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Allocation Bitmap</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0_bts_prmode</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <Condition>allo_flag#0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>P0 BTS PR Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ccm</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Channel Coding Command</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tlli_bcc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TLLI Block Channel Coding</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Alpha</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gamma</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Gamma</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ta_idx</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Timing Advance Index</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tbf_start_time</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>TBF Starting Time</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>CAN</Author>
                <Comment>Allocation Bitmap bit len set to 1</Comment>
            </History>
            <History>
                <Date Day="3" Month="2" Year="2002"/>
                <Author>MPA</Author>
                <Comment>add alpha/gamma/sti/ta_i</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The TFI Assignment and RLC Mode field is part of the packet Downlink assignment of IA rest octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>tfi_ass_rlc</Name>
                <Comment>TFI Assignment and RLC Mode</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tfi</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TFI Assignment</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rlc_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RLC Mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Alpha</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gamma</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Gamma</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>poll</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Polling</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ta_valid</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Timing Advance Valid</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The USF For Timeslot And Gamma field contains an uplink state flag and a gamma value.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>usf_gamma_csn1</Name>
                <Comment>USF For Timeslot And Gamma (CSN1)</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>usf_gamma</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>USF For Timeslot And Gamma</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="23" Month="10" Year="2000"/>
                <Author>FRI</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The USF For Timeslot And Gamma field contains an uplink state flag and a gamma value.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>usf_gamma</Name>
                <Comment>USF For Timeslot And Gamma</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>usf</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Uplink State Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gamma</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Gamma</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="10" Year="2000"/>
                <Author>FRI</Author>
                <Comment>removed CSN1_S1 for usf (s. 5.107)</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The UTRAN frequency list information element provides the mobile station with a list of UTRAN frequencies used by the network. These frequencies may be used in the cell selection procedure.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.1d</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>utran_freq_list</Name>
                <Version>REL99</Version>
                <Comment>UTRAN Freq List</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>length</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Count</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>fdd_arfcn</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_FDD]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>FDD_ARFCN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>tdd_arfcn</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_TDD]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>TDD_ARFCN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>0</CmdSequence>
                </Control>
                <SpecRef/>
                <Comment>Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="02" Month="05" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">VBS/VGCS Options are sent as part of SI6 rest octets.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>vbs_vgcs_opt</Name>
                <Comment>VBS/VGCS Options</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>inband_not</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Inband Notification</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>inband_pag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Inband pagings</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note: The recommendation is ambiguous: In text is explained "... is a type 3 information element with 2 octets length", but in message desciptions and in the desciptions of the IE occurs a length.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.42a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>vgcs_tmi</Name>
                <Comment>VGCS Target Mode Indication</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tm</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Target mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>group_ckn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Group Cipher Key Number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>11</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="28" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Fixed Allocation information element contains parameters necessary to define the radio resources of a fixed allocation.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>fa_blk_ia</Name>
                <Comment>Fixed Allocation Block Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>blp</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Blocks Or Block Periods</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>allo_len7</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Allocation Bitmap Length</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>allo_bmp7</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[allo_len7..127]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Allocation Bitmap</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>CAN</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">XXXThe Fixed Allocation information element contains parameters necessary to define the radio resources of a fixed allocation.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>sngl_block_alloc</Name>
                <Comment>Single Block Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Alpha</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>gamma</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Gamma</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>01</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>tbf_start_time</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TBF Starting Time</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0_bts_prmode</Name>
                </ItemLink>
                <Type>CSN1_SHL</Type>
                <SpecRef>-</SpecRef>
                <Comment>P0 BTS PR Mode</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>CAN</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Classmark Enquiry mask defines the information to be returned to the network. The bit mask defines the specific information to be returned, such as UTRAN specific information and/or CDMA2000 capability and/or requests the sending of the CLASSMARK CHANGE message.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.7c</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>class_enq_mask</Name>
                <Version>REL99</Version>
                <Comment>Classmark enquiry mask</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>class_req</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Classmark change request</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>utran_class_req</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Utran Classmark change request</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>cdma_class_req</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CDMA2000 Classmark change request</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="16" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="04" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Removed REL99 feature flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Extension Bits information element is used to provide a generalized means for possible future extension within a message. This information element is variable length and contains the length indicator and spare bits.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si2q_extn_bits</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>SI 2 Quater Extension Info</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>ext_length</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Extension len</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si2q_extn_info</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[.ext_length+1..256]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>SI 2 Quater Extension Info</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Extension Bits information element is used to provide a generalized means for possible future extension within a message. This information element is variable length and contains the length indicator and spare bits.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si2q_extn_info</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>SI 2 Quater Extension Info</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ccn_support_description</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>CCN Support Desc</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">L Neither UTRAN nor cdma2000 classmark change message shall be sent with the Early classmark sending H The sending of UTRAN and CDMA2000 Classmark Sending messages is controlled by the Early Classmark Sending Control parameter</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>threeg_es_tag_ind</Name>
                <Version>REL99</Version>
                <Comment>3G Early Classmark Sending Restriction (1 bit field)</Comment>
            </MsgStructElemDef>
            <History>
                <Date Day="27" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"> The presence of this field indicates that the SI2quater message is broadcast. </XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si2quater_ind</Name>
                <Version>REL99</Version>
                <Comment>SI2quater Indicator struct</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>si2quater_pos</Name>
                </ItemLink>
                <Version>REL99</Version>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="27" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field consists of parameters for TBF assigned using dynamic allocation.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>d_alloc</Name>
                <Version>REL99</Version>
                <Comment>Dynamic Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>usf</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Uplink State Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>usf_gran</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>USF Granularity</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0_prmode</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>P0 and PR Mode</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field consists of parameters for TBF assigned using fixed allocation.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>f_alloc</Name>
                <Version>REL99</Version>
                <Comment>Fixed Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>allo_len5</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Allocation Bitmap Length</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>allo_bmp5</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[allo_len5..31]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>Allocation Bitmap</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>p0_bts_prmode</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>P0 BTS PR Mode</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <DocLink DocType="OTHER">
                        <Name/>
                    </DocLink>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si6_rest_oct_dtm</Name>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>Structured Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>rac</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>RAC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr</DocName>
                    <Name>max_lapdm</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>MAX LAPDm</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="04" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
    </MsgStructElementsSection>
    <MsgBasicElementsSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all basic elements that are defined for the RR AIM</XHTMLElement>
            </DocElement>
        </Description>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.5 (Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>arfcn</Name>
                <BitLen>10</BitLen>
                <Comment>Absolute RF Channel Number</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The ACCESS_BURST_TYPE field indicates if 8 or 11 bit access burst shall be used on PRACH and in the PACKET CONTROL ACKNOWLEDGMENT message when the format is four access bursts.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets), [GSM_04.60] section 12.24 (GPRS Cell Options)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ab_type</Name>
                <BitLen>1</BitLen>
                <Comment>Access Burst Type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_ab_type</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.1.29 (RACH Control Parameters)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ac</Name>
                <BitLen>16</BitLen>
                <Comment>Access Control Class</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the access technology type to be associated with the following access capabilities</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.16 (Immediate Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>acc_tt</Name>
                <BitLen>4</BitLen>
                <Version>REL99</Version>
                <Comment>Access Technology Type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_acc_tt</Name>
            </ValuesLink>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.28a (Power Command and Access Type)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>atc</Name>
                <BitLen>1</BitLen>
                <Comment>Access Type Control</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_atc</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.1.9 (Descriptive Group Or Broadcast Call Reference), 10.5.2.22c (NT/N Rest octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>af</Name>
                <BitLen>1</BitLen>
                <Comment>Acknowledge Flag</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_af</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Additional reselect parameter indication.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.4 (Cell Selection Parameters)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>acs</Name>
                <BitLen>1</BitLen>
                <Comment>Additional reselect parameter indication</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_acs</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.9 (Cipher Mode Setting)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>algo_ident</Name>
                <BitLen>3</BitLen>
                <Comment>algorithm identifier</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_algo_ident</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Alpha field is used for power output control.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>alpha</Name>
                <BitLen>4</BitLen>
                <Comment>Alpha</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_alpha</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets), section 10.5.2.22c (RR Packet Uplink Assignment), section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>allo_bmp5</Name>
                <BitLen>1</BitLen>
                <Comment>Allocation Bitmap</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>CAN</Author>
                <Comment>bit len set to 1</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets), section 10.5.2.22c (RR Packet Uplink Assignment), section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>allo_bmp6</Name>
                <BitLen>1</BitLen>
                <Comment>Allocation Bitmap</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>CAN</Author>
                <Comment>bit len set to 1</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets), section 10.5.2.22c (RR Packet Uplink Assignment), section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>allo_bmp7</Name>
                <BitLen>1</BitLen>
                <Comment>Allocation Bitmap</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>CAN</Author>
                <Comment>bit len set to 1</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Allocation Bitmap Length describes the length of Allocation Bitmap.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets), section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>allo_len5</Name>
                <BitLen>5</BitLen>
                <Comment>Allocation Bitmap Length</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Allocation Bitmap Length describes the length of Allocation Bitmap.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets), section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>allo_len6</Name>
                <BitLen>6</BitLen>
                <Comment>Allocation Bitmap Length</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Allocation Bitmap Length describes the length of Allocation Bitmap.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets), section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>allo_len7</Name>
                <BitLen>7</BitLen>
                <Comment>Allocation Bitmap Length</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>allo_var</Name>
                <BitLen>1</BitLen>
                <Comment>Allocation Bitmap Var</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="10" Year="2000"/>
                <Author>FRI</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>CAN</Author>
                <Comment>bit len set to 1</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets) [GSM_04.60] section 12.10a (GPRS Mobile Allocation)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>arfcn_idx</Name>
                <BitLen>6</BitLen>
                <Comment>ARFCN Index</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="28" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.11 (Control Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>att</Name>
                <BitLen>1</BitLen>
                <Comment>Attach / detach allowed</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_att</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.18] section 10.5.2.50 (APDU Data) Table 10.5.2.50 APDU Data information element format</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>apdu_info</Name>
                <BitLen>8</BitLen>
                <Comment>APDU Information</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="19" Month="7" Year="2002"/>
                <Author>OTH</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ba_ind</Name>
                <BitLen>1</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>BA_ind</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.20 (Measurement Results)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ba_used</Name>
                <BitLen>1</BitLen>
                <Comment>BA-USED</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.2 (Cell Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bcch_arfcn_hi</Name>
                <BitLen>2</BitLen>
                <Comment>BCCH ARFCN</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="3" Month="2" Year="1998"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.2 (Cell Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bcch_arfcn_lo</Name>
                <BitLen>8</BitLen>
                <Comment>BCCH ARFCN</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="3" Month="2" Year="1998"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the status of the information an the BCCH. The value of this field may be changed when information on BCCH is changed.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37b (SI 13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bcch_cm</Name>
                <BitLen>3</BitLen>
                <Comment>BCCH Change Mark</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.20 (Measurement Result)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bcch_ncell</Name>
                <BitLen>5</BitLen>
                <Comment>BCCH Frequency Ncell</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37a (SI 9 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bcch_type</Name>
                <BitLen>1</BitLen>
                <Comment>BCCH Type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_bcch_type</Name>
            </ValuesLink>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bep_period</Name>
                <BitLen>4</BitLen>
                <Version>REL99</Version>
                <Comment>BEP Period 2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This information field indicates whether the allocation bit map is to be interpreted as blocks or as block periods.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>blp</Name>
                <BitLen>1</BitLen>
                <Comment>Blocks Or Block Periods</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_blp</Name>
            </ValuesLink>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.11 (Control Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bs_ag_blks_res</Name>
                <BitLen>3</BitLen>
                <Comment>BS Access Grant Blocks reserved</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The BCC field is coded as the binary representation of the BS colour code (see TS. GSM 03.03).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.2 (Cell Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bcc</Name>
                <BitLen>3</BitLen>
                <Comment>BS Colour Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">CV - countdown value</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets), [GSM_04.60] section 12.24 (GPRS Cell Options)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bs_cv_max</Name>
                <BitLen>4</BitLen>
                <Comment>BS_CV_MAX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.20 (Measurement Results)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[GSM_04.08] section 9.1.30 (Synchronisation Channel Information)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bsic</Name>
                <BitLen>6</BitLen>
                <Comment>BSIC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.11 (Control Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bs_pa_mfrms</Name>
                <BitLen>3</BitLen>
                <Comment>BS Paging Multiframes</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The  BTS Power Control Mode field indicates the power control mode used by the network as defined in GSM 05.08.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pwr_ctrl_mode</Name>
                <BitLen>1</BitLen>
                <Comment>BTS Power Control Mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_pwr_ctrl_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The C Value field is the C parameter as defined in GSM 05.08.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.20a (GPRS Measurement Results)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>c_val</Name>
                <BitLen>6</BitLen>
                <Comment>C Value</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.1.9 (Descriptive group or broadcast call reference), 10.5.1.11 (Priority level), 10.5.2.23 (P1 rest octets), 10.5.2.24 (P2 rest octets), 10.5.2.25 (P3 rest octets), 10.5.2.35a (SI 6 rest octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>call_prio</Name>
                <BitLen>3</BitLen>
                <Comment>Call Priority</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_call_prio</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.29 (RACH Control Parameters)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>re</Name>
                <BitLen>1</BitLen>
                <Comment>Call Reestablishment allowed</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_re</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to control mobile station cell selection and reselection.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34 (SI3 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cell_bar_qual</Name>
                <BitLen>1</BitLen>
                <Comment>Cell Bar Qualify</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_cell_bar_qual</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.29 (RACH Control Parameters)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cell_bar_access</Name>
                <BitLen>1</BitLen>
                <Comment>Cell Barred for Access</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_cell_bar_access</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Cell Channel Description information element is to provide the reference frequency list to be used to decode the mobile allocation information element. There are several formats for the Cell Channel Description information element, distinguished by the "format indicator" subfield. Some formats are frequency bit maps, the others use a special encoding scheme. NOTE: No more than 64 RF channels should be encoded in the Cell Allocation since this is the maximum number of RF channels which can be referenced in the Mobile Allocation IE.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.1b (Cell Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cell_chan_desc</Name>
                <BitLen>128</BitLen>
                <Comment>Cell Channel Description</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Cell Identity information element is to identify a cell within a location area.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.1.1 (Cell Identity)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cell_ident</Name>
                <BitLen>16</BitLen>
                <Comment>Cell identity</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>length of cell identity is 16 bit</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The usage of this information is defined in TS GSM 05.08.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.4 (Cell Selection Parameters)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cell_resel_hyst</Name>
                <BitLen>3</BitLen>
                <Comment>CELL-RESELECT HYSTERESIS</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_cell_resel_hyst</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used by the mobile station to apply an offset to the value of C2.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34 (SI3 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cell_resel_offs</Name>
                <BitLen>6</BitLen>
                <Comment>Cell Reselect Offset</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is the binary representation of the allowed value of the SI change mark associated with the GPRS mobile allocation to which the MA number refers.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25a (Packet Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ch_mark1</Name>
                <BitLen>2</BitLen>
                <Comment>Change Mark 1</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.5 (Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_type</Name>
                <BitLen>5</BitLen>
                <Comment>Channel type and TDMA offset</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_chan_type</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>added values for channel description 2</Comment>
            </History>
            <History>
                <Date Day="22" Month="6" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Corrected value description for CBCH</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.8 (Channel Needed) (cn1 and cn2),  section 10.5.2.24 (P2 Rest Octets), section 10.5.2.25 (P3 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cn1</Name>
                <BitLen>2</BitLen>
                <Comment>Channel Needed for Mobile ID 1</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_cn1</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>added cn3 and cn4</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.8 (Channel Needed) (cn1 and cn2),  section 10.5.2.24 (P2 Rest Octets), section 10.5.2.25 (P3 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cn2</Name>
                <BitLen>2</BitLen>
                <Comment>Channel Needed for Mobile ID 2</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_cn1</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>added cn3 and cn4</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.8 (Channel Needed) (cn1 and cn2),  section 10.5.2.24 (P2 Rest Octets), section 10.5.2.25 (P3 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cn3</Name>
                <BitLen>2</BitLen>
                <Comment>Channel Needed for Mobile ID 3</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_cn1</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>added cn3 and cn4</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.8 (Channel Needed) (cn1 and cn2),  section 10.5.2.24 (P2 Rest Octets), section 10.5.2.25 (P3 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cn4</Name>
                <BitLen>2</BitLen>
                <Comment>Channel Needed for Mobile ID 4</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_cn1</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>added cn3 and cn4</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Channel Mode information element gives information of the mode on coding/decoding and transcoding. The exact mode is determined by the contents of this IE and the channel type.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.6</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_mode</Name>
                <BitLen>8</BitLen>
                <Comment>Channel Mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_chan_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Add some new 'Values', CM_SPEECH is depreciated -&gt; use CM_SPEECH_VER1 instead</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>added chan_mode2 till chan_mode8</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Channel Mode information element gives information of the mode on coding/decoding and transcoding. The exact mode is determined by the contents of this IE and the channel type.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.6</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_mode2</Name>
                <BitLen>8</BitLen>
                <Comment>Mode Of  2nd Channel Set</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_chan_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Add some new 'Values', CM_SPEECH is depreciated -&amp;gt; use CM_SPEECH_VER1 instead</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>added chan_mode2 till chan_mode8</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Channel Mode information element gives information of the mode on coding/decoding and transcoding. The exact mode is determined by the contents of this IE and the channel type.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.6</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_mode3</Name>
                <BitLen>8</BitLen>
                <Comment>Mode Of  3rd Channel Set</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_chan_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Add some new 'Values', CM_SPEECH is depreciated -&amp;gt; use CM_SPEECH_VER1 instead</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>added chan_mode2 till chan_mode8</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Channel Mode information element gives information of the mode on coding/decoding and transcoding. The exact mode is determined by the contents of this IE and the channel type.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.6</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_mode4</Name>
                <BitLen>8</BitLen>
                <Comment>Mode Of  4th Channel Set</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_chan_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Add some new 'Values', CM_SPEECH is depreciated -&amp;gt; use CM_SPEECH_VER1 instead</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>added chan_mode2 till chan_mode8</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Channel Mode information element gives information of the mode on coding/decoding and transcoding. The exact mode is determined by the contents of this IE and the channel type.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.6</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_mode5</Name>
                <BitLen>8</BitLen>
                <Comment>Mode Of  5th Channel Set</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_chan_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Add some new 'Values', CM_SPEECH is depreciated -&amp;gt; use CM_SPEECH_VER1 instead</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>added chan_mode2 till chan_mode8</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Channel Mode information element gives information of the mode on coding/decoding and transcoding. The exact mode is determined by the contents of this IE and the channel type.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.6</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_mode6</Name>
                <BitLen>8</BitLen>
                <Comment>Mode Of  6th Channel Set</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_chan_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Add some new 'Values', CM_SPEECH is depreciated -&amp;gt; use CM_SPEECH_VER1 instead</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>added chan_mode2 till chan_mode8</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Channel Mode information element gives information of the mode on coding/decoding and transcoding. The exact mode is determined by the contents of this IE and the channel type.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.6</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_mode7</Name>
                <BitLen>8</BitLen>
                <Comment>Mode Of  7th Channel Set</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_chan_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Add some new 'Values', CM_SPEECH is depreciated -&amp;gt; use CM_SPEECH_VER1 instead</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>added chan_mode2 till chan_mode8</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Channel Mode information element gives information of the mode on coding/decoding and transcoding. The exact mode is determined by the contents of this IE and the channel type.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.6</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_mode8</Name>
                <BitLen>8</BitLen>
                <Comment>Mode Of  8th Channel Set</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_chan_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Add some new 'Values', CM_SPEECH is depreciated -&amp;gt; use CM_SPEECH_VER1 instead</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>added chan_mode2 till chan_mode8</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Channel Mode 2 information element gives information of the mode of coding/decoding and transcoding.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_mode_2</Name>
                <BitLen>8</BitLen>
                <Comment>Channel Mode 2</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_chan_mode_2</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Add some new 'Values', CM2_SPEECH_HALF is depreciated -&gt; use CM2_SPEECH_HALF_VER1 instead</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.8a (Channel Request Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>crd_prio</Name>
                <BitLen>2</BitLen>
                <Comment>Channel Request Description Priority</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_crd_prio</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">If bit m of Channel Set Bitmap field n is set to 1 then timeslot m-1 is included in channel set n.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21b (Multislot Allocation)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_set</Name>
                <BitLen>8</BitLen>
                <Comment>Channel Set Bitmap</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.10 (Cipher Response)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cr</Name>
                <BitLen>1</BitLen>
                <Comment>Cipher Response Info</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_cr</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is coded as the binary representation of the hysteresis value associated to the codec  threshold, as defined in GSM 05.09.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21aa (Multirate Configuration)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>codec_hyst</Name>
                <BitLen>4</BitLen>
                <Comment>Codec Hysteresis</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is coded as the binary representation of value N. N corresponds to the threshold of C/I in dB, as defined in GSM 05.09.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21aa (Multirate Configuration)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>codec_thr</Name>
                <BitLen>6</BitLen>
                <Comment>Codec Threshold</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter defines channel coding scheme to be used on the downlink.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.4a (MAC Mode and Channel Coding Requested), section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cod_scheme</Name>
                <BitLen>2</BitLen>
                <Comment>Coding Scheme</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_cod_scheme</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter defines channel coding scheme to be used on the downlink.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.4a (MAC Mode and Channel Coding Requested), section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ccm</Name>
                <BitLen>2</BitLen>
                <Comment>Channel Coding Command</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_cod_scheme</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.18] section 10.5.2.49 (APDU Flags)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>c_r</Name>
                <BitLen>1</BitLen>
                <Comment>Command/Final Response</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_c_r</Name>
            </ValuesLink>
            <History>
                <Date Day="19" Month="7" Year="2002"/>
                <Author>OTH</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.11 (Control Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ccch_conf</Name>
                <BitLen>3</BitLen>
                <Comment>Common Control Channel Configuration</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_ccch_conf</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of the default format of the PACKET CONTROL ACKNOWLEDGMENT message.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets), [GSM_04.60] section 12.24 (GPRS Cell Options)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ctrl_ack_type</Name>
                <BitLen>1</BitLen>
                <Comment>CONTROL_ACK_TYPE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_ctrl_ack_type</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.25b (Dedicated Mode Or TBF)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>d_t</Name>
                <BitLen>1</BitLen>
                <Comment>Dedicated Mode or TBF</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_d_t</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.3 (Cell Options (BCCH))</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dtx_b</Name>
                <BitLen>2</BitLen>
                <Comment>Discontinuous Transmission (BCCH)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_dtx_b</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.3a (Cell Options (SACCH))</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dtx2_s</Name>
                <BitLen>1</BitLen>
                <Comment>Discontinuous Transmission (SACCH) MSB</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note : the DTX indicator sent on the SACCH is split into two parts. The values defined here are applicable for the union of part I and II of the DTX indicator.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.3a (Cell Options (SACCH))</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dtx_s</Name>
                <BitLen>2</BitLen>
                <Comment>Discontinuous Transmission (SACCH) MSB</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_dtx_s</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.20 (Measurement Results)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dtx_used</Name>
                <BitLen>1</BitLen>
                <Comment>DTX USED</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_dtx_used</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.25b (Dedicated Mode Or TBF)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dl</Name>
                <BitLen>1</BitLen>
                <Comment>Downlink Assignment</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_dl</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.21b (Multislot Configuration)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dab</Name>
                <BitLen>7</BitLen>
                <Comment>Downlink Assignment Bitmap</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.21b (Multislot Configuration)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>uab</Name>
                <BitLen>7</BitLen>
                <Comment>Uplink Assignment Bitmap</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of the parameter DRX_TIMER_MAX. Range: 0 to 7. The parameter value is given as two taken to the power of the binary value minus one (2 (bv - 1) in units of 1 second. The binary value zero indicates that non-DRX mode is not supported in the cell. (E.g. the parameter takes the values: 'not supported', 1 s, 2 s, 4 s, .. 64 s.)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets), [GSM_04.60] section 12.24 (GPRS Cell Options)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>drx_t_max</Name>
                <BitLen>3</BitLen>
                <Comment>DRX_TIMER_MAX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>e_window</Name>
                <BitLen>5</BitLen>
                <Version>REL99</Version>
                <Comment>EGPRS Window Size</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_e_window</Name>
            </ValuesLink>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This bits indicates the medium access mode to be used during TBF.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ext_dyn_all</Name>
                <BitLen>1</BitLen>
                <Comment>Extended Dynamic Allocation</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_ext_dyn_all</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Extended Measurement Frequency List information element is to provide the absolute radio frequency channel numbers of carriers to measure signal strength to.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.46</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ext_meas_freq</Name>
                <BitLen>128</BitLen>
                <Comment>Extended Measurement Frequency List</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="28" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Extended RA (5 bit field) is the Extended Random Access information. This is an unformatted 5 bit field, whose content is coded as the 5 least significant bits of the the EGPRS PACKET CHANNEL REQUEST message defined in 3GPP TS 04.60.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.16 (Immediate Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ext_ra</Name>
                <BitLen>5</BitLen>
                <Comment>Extended RA</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="27" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The length of the extension.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.37b (SI13 Rest Octets), [GSM_04.60] section 12.24 (GPRS Cell Options), [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ext_length</Name>
                <BitLen>8</BitLen>
                <Comment>Extension Length2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="22" Month="03" Year="2006"/>
                <Author>xparagu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This bits indicates whether the allocation is the last allocation of the TBF or not.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>final</Name>
                <BitLen>1</BitLen>
                <Comment>Final Allocation</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_final</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.18] section 10.5.2.49 (APDU Flags)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>f_seg</Name>
                <BitLen>1</BitLen>
                <Comment>First segment</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_f_seg</Name>
            </ValuesLink>
            <History>
                <Date Day="19" Month="7" Year="2002"/>
                <Author>OTH</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This bits indicates whether an information is present or not.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>flag</Name>
                <BitLen>1</BitLen>
                <Comment>Flag</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_flag</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This bits indicates whether an information is present or not.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>flag1</Name>
                <BitLen>1</BitLen>
                <Comment>Flag1</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_flag</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This bits indicates whether an information is present or not.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>flag2</Name>
                <BitLen>1</BitLen>
                <Comment>Flag2</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_flag</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This bits indicates whether an information is present or not.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>allo_flag</Name>
                <BitLen>1</BitLen>
                <Comment>Allocation Flag</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_flag</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This bits indicates whether an information is present or not.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>flag_pp</Name>
                <BitLen>1</BitLen>
                <Comment>Flag Parameters Present</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_flag</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This bits indicates whether an information is present or not.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>flag_2bit</Name>
                <BitLen>2</BitLen>
                <Comment>Flag twobit</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Content of a frequency list</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.13</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>flist</Name>
                <BitLen>8</BitLen>
                <Comment>Frequency List Contents</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="8" Month="2" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.1a (BA Range)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>freq_lower</Name>
                <BitLen>10</BitLen>
                <Comment>Frequency Range Lower</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.1a (BA Range)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>freq_higher</Name>
                <BitLen>10</BitLen>
                <Comment>Frequency Range Higher</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Frequency Short List information element is to provide the list of the absolute radio frequency channel numbers used in a frequency hopping sequence, in a small fixed length information element to obtain when possible the HANDOVER COMMAND message in a single block. The Frequency Short List information element is a type 3 information element of 10 octet length. This element is encoded exactly as the Frequency List information element, except that it has a fixed length instead of a variable length and does not contain a length indicator and that it shall not be encoded in bitmap 0 format.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.14</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>freq_short_list_before</Name>
                <BitLen>72</BitLen>
                <Comment>Frequency Short List</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Frequency Short List information element is to provide the list of the absolute radio frequency channel numbers used in a frequency hopping sequence, in a small fixed length information element to obtain when possible the HANDOVER COMMAND message in a single block. The Frequency Short List information element is a type 3 information element of 10 octet length. This element is encoded exactly as the Frequency List information element, except that it has a fixed length instead of a variable length and does not contain a length indicator and that it shall not be encoded in bitmap 0 format.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.14</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>freq_short_list_after</Name>
                <BitLen>72</BitLen>
                <Comment>Frequency Short List</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Frequency Short List information element is to provide the list of the absolute radio frequency channel numbers used in a frequency hopping sequence, in a small fixed length information element to obtain when possible the NOTIFICATION FACCH message in a single block. The Frequency Short List 2 information element is a type 3 information element of 8 octet length. This element is encoded exactly as the Frequency List information element, except that it has a fixed length instead of a variable length and does not contain a length indicator and that it shall not be encoded in bitmap 0 format.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.14a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>freq_short_list2</Name>
                <BitLen>56</BitLen>
                <Comment>Frequency Short List 2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Gamma field is used for power output control in units of 2 dB.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>gamma</Name>
                <BitLen>5</BitLen>
                <Comment>Gamma</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.1.9 (Descriptive Group or Broadcast Call Reference)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>gcr</Name>
                <BitLen>27</BitLen>
                <Comment>Group Call Reference</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Group Cipher Key Number information element is to provide information on the group cipher key to be used for ciphering and deciphering by the mobile station.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.1.10</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>group_ckn</Name>
                <BitLen>4</BitLen>
                <Comment>Group Cipher Key Number</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This information field indicates, for multislot classes 19 to 29, whether the mobile station shall operate in half duplex mode.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>hdm</Name>
                <BitLen>1</BitLen>
                <Comment>Half Duplex Mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_hdm</Name>
            </ValuesLink>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Handover Reference information element is to provide a handover reference value used for access identification.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.15</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>handov_ref</Name>
                <BitLen>8</BitLen>
                <Comment>Handover Reference</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.5 (Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>hop</Name>
                <BitLen>1</BitLen>
                <Comment>Hopping</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_hop</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Swap HOP_NO and HOP_YES</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.5 (Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>hsn</Name>
                <BitLen>6</BitLen>
                <Comment>Hopping Sequence Number</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.1.4 (Mobile Identity)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ident_dig</Name>
                <BitLen>4</BitLen>
                <Comment>Identity digit</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to locate the blocks where SYSTEM INFORMATION TYPE 9 messages are sent</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>if_and_where</Name>
                <BitLen>3</BitLen>
                <Comment>If And Where</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to indicate possible channels for notifications of VBS/VGCS calls.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35a (SI 6 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>inband_not</Name>
                <BitLen>1</BitLen>
                <Comment>Inband Notification</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_inband_not</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to indicate possible channels for paging of point-to-point calls.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35a (SI 6 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>inband_pag</Name>
                <BitLen>1</BitLen>
                <Comment>Inband pagings</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_inband_pag</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The increment skip ARFCN n is coded as the binary representation of the increment of the preceding absolute RF channel number appearing in the sequence of channels used in the frequency hopping: n = 1,...,16.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Range: 0 to 15</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The value 0 indicates that the increment value is 15 but the concerned channel is not used and the next field, i.e. Increment skip ARFCN n+1 (if present) must be added to the increment to determine the next absolute RF channel number in the sequence of channels used in the frequency hopping.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.12 (Frequency Channel Sequence)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>inc_skip</Name>
                <BitLen>4</BitLen>
                <Comment>inc skip of ARFCNn</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25a (Packet Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>indir</Name>
                <BitLen>1</BitLen>
                <Comment>Indirect</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_indir</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">All values indicate unknown, unnecessary information and are reserved for future use</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37a (SI 9 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>it4</Name>
                <BitLen>4</BitLen>
                <Comment>Info Type 4</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">All values indicate unknown, unnecessary information and are reserved for future use</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37a (SI 9 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>it6</Name>
                <BitLen>6</BitLen>
                <Comment>Info Type 6</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37a (SI 9 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>it5</Name>
                <BitLen>5</BitLen>
                <Comment>Info Type 5</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_it5</Name>
            </ValuesLink>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21aa (Multirate Configuration)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>icmi</Name>
                <BitLen>1</BitLen>
                <Comment>Initial Codec Mode Indicator</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_icmi</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>inv_bsic_rep</Name>
                <BitLen>1</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Invalid BSIC reporting</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.1.2 (Ciphering Key Sequence Number)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>key_seq</Name>
                <BitLen>3</BitLen>
                <Comment>key sequence</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_key_seq</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.18] section 10.5.2.49 (APDU Flags)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>l_seg</Name>
                <BitLen>1</BitLen>
                <Comment>Last segment</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_l_seg</Name>
            </ValuesLink>
            <History>
                <Date Day="19" Month="7" Year="2002"/>
                <Author>OTH</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Length specifier for UTRAN frequency list.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>length</Name>
                <BitLen>8</BitLen>
                <Version>REL99</Version>
                <Comment>UTRAN frequency list length</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="02" Month="05" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>fp_len</Name>
                <BitLen>6</BitLen>
                <Comment>Length Of Frequency Parameters</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field determines the measurements to be included within the EGPRS Timeslot Link Quality Measurements IE.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.16 (IA rest octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>lqm_mode</Name>
                <BitLen>2</BitLen>
                <Version>REL99</Version>
                <Comment>Link Quality Measurement Mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_lqm_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="02" Month="05" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.8a (Channel Request Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>llc_fr_type</Name>
                <BitLen>1</BitLen>
                <Comment>LLC Frame Type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_llc_fr_type</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.1.3 (Location Area Identification)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>lac</Name>
                <BitLen>16</BitLen>
                <Comment>Location Area Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The lowest ARFCN field is coded as the binary representation of the lowest absolute RF channel number appearing in the sequence of channels used in the frequency hopping.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.1.12 (Frequency Channel Sequence)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>low_arfcn</Name>
                <BitLen>7</BitLen>
                <Comment>Lowest ARFCN</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_low_arfcn</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to identify the LSA.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35 (SI4 rest octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>lsa_id</Name>
                <BitLen>24</BitLen>
                <Comment>LSA ID</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to identify the LSA.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35 (SI4 rest octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>lsa_id_add</Name>
                <BitLen>24</BitLen>
                <Comment>Additional LSA IDs</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter defines an offset for LSA reselection between cells with same LSA priorities.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35 (SI4 rest octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>lsa_offs</Name>
                <BitLen>3</BitLen>
                <Comment>LSA Offset</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter defines the medium access method to be used during the TBF.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.4a ()MAC Mode and Channel Coding Requested), [GSM_04.60] section 11.2.7 (Packet Downlink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mac_mode</Name>
                <BitLen>2</BitLen>
                <Comment>MAC Mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_mac_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.25a (Packet Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ma_num</Name>
                <BitLen>1</BitLen>
                <Comment>MA Number Indication</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_ma_num</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.1.29 (RACH Control Parameters)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>max_retrans</Name>
                <BitLen>2</BitLen>
                <Comment>Maximum Number of Retransmissions</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_max_retrans</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Measurement Bitmap field indicates the timeslots for use during a measurement periods. A bit set in the field means that the MS shall make measurements during the timeslot, a bit reset means that the MS shall receive downlink data during the timeslot.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.25d (RR Packet Downlink Assignment), [GSM_04.60] section 11.2.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>meas_bmp</Name>
                <BitLen>8</BitLen>
                <Comment>Measurement Bitmap</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Measurement Interval field indicates the number of block periods from the start of one assigned measurement period to the beginning of the next measurement period.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.25d (RR Packet Downlink Assignment), [GSM_04.60] section 11.2.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>meas_int</Name>
                <BitLen>5</BitLen>
                <Comment>Measurement Interval</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.20 (Measurement Results)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>meas_valid</Name>
                <BitLen>1</BitLen>
                <Comment>Measurement valid</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_meas_valid</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.4</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>msg_type</Name>
                <BitLen>8</BitLen>
                <Comment>Message Type</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.21 (Mobile Allocation)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mac</Name>
                <BitLen>8</BitLen>
                <Comment>Mobile Allocation Contents</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.5 (Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>maio</Name>
                <BitLen>6</BitLen>
                <Comment>Mobile Allocation Index Offset</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 9.1.21a (Notification/FACCH), 10.2.22c (NT/N Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ma_len</Name>
                <BitLen>8</BitLen>
                <Comment>Mobile Allocation Length</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="8" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.1.3 (Location Area Identification)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mcc</Name>
                <BitLen>4</BitLen>
                <Comment>Mobile Country Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mcs</Name>
                <BitLen>4</BitLen>
                <Version>REL99</Version>
                <Comment>EGPRS Modulation and coding Scheme</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_mcs</Name>
            </ValuesLink>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.1.3 (Location Area Identification)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mnc</Name>
                <BitLen>4</BitLen>
                <Comment>Mobile Network Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Modulus field encodes the position modulus.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Let M be the encoded value.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">If  M=0, the position modulus is 0,</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">if  M&gt;0, the  position modulus is 2M+1.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37a (SI 9 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mod</Name>
                <BitLen>4</BitLen>
                <Comment>Modulus</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mp_change_mark</Name>
                <BitLen>1</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>MP change mark</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.11 (Control Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mscr</Name>
                <BitLen>1</BitLen>
                <Comment>MSC Release</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_mscr</Name>
            </ValuesLink>
            <History>
                <Date Day="27" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MS-TXPWR-MAX-CCH field is coded as the binary representation of the "power control level" in TS GSM 05.05 corresponding to the maximum TX power level an MS may use when accessing on a Control Channel CCH. This value shall be used by the Mobile Station according to TS GSM 05.08.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.4 (Cell Selection Parameters)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ms_txpwr_max_cch</Name>
                <BitLen>5</BitLen>
                <Comment>MS-TXPWR-MAX-CCH</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.8a (Channel Request Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>or_ty</Name>
                <BitLen>1</BitLen>
                <Comment>MT/MO Origination type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_or_ty</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This element is part of the Structured Element 'Add Multiband', which is not used in this implementation.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.44 (Additional Multiband Information)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mr</Name>
                <BitLen>2</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Multiband Reporting</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21aa (Multirate Configuration)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mr_vers</Name>
                <BitLen>3</BitLen>
                <Comment>Multi Rate Speech Version</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_mr_vers</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets).</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>n_avg_i</Name>
                <BitLen>4</BitLen>
                <Comment>N_AVG_I Value</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>CAN</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21c (NC Mode)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ncm</Name>
                <BitLen>2</BitLen>
                <Comment>NC Mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_ncm</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">his field indicates the minimum time the mobile station shall stay in non-DRX mode after an NC-measurement report has been sent. Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nc_non_drx</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>NC Non DRX period</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_nc_non_drx</Name>
            </ValuesLink>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">These fields indicate the time period for cell reselection measurement reporting for packet idle mode (I) and packet transfer mode (T), respectively.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nc_rep_t</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>NC reporting period T</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_nc_rep_i</Name>
            </ValuesLink>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">These fields indicate the time period for cell reselection measurement reporting for packet idle mode (I) and packet transfer mode (T), respectively.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nc_rep_i</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>NC reporting period I</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_nc_rep_i</Name>
            </ValuesLink>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the NCC Permitted information element is to provide a definition of the allowed NCCs on the BCCH carriers to be reported in the MEASUREMENT REPORT message by the mobile stations in the cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.27</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ncc_permit</Name>
                <BitLen>8</BitLen>
                <Comment>NCC Permitted</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>bit len instead of len</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The values of the NCH position field indicates the block number of the CCCH block which is used for the first NCH block and the number of blocks used for the NCH.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.32 (S1 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nch_position</Name>
                <BitLen>5</BitLen>
                <Comment>NCH Position</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_nch_position</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Neighbour Cells Description information element is to provide the absolute radio frequency channel numbers of the BCCH carriers to be monitored by the mobile stations in the cell.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.22</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>neigh_cell_desc</Name>
                <BitLen>NCELL_DESC_BIT_LEN</BitLen>
                <Comment>Neighbour Cells Description</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>bit len instead of len</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Half rate support.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.4 (Cell Selection Parameters)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>neci</Name>
                <BitLen>1</BitLen>
                <Comment>Half rate support</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_neci</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nco</Name>
                <BitLen>2</BitLen>
                <Comment>Network Control Order</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_nco</Name>
            </ValuesLink>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of the Network Mode of Operation, see GSM 03.60.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets), [GSM_04.60] section 12.24 (GPRS Cell Options)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nmo</Name>
                <BitLen>2</BitLen>
                <Comment>NMO</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_nmo</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.18] section 10.5.2.21aa (MultiRate configuration IEI Indication)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nscb</Name>
                <BitLen>1</BitLen>
                <Comment>Noise Suppression Control Bit</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_nscb</Name>
            </ValuesLink>
            <History>
                <Date Day="23" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The notification list number is a counter modulo 4 for a notification of a new VGCS or VBS call.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 3.3.3.3 (Notification Procedure)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nln_pch</Name>
                <BitLen>2</BitLen>
                <Comment>Notification List Number PCH</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The notification list number is a counter modulo 4 for a notification of a new VGCS or VBS call.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 3.3.3.3 (Notification Procedure)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nln_nch</Name>
                <BitLen>2</BitLen>
                <Comment>Notification List Number NCH</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The notification list number is a counter modulo 4 for a notification of a new VGCS or VBS call.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 3.3.3.3 (Notification Procedure)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nln_sacch</Name>
                <BitLen>2</BitLen>
                <Comment>Notification List Number SACCH</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">A change of the notification list number status indicates a change of information on the NCH which is not related to a new  VGCS or VBS call.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 3.3.3.3 (Notification Procedure)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nln_status</Name>
                <BitLen>1</BitLen>
                <Comment>Notification List Number Status</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.39 (Synchronisation Indication)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nci</Name>
                <BitLen>1</BitLen>
                <Comment>Normal cell indication</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_nci</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The number of Ranges parameter indicates in binary the number of ranges to be transmitted in the BA Range IE. It shall have a minimum value of 1.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.1a (BA Range)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>num_range</Name>
                <BitLen>8</BitLen>
                <Comment>Number of Ranges</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_num_range</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.20 (Measurement Results)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>num_ncell</Name>
                <BitLen>3</BitLen>
                <Comment>Number of Cells</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the number of blocks reserved for uplink transmission.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.16 (Immediate Asignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nr_rb</Name>
                <BitLen>2</BitLen>
                <Version>REL99</Version>
                <Comment>Number of Radio Blocks</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_nr_rb</Name>
            </ValuesLink>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.1.4 (Mobile Identity)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>odd_even</Name>
                <BitLen>1</BitLen>
                <Comment>Odd/ Even indication</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_odd_even</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The P0 field is used to code an optional downlink power control parameter. Its meaning is specific to downlink power control modes A and B. The fields range is 0 to 15, coding 0 dB to 30 dB in steps of 2 dB.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.16 (IA Rest Octets), [GSM_04.60] section 11.2.29 (Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>p0</Name>
                <BitLen>4</BitLen>
                <Comment>P0</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.25a (Packet Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pck_chan_type</Name>
                <BitLen>5</BitLen>
                <Comment>Packet Channel type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_pck_chan_type</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.35a (SI 6 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pch_restruct</Name>
                <BitLen>1</BitLen>
                <Comment>Paging Channel Restructuring</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_pch_restruct</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.26 (Page Mode)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pm</Name>
                <BitLen>2</BitLen>
                <Comment>Page Mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_pm</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets), [GSM_04.60] section 12.24 (GPRS Cell Options)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dec</Name>
                <BitLen>3</BitLen>
                <Comment>PAN_DEC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets), [GSM_04.60] section 12.24 (GPRS Cell Options)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>inc</Name>
                <BitLen>3</BitLen>
                <Comment>PAN_INC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets), [GSM_04.60] section 12.24 (GPRS Cell Options)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pmax</Name>
                <BitLen>3</BitLen>
                <Comment>PAN_MAX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Pb field is used to code an power reduce value used by the BTS on PBCCH blocks, relative to the output power used of the BCCH. The fields range is 0 to 15, coding 0 dB to -30 dB in steps of -2 dB.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets), [GSM_04.60] section 12.9 (Global Power Control Parameters)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pb</Name>
                <BitLen>4</BitLen>
                <Comment>Pb</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets).</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pc_meas_chan</Name>
                <BitLen>1</BitLen>
                <Comment>PC_MEAS_CHAN</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_pc_meas_chan</Name>
            </ValuesLink>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>CAN</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used by the mobile station to apply an offset to the value of C2 during penalty time.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34 (SI3 Rest Octets), section 10.5.2.35 (SI4 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>penalty_time</Name>
                <BitLen>5</BitLen>
                <Comment>Penalty Time</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The NCC field is coded as the binary representation of the PLMN colour code (see TS. GSM 03.03)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.2 (Cell Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ncc</Name>
                <BitLen>3</BitLen>
                <Comment>PLMN Colour Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is in packet uplink assignment and packet downlink assignment of IA Rest Octets. It indicates if the mobile station is polled for a PACKET CONTROL ACKNOWLEDGEMENT.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.16. (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>poll</Name>
                <BitLen>1</BitLen>
                <Comment>Polling</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_poll</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.3 (Cell Options (BCCH))</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[GSM_04.08] section 10.5.2.3a (Cell Options (SACCH))</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pow_ctrl</Name>
                <BitLen>1</BitLen>
                <Comment>Power Control</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_pow_ctrl</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.28 (Power Command)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">: [GSM_04.08] section 10.5.2.28a (Power Command and Access Type)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pow</Name>
                <BitLen>5</BitLen>
                <Comment>Power Level</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used by DCS 1800 Class 3 MSs to add a power offset to the value of MS_TXPWR_MAX_CCH.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34 (SI 3 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pow_offs</Name>
                <BitLen>2</BitLen>
                <Comment>Power Offset</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_pow_offs</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">XXX</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section XXX (XXX)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pr_mode</Name>
                <BitLen>1</BitLen>
                <Comment>PR Mode</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="19" Month="9" Year="2000"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>prio_acc_thr</Name>
                <BitLen>3</BitLen>
                <Comment>Priority Access Threshold</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_prio_acc_thr</Name>
            </ValuesLink>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to determine whether the mobile shall apply prioritized cell re-selection.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35 (SI4 Rest Octets), section 10.5.2.37e (SI16 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>prio_thr</Name>
                <BitLen>3</BitLen>
                <Comment>Priority Threshold</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.18] section 10.5.2.48 (APDU ID)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>protoc_ident</Name>
                <BitLen>4</BitLen>
                <Comment>Protocol Identifier</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_protoc_ident</Name>
            </ValuesLink>
            <History>
                <Date Day="19" Month="7" Year="2002"/>
                <Author>OTH</Author>
                <Comment>Initial - add protocol identifier</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets).</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>psi1_period</Name>
                <BitLen>4</BitLen>
                <Comment>PSI1 Repeat Period</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>CAN</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used by the mobile station to decide whether two cell belong to different routing areas.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34 (SI3 Rest Octets), section 10.5.2.35 (SI4 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ra_color</Name>
                <BitLen>3</BitLen>
                <Comment>RA color</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The precise meaning of RADIO-LINK-TIMEOUT parameter can be found in Technical</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Specification GSM 05.08.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.3 (Cell Options (BCCH))</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[GSM_04.08] section 10.5.2.3a (Cell Options (SACCH))</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rlt</Name>
                <BitLen>4</BitLen>
                <Comment>Radio Link Timeout</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Content of a previous channel request message.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.30 (Request Reference)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ra</Name>
                <BitLen>8</BitLen>
                <Comment>Random Access Information</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The length of this field depends on the value M of Modulus field. It contains a non-negative integer number &lt; 2M+1, if M is greater than 0.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37a (SI 9 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rel_pos</Name>
                <BitLen>16</BitLen>
                <Comment>Relative Position</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="3" Month="5" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>reporting_rate</Name>
                <BitLen>1</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting rate</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.39 (Synchronisation Indication)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rot</Name>
                <BitLen>1</BitLen>
                <Comment>Report Observed Time Difference</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_rot</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>report_type</Name>
                <BitLen>1</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Report type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_report_type</Name>
            </ValuesLink>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The requested bandwidth is the binary encoding of the bit rate information expressed in 100 bit/s, starting from 0*100 bit/s until 65535 * 100 bit/s.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.8a (Channel Request Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rbw</Name>
                <BitLen>16</BitLen>
                <Comment>Requested Bandwidth</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Resegment Bit defines whether retransmitted uplink RLC data blocks shall be re-segmented or not.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>resegm</Name>
                <BitLen>1</BitLen>
                <Version>REL99</Version>
                <Comment>Resegment Bit</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_resegm</Name>
            </ValuesLink>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The ACK field is the binary acknowledge of a successful resumption of GPRS services.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.14c (GPRS Resumption)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>res_ack</Name>
                <BitLen>1</BitLen>
                <Comment>Resumption ACK</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_res_ack</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Reference Frequency List Number field contains a reference frequency.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets) [GSM_04.60] section 12.10a (GPRS Mobile Allocation)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rfln</Name>
                <BitLen>4</BitLen>
                <Comment>RFL Number</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="28" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the number of RLC data blocks the mobile station shall transfer. The number of blocks to transmit is coded as the binary representation of the count minus 9.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rlc_blks</Name>
                <BitLen>8</BitLen>
                <Comment>RLC Data Blocks Granted</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.8a (Channel Request Description), section 10.5.2.16 (IA rest octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rlc_mode</Name>
                <BitLen>1</BitLen>
                <Comment>RLC Mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_rlc_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the number of octets of RLC data the mobile station wishes to transfer.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.8a (Channel Request Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rlc_c_oct</Name>
                <BitLen>16</BitLen>
                <Comment>RLC Octet Count</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="20" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field identifies the routing area.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets), [GSM_03.03]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rac</Name>
                <BitLen>8</BitLen>
                <Comment>Routing Area Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the RR Cause information element is to provide the reason for release or the reason for completion of an assignment or handover.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.31</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rr_cause</Name>
                <BitLen>8</BitLen>
                <Comment>RR Cause</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_rr_cause</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>bit len instead of len</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The RXLEV-ACCESS-MIN field is coded as the binary representation of the minimum received signal level at the MS for which it is permitted to access the system.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.4 (Cell Selection Parameters)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rxlev_access_min</Name>
                <BitLen>6</BitLen>
                <Comment>RX Level Access Minimum</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.20 (Measurement Result)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rxlev_full</Name>
                <BitLen>6</BitLen>
                <Comment>RX Level Full Serving Cell</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.20 (Measurement Result)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rxlev_sub</Name>
                <BitLen>6</BitLen>
                <Comment>RX Level Sub Serving Cell</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.20 (Measurement Result)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rx_lev_ncell</Name>
                <BitLen>6</BitLen>
                <Comment>RX Level Ncell</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.20 (Measurement Result), 10.5.2.20a (GPRS Measurement Result)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rxqual_full</Name>
                <BitLen>3</BitLen>
                <Comment>RX Quality Full Serving Cell</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>rxqual added</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.20 (Measurement Result), 10.5.2.20a (GPRS Measurement Result)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rxqual</Name>
                <BitLen>3</BitLen>
                <Comment>RX Quality</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>rxqual added</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.20 (Measurement Result)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rxqual_sub</Name>
                <BitLen>3</BitLen>
                <Comment>RX Quality Sub Serving Cell</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>scale_ord</Name>
                <BitLen>2</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Scale ord</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_scale_ord</Name>
            </ValuesLink>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Sequence Code Used indicates the value of the SEQ-CODE in the extended measurement frequency list information element used for defining the list of frequencies reported on.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.45 (Extended Measurement Results)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>sc_used</Name>
                <BitLen>1</BitLen>
                <Comment>Sequence Code Used</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="28" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>serv_band_rep</Name>
                <BitLen>2</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Serving band reporting</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.1.9 (Descriptive Group or Broadcast Call Reference)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>sf</Name>
                <BitLen>1</BitLen>
                <Comment>Service Flag</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_sf</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to indicate the presence or absence of codecs of certain rates.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21aa (Multirate Configuration)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>set_amr</Name>
                <BitLen>8</BitLen>
                <Comment>Set of AMR Codec Modes</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_set_amr</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>si2qua_count</Name>
                <BitLen>4</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>SI2quater_count</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>si2qua_index</Name>
                <BitLen>4</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>SI2quater_index</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to indicate version of the release used.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>sgsnr</Name>
                <BitLen>1</BitLen>
                <Version>REL99</Version>
                <Comment>SGSNR Bit</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_sgsnr</Name>
            </ValuesLink>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used to indicate where SYSTEM INFORMATION TYPE 13 is sent.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34 (SI3 Rest Octets), section 10.5.2.35 (SI4 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>si13_pos</Name>
                <BitLen>1</BitLen>
                <Comment>SI13 Position</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_si13_pos</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of the SI change mark identifying the GPRS Mobile Allocation provided in SI13 and PSI13 messages.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>si13_cm</Name>
                <BitLen>2</BitLen>
                <Comment>SI 13 Change Mark</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of which information was changed at the last indication in BCCH Change Mark field.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>si_cf</Name>
                <BitLen>4</BitLen>
                <Comment>SI Change Field</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_si_cf</Name>
            </ValuesLink>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Signal Variance field contains the signal variance parameter calculated by the mobile station as defined in GSM 05.08.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.20a (GPRS Measurement Results)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>sign_var</Name>
                <BitLen>6</BitLen>
                <Comment>Signal Variance</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter defines an offset for LSA reselection between cells with same LSA priorities.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.35 (SI4 Rest Octets), section 10.5.2.37e (SI16 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>solsa_exc_acc</Name>
                <BitLen>1</BitLen>
                <Comment>SoLSA Exclusive Access</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_solsa_exc_acc</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>spgc</Name>
                <BitLen>1</BitLen>
                <Comment>Split PG Cycle Support</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_spgc</Name>
            </ValuesLink>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.9 (Cipher Mode Setting)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>sc</Name>
                <BitLen>1</BitLen>
                <Comment>Start Ciphering</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_sc</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21aa (Multirate Configuration), [GSM_05.09] section 3.4.1</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>st_mode</Name>
                <BitLen>2</BitLen>
                <Comment>Start Mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_st_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Suspension Cause information element is to provide the reason for the establishment of the dedicated circuit which generated the GPRS suspension.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.47 (Suspension Cause)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>susp_cause</Name>
                <BitLen>8</BitLen>
                <Comment>Suspension Cause</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_susp_cause</Name>
            </ValuesLink>
            <History>
                <Date Day="28" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.39 (Synchronisation Indication)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>si</Name>
                <BitLen>2</BitLen>
                <Comment>Synchronisation indication</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_si</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.30 (Request Reference)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t1</Name>
                <BitLen>5</BitLen>
                <Comment>T1'</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.30 (Request Reference)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t2</Name>
                <BitLen>5</BitLen>
                <Comment>T2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.30 (Request Reference)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t3</Name>
                <BitLen>6</BitLen>
                <Comment>T3</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Wait Indication information element is to provide the time the mobile station shall wait before attempting another channel request.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.43</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t3122</Name>
                <BitLen>8</BitLen>
                <Comment>T 3122 Wait Indication</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Wait Indication information element is to provide the time the mobile station shall wait before attempting another channel request.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.43</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t3122_2</Name>
                <BitLen>8</BitLen>
                <Comment>T 3122 Wait Indication</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Wait Indication information element is to provide the time the mobile station shall wait before attempting another channel request.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.43</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t3122_3</Name>
                <BitLen>8</BitLen>
                <Comment>T 3122 Wait Indication</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Wait Indication information element is to provide the time the mobile station shall wait before attempting another channel request.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.43</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t3122_4</Name>
                <BitLen>8</BitLen>
                <Comment>T 3122 Wait Indication</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of the timeout value of timer T3168. Range: 0 to 7. The timeout value is given as the binary value plus one in units of 500 millisecond.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets), [GSM_04.60] section 12.24</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t3168</Name>
                <BitLen>3</BitLen>
                <Comment>T3168</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of the timeout value of timer T3192. Range: 0 to 7. The timeout value is given as the binary value plus one in units of 500 millisecond.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets), [GSM_04.60] section 12.24</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t3192</Name>
                <BitLen>3</BitLen>
                <Comment>T3192</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.11 (Control Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t3212</Name>
                <BitLen>8</BitLen>
                <Comment>T 3212 time-out value</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets).</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t_avg_t</Name>
                <BitLen>5</BitLen>
                <Comment>T_AVG_T Value</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>CAN</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.37b (SI13 Rest Octets).</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t_avg_w</Name>
                <BitLen>5</BitLen>
                <Comment>T_AVG_W Value</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>CAN</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.42a (VGCS Target Mode Indication)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tm</Name>
                <BitLen>2</BitLen>
                <Comment>Target mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_tm</Name>
            </ValuesLink>
            <History>
                <Date Day="28" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The coding of TLLI (temporary logical link identifier) is left to each administration.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA rest Octets), [GSM_03.03]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ded_tlli</Name>
                <BitLen>32</BitLen>
                <Comment>Temporary Logical Link Identifier</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is used by the mobile station to apply an offset to the value of C2 during penalty time.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.34 (SI3 Rest Octets), section 10.5.2.35 (SI4 Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>temp_offs</Name>
                <BitLen>3</BitLen>
                <Comment>Temporary Offset</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="5" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The TFI Assignment field is the binary representation of Temporary Flow Identity.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA rest Octets), [GSM_04.60]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tfi</Name>
                <BitLen>5</BitLen>
                <Comment>TFI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>threeg_ba_ind</Name>
                <BitLen>1</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>ThreeG BA ind</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter defines the mobile observed time difference in half bits.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.21a (Mobile Time Difference)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>diff</Name>
                <BitLen>21</BitLen>
                <Comment>Time difference</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="2" Month="6" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Time Difference information element is to provide information about the synchronization difference between the time bases of two Base Stations. This type of information element is used in relation with the pseudo-synchronization scheme, see TS GSM 05.10.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.41</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>time_diff</Name>
                <BitLen>8</BitLen>
                <Comment>Time Difference</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The TN field is coded as the binary representation of the timeslot number as defined in TS GSM 05.10.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.5 (Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tn</Name>
                <BitLen>3</BitLen>
                <Comment>Time Slot</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>dl_ctrl_tn added</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The TN field is coded as the binary representation of the timeslot number as defined in TS GSM 05.10.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.5 (Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dl_ctrl_tn</Name>
                <BitLen>3</BitLen>
                <Comment>Downlink Control Timeslot</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="27" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>dl_ctrl_tn added</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Timeslot Allocation field indicates whether a timeslot is used in a TBF or an PCCCH or not. A bit set in the field means that the appropriate timeslot is assigned.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ts_all</Name>
                <BitLen>8</BitLen>
                <Comment>Timeslot Allocation</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.16 (IA Rest Octets), section 10.5.2.25c (RR Packet Uplink Assignment), [GSM_04.60] section 12.12 (Packet Timing Advance)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ta_idx</Name>
                <BitLen>4</BitLen>
                <Comment>Timing Advance Index</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.25c (RR Packet Uplink Assignment), [GSM_04.60] section 12.12 (Packet Timing Advance)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ta_nm</Name>
                <BitLen>3</BitLen>
                <Comment>Timing Advance Timeslot Number</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Timing Advance Valid field indicates the validity of the timing advance value given in the Timing Advance IE.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ta_valid</Name>
                <BitLen>1</BitLen>
                <Comment>Timing Advance Valid</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_ta_valid</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.40 (Timing Advance)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ta</Name>
                <BitLen>6</BitLen>
                <Comment>Timing advance value</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter indicates the channel coding to be used for RLC data block comprising TLLI for contention resolution.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA rest Octets), [GSM_03.03]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tlli_bcc</Name>
                <BitLen>1</BitLen>
                <Comment>TLLI Block Channel Coding</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_tlli_bcc</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter contains the length information (L) of a TLV type. This IE does not occure in the air message. It is to set by the CCD caller for ecoding. It will be set by CCD while decoding.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tlv_len</Name>
                <BitLen>16</BitLen>
                <Comment>TLV length information</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="27" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the TMSI information element is to provide the Temporary Mobile Subscriber Identity for paging purposes.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.42</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tmsi_1</Name>
                <BitLen>32</BitLen>
                <Comment>TMSI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="16" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change name of "imsi" to "imsi_1" to avoid confusion</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the TMSI information element is to provide the Temporary Mobile Subscriber Identity for paging purposes.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.42</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tmsi_2</Name>
                <BitLen>32</BitLen>
                <Comment>TMSI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="16" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change name of "imsi" to "imsi_1" to avoid confusion</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the TMSI information element is to provide the Temporary Mobile Subscriber Identity for paging purposes.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.42</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tmsi_3</Name>
                <BitLen>32</BitLen>
                <Comment>TMSI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="16" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change name of "imsi" to "imsi_1" to avoid confusion</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the TMSI information element is to provide the Temporary Mobile Subscriber Identity for paging purposes.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.42</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tmsi_4</Name>
                <BitLen>32</BitLen>
                <Comment>TMSI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="16" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change name of "imsi" to "imsi_1" to avoid confusion</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the TMSI information element is to provide the Temporary Mobile Subscriber Identity for paging purposes.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.42</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ptmsi</Name>
                <BitLen>32</BitLen>
                <Version>REL99</Version>
                <Comment>P_TMSI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="17" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The TSC field is coded as the binary representation of the Training Sequence code as defined in TS GSM 05.03</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.5 (Channel Description)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tsc</Name>
                <BitLen>3</BitLen>
                <Comment>Training Sequence Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.25b (Dedicated Mode Or TBF)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tma</Name>
                <BitLen>1</BitLen>
                <Comment>Two-message Assignment</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_tma</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.2.29 (RACH Control Parameters)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tx_integer</Name>
                <BitLen>4</BitLen>
                <Comment>Tx-integer</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_tx_integer</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.1.4 (Mobile Identity)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ident_type</Name>
                <BitLen>3</BitLen>
                <Comment>Type of identity</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_ident_type</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter is the binary representation of the uplink state flag.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>usf</Name>
                <BitLen>3</BitLen>
                <Comment>Uplink State Flag</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter indicates the USF granularity to be applied by the mobile station when it is assigned a TBF using Dynamic Allocation.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [GSM_04.08] section 10.5.2.16 (IA Rest Octets)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>usf_gran</Name>
                <BitLen>1</BitLen>
                <Comment>USF Granularity</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_usf_gran</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="4" Year="2000"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Break Indicator indicates if parameters in addition to those in SI 4 rest octets are sent in SI7 and SI8  L Additional parameters are not sent in SYSTEM INFORMATION TYPE 7 and 8  H Additional parameters SI4 Rest Octets_S are sent in SYSTEM INFORMATION TYPE 7 and 8</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>break_ind</Name>
                <BitLen>1</BitLen>
                <Comment>Break Indicator</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_break_ind</Name>
            </ValuesLink>
            <History>
                <Date Day="27" Month="01" Year="2005"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.7c (Classmark Enquiry Mask)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>class_req</Name>
                <BitLen>1</BitLen>
                <Version>REL99</Version>
                <Comment>Classmark change request</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_class_req</Name>
            </ValuesLink>
            <History>
                <Date Day="16" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="04" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Removed REL99 feature flag</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.7c (Classmark Enquiry Mask)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>utran_class_req</Name>
                <BitLen>3</BitLen>
                <Version>REL99</Version>
                <Comment>Utran Classmark change request</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_utran_class_req</Name>
            </ValuesLink>
            <History>
                <Date Day="16" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="04" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Removed REL99 feature flag</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.7c (Classmark Enquiry Mask)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cdma_class_req</Name>
                <BitLen>1</BitLen>
                <Version>REL99</Version>
                <Comment>CDMA2000 Classmark change request</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_cdma_class_req</Name>
            </ValuesLink>
            <History>
                <Date Day="16" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="04" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Removed REL99 feature flag</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates where the SYSTEM INFORMATION TYPE 2 quater message is sent:  0 SYSTEM INFORMATION TYPE 2 quater message is sent on BCCH Norm  1 SYSTEM INFORMATION TYPE 2 quater message is sent on BCCH Ext.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>si2quater_pos</Name>
                <BitLen>1</BitLen>
                <Version>REL99</Version>
                <Comment>SI2quater_POSITION </Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="27" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">See 3GPP TS 05.05 for definition of this field. Reference : [2] section 11.2.18</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>band_indicator</Name>
                <BitLen>1</BitLen>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>BAND_INDICATOR</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_band_indicator</Name>
            </ValuesLink>
            <History>
                <Date Day="21" Month="04" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <DocLink DocType="OTHER">
                        <Name/>
                    </DocLink>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>max_lapdm</Name>
                <BitLen>3</BitLen>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>Max LAPDm frames on which a layer 3 can be segmented</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr</DocName>
                <Name>VAL_max_lapdm</Name>
            </ValuesLink>
            <History>
                <Date Day="21" Month="04" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
    </MsgBasicElementsSection>
    <ValuesSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all sets of values that are defined for the RR AIM</XHTMLElement>
            </DocElement>
        </Description>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ab_type</Name>
                <Comment>values for ab_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>AB_8_BIT</Alias>
                <Comment>8 bit access burst shall be used</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>AB_11_BIT</Alias>
                <Comment>11 bit access burst shall be used</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_acc_tt</Name>
                <Version>REL99</Version>
                <Comment>values for acc_tt</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ACC_TT_GSM_P</Alias>
                <Comment>GSM P</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ACC_TT_GSM_E</Alias>
                <Comment>GSM E  --note that GSM E covers GSM P</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>ACC_TT_GSM_R</Alias>
                <Comment>GSM E  --note that GSM R covers GSM E and GSM P</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>ACC_TT_GSM_1800</Alias>
                <Comment>GSM 1800</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>ACC_TT_GSM_1900</Alias>
                <Comment>GSM 1900</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>ACC_TT_GSM_450</Alias>
                <Comment>GSM 450</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>ACC_TT_GSM_480</Alias>
                <Comment>GSM 480</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>ACC_TT_GSM_850</Alias>
                <Comment>GSM 850</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>ACC_TT_GSM_ADD</Alias>
                <Comment>Additional Access Technologies</Comment>
            </ValuesItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_atc</Name>
                <Comment>values for atc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ATC_HANDOV_MAN</Alias>
                <Comment>Sending of Handover access is mandatory</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ATC_HANDOV_OPT</Alias>
                <Comment>Sending of Handover access is optional</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_af</Name>
                <Comment>values for af</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>AF_NO</Alias>
                <Comment>acknowledgement is not required</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>AF_YES</Alias>
                <Comment>acknowledgement is required</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_acs</Name>
                <Comment>values for acs</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ACS_USE_SI4</Alias>
                <Comment>The SI 4 rest octets, if present, shall be used to derive the value of PI and possibly C2 parameters and/or other parameters</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ACS_USE_SI7</Alias>
                <Comment>The value of PI and possibly C2 parameters and/or other parameters in a System information type 7 or type 8 message shall be used</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_algo_ident</Name>
                <Comment>values for algo_ident</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ALGO_A5_1</Alias>
                <Comment>cipher with algorithm A5/1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ALGO_A5_2</Alias>
                <Comment>cipher with algorithm A5/2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>ALGO_A5_3</Alias>
                <Comment>cipher with algorithm A5/3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>ALGO_A5_4</Alias>
                <Comment>cipher with algorithm A5/4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>ALGO_A5_5</Alias>
                <Comment>cipher with algorithm A5/5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>ALGO_A5_6</Alias>
                <Comment>cipher with algorithm A5/6</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>ALGO_A5_7</Alias>
                <Comment>cipher with algorithm A5/7</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_alpha</Name>
                <Comment>values for alpha</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>10</MaxValue>
                <Comment>binary representation of tenth of alpha (measured in dB)</Comment>
            </ValuesRange>
            <ValuesDefault>
                <Comment>Reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_att</Name>
                <Comment>values for att</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CCD_ATT_NO</Alias>
                <Comment>MSs are not allowed to apply IMSI attach and detach procedure.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CCD_ATT_YES</Alias>
                <Comment>MSs in the cell shall apply IMSI attach and detach procedure.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_bcch_type</Name>
                <Comment>values for bcch_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>BCCH_NORM</Alias>
                <Comment>on BCCH Norm</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>BCCH_EXT</Alias>
                <Comment>on BCCH Ext.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_blp</Name>
                <Comment>values for blp</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>BLP_BLK</Alias>
                <Comment>The allocation bitmap is to be interpreted as blocks.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>BLP_PER</Alias>
                <Comment>The allocation bitmap is to be interpreted as block periods.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pwr_ctrl_mode</Name>
                <Comment>values for pwr_ctrl_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PWR_CTR_A</Alias>
                <Comment>mode A</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PWR_CTR_B</Alias>
                <Comment>mode B</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_call_prio</Name>
                <Comment>values for call_prio</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CALL_PRIO_NO</Alias>
                <Comment>no priority applied</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CALL_PRIO_LEV_4</Alias>
                <Comment>call priority level 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CALL_PRIO_LEV_3</Alias>
                <Comment>call priority level 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CALL_PRIO_LEV_2</Alias>
                <Comment>call priority level 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CALL_PRIO_LEV_1</Alias>
                <Comment>call priority level 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>CALL_PRIO_LEV_0</Alias>
                <Comment>call priority level 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>CALL_PRIO_LEV_A</Alias>
                <Comment>call priority level A</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>CALL_PRIO_LEV_B</Alias>
                <Comment>call priority level B</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_re</Name>
                <Comment>values for re</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>REESTAB_YES</Alias>
                <Comment>Call Reestablishment allowed in the cell</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>REESTAB_NO</Alias>
                <Comment>Call Reestablishment not allowed in the cell</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_cell_bar_qual</Name>
                <Comment>values for cell_bar_qual</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CBQ_NO</Alias>
                <Comment>cell selection and reselection depending on cell bar access</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CBQ_YES</Alias>
                <Comment>cell selection priority always low, reselection always normal</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_cell_bar_access</Name>
                <Comment>values for cell_bar_access</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>BARRED_NO</Alias>
                <Comment>The cell is not barred</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>BARRED_YES</Alias>
                <Comment>The cell is barred</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_cell_resel_hyst</Name>
                <Comment>values for cell_resel_hyst</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CELL_HYST_0_DB</Alias>
                <Comment>0 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CELL_HYST_2_DB</Alias>
                <Comment>2 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CELL_HYST_4_DB</Alias>
                <Comment>4 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CELL_HYST_6_DB</Alias>
                <Comment>6 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CELL_HYST_8_DB</Alias>
                <Comment>8 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>CELL_HYST_10_DB</Alias>
                <Comment>10 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>CELL_HYST_12_DB</Alias>
                <Comment>12 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>CELL_HYST_14_DB</Alias>
                <Comment>14 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_chan_type</Name>
                <Comment>values for chan_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>TCH_F</Alias>
                <Comment>TCH/F + ACCHs</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>TCH_H_S0</Alias>
                <Comment>TCH/H + ACCHs, subchannel 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>TCH_H_S1</Alias>
                <Comment>TCH/H + ACCHs, subchannel 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SDCCH_4_S0</Alias>
                <Comment>SDCCH/4 + SDCCH/C4, subchannel 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SDCCH_4_S1</Alias>
                <Comment>SDCCH/4 + SDCCH/C4, subchannel 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>SDCCH_4_S2</Alias>
                <Comment>SDCCH/4 + SDCCH/C4, subchannel 2 or CBCH (SDCCH/4)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>SDCCH_4_S3</Alias>
                <Comment>SDCCH/4 + SDCCH/C4, subchannel 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>SDCCH_8_S0</Alias>
                <Comment>SDCCH/8 + SDCCH/C8, subchannel 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>SDCCH_8_S1</Alias>
                <Comment>SDCCH/8 + SDCCH/C8, subchannel 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>SDCCH_8_S2</Alias>
                <Comment>SDCCH/8 + SDCCH/C8, subchannel 2 or CBCH (SDCCH/8)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>SDCCH_8_S3</Alias>
                <Comment>SDCCH/8 + SDCCH/C8, subchannel 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>SDCCH_8_S4</Alias>
                <Comment>SDCCH/8 + SDCCH/C8, subchannel 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">13</Value>
                <Alias>SDCCH_8_S5</Alias>
                <Comment>SDCCH/8 + SDCCH/C8, subchannel 5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias>SDCCH_8_S6</Alias>
                <Comment>SDCCH/8 + SDCCH/C8, subchannel 6</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>SDCCH_8_S7</Alias>
                <Comment>SDCCH/8 + SDCCH/C8, subchannel 7</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">16</Value>
                <Alias>TCH_F_NO_ADD</Alias>
                <Comment>TCH/F + FACCH/F + SACCH/M, no additional timeslots</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">17</Value>
                <Alias>TCH_F_ADD_BI1</Alias>
                <Comment>TCH/F+ACCHs, additional bidirectional TCH/F/SACCH/M on timeslot n-1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">18</Value>
                <Alias>TCH_F_ADD_BI2</Alias>
                <Comment>TCH/F+ACCHs, additional bidirectional TCH/F/SACCH/M on timeslot n+1, n-1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">19</Value>
                <Alias>TCH_F_ADD_BI3</Alias>
                <Comment>TCH/F+ACCHs, additional bidirectional TCH/F/SACCH/M on timeslot n+1, n-1, n-2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">20</Value>
                <Alias>TCH_F_ADD_BI4</Alias>
                <Comment>TCH/F+ACCHs, additional bidirectional TCH/F/SACCH/M on timeslot n+1, n-1 until n-3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">21</Value>
                <Alias>TCH_F_ADD_BI5</Alias>
                <Comment>TCH/F+ACCHs, additional bidirectional TCH/F/SACCH/M on timeslot n+1, n-1 until n-4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">22</Value>
                <Alias>TCH_F_ADD_BI6</Alias>
                <Comment>TCH/F+ACCHs, additional bidirectional TCH/F/SACCH/M on timeslot n+1, n-1 until n-5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">23</Value>
                <Alias>TCH_F_ADD_BI7</Alias>
                <Comment>TCH/F+ACCHs, additional bidirectional TCH/F/SACCH/M on timeslot n+1, n-1 until n-6</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">24</Value>
                <Alias>TCH_F_ADD_UNI1</Alias>
                <Comment>TCH/F+ACCHs, additional unidirectional TCH/FD/SACCH/MD on timeslot n-1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">25</Value>
                <Alias>TCH_F_ADD_UNI2</Alias>
                <Comment>TCH/F+ACCHs, additional unidirectional TCH/FD/SACCH/MD on timeslot n+1, n-1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">26</Value>
                <Alias>TCH_F_ADD_UNI3</Alias>
                <Comment>TCH/F+ACCHs, additional unidirectional TCH/FD/SACCH/MD on timeslot n+1, n-1 , n-2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">30</Value>
                <Alias>TCH_F_ADD_BI_UNI</Alias>
                <Comment>TCH/F+ACCHs, additional bidirectional TCH/F/SACCH/M and unidirectional TCH/FD/SACCH/MD on timeslot n+1, n-1</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>channel not defined</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_cn1</Name>
                <Comment>values for cn1</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CN_ANY_CHAN</Alias>
                <Comment>Any channel.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CN_SDCCH</Alias>
                <Comment>SDCCH.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CN_TCH_F</Alias>
                <Comment>TCH/F (Full rate).</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CN_TCH</Alias>
                <Comment>TCH/H or TCH/F (Dual rate).</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_chan_mode</Name>
                <Comment>values for chan_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CM_SIG_ONLY</Alias>
                <Comment>signaling only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CM_SPEECH</Alias>
                <Comment>speech (full rate or half rate), version 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias>CM_SPEECH_VER1</Alias>
                <Comment>speech (full rate or half rate), version 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100001</Value>
                <Alias>CM_SPEECH_VER2</Alias>
                <Comment>speech (full rate or half rate), version 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01000001</Value>
                <Alias>CM_SPEECH_VER3</Alias>
                <Comment>speech (full rate or half rate), version 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00001111</Value>
                <Alias>CM_DATA_14_5</Alias>
                <Comment>data, 14.5 kbit/s radio interface rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000011</Value>
                <Alias>CM_DATA_12_0</Alias>
                <Comment>data, 12.0 kbit/s radio interface rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00001011</Value>
                <Alias>CM_DATA_6_0</Alias>
                <Comment>data, 6.0 kbit/s radio interface rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00010011</Value>
                <Alias>CM_DATA_3_6</Alias>
                <Comment>data, 3.6 kbit/s radio interface rate</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved mode</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_chan_mode_2</Name>
                <Comment>values for chan_mode_2</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CM2_SIG_ONLY</Alias>
                <Comment>signaling only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>CM2_SPEECH_HALF</Alias>
                <Comment>speech half rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000101</Value>
                <Alias>CM2_SPEECH_VER1</Alias>
                <Comment>speech (full rate or half rate), version 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100101</Value>
                <Alias>CM2_SPEECH_VER2</Alias>
                <Comment>speech (full rate or half rate), version 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01000101</Value>
                <Alias>CM2_SPEECH_VER3</Alias>
                <Comment>speech (full rate or half rate), version 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00001111</Value>
                <Alias>CM2_DATA_6_0</Alias>
                <Comment>data, 6.0 kbit/s radio interface rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00010111</Value>
                <Alias>CM2_DATA_3_6</Alias>
                <Comment>data, 3.6 kbit/s radio interface rate</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved mode</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_crd_prio</Name>
                <Comment>values for crd_prio</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CRD_PRIO_1</Alias>
                <Comment>priority level 1 (highest priority)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CRD_PRIO_2</Alias>
                <Comment>priority level 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CRD_PRIO_3</Alias>
                <Comment>priority level 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CRD_PRIO_4</Alias>
                <Comment>priority level 4 (lowest priority)</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_cr</Name>
                <Comment>values for cr</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>INC_IMEISV_NO</Alias>
                <Comment>IMEISV shall not be included</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>INC_IMEISV_YES</Alias>
                <Comment>IMEISV shall be included</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_cod_scheme</Name>
                <Comment>values for cod_scheme</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>COD_S_1</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>COD_S_2</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>COD_S_3</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>COD_S_4</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_c_r</Name>
                <Comment>values for c_r</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CMD_FRESP</Alias>
                <Comment>Command or Final Response</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NCMD_FRESP</Alias>
                <Comment>Not Command or Final Response</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ccch_conf</Name>
                <Comment>values for ccch_conf</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CCD_CCCH_1_NOT_COMB</Alias>
                <Comment>1 basic channel used for CCCH, not combined with SDCCHs</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CCD_CCCH_1_COMB</Alias>
                <Comment>1 basic channel used for CCCH, combined with SDCCHs</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CCD_CCCH_2_NOT_COMB</Alias>
                <Comment>2 basic channel used for CCCH, not combined with SDCCHs</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CCD_CCCH_3_NOT_COMB</Alias>
                <Comment>3 basic channel used for CCCH, not combined with SDCCHs</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>CCD_CCCH_4_NOT_COMB</Alias>
                <Comment>4 basic channel used for CCCH, not combined with SDCCHs</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ctrl_ack_type</Name>
                <Comment>values for ctrl_ack_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>default format is four access bursts</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>default format is RLC/MAC control block.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_d_t</Name>
                <Comment>values for d_t</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>D_T_DED</Alias>
                <Comment>the message assigns a resource in dedicated mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>D_T_TBF</Alias>
                <Comment>the message assigns a TBF</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_dtx_b</Name>
                <Comment>values for dtx_b</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>B_DTX_MAY_USE</Alias>
                <Comment>The MSs may use uplink DTX</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>B_DTX_SHALL_USE</Alias>
                <Comment>The MSs shall use uplink DTX</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>B_DTX_DONT_USE</Alias>
                <Comment>The MS shall not use uplink DTX</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>invalid DTX indicator</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_dtx_s</Name>
                <Comment>values for dtx_s</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>S_DTX_F_MAYUSE_H_DONTUSE</Alias>
                <Comment>May use DTX on TCH-F. Don't use DTX on TCH-H.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>S_DTX_F_USE_H_DONTUSE</Alias>
                <Comment>Do use DTX on TCH-F. Don't use DTX on TCH-H.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>S_DTX_F_DONTUSE_H_DONTUSE</Alias>
                <Comment>Don't use DTX on TCH-F. Don't use DTX on TCH-H.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>S_DTX_F_USE_H_MAYUSE</Alias>
                <Comment>Do use DTX on TCH-F. May use DTX on TCH-H.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>S_DTX_F_MAYUSE_H_MAYUSE</Alias>
                <Comment>May use DTX on TCH-F. May use DTX on TCH-H.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>S_DTX_F_USE_H_USE</Alias>
                <Comment>Do use DTX on TCH-F.    Do use DTX on TCH-H.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>S_DTX_F_DONTUSE_H_USE</Alias>
                <Comment>Don't use DTX on TCH-F. Do use DTX on TCH-H.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>S_DTX_F_MAYUSE_H_USE</Alias>
                <Comment>May use DTX on TCH-F. Do use DTX on TCH-H.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_dtx_used</Name>
                <Comment>values for dtx_used</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DTX_USED_NO</Alias>
                <Comment>DTX was not used</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DTX_USED_YES</Alias>
                <Comment>DTX was used</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_dl</Name>
                <Comment>values for dl</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DL_0</Alias>
                <Comment>no meaning</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DL_1</Alias>
                <Comment>the message assigns a resource to the MS identified by the IA rest octets</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_e_window</Name>
                <Version>REL99</Version>
                <Comment>values for e_window</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>E_WIN_64</Alias>
                <Comment>EGPRS Window Size 64</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>E_WIN_96</Alias>
                <Comment>EGPRS Window Size 96</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>E_WIN_128</Alias>
                <Comment>EGPRS Window Size 128</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>E_WIN_160</Alias>
                <Comment>EGPRS Window Size 160</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>E_WIN_192</Alias>
                <Comment>EGPRS Window Size 192 (maximum window size for a 1 timeslot TBF)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>E_WIN_224</Alias>
                <Comment>EGPRS Window Size 224</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>E_WIN_256</Alias>
                <Comment>EGPRS Window Size 256 (maximum window size for a 2 timeslot TBF)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>E_WIN_288</Alias>
                <Comment>EGPRS Window Size 288</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>E_WIN_320</Alias>
                <Comment>EGPRS Window Size 320</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>E_WIN_352</Alias>
                <Comment>EGPRS Window Size 352</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>E_WIN_384</Alias>
                <Comment>EGPRS Window Size 384 (maximum window size for a 3 timeslot TBF)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>E_WIN_416</Alias>
                <Comment>EGPRS Window Size 416</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>E_WIN_448</Alias>
                <Comment>EGPRS Window Size 448</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">13</Value>
                <Alias>E_WIN_480</Alias>
                <Comment>EGPRS Window Size 480</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias>E_WIN_512</Alias>
                <Comment>EGPRS Window Size 512 (maximum window size for a 4 timeslot TBF)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>E_WIN_544</Alias>
                <Comment>EGPRS Window Size 544</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">16</Value>
                <Alias>E_WIN_576</Alias>
                <Comment>EGPRS Window Size 576</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">17</Value>
                <Alias>E_WIN_608</Alias>
                <Comment>EGPRS Window Size 608</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">18</Value>
                <Alias>E_WIN_640</Alias>
                <Comment>EGPRS Window Size 640 (maximum window size for a 5 timeslot TBF)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">19</Value>
                <Alias>E_WIN_672</Alias>
                <Comment>EGPRS Window Size 672</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">20</Value>
                <Alias>E_WIN_704</Alias>
                <Comment>EGPRS Window Size 704</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">21</Value>
                <Alias>E_WIN_736</Alias>
                <Comment>EGPRS Window Size 736</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">22</Value>
                <Alias>E_WIN_768</Alias>
                <Comment>EGPRS Window Size 768 (maximum window size for a 6 timeslot TBF)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">23</Value>
                <Alias>E_WIN_800</Alias>
                <Comment>EGPRS Window Size 800</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">24</Value>
                <Alias>E_WIN_832</Alias>
                <Comment>EGPRS Window Size 832</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">25</Value>
                <Alias>E_WIN_864</Alias>
                <Comment>EGPRS Window Size 864</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">26</Value>
                <Alias>E_WIN_896</Alias>
                <Comment>EGPRS Window Size 896 (maximum window size for a 7 timeslot TBF)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">27</Value>
                <Alias>E_WIN_928</Alias>
                <Comment>EGPRS Window Size 928</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">28</Value>
                <Alias>E_WIN_960</Alias>
                <Comment>EGPRS Window Size 960</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">29</Value>
                <Alias>E_WIN_992</Alias>
                <Comment>EGPRS Window Size 992</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">30</Value>
                <Alias>E_WIN_1024</Alias>
                <Comment>EGPRS Window Size 1024  (maximum window size for a 8 timeslot TBF)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">31</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ext_dyn_all</Name>
                <Comment>values for ext_dyn_all</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EXT_DYN_NO</Alias>
                <Comment>Dynamic Allocation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EXT_DYN_YES</Alias>
                <Comment>Extended Dynamic Allocation</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_final</Name>
                <Comment>values for final</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>FINAL_NO</Alias>
                <Comment>allocation is not the last Allocation of TBF</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>FINAL_YES</Alias>
                <Comment>allocation is the last Allocation of TBF</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_f_seg</Name>
                <Comment>values for f_seg</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>F_SEG</Alias>
                <Comment>First or only segment</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NF_SEG</Alias>
                <Comment>Not first or only segment</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_flag</Name>
                <Comment>values for flag</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PRES_NO</Alias>
                <Comment>information is not present</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PRES_YES</Alias>
                <Comment>information is present</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_hdm</Name>
                <Comment>values for hdm</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>HDM_NO</Alias>
                <Comment>The mobile station shall not  operate in half duplex mode.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>HDM_YES</Alias>
                <Comment>The mobile station shall operate in half duplex mode.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_hop</Name>
                <Comment>values for hop</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>HOP_NO</Alias>
                <Comment>frequency hopping is off</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>HOP_YES</Alias>
                <Comment>frequency hopping is on</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_inband_not</Name>
                <Comment>values for inband_not</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>IN_BAND_NOT_NCH</Alias>
                <Comment>notifications are sent on NCH only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>IN_BAND_NOT_FACCH</Alias>
                <Comment>notifications are sent on FACCH too</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_inband_pag</Name>
                <Comment>values for inband_pag</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>IN_BAND_PAG_PCH</Alias>
                <Comment>pagings are sent on PCH only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>IN_BAND_PAG_FACCH</Alias>
                <Comment>pagings are sent on FACCH too</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_indir</Name>
                <Comment>values for indir</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>INDIR_NO</Alias>
                <Comment>non hopping configuration</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>INDIR_YES</Alias>
                <Comment>indirect encoding of hopping RF channel configuration</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_it5</Name>
                <Comment>values for it5</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>IT5_1</Alias>
                <Comment>System Information Type 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>IT5_2</Alias>
                <Comment>System Information Type 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>IT5_2BIS</Alias>
                <Comment>System Information Type 2bis</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>IT5_2TER</Alias>
                <Comment>System Information Type 2ter</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>IT5_3</Alias>
                <Comment>System Information Type 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>IT5_4</Alias>
                <Comment>System Information Type 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>IT5_7</Alias>
                <Comment>System Information Type 7</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>IT5_8</Alias>
                <Comment>System Information Type 8</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>IT5_9</Alias>
                <Comment>System Information Type 9</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>IT5_13</Alias>
                <Comment>System Information Type 13</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>IT5_14</Alias>
                <Comment>System Information Type 14</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_icmi</Name>
                <Comment>values for icmi</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ICMI_IMPL</Alias>
                <Comment>initial codec mode defined by implicit rule provided in GSM 05.09</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ICMI_START_MODE</Alias>
                <Comment>initial codec mode defined by start mode field</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_key_seq</Name>
                <Comment>values for key_seq</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias/>
                <Comment>No key is available (MS to network); Reserved (network to MS)</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>6</MaxValue>
                <Comment/>
            </ValuesRange>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_l_seg</Name>
                <Comment>values for l_seg</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>L_SEG</Alias>
                <Comment>Last or only segment</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NL_SEG</Alias>
                <Comment>Not last or only segment</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_lqm_mode</Name>
                <Version>REL99</Version>
                <Comment>values for lqm_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>LQM_NOTHING</Alias>
                <Comment>The MS shall not report either interference measurements or per slot BEP measurements</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>LQM_GAMMA</Alias>
                <Comment>The MS shall report available interference measurements</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>LQM_BEP</Alias>
                <Comment>The MS shall report mean BEP on each allocated time slot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>LQM_ALTERNATE</Alias>
                <Comment>The MS shall report mean BEP on each allocated time slot alternating slots 1-3 and 4-7</Comment>
            </ValuesItem>
            <History>
                <Date Day="02" Month="05" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_llc_fr_type</Name>
                <Comment>values for llc_fr_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>LLC_IS_ACK</Alias>
                <Comment>LLC frame is SACK or NACK</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>LLC_NOT_ACK</Alias>
                <Comment>LLC frame is not SACK or NACK</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_low_arfcn</Name>
                <Comment>values for low_arfcn</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>124</MaxValue>
                <Comment/>
            </ValuesRange>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_mac_mode</Name>
                <Comment>values for mac_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MAC_DYN_ALLOC</Alias>
                <Comment>dynamic allocation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MAC_EXT_DYN_ALLOC</Alias>
                <Comment>extended dynamic allocation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MAC_FIX_ALLOC_NOT_HALF</Alias>
                <Comment>fixed allocation, not half duplex mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MAC_FIX_ALLOC</Alias>
                <Comment>fixed allocation, half duplex mode</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ma_num</Name>
                <Comment>values for ma_num</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MA_NUM_14</Alias>
                <Comment>MA_NUMBER = 14</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MA_NUM_15</Alias>
                <Comment>MA_NUMBER = 15</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_max_retrans</Name>
                <Comment>values for max_retrans</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MAX_RETRANS_1</Alias>
                <Comment>Maximum 1 retransmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MAX_RETRANS_2</Alias>
                <Comment>Maximum 2 retransmissions</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MAX_RETRANS_4</Alias>
                <Comment>Maximum 4 retransmissions</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MAX_RETRANS_7</Alias>
                <Comment>Maximum 7 retransmissions</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_meas_valid</Name>
                <Comment>values for meas_valid</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MEAS_VALID_YES</Alias>
                <Comment>The measurement results are valid</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MEAS_VALID_NO</Alias>
                <Comment>the measurement results are not valid</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_mcs</Name>
                <Version>REL99</Version>
                <Comment>values for mcs</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MCS1</Alias>
                <Comment>MCS-1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MCS2</Alias>
                <Comment>MCS-2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MCS3</Alias>
                <Comment>MCS-3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MCS4</Alias>
                <Comment>MCS-4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>MCS5</Alias>
                <Comment>MCS-5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>MCS6</Alias>
                <Comment>MCS-6</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>MCS7</Alias>
                <Comment>MCS-7</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>MCS8</Alias>
                <Comment>MCS-8</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>MCS9</Alias>
                <Comment>MCS-9</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>MCS5_7</Alias>
                <Comment>MCS-5-7</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>MCS6_9</Alias>
                <Comment>MCS-6-9</Comment>
            </ValuesItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_mscr</Name>
                <Comment>Values</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MSCR_98</Alias>
                <Comment>MSC is Release '98 or older</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MSCR_99</Alias>
                <Comment>MSC is Release '99 onwards</Comment>
            </ValuesItem>
            <History>
                <Date Day="27" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_or_ty</Name>
                <Comment>values for or_ty</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>OR_TY_MT</Alias>
                <Comment>Mobile terminated</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>OR_TY_MO</Alias>
                <Comment>Mobile originated</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_mr_vers</Name>
                <Comment>values for mr_vers</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MR_VERS_1</Alias>
                <Comment>Adaptive Multirate speech version 1</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ncm</Name>
                <Comment>values for ncm</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NC_0</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NC_1</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>NC_2</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>NC_TARGET</Alias>
                <Comment>information on NC mode to be gathered from the target cell</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_nc_non_drx</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>values for nc_non_drx</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NC_NO_DRX</Alias>
                <Comment>No non-DRX mode after a measurement report has been sent.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NC_0_24S</Alias>
                <Comment>NC 0.24 s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>NC_0_48S</Alias>
                <Comment>NC 0.48 s (default value)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>NC_0_72S</Alias>
                <Comment>NC 0.72 s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>NC_0_96S</Alias>
                <Comment>NC 0.96 s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>NC_1_20S</Alias>
                <Comment>NC 1.20 s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>NC_1_44S</Alias>
                <Comment>NC 1.44 s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>NC_1_92S</Alias>
                <Comment>NC 1.92 s</Comment>
            </ValuesItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>GP</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_nc_rep_i</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>values for nc_rep_i</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NC_I_0_48S</Alias>
                <Comment>NC 0.48 S</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NC_I_0_96S</Alias>
                <Comment>NC 0.96 s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>NC_I_1_92S</Alias>
                <Comment>NC 1.92 s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>NC_I_3_84S</Alias>
                <Comment>NC 3.84 s (default value for NC_REPORTING_PERIOD_T)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>NC_I_7_68S</Alias>
                <Comment>NC 7.68 s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>NC_I_15_36S</Alias>
                <Comment>NC 15.36 s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>NC_I_30_72S</Alias>
                <Comment>NC 30.72 s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>NC_I_61_44S</Alias>
                <Comment>NC 61.44 s (default value for NC_REPORTING_PERIOD_I)</Comment>
            </ValuesItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_nch_position</Name>
                <Comment>values for nch_position</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NCH_1BLK_NR0</Alias>
                <Comment>1 block / first is block 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NCH_1BLK_NR1</Alias>
                <Comment>1 block / first is block 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>NCH_1BLK_NR2</Alias>
                <Comment>1 block / first is block 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>NCH_1BLK_NR3</Alias>
                <Comment>1 block / first is block 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>NCH_1BLK_NR4</Alias>
                <Comment>1 block / first is block 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>NCH_1BLK_NR5</Alias>
                <Comment>1 block / first is block 5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>NCH_1BLK_NR6</Alias>
                <Comment>1 block / first is block 6</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>NCH_2BLK_NR0</Alias>
                <Comment>2 blocks / first is block 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>NCH_2BLK_NR1</Alias>
                <Comment>2 blocks / first is block 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>NCH_2BLK_NR2</Alias>
                <Comment>2 blocks / first is block 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>NCH_2BLK_NR3</Alias>
                <Comment>2 blocks / first is block 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>NCH_2BLK_NR4</Alias>
                <Comment>2 blocks / first is block 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>NCH_2BLK_NR5</Alias>
                <Comment>2 blocks / first is block 5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">13</Value>
                <Alias>NCH_3BLK_NR0</Alias>
                <Comment>3 blocks / first is block 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias>NCH_3BLK_NR1</Alias>
                <Comment>3 blocks / first is block 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>NCH_3BLK_NR2</Alias>
                <Comment>3 blocks / first is block 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">16</Value>
                <Alias>NCH_3BLK_NR3</Alias>
                <Comment>3 blocks / first is block 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">17</Value>
                <Alias>NCH_3BLK_NR4</Alias>
                <Comment>3 blocks / first is block 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">18</Value>
                <Alias>NCH_4BLK_NR0</Alias>
                <Comment>4 blocks / first is block 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">19</Value>
                <Alias>NCH_4BLK_NR1</Alias>
                <Comment>4 blocks / first is block 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">20</Value>
                <Alias>NCH_4BLK_NR2</Alias>
                <Comment>4 blocks / first is block 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">21</Value>
                <Alias>NCH_4BLK_NR3</Alias>
                <Comment>4 blocks / first is block 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">22</Value>
                <Alias>NCH_5BLK_NR0</Alias>
                <Comment>5 blocks / first is block 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">23</Value>
                <Alias>NCH_5BLK_NR1</Alias>
                <Comment>5 blocks / first is block 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">24</Value>
                <Alias>NCH_5BLK_NR2</Alias>
                <Comment>5 blocks / first is block 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">25</Value>
                <Alias>NCH_6BLK_NR0</Alias>
                <Comment>6 blocks / first is block 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">26</Value>
                <Alias>NCH_6BLK_NR1</Alias>
                <Comment>6 blocks / first is block 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">27</Value>
                <Alias>NCH_7BLK_NR0</Alias>
                <Comment>7 blocks / first is block 0</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_neci</Name>
                <Comment>values for neci</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NECI_NO</Alias>
                <Comment>New establishment causes are not supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NECI_YES</Alias>
                <Comment>New establishment causes are supported</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_nco</Name>
                <Comment>values for nco</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NCO_NO_REP</Alias>
                <Comment>MS controlled cell reselection, no measurement reporting</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NCO_MS_RESEL</Alias>
                <Comment>MS controlled cell reselection, MA sends measurement reports</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>NCO_NET_RESEL</Alias>
                <Comment>Network controlled cell reselection, MA sends measurement reports</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_nmo</Name>
                <Comment>values for nmo</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias/>
                <Comment>Network Mode 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias/>
                <Comment>Network Mode 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10</Value>
                <Alias/>
                <Comment>Network Mode 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_nscb</Name>
                <Comment>values for nscb</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NSCB_ON</Alias>
                <Comment>NSCB can be used (default)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NSCB_OFF</Alias>
                <Comment>NSCB shall be turned off</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_nci</Name>
                <Comment>values for nci</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NCI_IGNORE</Alias>
                <Comment>Out of range timing advance is ignored</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NCI_TRIGGER</Alias>
                <Comment>Out of range timing advance shall trigger a handover failure</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_num_range</Name>
                <Comment>values for num_range</Comment>
            </ValuesDef>
            <ValuesRange ValueType="ALPHA">
                <MinValue>1</MinValue>
                <MaxValue>N_MAX_RANGE</MaxValue>
                <Comment>number of frequency ranges</Comment>
            </ValuesRange>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_nr_rb</Name>
                <Version>REL99</Version>
                <Comment>values for nr_rb</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NR_RB_1</Alias>
                <Comment>1 radio block reserved for uplink transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NR_RB_2</Alias>
                <Comment>2 radio blocks reserved for uplink transmission</Comment>
            </ValuesItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_odd_even</Name>
                <Comment>values for odd_even</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EVEN</Alias>
                <Comment>even</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ODD</Alias>
                <Comment>odd</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pck_chan_type</Name>
                <Comment>values for pck_chan_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PCK_CH_1</Alias>
                <Comment>for backward compatibility</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pch_restruct</Name>
                <Comment>values for pch_restruct</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PCH_RESTRUCT_NO</Alias>
                <Comment>paging channel is restructured</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PCH_RESTRUCT_YES</Alias>
                <Comment>paging channel is not restructured</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pm</Name>
                <Comment>values for pm</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PAGING_NORM</Alias>
                <Comment>Normal paging.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PAGING_EXT</Alias>
                <Comment>Extended paging.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PAGING_REORG</Alias>
                <Comment>Paging reorganization.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>PAGING_SAME</Alias>
                <Comment>Same as before.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pc_meas_chan</Name>
                <Comment>values for pc_meas_chan</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PC_MEAS_BCCH</Alias>
                <Comment>BCCH shall be used for downlink measurements for power control</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PC_MEAS_PDCH</Alias>
                <Comment>PDCH shall be used for downlink measurements for power control</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_poll</Name>
                <Comment>values for poll</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>POLL_NO_ACTION</Alias>
                <Comment>no action required from MS</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>POLL_SEND_ACK</Alias>
                <Comment>MS shall send a PACKET CONTROL ACKNOWLEDGEMENT</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pow_ctrl</Name>
                <Comment>values for pow_ctrl</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>POW_CTRL_NO</Alias>
                <Comment>PWRC is not set</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>POW_CTRL_YES</Alias>
                <Comment>PWRC is set</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pow_offs</Name>
                <Comment>values for pow_offs</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>POW_OFFS_0_DB</Alias>
                <Comment>offset 0 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>POW_OFFS_2_DB</Alias>
                <Comment>offset 2 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>POW_OFFS_4_DB</Alias>
                <Comment>offset 4 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>POW_OFFS_6_DB</Alias>
                <Comment>offset 6 dB</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_prio_acc_thr</Name>
                <Comment>values for prio_acc_thr</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PAT_NO</Alias>
                <Comment>Packet access not allowed in the cell</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PAT_SPARE1</Alias>
                <Comment>Spare, shall be interpreted as 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PAT_SPARE2</Alias>
                <Comment>Spare, shall be interpreted as 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>PAT_ACC1</Alias>
                <Comment>packet access allowed for priority level 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>PAT_ACC2</Alias>
                <Comment>packet access allowed for priority level 1 to 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>PAT_ACC3</Alias>
                <Comment>packet access allowed for priority level 1 to 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>PAT_ACC4</Alias>
                <Comment>packet access allowed for priority level 1 to 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>PAT_SPARE6</Alias>
                <Comment>Spare, shall be interpreted as 6</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_protoc_ident</Name>
                <Comment>values for protoc_ident</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>RRLP_LCS</Alias>
                <Comment>Radio Resource Location Service Protocol</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_reporting_rate</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>values for reporting_rate</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NORMAL_RATE</Alias>
                <Comment>Normal reporting rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>REDUCED_RATE</Alias>
                <Comment>Reduced reporting rate</Comment>
            </ValuesItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>GP</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rot</Name>
                <Comment>values for rot</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TIME_DIFF_NO</Alias>
                <Comment>Mobile Time Difference IE shall not be included in the HANDOVER COMPLETE message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>TIME_DIFF_YES</Alias>
                <Comment>Mobile Time Difference IE shall be included in the HANDOVER COMPLETE message</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_report_type</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>values for report_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ENHANCED_MEAS</Alias>
                <Comment>The MS shall use the Enhanced Measurement Report message for reporting if at least one BSIC is allocated to each BA (list) frequency. Otherwise, the Measurement Report message shall be used.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NORMAL_MEAS</Alias>
                <Comment>The MS shall use the Measurement Report message for reporting.</Comment>
            </ValuesItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_resegm</Name>
                <Version>REL99</Version>
                <Comment>values for resegm</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>RESEGM_NO</Alias>
                <Comment>Retransmitted RLC data blocks shall not be re-segmented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>RESEGM_YES</Alias>
                <Comment>Retransmitted RLC data blocks shall be re-segmented according to commanded MCS</Comment>
            </ValuesItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_res_ack</Name>
                <Comment>values for res_ack</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>RES_ACK_NO</Alias>
                <Comment>resumption of GPRS services not successfully acknowledged</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>RES_ACK_YES</Alias>
                <Comment>resumption of GPRS services successfully acknowledged</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rlc_mode</Name>
                <Comment>values for rlc_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>RLC_ACK_MODE</Alias>
                <Comment>RLC acknowledged mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>RLC_UNACK_MODE</Alias>
                <Comment>RLC unacknowledged mode</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rr_cause</Name>
                <Comment>values for rr_cause</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>RRC_NORMAL_EVENT</Alias>
                <Comment>Normal event</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias>RRC_UNSPECIFIED</Alias>
                <Comment>Abnormal release, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000010</Value>
                <Alias>RRC_CHAN_UNACCEPT</Alias>
                <Comment>Abnormal release, channel unacceptable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000011</Value>
                <Alias>RRC_TIMER_EXPIRED</Alias>
                <Comment>Abnormal release, timer expired</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000100</Value>
                <Alias>RRC_NO_ACTIVITY</Alias>
                <Comment>Abnormal release, no activity on the radio path</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000101</Value>
                <Alias>RRC_PREEMEPT</Alias>
                <Comment>Preemptive release</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00001000</Value>
                <Alias>RRC_TIME_ADVANCE</Alias>
                <Comment>Handover impossible, timing advance out of range</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00001001</Value>
                <Alias>RRC_CHANNEL_MODE</Alias>
                <Comment>Channel mode unacceptable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00001010</Value>
                <Alias>RRC_FREQ_NOT_IMPL</Alias>
                <Comment>Frequency not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00001100</Value>
                <Alias>RRC_LOWER_LAYER_FAIL</Alias>
                <Version>REL99 AND FF_BHO</Version>
                <Comment>Lower layer failure</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01000001</Value>
                <Alias>RRC_CALL_CLEARED</Alias>
                <Comment>Call already cleared</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01011111</Value>
                <Alias>RRC_INCORRECT_MSG</Alias>
                <Comment>Semantically incorrect message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01100000</Value>
                <Alias>RRC_INVALID_MAN_INFO</Alias>
                <Comment>Invalid mandatory information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01100001</Value>
                <Alias>RRC_MSG_NOT_IMPL</Alias>
                <Comment>Message type non-existent or not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01100010</Value>
                <Alias>RRC_MSG_NOT_COMPAT</Alias>
                <Comment>Message type not compatible with protocol state</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01100100</Value>
                <Alias>RRC_COND_IE_ERROR</Alias>
                <Comment>Conditional IE error</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01100101</Value>
                <Alias>RRC_NO_CELL_ALLOC</Alias>
                <Comment>No cell allocation available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01101111</Value>
                <Alias>RRC_PROT_UNSPECIFIED</Alias>
                <Comment>Protocol error unspecified</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_scale_ord</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>values for scale_ord</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SC_ORD_ZERO_DB</Alias>
                <Comment>0 dB offset, which shall be used for the reported RXLEV values</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SC_ORD_TEN_DB</Alias>
                <Comment>+10 dB offset, which shall be used for the reported RXLEV values</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SC_ORD_AUTOMATIC</Alias>
                <Comment>automatic offset, which shall be used for the reported RXLEV values</Comment>
            </ValuesItem>
            <History>
                <Date Day="21" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_sf</Name>
                <Comment>values for sf</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SF_VBS</Alias>
                <Comment>broadcast call reference</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SF_VGCS</Alias>
                <Comment>group call reference</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_set_amr</Name>
                <Comment>values for set_amr</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">80</Value>
                <Alias>SET_AMR_12_2</Alias>
                <Comment>codec 12.2 kbit/s is part of subset</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">40</Value>
                <Alias>SET_AMR_10_2</Alias>
                <Comment>codec 10.2 kbit/s is part of subset</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">20</Value>
                <Alias>SET_AMR_7_95</Alias>
                <Comment>codec 7.95 kbit/s is part of subset</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">10</Value>
                <Alias>SET_AMR_7_4</Alias>
                <Comment>codec 7.4 kbit/s is part of subset</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">08</Value>
                <Alias>SET_AMR_6_7</Alias>
                <Comment>codec 6.7 kbit/s is part of subset</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>SET_AMR_5_9</Alias>
                <Comment>codec 5.9 kbit/s is part of subset</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>SET_AMR_5_15</Alias>
                <Comment>codec 5.15 kbit/s is part of subset</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>SET_AMR_4_75</Alias>
                <Comment>codec 4 .75 kbit/s is part of subset</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_sgsnr</Name>
                <Version>REL99</Version>
                <Comment>values for sgsnr</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SGSNR_98</Alias>
                <Comment>SGSN is Release '98 or older</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SGSNR_99</Alias>
                <Comment>SGSN is Release '99 onwards</Comment>
            </ValuesItem>
            <History>
                <Date Day="28" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_si13_pos</Name>
                <Comment>values for si13_pos</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SI13_ON_BCCH_NORM</Alias>
                <Comment>on BCCH Norm</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SI13_ON_BCCH_EXT</Alias>
                <Comment>on BCCH Ext.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_si_cf</Name>
                <Comment>values for si_cf</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SI_CF_UNSPEC</Alias>
                <Comment>Update of unspecified SI message(s)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SI_CF_1</Alias>
                <Comment>Update of SI1 message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SI_CF_2X</Alias>
                <Comment>Update of SI2, SI2bis or SI2ter message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SI_CF_3UNTIL8</Alias>
                <Comment>Update of SI3, SI4, SI7 or SI8 message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SI_CF_9</Alias>
                <Comment>Update of SI9 message</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Update of unknown SI message type</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_solsa_exc_acc</Name>
                <Comment>values for solsa_exc_acc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SOLSA_EXCLUSIVE_NO</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SOLSA_EXCLUSIVE_YES</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_spgc</Name>
                <Comment>values for spgc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SPGC_NO</Alias>
                <Comment>SPLIT_PG_CYCLE is not supported on CCCH in this cell</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SPGC_YES</Alias>
                <Comment>SPLIT_PG_CYCLE is supported on CCCH in this cell</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_sc</Name>
                <Comment>values for sc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>START_CIPH_NO</Alias>
                <Comment>No ciphering</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>START_CIPH_YES</Alias>
                <Comment>Start ciphering</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_st_mode</Name>
                <Comment>values for st_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CODEC_MODE_1</Alias>
                <Comment>lowest bit rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CODEC_MODE_2</Alias>
                <Comment>second lowest rate if codec includes more then 1 mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CODEC_MODE_3</Alias>
                <Comment>third lowest rate if codec includes more then 2 modes</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CODEC_MODE_4</Alias>
                <Comment>highest mode if codec includes 4 modes</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_susp_cause</Name>
                <Comment>values for susp_cause</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SUSP_C_CALL</Alias>
                <Comment>Mobile originated or mobile terminated call</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SUSP_C_LU</Alias>
                <Comment>Location Update</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SUSP_C_SMS</Alias>
                <Comment>Short message service</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SUSP_C_SS</Alias>
                <Comment>Supplementary service activation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SUSP_C_VBS</Alias>
                <Comment>Voice broadcast or group call</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SUSP_C_MT_CALL</Alias>
                <Comment>Mobile terminated call</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>SUSP_C_DTM</Alias>
                <Comment>DTM not supported</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>shall be treated as 0</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_si</Name>
                <Comment>values for si</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SYI_NON_SYNCH</Alias>
                <Comment>Non-synchronized</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SYI_NORM_SYNCH</Alias>
                <Comment>Synchronized</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SYI_PRE_SYNCH</Alias>
                <Comment>Pre-synchronised</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SYI_PSEUDO_SYNCH</Alias>
                <Comment>Pseudo-synchronised</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_tm</Name>
                <Comment>values for tm</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TM_DED</Alias>
                <Comment>dedicated mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>TM_GROUP</Alias>
                <Comment>group transmit mode</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_threeg_prio</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>values for threeg_prio</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NO_SEACH</Alias>
                <Comment>Seach not allowed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>YES_SEACH</Alias>
                <Comment>Seach allowed</Comment>
            </ValuesItem>
            <History>
                <Date Day="22" Month="03" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ta_valid</Name>
                <Comment>values for ta_valid</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TA_VALID_NO</Alias>
                <Comment>the value is not valid</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>TA_VALID_YES</Alias>
                <Comment>the value is valid</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_tlli_bcc</Name>
                <Comment>values for tlli_bcc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TLLI_BCC1</Alias>
                <Comment>mobile station shall use CS-1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>TLLI_BCC_CODED</Alias>
                <Comment>mobile station shall use CS specified by Channel Coding</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_tma</Name>
                <Comment>values for tma</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TMA_0</Alias>
                <Comment>no meaning</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>TMA_1</Alias>
                <Comment>the message is the first of two in a two message assignment</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_tx_integer</Name>
                <Comment>values for tx_integer</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SPREAD_TRANS_3</Alias>
                <Comment>3 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SPREAD_TRANS_4</Alias>
                <Comment>4 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SPREAD_TRANS_5</Alias>
                <Comment>5 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SPREAD_TRANS_6</Alias>
                <Comment>6 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SPREAD_TRANS_7</Alias>
                <Comment>7 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SPREAD_TRANS_8</Alias>
                <Comment>8 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>SPREAD_TRANS_9</Alias>
                <Comment>9 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>SPREAD_TRANS_10</Alias>
                <Comment>10 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>SPREAD_TRANS_11</Alias>
                <Comment>11 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>SPREAD_TRANS_12</Alias>
                <Comment>12 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>SPREAD_TRANS_14</Alias>
                <Comment>14slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>SPREAD_TRANS_16</Alias>
                <Comment>16 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>SPREAD_TRANS_20</Alias>
                <Comment>20 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">13</Value>
                <Alias>SPREAD_TRANS_25</Alias>
                <Comment>25 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias>SPREAD_TRANS_32</Alias>
                <Comment>32 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>SPREAD_TRANS_50</Alias>
                <Comment>50 slots used to spread transmission</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ident_type</Name>
                <Comment>values for ident_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ID_TYPE_NO_IDENT</Alias>
                <Comment>No Identity</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ID_TYPE_IMSI</Alias>
                <Comment>IMSI</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>ID_TYPE_IMEI</Alias>
                <Comment>IMEI</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>ID_TYPE_IMEISV</Alias>
                <Comment>IMEISV</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>ID_TYPE_TMSI</Alias>
                <Comment>TMSI</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_usf_gran</Name>
                <Comment>values for usf_gran</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>USF_GRAN1</Alias>
                <Comment>the mobile shall send one RLC/MAC block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>USF_GRAN4</Alias>
                <Comment>the mobile shall send four consecutive RLC/MAC blocks</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Break Indicator indicates if parameters in addition to those in SI 4 rest octets are sent in SI7 and SI8  L Additional parameters are not sent in SYSTEM INFORMATION TYPE 7 and 8  H Additional parameters SI4 Rest Octets_S are sent in SYSTEM INFORMATION TYPE 7 and 8</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_break_ind</Name>
                <Comment>Break Indicator value</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>BREAK_IND_NO</Alias>
                <Comment>Additional parameters are not sent in SYSTEM INFORMATION TYPE 7 and 8</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>BREAK_IND_YES</Alias>
                <Comment>Additional parameters SI4 Rest Octets_S are sent in SYSTEM INFORMATION TYPE 7 and 8</Comment>
            </ValuesItem>
            <History>
                <Date Day="27" Month="01" Year="2005"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_class_req</Name>
                <Version>REL99</Version>
                <Comment>values for class_req</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CLASS_CHANGE_REQ</Alias>
                <Comment>the mobile shall send CLASSMARK CHANGE message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CLASS_CHANGE_NOTREQ</Alias>
                <Comment>the mobile shall not send CLASSMARK CHANGE message</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="03" Year="2006"/>
                <Author>GP</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_utran_class_req</Name>
                <Version>REL99</Version>
                <Comment>values for utran_class_req</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>UTRAN_CLASS_CHANGE_REQ</Alias>
                <Comment>the mobile shall send CDMA2000 CLASSMARK CHANGE message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>UTRAN_CLASS_CHANGE_NOTREQ</Alias>
                <Comment>the mobile shall not send CDMA2000 CLASSMARK CHANGE message</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="03" Year="2006"/>
                <Author>GP</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_cdma_class_req</Name>
                <Version>REL99</Version>
                <Comment>values for cdma_class_req</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CDMA_CLASS_CHANGE_REQ</Alias>
                <Comment>the mobile shall send CDMA2000 CLASSMARK CHANGE message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CDMA_CLASS_CHANGE_NOTREQ</Alias>
                <Comment>the mobile shall not send CDMA2000 CLASSMARK CHANGE message</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="03" Year="2006"/>
                <Author>GP</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <DocLink DocType="OTHER">
                        <Name/>
                    </DocLink>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_band_indicator</Name>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>values for band_indicator</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>BAND_IND_1800</Alias>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>ARFCN indicates 1800 band</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>BAND_IND_1900</Alias>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>ARFCN indicates 1900 band</Comment>
            </ValuesItem>
            <History>
                <Date Day="21" Month="04" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <DocLink DocType="OTHER">
                        <Name/>
                    </DocLink>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_max_lapdm</Name>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>Values for max LAPDm frames</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>LAPDM_FRAMES_5</Alias>
                <Comment>Upto 5 LAPDM FRAMES</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>LAPDM_FRAMES_6</Alias>
                <Comment>Upto 6 LAPDM FRAMES</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>LAPDM_FRAMES_7</Alias>
                <Comment>Upto 7 LAPDM FRAMES</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>LAPDM_FRAMES_8</Alias>
                <Comment>Upto 8 LAPDM FRAMES</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>LAPDM_FRAMES_9</Alias>
                <Comment>Upto 9 LAPDM FRAMES</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>LAPDM_FRAMES_10</Alias>
                <Comment>Upto 10 LAPDM FRAMES</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>LAPDM_FRAMES_11</Alias>
                <Comment>Upto 11 LAPDM FRAMES</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>LAPDM_FRAMES_12</Alias>
                <Comment>Upto 12 LAPDM FRAMES</Comment>
            </ValuesItem>
            <History>
                <Date Day="21" Month="04" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
    </ValuesSection>
</AIM>
