<?xml version="1.0" encoding="UTF-8"?>
<!-- edited with SAPE SAP Editor -->
<AIM xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="aim.xsd">
    <DocInfoSection>
        <DocName DocType="AIM">rr_com</DocName>
        <DocNum Number="606" Project="8010"/>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">The Air Interface Message (AIM) for an interface defines the air messages supported by that interface in order to gain access to these messages. This document contains a specification of the RR_COM AIM for the RR_COM interface in the Texas Instruments Dual mode protocol stack.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This document has five primary sections. The first section contains a specification of constants used in the messages, which are not specific to the value of a particular parameter. Such constants are typically size fields, specifying array or element sizes.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">The second primary section contains common types used in the description of the primitives contained in this AIM.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">The third primary section contains a top-level description of the air messages defined for this interface. For each primitive its function is described, and a parameter list is given.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">For any messages using complex structures or parameters with identified values, references will be given to subsections of the fifth and sixth primary sections. Section 5 contains structured elements and section 6 contains basic elements.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">For all messages included in this AIM, it is a sad but unavoidable fact that as the world of 3G evolves, some changes to this interface may be necessary. However, as this document is the basis for the RR_COM AIM it will be fully maintained and all necessary changes will result in updated versions of this document.</XHTMLElement>
            </DocElement>
        </Description>
        <DocHistory>
            <DocVersion Number="001" Year="02"/>
            <Date Day="6" Month="12" Year="2002"/>
            <Author>FLF</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Initial version. based on 8443.250.02.008 and 8443.250.02.008_review_report</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="002" Year="02"/>
            <Date Day="9" Month="12" Year="2002"/>
            <Author>JMM</Author>
            <DocStatus State="APPROVED"/>
            <Comment>Status changed to Accepted after FLFs deskcheck</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="003" Year="02"/>
            <Date Day="31" Month="1" Year="2003"/>
            <Author>GSO</Author>
            <DocStatus State="APPROVED"/>
            <Comment>Updated references to 8010</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="004" Year="02"/>
            <Date Day="24" Month="6" Year="2003"/>
            <Author>LOE</Author>
            <DocStatus State="APPROVED"/>
            <Comment>Corrected minor problems.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="005" Year="02"/>
            <Date Day="26" Month="6" Year="2003"/>
            <Author>CLA</Author>
            <DocStatus State="APPROVED"/>
            <Comment>Added PRAGMA section for tool compatibility.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="006" Year="02"/>
            <Date Day="2" Month="7" Year="2003"/>
            <Author>CLA</Author>
            <DocStatus State="APPROVED"/>
            <Comment>Section 6.2: Added prefix REV_LEV due to clash with other AIMs.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="007" Year="02"/>
            <Date Day="14" Month="11" Year="2003"/>
            <Author>LG</Author>
            <DocStatus State="APPROVED"/>
            <Comment>Moved IE's common to RR AIM and RR_SHORT_PD AIM to this document, reordered structure and basic element sections.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="008" Year="02"/>
            <Date Day="16" Month="01" Year="2004"/>
            <Author>x0abuali</Author>
            <DocStatus State="APPROVED"/>
            <Comment>Added Rel4 extension in CM3,GPRS Cell options,MS Radio Access capability</Comment>
        </DocHistory>
    </DocInfoSection>
    <PragmasSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all pragmas that are defined for the RR_COM AIM</XHTMLElement>
            </DocElement>
        </Description>
        <Pragma>
            <Name>CCDNAME</Name>
            <Value ValueType="ALPHA">RR_COM</Value>
            <Comment>CCD name tag</Comment>
        </Pragma>
        <Pragma>
            <Name>ALLWAYS_ENUM_IN_VAL_FILE</Name>
            <Value ValueType="ALPHA">NO</Value>
            <Comment>Adds enumerations in the .val file.</Comment>
        </Pragma>
        <History>
            <Date Day="8" Month="12" Year="2002"/>
            <Author>FLF</Author>
            <Comment>Initial</Comment>
        </History>
        <History>
            <Date Day="24" Month="6" Year="2003"/>
            <Author>LOE</Author>
            <Comment>Removed constants</Comment>
        </History>
        <History>
            <Date Day="28" Month="6" Year="2003"/>
            <Author>CLA</Author>
            <Comment>Added PRAGMA section</Comment>
        </History>
        <History>
            <Date Day="14" Month="11" Year="2003"/>
            <Author>LG</Author>
            <Comment>Added MAX_BSIC, MAX_NNC and MAXRTDxy</Comment>
        </History>
    </PragmasSection>
    <ConstantsSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all constants that are defined for the RR_COM AIM</XHTMLElement>
            </DocElement>
        </Description>
        <Constant>
            <Alias>MAX_ADD_RA_CAP</Alias>
            <Value ValueType="DEC">4</Value>
            <Comment>number of RA caps is MAX_ADD_RA_CAP+1</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NUM_ACC_TYPE</Alias>
            <Value ValueType="DEC">16</Value>
            <Comment>Maximum number of access technologies that can be requested by NW in Packet Uplink assignment message</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_BSIC</Alias>
            <Value ValueType="DEC">18</Value>
            <Comment>Maximum number of bsic_struct in Measurement Information message ((23*8-28-14)/7 = 20) and in SI 2quater Rest Octets IE ((20*8-22-14)/7 = 17)</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NNC</Alias>
            <Value ValueType="DEC">96</Value>
            <Comment>Maximum number of cells in Neighbour cell list for Enhanced Measurements</Comment>
        </Constant>
        <Constant>
            <Alias>MAXRTDS6</Alias>
            <Value ValueType="DEC">20</Value>
            <Comment>Maximum number of 6 Bit Real Time Difference structures in Measurement Information message and in SI 2quater Rest Octets IE (assuming 1 value per structure)</Comment>
        </Constant>
        <Constant>
            <Alias>MAXRTDS12</Alias>
            <Value ValueType="DEC">10</Value>
            <Comment>Maximum number of 12 Bit Real Time Difference structures in Measurement Information message and in SI 2quater Rest Octets IE  (assuming 1 value per structure)</Comment>
        </Constant>
        <Constant>
            <Alias>MAXRTD6</Alias>
            <Value ValueType="DEC">8</Value>
            <Comment>Maximum number of 6 Bit Real Time Difference values per 6 Bit RTD structure (assumed value, theoretical maximum: 21)</Comment>
        </Constant>
        <Constant>
            <Alias>MAXRTD12</Alias>
            <Value ValueType="DEC">6</Value>
            <Comment>Maximum number of 12 Bit Real Time Difference values per 12 Bit RTD structure (assumed value, theoretical maximum: 11)</Comment>
        </Constant>
        <Constant>
            <Alias>BIT7_MAX</Alias>
            <Value ValueType="DEC">128</Value>
            <Comment>7 bit max</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_TDD_CELLS</Alias>
            <Value ValueType="DEC">21</Value>
            <Comment>Maximum number of TDD cell info in 3G neighbour cell info</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_FDD_CELLS</Alias>
            <Value ValueType="DEC">17</Value>
            <Comment>Maximum number of FDD cell info in 3G neighbour cell info</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_FDD</Alias>
            <Value ValueType="DEC">131</Value>
            <Comment>(L3MAX_ACK-3-1-1)*8/(14+1) = 131,2</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_TDD</Alias>
            <Value ValueType="DEC">131</Value>
            <Comment>(L3MAX_ACK-3-1-1)*8/(14+1) = 131,2</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CDMA2K_NEIGH_CELLS</Alias>
            <Value ValueType="DEC">64</Value>
            <Comment>maximum value 3 uarfcn times 32 cells</Comment>
        </Constant>
        <History>
            <Date Day="8" Month="12" Year="2002"/>
            <Author>FLF</Author>
            <Comment>Initial</Comment>
        </History>
        <History>
            <Date Day="24" Month="6" Year="2003"/>
            <Author>LOE</Author>
            <Comment>Removed constants</Comment>
        </History>
        <History>
            <Date Day="28" Month="6" Year="2003"/>
            <Author>CLA</Author>
            <Comment>Added PRAGMA section</Comment>
        </History>
        <History>
            <Date Day="14" Month="11" Year="2003"/>
            <Author>LG</Author>
            <Comment>Added MAX_BSIC, MAX_NNC and MAXRTDxy</Comment>
        </History>
    </ConstantsSection>
    <MessagesSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all messages that are defined for the RR_COM AIM</XHTMLElement>
            </DocElement>
        </Description>
        <Message>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure defines the RF capability (available bands and radio power class?) of the MS. This structure must be filled by the customer and stored in the permanent configuration memory. From this structure the MS reads the available values on run time and use it to fill the classmark info elements 1 to 3 depend on the found frequency band.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgDef>
                <Name>ms_rf_capability</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000001</MsgID>
                <Comment>Mobile Station RF Capabilities</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>-</SpecRef>
                <Comment>Message type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rf_cap</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>-</SpecRef>
                <Comment>MS RF capability</Comment>
            </MsgItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
    </MessagesSection>
    <MsgStructElementsSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all structured elements that are defined for the RR_COM AIM</XHTMLElement>
            </DocElement>
        </Description>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field describes the availability of the encryption algorithm A5.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">No definition of this field (zero as CSN1_S1) means that the same values apply for parameters as in the immediately preceding Access capabilities field within this IE. The presence of the A5 bits is mandatory in the first access capability struct within this IE</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>a5_bits</Name>
                <Comment>A5 bits</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/1; Encryption algorithm A5/1.  Note inverse logic for the A5/1 encryption algorithm between classmark 1 and 2 on the one hand  (available=0 or not=1) and radio access capability on the other hand (available=1 or not=0).</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/2; Encryption algorithm A5/2 available (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_3</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/3; Encryption algorithm A5/3 available (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_4</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/4; Encryption algorithm A5/4 available (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_5</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/5; Encryption algorithm A5/5 available (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_6</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/6; Encryption algorithm A5/6 available (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_7</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/7; Encryption algorithm A5/7 available (1) or not (0)</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This element is a member from MS RA Capability value part</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>acc_cap</Name>
                <Comment>Access capabilities</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>pow_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RF Power Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_bits</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>A5 bits</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>es_ind</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Early Classmark Sending</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ps</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Pseudo Synchronisation capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>vgcs</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Voice Group Call Service</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>vbs</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Voice Broadcast Service</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ms_struct</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Multi Slot Capability Struct</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>pow_8psk_cap</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>Modulation 8-PSK Power Capabilty</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>compact</Name>
                </ItemLink>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>COMPACT Interference Measurement Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rev99</Name>
                </ItemLink>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>Revision Level Indicator (R99)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>umts_fdd</Name>
                </ItemLink>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>UMTS FDD Radio Access Technology</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>umts_tdd</Name>
                </ItemLink>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>UMTS TDD 3.84 Radio Access Technology</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cdma2000</Name>
                </ItemLink>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>CDMA 2000 Radio Access Technology</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Added Rel 4 extensioms</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Access technologies that are requested by network for reporting in MA Radio access capability. This is a recursive structure as defined in sec.11.2.29. Since the access type field is 4 bit, the recursiveness is limited to 16. Access type field is defined in RR.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>acc_tech_req</Name>
                <Version>REL99</Version>
                <Comment>Access Technologies Request</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>acc_tech_typ</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_NUM_ACC_TYPE]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Access Technology Type</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="8" Year="2003"/>
                <Author>Created</Author>
                <Comment>for EGPRS support</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure contains the GMSK Power Class and 8PSK Power Class for an additional Access Technology. All other capabilities for this indicated Access Technology are the same as the capabilities indicated by the preceding Access capabilities structure.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>add_acc_tech</Name>
                <Version>REL99</Version>
                <Comment>Additonal Access Technologies</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>add_acc_tech_elem</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[1.. MAX_ADD_RA_CAP]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Additional Access Technology Element</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="24" Month="7" Year="2003"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure contains the GMSK Power Class and 8PSK Power Class for an additional Access Technology. All other capabilities for this indicated Access Technology are the same as the capabilities indicated by the preceding Access capabilities structure.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP_TS24.008] section 10.5.5.12a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>add_acc_tech_elem</Name>
                <Version>REL99</Version>
                <Comment>Additonal Access Technologies Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>acc_tech_typ</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Access Technology Type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>pow_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GMSK Power Class</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>pow_8psk_cap</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>8PSK Power Class</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="24" Month="7" Year="2003"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This element defines the actual contents MS Radio Access Capability, which is used in the first and in the following MS RA capabilities.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ra_cap_values</Name>
                <Version>REL99</Version>
                <Comment>Actual MS RA capability value part</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>acc_tech_typ</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Access Technology Type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>acc_cap</Name>
                </ItemLink>
                <Type>GSM7_LV</Type>
                <Control>
                    <Condition>acc_tech_typ # 15</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Access Capabilities</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>add_acc_tech</Name>
                </ItemLink>
                <Type>GSM7_LV</Type>
                <Control>
                    <Condition>acc_tech_typ = 15</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Additional Access Technologies</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="15" Month="8" Year="2003"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>bsic_struct</Name>
                <Version>REL99</Version>
                <Comment>BSIC Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>freq_scroll</Name>
                </ItemLink>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>Frequency Scrolling</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BSIC</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_bsic</Name>
                <Version>REL99</Version>
                <Comment>GPRS BSIC Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ba_start_bsic</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>BA Index Start BSIC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BSIC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rem_bsic</Name>
                </ItemLink>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>Number Remaining BSIC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>bsic_struct</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[rem_bsic.. MAX_BSIC]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>BSIC Structure</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure is used in optional extension information structure. Reference: [2] 12.24</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_ext_info</Name>
                <Version>REL99</Version>
                <Comment>GPRS cell options Extension Information</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egprs_pck_ch_req_bep_per</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>EGPRS packet channel and BEP period structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>pfc_feature_mode</Name>
                </ItemLink>
                <Control>
                    <Condition> (TAKE, 1) &gt;0 AND flag=0 OR (TAKE, 1) &gt;5</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>PFC feature support by the N/W</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_support</Name>
                </ItemLink>
                <Control>
                    <Condition> (TAKE, 1) &gt;1 AND flag=0 OR (TAKE, 1) &gt;6</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>DTM support by the cell</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>bss_paging_coord</Name>
                </ItemLink>
                <Control>
                    <Condition>(TAKE, 1) &gt;2 AND flag=0 OR (TAKE, 1) &gt;7</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>BSS paging co-ordination</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ccn_active</Name>
                </ItemLink>
                <Control>
                    <Condition>(TAKE, 1) &gt;3 AND flag=0 OR (TAKE, 1) &gt;8</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>CCN_ACTIVE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>nw_ext_ul_tbf</Name>
                </ItemLink>
                <Control>
                    <Condition>(TAKE, 1) &gt;4 AND flag=0 OR (TAKE, 1) &gt;9</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>NW_EXT_UTBF</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="24" Month="8" Year="2003"/>
                <Author>XBOREGOW</Author>
                <Comment>Initial version release 99</Comment>
            </History>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>xabuali</Author>
                <Comment>Added Rel 4 extensions</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Extension Bits information element is used to provide a generalized means for possible future extension within a message. This information element is variable length and contains the length indicator and spare bits.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_ext_bits</Name>
                <Comment>GPRS cell options extensions Bits IE</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ext_len</Name>
                </ItemLink>
                <Control>
                    <CmdSequence>KEEP,1</CmdSequence>
                </Control>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>Extension length</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gprs_ext_info</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[.ext_len+1..64]</TypeModifier>
                </Control>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>GPRS cell options extension Information and spare bit(s)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ext_len</Name>
                </ItemLink>
                <Version>!REL99</Version>
                <SpecRef/>
                <Comment>Extension length</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>spare_ext</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[ext_len+1..64]</TypeModifier>
                </Control>
                <Version>!REL99</Version>
                <SpecRef/>
                <Comment>spare bit extensions IE</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="24" Month="8" Year="2003"/>
                <Author>XBOREGOW</Author>
                <Comment>Initial version release 99</Comment>
            </History>
            <History>
                <Date Day="06" Month="01" Year="2004"/>
                <Author>XGULALIT</Author>
                <Comment>Modified gprs_ext_info for &amp; type modifier</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The GPRS Cell Options information element is used to control a set of cell options related to GPRS.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_cell_opt</Name>
                <Comment>GPRS Cell Options</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>nmo</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NMO</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>t3168</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T3168</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>t3192</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T3192</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>drx_t_max</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DRX_TIMER_MAX</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ab_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ACCESS_BURST_TYPE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ctrl_ack_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CONTROL_ACK_TYPE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>bs_cv_max</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BS_CV_MAX</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>pan_struct</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>PAN Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gprs_ext_bits</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS cell options extension Bits IE</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>xboregow</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Mobile Station Classmark 1 information element is to provide the network with information concerning aspects of high priority of the mobile station equipment. This affects the manner in which the network handles the operation of the mobile station.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note : not used in GSM RR.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [1] section 10.5.1.5</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>mob_class_1</Name>
                <Comment>Mobile Station Classmark 1</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rev_lev</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Revision level</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>es_ind</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Early Classmark Sending</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/1; Encryption algorithm A5/1 available (0) or not (1).  Please note the inverse logic!</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rf_pow_cap</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RF power capability</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Mobile Station Classmark 2 information element is to provide the network with information concerning aspects of both high and low priority of the mobile station equipment. This affects the manner in which the network handles the operation of the mobile station.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.6</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>mob_class_2</Name>
                <Comment>Mobile Station Classmark 2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rev_lev</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Revision level; Indicates the revision level of the MS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>es_ind</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Early Classmark Sending; "Controlled Early Classmark Sending" option is implementation (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/1; Encryption algorithm A5/1 available (0) or not (1). Please note the inverse logic!</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rf_pow_cap</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RF power capability (CM2); Indication of the RF power capabilities corresponding to the supported band</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ps</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Pseudo Synchronisation capability; PS capability present (1) or not present (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ss_screen</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SS Screen. Indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mt_pp_sms</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Short Message capability; MS does supports (1) MT point to point SMS or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>vbs</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>VBS Notification Reception; VBS capability and notifications wanted (1) or vice versa (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>vgcs</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>VGCS Notification Reception; VGCS capability and notifications wanted (1) or vice versa (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egsm</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Frequency capability; When the GSM 850 or DCS 1800 or PCS 1900 band is used, this bit shall be sent with the value '0'. When a GSM 900 band is used, this bit describes the support of the extension band</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>class3</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Classmark 3; The MS supports options that are indicated in classmark 3 (1) or it does not support any classmark 3 options (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>lcsva</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>LCSVA capability; LCS value added location request notification supported (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ucs2_treat</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>UCS2 treatment; Indicates the likely treatment by the MS of UCS2 encoded</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>solsa</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SoLSA Supported; MS supports SoLSA (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cmsp</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CMSP Supported; MS supports (1) CM service Prompt (network initiated MO CM connection request) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_3</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/3; Encryption algorithm A5/3 available (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/2; Encryption algorithm A5/2 available (1) or not (0)</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The purpose of the Mobile Station Classmark 3 information element is to provide the network with information concerning aspects of the mobile station. The contents might affect the manner in which the network handles the operation of the mobile station.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>mob_class_3</Name>
                <Comment>Mobile Station Classmark 3</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mb_value</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Multiband Support</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_7</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/7</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_6</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/6</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_5</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/5</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_4</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5/4</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>radio_cap_2</Name>
                </ItemLink>
                <Control>
                    <Condition>mb_value=5 OR mb_value=6</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Associated Radio Capability 2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <Control>
                    <Condition>mb_value=1 OR mb_value=2 OR mb_value=4</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>radio_cap_1</Name>
                </ItemLink>
                <Control>
                    <Condition>mb_value=1 OR mb_value=2 OR mb_value=4 OR mb_value=5 OR mb_value=6</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Associated Radio Capability 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rgsm_class</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>R Support (R-GSM Class)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ms_class</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Multi Slot Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ucs2_treat</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>UCS2 Treatment</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ext_meas</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Extended Measurement Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>measurement</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Measurement Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>pos_method</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>MS Positioning Method Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>edge_ms_class</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>EGDE Multi Slot Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egde_struct</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>EGDE Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gsm400_struct</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GSM 400 Bands Supported Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gsm850_cap</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GSM 850 Associated Radio Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>pcs1900_cap</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>PCS 1900 Associated Radio Cap.</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>umts_fdd</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>UMTS FDD Radio Access Technology</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>umts_tdd</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>UMTS TDD Radio Access Technology</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cdma2000</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CDMA 2000 Radio Access Technology</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_ms</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>DTM Multislot Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>single_band</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Single Band Support</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gsm700_cap</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>GSM 700 Associated Radio Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>umts_tdd_128</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>UMTS 1.28 TDD Radio Access Technology</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>geran_feat_pack_1</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>GERAN Feature 1 Package</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ext_dtm_ms</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>Extended DTM Multislot Structure </Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>high_ms_cap</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>High Multislot Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>geran_iu_mod_cap</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>GERAN Iu Mode Capabilities</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>geran_feat_pack_2</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>GERAN Feature Package 2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gmsk_ms_pwr_prof</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>GMSK Multislot Power Profile</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>psk8_ms_pwr_prof</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>8-PSK Multislot Power Profile</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>t_gsm400_struct</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>T-GSM 400 Bands Supported Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>t_gsm900_cap</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>T-GSM 900 Associated Radio Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dl_adv_rx_per</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Downlink Advanced Receiver Performance</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_enhance_cap</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>DTM Enhancements Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_high_ms</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>DTM (E)GPRS High Multi Slot Class </Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rep_acch_cap</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Repeated ACCH Capability : bit</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00000000</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING</Type>
                <Control>
                    <CmdSequence>0</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>N Spare Padding</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Added Rel 4 extensions</Comment>
            </History>
            <History>
                <Date Day="07" Month="03" Year="2007"/>
                <Author>Manjunath</Author>
                <Comment>Added Repeated ACCH capability field</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The DTM Multislot Struct contains GPRS related capabilities.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>dtm_ms</Name>
                <Comment>DTM Multislot Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_g_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DTM GPRS Multi Slot Sub-Class</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mac_support</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MAC Mode support</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_e_ms_class</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>DTM EGPRS Multi Slot Sub-Class</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The DTM High Multislot Struct contains GPRS and EGPRS related capabilities.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>dtm_high_ms</Name>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>DTM High Multislot Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_g_high_ms_class</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>DTM GPRS High Multi Slot Sub-Class</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>offset_required</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Offset Required</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_e_high_ms_class</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>DTM EGPRS High Multi Slot Sub-Class</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The EDGE Struct contains the Modulation Capability field, which indicates the supported modulation scheme by an EDGE MS in addition to GMSK. If 8-PSK modulation is supported for both uplink and downlink, the additional EDGE RF Power Capability fields indicate the radio capability for 8-PSK modulation in GSM400, GSM850, GSM900, DCS1800 or PCS1900.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field shall be sent only the MS support EDGE (edge_cap)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>egde_struct</Name>
                <Comment>EGDE Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mod</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EDGE Modulation Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egde_pow1</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>EGDE RF Power Capability 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egde_pow2</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>EGDE RF Power Capability 2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rtdd</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>GPRS Real Time Difference Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rtdd6</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Real Time Difference Description 6 Bit</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rtdd12</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Real Time Difference Description 12 Bit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_rep_prio</Name>
                <Version>REL99</Version>
                <Comment>GPRS REPORT PRIORITY Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>num_cells</Name>
                </ItemLink>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>Number cells</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rep_priority</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[num_cells.. MAX_NNC]</TypeModifier>
                </Control>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>Reporting Priority</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This information field indicates which GSM 400 bands the MS supports and the associated Radio Access Capability for that/those band(s). It is contained in the classmark 3 IE only if the MS supports the GSM 450 and/or the GSM 480 band.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gsm400_struct</Name>
                <Comment>GSM 400 Bands Supported Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gsm400_supp</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GSM 400 Bands Supported</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gsm400_cap</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GSM 400 Associated Radio Capability</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This information field indicates which GSM 400 bands the MS supports and the associated Radio Access Capability for that/those band(s). It is contained in the classmark 3 IE only if the MS supports the GSM 450 and/or the GSM 480 band.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>t_gsm400_struct</Name>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>GSM 400 Bands Supported Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>t_gsm400_supp</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>T-GSM 400 Bands Supported</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>t_gsm400_cap</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>T-GSM 400 Associated Radio Capability</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The information field contains values about the measurement capabilities. The SMS field indicates the time for the MS to switch from one radio channel to another, perform a neighbour cell power measurement, and the switch from that radio channel to another radio channel. The SM field indicates the time needed for the MS to switch from one radio channel to another and perform a neighbour cell power measurement.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>measurement</Name>
                <Comment>Measurement Capability</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>sms_val</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Switch-Measure-Switch-Value</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>sm_val</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Switch-Measure-Value</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This information field indicates which positiong method(s) are supported by the mobil station. This shall be sent only if the MS supports positioning methods.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pos_method</Name>
                <Comment>MS Positioning Method</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>assist_eotd</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS assisted E-OTD; bit 5</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>based_eotd</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS based E-OTD; bit 4</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>assist_gps</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS assisted GPS; bit 3</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>based_gps</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS based GPS; bit 2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>conv_gps</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS conventional GPS; bit 1</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure defines the RF capability (available bands and radio power class?) of the MS. This structure must be filled by the customer and store in the permanent configuration memory. From this structure the MS reads the available values on run time and use it to fill the classmark info elements 1 to 3 depend on the found frequency band.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pow_class4</Name>
                <Comment>RF Power Capability (4 bits); Power Class of GSM 400, GSM 850, GSM 900, DCS 1800, PCS 1900</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>pow_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RF Power Capability</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This element defines the MS Radio Access Capability. It provides the radio part of the network with information concerning radio aspect of the mobile station. The content might affect the manner in which the network handles the operation of the mobile station.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This definition is used by links from the GRR and GMM message interface.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ra_cap</Name>
                <Comment>MS RA capability value part</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ra_cap_values</Name>
                </ItemLink>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>Actual MS RA capability value part</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ra_cap_r</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0.. MAX_ADD_RA_CAP]</TypeModifier>
                </Control>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>Recursive MS RA capability value</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>acc_tech_typ</Name>
                </ItemLink>
                <Version>!REL99</Version>
                <SpecRef/>
                <Comment>Access Technology Type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>acc_cap</Name>
                </ItemLink>
                <Type>GSM7_LV</Type>
                <Version>!REL99</Version>
                <SpecRef/>
                <Comment>Access Capabilities</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>flag_ra_cap2</Name>
                </ItemLink>
                <Version>!REL99</Version>
                <SpecRef/>
                <Comment>Valid flag for MS RA capability value part II</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ra_cap2</Name>
                </ItemLink>
                <Control>
                    <Condition>flag_ra_cap2=1</Condition>
                </Control>
                <Version>!REL99</Version>
                <SpecRef/>
                <Comment>MS RA capability value part II</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="2003"/>
                <Author>MPA</Author>
                <Comment>add additional access capabilities</Comment>
            </History>
            <History>
                <Date Day="15" Month="8" Year="2003"/>
                <Author>MPA</Author>
                <Comment>make RA cap recursive</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This element defines the MS Radio Access Capability. It?s the same as MS RA capability value part. The Specification allows any number of access technologies by recursive use of this structure.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ra_cap_r</Name>
                <Version>REL99</Version>
                <Comment>Recursive MS RA capability value part</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ra_cap_values</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Actual MS RA capability value part</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="15" Month="8" Year="2003"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ra_cap2</Name>
                <Version>!REL99</Version>
                <Comment>RAC structure for R97</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>acc_tech_typ</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Access Technology Type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>acc_cap</Name>
                </ItemLink>
                <Type>GSM7_LV</Type>
                <SpecRef/>
                <Comment>Access Capabilities</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef/>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="19" Month="04" Year="2006"/>
                <Author>Gopinath</Author>
                <Comment>R97 structure fot RAC</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">No definition of this field (zero as CSN1_S1) means that the same values for multislot parameters as given in an earlier Access capabilities field within this IE apply also here</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ms_struct</Name>
                <Comment>Multislot Capability Struct</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>hscsd_ms_class</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>HSCSD multislot class</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gprs_struct</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS multislot class and Extended Dynamic Allocation Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>sms_sm_value</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>MS Measurement Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ecsd_ms_class</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>ECSD multislot class</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egprs_struct</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>EGPRS multislot class and Extended Dynamic Allocation Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_struct</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Version>REL99</Version>
                <SpecRef>-</SpecRef>
                <Comment>DTM (E-)GPRS Multislot Sub-Class and MAC Mode Support</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the GPRS and EGPRS DTM capabilities of the MS. The DTM Multislot Sub-Class is independent from the Multislot capabilities. This field indicates also whether the MS supports Dynamic and Fixed Allocation or only supports Excusive Allocation.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>dtm_struct</Name>
                <Version>REL99</Version>
                <Comment>DTM (E-)GPRS Multislot Sub-Class and MAC Mode Support</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_g_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DTM GPRS Multi Slot Sub-Class</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mac_support</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MAC Mode support</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_e_ms_class</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>DTM EGPRS Multi Slot Sub-Class</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the Multislot Class and the Extended Dynamic Allocation Capability for EGPRS. The Multislot Class is coded as the binary representation defined in 3GPP TS GSM 05.02-</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_05.02]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>egprs_struct</Name>
                <Version>REL99</Version>
                <Comment>GPRS Multislot Class and Extended Dynamic Allocation Capability</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egprs_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EGPRS multislot class</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egprs_eda</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EGPRS Extended Dynamic Allocation Capability</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the Multislot Class and the Extended Dynamic Allocation Capability for GPRS. The Multislot Class is coded as the binary representation defined in 3GPP TS GSM 05.02-</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_05.02]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_struct</Name>
                <Comment>GPRS Multislot Class and Extended Dynamic Allocation Capability</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gprs_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS multislot class</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gprs_eda</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Extended Dynamic Allocation Capability</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure defines the RF multi slot capability and classes of the MS. This is a sub-structure of the MS RF Capability structure.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rf_ms</Name>
                <Comment>MS RF Multi Slot Capability</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gsm_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GSM Multi Slot Class; Zero indicates that MS doesn?t supports the use of multiple timeslots</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>edge_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EDGE Multi Slot Class; Zero indicates that MS doesn?t supports the use of multiple timeslots</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>hscsd_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>HSCSD Multi Slot Class; Zero indicates that MS doesn?t supports the use of multiple timeslots</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gprs_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Multi Slot Class; Zero indicates that MS doesn?t supports the use of multiple timeslots</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_g</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DTM GPRS Multi Slot Capability; GPRS MS does supports dual transfer mode (DTM)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_g_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DTM GPRS Multi Slot Sub-Class; DTM GPRS Multi Slot Sub-Class (independent from the Multi Slot Capabilities field.)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ecsd_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ECSD Multi Slot Class; Zero indicates that MS doesn?t supports the use of multiple timeslots</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egprs_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EGPRS Multi Slot Class; Zero indicates that MS doesn?t supports the use of multiple timeslots</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_e</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DTM EGPRS Multi Slot Capability; Enhanced GPRS MS does supports dual transfer mode (DTM)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dtm_e_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DTM EGPRS Multi Slot Sub-Class; DTM EGPRS Multi Slot Sub-Class (independent from the Multi Slot Capabilities field.)</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rtdd6</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Real Time Difference Description 6 Bit</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ba_start_rtd</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>BA Index Start RTD</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rtds6</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Real Time Difference Structure 6 Bit</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rtds6_add</Name>
                </ItemLink>
                <Type>CSN1_S0</Type>
                <Control>
                    <TypeModifier>[0..MAXRTDS6]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Real Time Difference Structure 6 Bit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rtdd12</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Real Time Difference Description 12 Bit</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ba_start_rtd</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>BA Index Start RTD</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rtds12</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Real Time Difference Structure 12 Bit</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rtds12_add</Name>
                </ItemLink>
                <Type>CSN1_S0</Type>
                <Control>
                    <TypeModifier>[0..MAXRTDS12]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Real Time Difference Structure 12 Bit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rtds6</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Real Time Difference Structure 6 Bit</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>rtds6_add</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Real Time Difference Structure 6 Bit</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rtd6</Name>
                </ItemLink>
                <Type>CSN1_S0</Type>
                <Control>
                    <TypeModifier>[0..MAXRTD6]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Real Time Difference 6 Bit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rtds12</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Real Time Difference Structure 12 Bit</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>rtds12_add</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Real Time Difference Structure 12 Bit</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rtd12</Name>
                </ItemLink>
                <Type>CSN1_S0</Type>
                <Control>
                    <TypeModifier>[0..MAXRTD12]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Real Time Difference 12 Bit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field are used for measurements.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 11.2.23</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>report_900</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting 900</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rep_offset_900</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Reporting Offset 900</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>th_rep_900</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Reporting Threshold 900</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field are used for measurements.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 11.2.23</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>report_1800</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting 1800</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rep_offset_1800</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Reporting Offset 1800</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>th_rep_1800</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Reporting Threshold 1800</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field are used for measurements.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 11.2.23</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>report_400</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting 400</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rep_offset_400</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Reporting Offset 400</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>th_rep_400</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Reporting Treshold 400</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field are used for measurements.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 11.2.23</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>report_1900</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting 1900</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rep_offset_1900</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Reporting Offset 1900</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>th_rep_1900</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Reporting Threshold 1900</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field are used for measurements.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 11.2.23</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>report_850</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting 850</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rep_offset_850</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Reporting Offset 850</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>th_rep_850</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Reporting Threshold 850</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SMS field indicates the time needed for the mobile station to switch from one radio channel to another, perform a neighbor cell power measurement, and the switch from that radio channel to another radio channel.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SM field indicates the time needed for the mobile station to switch from one radio channel to another and perform a neighbour cell power measurement.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>sms_sm_value</Name>
                <Comment>MS Measurement Capability</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>sms_val</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Switch-Mesure-Switch Value</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>sm_val</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Switch-Measure-Value</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure defines the RF capability (available bands and radio power class?) of the MS. This structure must be filled by the customer and stored in the permanent configuration memory. From this structure the MS reads the available values on run time and use it to fill the classmark info elements 1 to 3 and the MS Radio Access Capability depend on the found frequency band.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rf_cap</Name>
                <Comment>MS RF Capability</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>setbands</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Set Frequency Bands; bitmask of set frequency bands</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>bands</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Supported Frequency Bands; bitmask of all available frequency bands</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rf_power</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS RF Power Classes; MS RF Power Classes</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rf_ms</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS RF Multi Slot Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>es_ind</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Early Classmark Sending; "Controlled Early Classmark Sending" option is implementation (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ps</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Pseudo Synchronisation capability; PS capability present (1) or not present (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mt_pp_sms</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Short Message capability; MS does supports (1) MT point to point SMS or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>lcsva</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>LCSVA capability; LCS value added location request notification supported (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>solsa</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SoLSA Supported; MS does supports SoLSA (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cmsp</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CMSP Supported; MS does supports (1) CM service Prompt (network initiated MO CM connection request) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mod</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EDGE Modulation Capability; The Modulation Capability field indicates the supported modulation scheme by MS in addition to GMSK. 8-PSK supported for downlink reception only (0) or for for uplink transmission and downlink reception (1)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>mac_support</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MAC Mode support; MS does supports Dynamic and Fixed Allocation (1) or only supports Exclusive Allocation (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>meas</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Measurement Capability; Indicates whether a IE shall contain any value about the measurement capabilities (1) or not (0).</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ext_meas</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Extended Measurement Capability; The MS does supports "Extended Measurement" (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>compact</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>COMPACT Interference Measurement Capability; The MS does support COMPACT Interference Measurement (1) or not (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>vbs</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>VBS Notification Reception; VBS capability and notifications wanted (1) or vice versa (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>vgcs</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>VGCS Notification Reception; VGCS capability and notifications wanted (1) or vice versa (0)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ucs2_treat</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>UCS2 treatment; Indicates the likely treatment by the MS of UCS2 encoded</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ss_screen</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SS Screen. Indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>sms_val</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Switch-Measure-Switch-Value</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>sm_val</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Switch-Measure-Value</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>a5_bits</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>A5 bits; Encryption algorithm A5/n available (0) or not (1)</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>assist_eotd</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS assisted E-OTD; bit 5</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>based_eotd</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS based E-OTD; bit 4</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>assist_gps</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS assisted GPS; bit 3</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>based_gps</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS based GPS; bit 2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>conv_gps</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS conventional GPS; bit 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>gprs_eda</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Extended Dynamic Allocation Capability; Extended Dynamic Allocation Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egprs_eda</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EGPRS Extended Dynamic Allocation Capability; Extended Dynamic Allocation Capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure defines the RF power classes for all available bands of the MS. This is a sub-structure of the MS RF Capability structure.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rf_power</Name>
                <Comment>MS RF Power Classes</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>pow_class4</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[5]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>RF Power Capability (4 bits); Power Class of GSM 400, GSM 850, GSM 900, DCS 1800, PCS 1900</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egde_pow1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EGDE RF Power Capability 1; 8-PSK Power Class of GSM 400, GSM 850, GSM 900</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egde_pow2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EGDE RF Power Capability 2; 8-PSK Power Class of DCS 1800, PCS 1900</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure contains parameter for handling of counter N3102 during Packet Data Transfer. At each cell reselection the mobile station shall set the counter N3102 to the value defined by the optional broadcast parameter PAN_MAX. Whenever the mobile station receives a Packet Ack/Nack that allows the advancement of V(S), the mobile station shall increment N3102 by the broadcast value PAN_INC, however N3102 shall never exceed the value PAN_MAX. Each time T3182 expires the mobile station shall decrement N3102 by the broadcast value PAN_DEC. When N3102 ??0 is reached, the mobile station shall perform an abnormal release with cell re-selection.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pan_struct</Name>
                <Comment>PAN Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>dec</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PAN_DEC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>inc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PAN_INC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>pmax</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PAN_MAX</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>xboregow</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ccn_support_description</Name>
                <Version>REL99</Version>
                <Comment>ccn support description towards all neighbour</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>num_cells</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Num of Cells</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ccn_support</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[num_cells..BIT7_MAX]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>CCN support</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="05" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"> Extended DTM Multislot Structure  </XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ext_dtm_ms</Name>
                <Version>REL99 OR TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>Extended DTM Multislot Structure </Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ext_dtm_g_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Extended DTM GPRS Multi Slot Sub-Class</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ext_dtm_e_ms_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Extended DTM EGPRS Multi Slot Sub-Class</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure defines the part of UTRAN TDD IE in which we use the mapping function q(x) to define the number of bits in 3G neighbourcell list.  ----------------------------------------------------------------------- IMPORTANT NOTE:  ----------------------------------------------------------------------- In this particular case, CCD performs more than just decoding of bits received in the air message. CCD performs   1. the mapping of NR_OF_TDD_CELLS using q(x),   2. gets the number of bits to be actually decoded,  3. extracts these bits from air message,   4. then decodes the 'Range 512 format' also and updates the array of NR_OF_TDD_CELLS elements.  Each of this array element is a 9 bit field (defined as USHORT field here).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Also note that the field NR_OF_TDD_CELLS is implicitly decoded by CCD when the coding type for tdd_ncell_data field is indicated as TDD_CI. Hence no need to define the field NR_OF_TDD_CELLS explicitly.  For the entity to know the count of NR_OF_TDD_CELLS, the generated counter can be used. </XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>tdd_ci_struct</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>TDD Neighbour cell information</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>tdd_indic0</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>tdd_ncell_data</Name>
                </ItemLink>
                <Type>TDD_CI</Type>
                <Control>
                    <TypeModifier>[0..MAX_TDD_CELLS]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="09" Month="06" Year="2004"/>
                <Author>XGIRIDHA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure defines the part of UTRAN FDD IE in which we use the mapping function p(x) to define the number of bits in 3G neighbourcell list.  ----------------------------------------------------------------------- IMPORTANT NOTE:  ----------------------------------------------------------------------- In this particular case, CCD performs more than just decoding of bits received in the air message. CCD performs   1. the mapping of NR_OF_FDD_CELLS using p(x),   2. gets the number of bits to be actually decoded,  3. extracts these bits from air message,   4. then decodes the 'Range 1024 format' also and updates the array of NR_OF_FDD_CELLS elements.  Each of this array element is a 10 bit field (defined as USHORT field here).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Also note that the field NR_OF_FDD_CELLS is implicitly decoded by CCD when the coding type for fdd_ncell_data field is indicated as FDD_CI. Hence no need to define the field NR_OF_FDD_CELLS explicitly.  For the entity to know the count of NR_OF_FDD_CELLS, the generated counter can be used.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>fdd_ci_struct</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>FDD Neighbour cell information</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>fdd_indic0</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>fdd_ncell_data</Name>
                </ItemLink>
                <Type>FDD_CI</Type>
                <Control>
                    <TypeModifier>[0..MAX_FDD_CELLS]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="09" Month="06" Year="2004"/>
                <Author>XGIRIDHA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rep_u_tdd_cells</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Repeated UTRAN TDD Neighbour cells</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>tdd_arfcn</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TDD_ARFCN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>tdd_arfcn_index</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TDD ARFCN index</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>tdd_ci_struct</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>TDD neighbour cell info</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="06" Year="2004"/>
                <Author>XGIRIDHA</Author>
                <Comment>Linked to new structure (tdd_ci_struct) supported by GPFv17</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rep_u_fdd_cells</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Repeated UTRAN FDD Neighbour cells</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>fdd_arfcn</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>FDD_ARFCN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>fdd_arfcn_index</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>FDD ARFCN index</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>fdd_ci_struct</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>FDD neighbour cell info</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="06" Year="2004"/>
                <Author>XGIRIDHA</Author>
                <Comment>Linked to new structure (fdd_ci_struct) supported by GPFv17</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>utran_tdd</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>UTRAN TDD description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>bw_tdd</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Bandwidth TDD</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rep_u_tdd_cells</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_TDD]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Repeated UTRAN TDD Neighbour cells</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>utran_fdd</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>UTRAN FDD description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>bw_fdd</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Bandwidth FDD</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>rep_u_fdd_cells</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_FDD]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Repeated UTRAN FDD Neighbour cells</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>threeg_cells</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>3G Neighbour Cell Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>index_start_3g</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Index Start 3G</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>abs_index_emr</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Absolute Index start EMR</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>utran_fdd</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>UTRAN FDD description</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>utran_tdd</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>UTRAN TDD description</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cd2k_str_000</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Structured Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>td_mode</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>td_power_level</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cd2k_str_001</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Structured Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>qof</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>walsh_len_a</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>aux_pilot_walsh</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[.walsh_len_a+6..8]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cd2k_str_010</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Structured Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>qof</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>walsh_len_b</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>aux_td_walsh</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[.walsh_len_b+6..8]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>aux_td_power_level</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>td_mode</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cd2k_str_011</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Structured Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>sr3_prim_pilot</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>sr3_pilot_power1</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>sr3_pilot_power2</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cd2k_str_110_1</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Structured Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>qof1</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>walsh_length1</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>aux_pilot_walsh1</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[.walsh_length1+6..8]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cd2k_str_110_2</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Structured Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>qof2</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>walsh_length2</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>aux_pilot_walsh2</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[.walsh_length2+6..8]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cd2k_str_110</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Structured Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cd2k_str_011</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>qof</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>walsh_len_c</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>aux_walsh_len</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[.walsh_len_c+6..8]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cd2k_str_110_1</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cd2k_str_110_2</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cd2k_str_all</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Structured Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>flag_3bit</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cd2k_str_000</Name>
                </ItemLink>
                <Control>
                    <Condition>flag_3bit=000</Condition>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cd2k_str_001</Name>
                </ItemLink>
                <Control>
                    <Condition>flag_3bit=001</Condition>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cd2k_str_010</Name>
                </ItemLink>
                <Control>
                    <Condition>flag_3bit=010</Condition>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cd2k_str_011</Name>
                </ItemLink>
                <Control>
                    <Condition>flag_3bit=011</Condition>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cd2k_str_110</Name>
                </ItemLink>
                <Control>
                    <Condition>flag_3bit=110</Condition>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cd2k_cell_str</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Structured Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>pilot_PN_offset</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cd2k_str_all</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This section contains description of neighbour cells which are of cdma2000 technology.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cdma2000_cell_desc</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>CDMA2000 neighbour cell description structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cdma2000_frequency_band </Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cdma2000_frequency</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>number_cdma2000_cells</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cd2k_cell_str</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[number_cdma2000_cells..MAX_CDMA2K_NEIGH_CELLS]</TypeModifier>
                </Control>
                <SpecRef/>
                <Comment>Structured Element Item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="11" Month="01" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field are used for measurements. Reference: [2] 11.2.23</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>fdd_report</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>FDD Reporting</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>fdd_rep_offset</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>FDD Reporting Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>fdd_rep_thres</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>FDD Reporting Threshold</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field are used for measurements. Reference: [2] 11.2.23</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>tdd_rep</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>TDD Reporting</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>tdd_rep_offset</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TDD Reporting Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>tdd_rep_thres</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TDD Reporting Threshold</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field are used for measurements. Reference: [2] 11.2.9b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cdma2000_rep</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Structured Element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cdma2000_rep_offset</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>CDMA2000 Reporting Offset</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>cdma2000_rep_thres</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>CDMA2000 Reporting Threshold</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="11" Month="01" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure is used in optional extension information structure. Reference: [2] 12.24</XHTMLElement>
                </DocElement>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>egprs_pck_ch_req_bep_per</Name>
                <Version>REL99</Version>
                <Comment>EGPRS packet channel and BEP period structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>egprs_packet_channel_request</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>EGPRS packet channel request message sent</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>bep_period</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Packet channel request message in two phase packet access</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="02" Month="05" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
    </MsgStructElementsSection>
    <MsgBasicElementsSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all basic elements that are defined for the RR_COM AIM</XHTMLElement>
            </DocElement>
        </Description>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The ACCESS_BURST_TYPE field indicates if the 8 or 11 bit format shall be used in the PACKET CHANNEL REQUEST message, the PTCCH uplink block (3GPP TS 04.04) and in the PACKET CONTROL ACKNOWLEDGMENT message when the format is four access bursts. The field is coded according to the following table.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ab_type</Name>
                <BitLen>1</BitLen>
                <Comment>Access Burst Type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ab_type</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the access technology type to be associated with the following access capabilities.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>acc_tech_typ</Name>
                <BitLen>4</BitLen>
                <Comment>Access Technology Type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_acc_tech_typ</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates whether the associated radio capability for a RF band. Note: the coding of the power class in associated radio capability is different to that used in the MS classmark 1 and 2 information elements (-&gt; 6.26).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS05.05] section 4.1.1 (Output power Mobile Station )</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pow_class</Name>
                <BitLen>3</BitLen>
                <Comment>RF Power Capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates whether the associated radio capability for a RF band. Note: the coding of the power class in associated radio capability is different to that used in the MS classmark 1 and 2 information elements (-&amp;gt; 6.26).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS05.05] section 4.1.1 (Output power Mobile Station )</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>radio_cap_1</Name>
                <BitLen>4</BitLen>
                <Comment>Associated Radio Capability 1</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates whether the associated radio capability for a RF band. Note: the coding of the power class in associated radio capability is different to that used in the MS classmark 1 and 2 information elements (-&amp;gt; 6.26).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS05.05] section 4.1.1 (Output power Mobile Station )</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>radio_cap_2</Name>
                <BitLen>4</BitLen>
                <Comment>Associated Radio Capability 2</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates whether the associated radio capability for a RF band. Note: the coding of the power class in associated radio capability is different to that used in the MS classmark 1 and 2 information elements (-&amp;gt; 6.26).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS05.05] section 4.1.1 (Output power Mobile Station )</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rgsm_class</Name>
                <BitLen>3</BitLen>
                <Comment>R Support (R-GSM Class)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates whether the associated radio capability for a RF band. Note: the coding of the power class in associated radio capability is different to that used in the MS classmark 1 and 2 information elements (-&amp;gt; 6.26).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS05.05] section 4.1.1 (Output power Mobile Station )</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>gsm400_cap</Name>
                <BitLen>4</BitLen>
                <Comment>GSM 400 Associated Radio Capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates whether the associated radio capability for a RF band. Note: the coding of the power class in associated radio capability is different to that used in the MS classmark 1 and 2 information elements (-&amp;gt; 6.26).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS05.05] section 4.1.1 (Output power Mobile Station )</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t_gsm400_cap</Name>
                <BitLen>4</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>T-GSM 400 Associated Radio Capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_class</Name>
            </ValuesLink>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates whether the associated radio capability for a RF band. Note: the coding of the power class in associated radio capability is different to that used in the MS classmark 1 and 2 information elements (-&amp;gt; 6.26).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS05.05] section 4.1.1 (Output power Mobile Station )</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t_gsm900_cap</Name>
                <BitLen>4</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>T-GSM 400 Associated Radio Capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_class</Name>
            </ValuesLink>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author/>
                <Comment>xparapgu</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates whether the associated radio capability for a RF band. Note: the coding of the power class in associated radio capability is different to that used in the MS classmark 1 and 2 information elements (-&amp;gt; 6.26).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS05.05] section 4.1.1 (Output power Mobile Station )</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>gsm850_cap</Name>
                <BitLen>4</BitLen>
                <Comment>GSM 850 Associated Radio Capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates whether the associated radio capability for a RF band. Note: the coding of the power class in associated radio capability is different to that used in the MS classmark 1 and 2 information elements (-&amp;gt; 6.26).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS05.05] section 4.1.1 (Output power Mobile Station )</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pcs1900_cap</Name>
                <BitLen>4</BitLen>
                <Comment>PCS 1900 Associated Radio Cap.</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ba_start_rtd</Name>
                <BitLen>5</BitLen>
                <Comment>BA Index Start RTD</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ba_start_bsic</Name>
                <BitLen>5</BitLen>
                <Comment>BA Index Start BSIC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MS shall report the mean BEP measurement corresponding to the modulation for which it has received a larger number of blocks since the previous report. The MS shall make BEP measurements only on Radio Blocks intended for it</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bep_period</Name>
                <BitLen>4</BitLen>
                <Comment>BEP Period</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bool</Name>
                <BitLen>1</BitLen>
                <Comment>Boolean; the value is set (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>support</Name>
                <BitLen>1</BitLen>
                <Comment>Feature Support; MS does supports a feature (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>es_ind</Name>
                <BitLen>1</BitLen>
                <Comment>Early Classmark Sending; 'controlled early classmark sending' option is implemented (1) or not (0) in the MS</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ps</Name>
                <BitLen>1</BitLen>
                <Comment>Pseudo Synchronisation capability; Pseudo synchronisation capabilty is present (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mt_pp_sms</Name>
                <BitLen>1</BitLen>
                <Comment>Short Message capability; MS does supports (1) MT point to point SMS or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>vgcs</Name>
                <BitLen>1</BitLen>
                <Comment>Voice Group Call Service; VGCS capability and notification wanted (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>vbs</Name>
                <BitLen>1</BitLen>
                <Comment>Voice Broadcast Service; VBS capability and notification wanted (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>class3</Name>
                <BitLen>1</BitLen>
                <Comment>Classmark 3; The MS supports options that are indicated in classmark 3 (1) or it does not support any classmark 3 options (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>lcsva</Name>
                <BitLen>1</BitLen>
                <Comment>LCSVA capability; LCS value added location request notification supported (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>solsa</Name>
                <BitLen>1</BitLen>
                <Comment>SoLSA Supported; MS does supports SoLSA (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cmsp</Name>
                <BitLen>1</BitLen>
                <Comment>CMSP Supported; MS does supports (1) CM service Prompt (network initiated MO CM connection request) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ext_meas</Name>
                <BitLen>1</BitLen>
                <Comment>Extended Measurement Capability; MS does supports 'extended measurements`(1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>meas</Name>
                <BitLen>1</BitLen>
                <Comment>Measurement Capability; Indicates whether the IE contains any value about the measurement capabilities or not</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pos</Name>
                <BitLen>1</BitLen>
                <Comment>MS Positioning Method Capability; Indicates whether MS does supports positioning method or not</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>edge</Name>
                <BitLen>1</BitLen>
                <Comment>EDGE Structure; Indicates whether MS does supports the EDGE or not</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>edge_ms</Name>
                <BitLen>1</BitLen>
                <Comment>Multi Slot Capability; Indicates whether MS does supports the use of multiple timeslots or not</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ms</Name>
                <BitLen>1</BitLen>
                <Comment>Multi Slot Capability; indicates whether MS does supports the use of multiple timeslots or not</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>hscsd_ms</Name>
                <BitLen>1</BitLen>
                <Comment>HSCSD Multi Slot Capability; indicates whether MS supports the use of multiple timeslots or not</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_ms</Name>
                <BitLen>1</BitLen>
                <Comment>GPRS Multi Slot Capability; indicates whether MS supports the use of multiple timeslots or not</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ecsd_ms</Name>
                <BitLen>1</BitLen>
                <Comment>ECSD Multi Slot Capability; indicates whether MS supports the use of multiple timeslots or not</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>egprs_ms</Name>
                <BitLen>1</BitLen>
                <Comment>EGPRS Multi Slot Capability; indicates whether MS supports the use of multiple timeslots or not</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mod</Name>
                <BitLen>1</BitLen>
                <Comment>Modulation Capability; MS does supports 8-PSK modulation for uplink and downlink (1) or only for downlink (0) in addition to GSMK</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>assist_eotd</Name>
                <BitLen>1</BitLen>
                <Comment>MS assisted E-OTD; MS does supports assisted E-OTD (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>based_eotd</Name>
                <BitLen>1</BitLen>
                <Comment>MS based E-OTD; MS does supports based E-OTD (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>assist_gps</Name>
                <BitLen>1</BitLen>
                <Comment>MS assisted GPS; MS does supports assisted GPS (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>based_gps</Name>
                <BitLen>1</BitLen>
                <Comment>MS based GPS; MS does supports based GPS (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>conv_gps</Name>
                <BitLen>1</BitLen>
                <Comment>MS conventional GPS; MS does supports conventional GPS (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>umts_fdd</Name>
                <BitLen>1</BitLen>
                <Comment>UMTS FDD Radio Access Technology; MS does supports  UMTS FDD (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>umts_tdd</Name>
                <BitLen>1</BitLen>
                <Comment>UMTS 3.84 Mcps TDD Radio Access Technology; MS does supports UMTS TDD (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cdma2000</Name>
                <BitLen>1</BitLen>
                <Comment>CDMA 2000 Radio Access Technology; MS does supports CDMA 2000 (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mac_support</Name>
                <BitLen>1</BitLen>
                <Comment>MAC Mode support; MS does supports dynamice and fixed allocation (1) or only exclusive allocation (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>compact</Name>
                <BitLen>1</BitLen>
                <Comment>COMPACT Interference Measurement Capability; COMPACT Interference Measurement Capability is implemented (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_eda</Name>
                <BitLen>1</BitLen>
                <Comment>GPRS Extended Dynamic Allocation Capability; MS does supports dynamice and fixed allocation (1) or only exclusive allocation (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>egprs_eda</Name>
                <BitLen>1</BitLen>
                <Comment>EGPRS Extended Dynamic Allocation Capability; MS does supports dynamice and fixed allocation (1) or only exclusive allocation (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_1</Name>
                <BitLen>1</BitLen>
                <Comment>A5/1; Encryption algorithm A5/1.  Note inverse logic for the A5/1 encryption algorithm between classmark 1 and 2 on the one hand  (available=0 or not=1) and radio access capability on the other hand (available=1 or not=0).</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_2</Name>
                <BitLen>1</BitLen>
                <Comment>A5/2; Encryption algorithm A5/2 available (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_3</Name>
                <BitLen>1</BitLen>
                <Comment>A5/3; Encryption algorithm A5/3 available (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_4</Name>
                <BitLen>1</BitLen>
                <Comment>A5/4; Encryption algorithm A5/4 available (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_5</Name>
                <BitLen>1</BitLen>
                <Comment>A5/5; Encryption algorithm A5/5 available (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_6</Name>
                <BitLen>1</BitLen>
                <Comment>A5/6; Encryption algorithm A5/6 available (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_7</Name>
                <BitLen>1</BitLen>
                <Comment>A5/7; Encryption algorithm A5/7 available (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dtm_g</Name>
                <BitLen>1</BitLen>
                <Comment>DTM GPRS Multi Slot Capability; GPRS MS does supports dual transfer mode (DTM)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dtm_e</Name>
                <BitLen>1</BitLen>
                <Comment>DTM EGPRS Multi Slot Capability; EGPRS MS does supports dual transfer mode (DTM)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This indicates whether the MS supports a feature or not respectively whether the value is set or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dummy_r99_ind</Name>
                <BitLen>1</BitLen>
                <Comment>Dummy R99 inclusion indicator; A dummy field to suppress R99 fields (esp.in MS RACAP)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This bit indicates whether an information is present or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>flag</Name>
                <BitLen>1</BitLen>
                <Comment>Flag</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_flag</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="9" Year="2003"/>
                <Author>xboregow</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.20 (Measurement Results)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54 (Measurement Information)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bsic</Name>
                <BitLen>6</BitLen>
                <Comment>BSIC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the network support of CS paging co-ordination in packet transfer mode during network mode of operation II and III. This field shall be ignored by the mobile station during network mode of operation I.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bss_paging_coord</Name>
                <BitLen>1</BitLen>
                <Comment>BSS paging co-ordination</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bss_paging_coord</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="2003"/>
                <Author>XBOREGOW</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of the parameter BS_CV_MAX. Range: 0 to 15. The value BS_CV_MAX=0 shall be interpreted as value BS_CV_MAX=1 for calculation of T3200 and N3104max values. CV - countdown value</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bs_cv_max</Name>
                <BitLen>4</BitLen>
                <Comment>BS_CV_MAX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of the default format of the PACKET CONTROL ACKNOWLEDGMENT message.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ctrl_ack_type</Name>
                <BitLen>1</BitLen>
                <Comment>CONTROL_ACK_TYPE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ctrl_ack_type</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of the parameter DRX_TIMER_MAX. Range: 0 to 7. The parameter value is given as two taken to the power of the binary value minus one (2 (bv - 1) in units of 1 second. The binary value zero indicates that non-DRX mode is not supported in the cell. (E.g. the parameter takes the values: 'not supported', 1 s, 2 s, 4 s, .. 64 s.)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>drx_t_max</Name>
                <BitLen>3</BitLen>
                <Comment>DRX_TIMER_MAX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the GPRS or EGPRS DTM capabilities of the MS. The GPRS or EGPRS DTM Multi Slot Sub-Class is independent from the Multi Slot Capabilities field. In case of EPGPRS this field shall be included only if the mobile station supports EGPRS DTM.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP_TS24.008] section section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dtm_g_ms_class</Name>
                <BitLen>2</BitLen>
                <Comment>DTM GPRS Multi Slot Sub-Class</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_dtm_g_ms_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the GPRS or EGPRS DTM capabilities of the MS. The GPRS or EGPRS DTM Multi Slot Sub-Class is independent from the Multi Slot Capabilities field. In case of EPGPRS this field shall be included only if the mobile station supports EGPRS DTM.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP_TS24.008] section section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dtm_e_ms_class</Name>
                <BitLen>2</BitLen>
                <Comment>DTM EGPRS Multi Slot Sub-Class; only if the MS supports EGPRS DTM</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_dtm_g_ms_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the GPRS or EGPRS DTM capabilities of the MS. The GPRS or EGPRS DTM Multi Slot Sub-Class is independent from the Multi Slot Capabilities field. In case of EPGPRS this field shall be included only if the mobile station supports EGPRS DTM.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dtm_g_high_ms_class</Name>
                <BitLen>3</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>DTM GPRS High Multi Slot Sub-Class</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_dtm_g_high_ms_class</Name>
            </ValuesLink>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the GPRS or EGPRS DTM capabilities of the MS. The GPRS or EGPRS DTM Multi Slot Sub-Class is independent from the Multi Slot Capabilities field. In case of EPGPRS this field shall be included only if the mobile station supports EGPRS DTM.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dtm_e_high_ms_class</Name>
                <BitLen>3</BitLen>
                <Comment>DTM EGPRS High Multi Slot Sub-Class; only if the MS supports EGPRS DTM</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <DocLink DocType="OTHER">
                        <Name>This field indicates whether the MS Supports Repeated SACCH and Repeated Downlink FACCH. It is coded as follows : 0 MS supports Repeated Downlink FACCH  1 MS supports Repeated SACCH and Repeated Downlink FACCH</Name>
                    </DocLink>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rep_acch_cap</Name>
                <BitLen>1</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>Indicates whether the MS supports Repeated SACCH and Repeated FACCH</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_rep_acch_cap</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="02" Year="2007"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates whether the cell supports DTM or not.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dtm_support</Name>
                <BitLen>1</BitLen>
                <Comment>DTM support by the cell</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_dtm_support</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="2003"/>
                <Author>XBOREGOW</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The length of the extension.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ext_len</Name>
                <BitLen>6</BitLen>
                <Comment>Extension Length</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="24" Month="8" Year="2003"/>
                <Author>XBOREGOW</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">That field will be defined during future extension.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>spare_ext</Name>
                <BitLen>1</BitLen>
                <Comment>Spare bits(s)</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="24" Month="8" Year="2003"/>
                <Author>XBOREGOW</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This bit is used in the message "System Information Type 1"  if EGPRS is supported by the cell.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>egprs_packet_channel_request</Name>
                <BitLen>1</BitLen>
                <Comment>EGPRS packet channel request message sent</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_egprs_packet_channel_request</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="2003"/>
                <Author>XBOREGOW</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines which frequency bands shall be measured. This parameter is not used in the current implementation but is introduced for future extensions. It is a bitmap indicating the frequency bands for which power measurements shall be carried out.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bands</Name>
                <BitLen>8</BitLen>
                <Comment>Supported Frequency Bands; bitmask of all available frequency bands</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bands</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines which frequency bands shall be measured. This parameter is not used in the current implementation but is introduced for future extensions. It is a bitmap indicating the frequency bands for which power measurements shall be carried out.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>setbands</Name>
                <BitLen>8</BitLen>
                <Comment>Set Frequency Bands; bitmask of set frequency bands</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bands</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">When the GSM 850 or DCS 1800 or PCS 1900 band is used, this bit shall be sent with the value '0'. When a GSM 900 band is used, this bit describes the support of the extension band.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.1.6 (Mobile Station Classmark 2)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>egsm</Name>
                <BitLen>1</BitLen>
                <Comment>Frequency capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_egsm</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18]</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>freq_scroll</Name>
                <BitLen>1</BitLen>
                <Comment>Frequency Scrolling</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_freq_scroll</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the support of the GSM 450 and GSM 480 bands.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>gsm400_supp</Name>
                <BitLen>2</BitLen>
                <Comment>GSM 400 Bands Supported</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_gsm400_supp</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the support of the GSM 450 and GSM 480 bands.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t_gsm400_supp</Name>
                <BitLen>2</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>T-GSM 400 Bands Supported</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.4</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>msg_type</Name>
                <BitLen>8</BitLen>
                <Comment>Message Type</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">If 8-PSK modulation is supported this field indicates the radio capability for 8-PSK.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note (Classmark 3): If 8-PSK modulation is supported for both uplink and downlink, the EDGE RF Power Capability 2 field indicates the radio capability for 8-PSK modulation in GSM400, GSM850, GSM900, DCS1800 or PCS1900 if supported, and is not included otherwise.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS05.05] section 4.1.1 (Output power Mobile Station for 8-PSK modulation)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pow_8psk_cap</Name>
                <BitLen>2</BitLen>
                <Comment>8-PSK Power Capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_8psk_cap</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">If 8-PSK modulation is supported this field indicates the radio capability for 8-PSK.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note (Classmark 3): If 8-PSK modulation is supported for both uplink and downlink, the EDGE RF Power Capability 2 field indicates the radio capability for 8-PSK modulation in GSM400, GSM850, GSM900, DCS1800 or PCS1900 if supported, and is not included otherwise.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS05.05] section 4.1.1 (Output power Mobile Station for 8-PSK modulation)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>egde_pow1</Name>
                <BitLen>2</BitLen>
                <Comment>EGDE RF Power Capability 1</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_8psk_cap</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">If 8-PSK modulation is supported this field indicates the radio capability for 8-PSK.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note (Classmark 3): If 8-PSK modulation is supported for both uplink and downlink, the EDGE RF Power Capability 2 field indicates the radio capability for 8-PSK modulation in GSM400, GSM850, GSM900, DCS1800 or PCS1900 if supported, and is not included otherwise.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS05.05] section 4.1.1 (Output power Mobile Station for 8-PSK modulation)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>egde_pow2</Name>
                <BitLen>2</BitLen>
                <Comment>EGDE RF Power Capability 2</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_8psk_cap</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The modulation capability field indicates the supported modulation scheme by MS in addition to GMSK</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mod_cap</Name>
                <BitLen>1</BitLen>
                <Comment>Modulation Capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_mod_cap</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the bands, which are supported together</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mb_value</Name>
                <BitLen>3</BitLen>
                <Comment>Multiband Support</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_mb_value</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Multi Slot Class is coded as the binary representation of the multislot class defined in TS GSM 05.02. The range are 1 to 29, all other values are reserved.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note For HSCSD, only multislot classes 1 to 18 are recognised. An MS with a higher multislot class number shall indicate a suitable multislot class less than 19 for HSCSD applications.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [GSM_05.02] Annex B.1 (MS classes for multislot capability)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ms_class</Name>
                <BitLen>5</BitLen>
                <Comment>Multi Slot Class</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ms_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Multi Slot Class is coded as the binary representation of the multislot class defined in TS GSM 05.02. The range are 1 to 29, all other values are reserved.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note For HSCSD, only multislot classes 1 to 18 are recognised. An MS with a higher multislot class number shall indicate a suitable multislot class less than 19 for HSCSD applications.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [GSM_05.02] Annex B.1 (MS classes for multislot capability)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>gsm_ms_class</Name>
                <BitLen>5</BitLen>
                <Comment>GSM Multi Slot Class</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ms_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Multi Slot Class is coded as the binary representation of the multislot class defined in TS GSM 05.02. The range are 1 to 29, all other values are reserved.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note For HSCSD, only multislot classes 1 to 18 are recognised. An MS with a higher multislot class number shall indicate a suitable multislot class less than 19 for HSCSD applications.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [GSM_05.02] Annex B.1 (MS classes for multislot capability)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>edge_ms_class</Name>
                <BitLen>5</BitLen>
                <Comment>EDGE Multi Slot Class</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ms_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Multi Slot Class is coded as the binary representation of the multislot class defined in TS GSM 05.02. The range are 1 to 29, all other values are reserved.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note For HSCSD, only multislot classes 1 to 18 are recognised. An MS with a higher multislot class number shall indicate a suitable multislot class less than 19 for HSCSD applications.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [GSM_05.02] Annex B.1 (MS classes for multislot capability)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>hscsd_ms_class</Name>
                <BitLen>5</BitLen>
                <Comment>HSCSD Multi Slot Class</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ms_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Multi Slot Class is coded as the binary representation of the multislot class defined in TS GSM 05.02. The range are 1 to 29, all other values are reserved.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note For HSCSD, only multislot classes 1 to 18 are recognised. An MS with a higher multislot class number shall indicate a suitable multislot class less than 19 for HSCSD applications.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [GSM_05.02] Annex B.1 (MS classes for multislot capability)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_ms_class</Name>
                <BitLen>5</BitLen>
                <Comment>GPRS Multi Slot Class</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ms_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Multi Slot Class is coded as the binary representation of the multislot class defined in TS GSM 05.02. The range are 1 to 29, all other values are reserved.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note For HSCSD, only multislot classes 1 to 18 are recognised. An MS with a higher multislot class number shall indicate a suitable multislot class less than 19 for HSCSD applications.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [GSM_05.02] Annex B.1 (MS classes for multislot capability)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ecsd_ms_class</Name>
                <BitLen>5</BitLen>
                <Comment>ECSD Multi Slot Class</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ms_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The Multi Slot Class is coded as the binary representation of the multislot class defined in TS GSM 05.02. The range are 1 to 29, all other values are reserved.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note For HSCSD, only multislot classes 1 to 18 are recognised. An MS with a higher multislot class number shall indicate a suitable multislot class less than 19 for HSCSD applications.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [GSM_05.02] Annex B.1 (MS classes for multislot capability)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>egprs_ms_class</Name>
                <BitLen>5</BitLen>
                <Comment>EGPRS Multi Slot Class</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ms_class</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of the Network Mode of Operation, see GSM 03.60.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nmo</Name>
                <BitLen>2</BitLen>
                <Comment>NMO</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_nmo</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.20 (Measurement Results)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.55</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>num_cells</Name>
                <BitLen>7</BitLen>
                <Comment>Number of Cells</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rem_bsic</Name>
                <BitLen>7</BitLen>
                <Comment>Number Remaining BSIC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">See PAN structure.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dec</Name>
                <BitLen>3</BitLen>
                <Comment>PAN_DEC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">See PAN structure.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>inc</Name>
                <BitLen>3</BitLen>
                <Comment>PAN_INC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">See PAN structure'.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pmax</Name>
                <BitLen>3</BitLen>
                <Comment>PAN_MAX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This bit will indicate if the Packet flow context procedures are supported by the network.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pfc_feature_mode</Name>
                <BitLen>1</BitLen>
                <Comment>PFC feature support by the N/W</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pfc_feature_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="2003"/>
                <Author>XBOREGOW</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54 (Measurement Information)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rtd6</Name>
                <BitLen>6</BitLen>
                <Comment>Real Time Difference 6 Bit</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54 (Measurement Information)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rtd12</Name>
                <BitLen>12</BitLen>
                <Comment>Real Time Difference 12 Bit</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rep_priority</Name>
                <BitLen>1</BitLen>
                <Comment>Reporting Priority</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_rep_priority</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MS shall indicate the RF power capability of the band for GSM 850, GSM 900 P or E, DCS 1800 or PCS 1900. Note: the coding of the power class in RF radio capability is different to that used in the MS classmark 3 or MS Radio Access Capability information elements (-&gt; 6.3).</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.5 (Mobile Station Classmark 1)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP_TS24.008] section 10.5.1.6 (Mobile Station Classmark 2)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rf_pow_cap</Name>
                <BitLen>3</BitLen>
                <Comment>RF power capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_rf_pow_cap</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Discrimination between GSM phase 1 or 2 or support of R99 or later versions.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS04.18] section 10.5.1.6 (Mobile Station Classmark 2)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rev_lev</Name>
                <BitLen>2</BitLen>
                <Comment>Revision Level</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_rev_lev</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="2" Month="7" Year="2003"/>
                <Author>CLA</Author>
                <Comment>Added prefix REV_LEV due to clash with other AIMs.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Discrimination whether the MS supports Release ?98 (or older) or Release ?99 onwards.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rev99</Name>
                <BitLen>1</BitLen>
                <Version>REL99</Version>
                <Comment>Revision Level</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_rev99</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates the band, which is supported together with UMTS.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note: This field shall be sent if the mobile station supports UMTS and one and only one GSM band with the exception of R-GSM; this field shall not be sent otherwise.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>single_band</Name>
                <BitLen>4</BitLen>
                <Comment>Single GSM Band Support</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_single_band</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SMS field indicates the time for the MS to switch from one radio channel to another, perform a neighbour cell power measurement, and the switch from that radio channel to another radio channel.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SM field indicates the time needed for the MS to switch from one radio channel to another and perform a neighbour cell power measurement.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>sms_val</Name>
                <BitLen>4</BitLen>
                <Comment>Switch-Measure-Switch-Value</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_sms_val</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SMS field indicates the time for the MS to switch from one radio channel to another, perform a neighbour cell power measurement, and the switch from that radio channel to another radio channel.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The SM field indicates the time needed for the MS to switch from one radio channel to another and perform a neighbour cell power measurement.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference [3GPP_TS24.008] section 10.5.1.7 (Mobile Station Classmark 3)</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.5.12a (MS Radio Access Capability)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>sm_val</Name>
                <BitLen>4</BitLen>
                <Comment>Switch-Measure-Value</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_sms_val</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Coding of SS screening indicator in mobile station classmark 2</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [GSM_04.08] section 10.5.1.6 (Mobile Station Classmark 2)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ss_screen</Name>
                <BitLen>2</BitLen>
                <Comment>SS Screening Indicator</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ss_screen</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of the timeout value of timer T3168. Range: 0 to 7. The timeout value is given as the binary value plus one in units of 500 millisecond.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t3168</Name>
                <BitLen>3</BitLen>
                <Comment>T3168</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field is the binary representation of the timeout value of timer T3192. Range: 0 to 7. The timeout value is given as the binary value plus one in units of 500 millisecond.</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>t3192</Name>
                <BitLen>3</BitLen>
                <Comment>T3192</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This information field indicates the likely treatment by the mobile station of UCS2 encoded character strings. For backward compatibility reasons, if this field is not included, the value 0 shall be assumed by the receiver.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.6 (Mobile Station Classmark 2)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ucs2_treat</Name>
                <BitLen>1</BitLen>
                <Comment>UCS2 treatment</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ucs2_treat</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="12" Year="2002"/>
                <Author>FLF</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rep_offset_900</Name>
                <BitLen>3</BitLen>
                <Comment>900 reporting offset</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_rep_offset_900</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rep_offset_1800</Name>
                <BitLen>3</BitLen>
                <Comment>1800 reporting offset</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_rep_offset_900</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rep_offset_400</Name>
                <BitLen>3</BitLen>
                <Comment>400 reporting offset</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_rep_offset_900</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rep_offset_1900</Name>
                <BitLen>3</BitLen>
                <Comment>1900 reporting offset</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_rep_offset_900</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>rep_offset_850</Name>
                <BitLen>3</BitLen>
                <Comment>850 reporting offset</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_rep_offset_900</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>th_rep_900</Name>
                <BitLen>3</BitLen>
                <Comment>900 reporting threshold</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_th_rep_900</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>th_rep_1800</Name>
                <BitLen>3</BitLen>
                <Comment>1800 reporting threshold</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_th_rep_900</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>th_rep_400</Name>
                <BitLen>3</BitLen>
                <Comment>400 reporting threshold</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_th_rep_900</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>th_rep_1900</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>1900 reporting threshold</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_th_rep_900</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference:  [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">[3GPP 04.18] section 9.1.54</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>th_rep_850</Name>
                <BitLen>3</BitLen>
                <Comment>850 reporting threshold</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_th_rep_900</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="11" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"> The bit indicates the support of NACC feature by Rel 4 network </XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ccn_active</Name>
                <BitLen>1</BitLen>
                <Comment>Indicates NACC support by rel 4 network</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ccn_active</Name>
            </ValuesLink>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Indicates Extended UL TBF support by Rel 4 network</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>nw_ext_ul_tbf</Name>
                <BitLen>1</BitLen>
                <Comment>Indicates Extended UL TBF support by rel 4 network</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_nw_ext_ul_tbf</Name>
            </ValuesLink>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"> This field indicates whether the associated radio capability for a RF band. Note: the coding of the power class in associated radio capability is different to that used in the MS classmark 1 and 2 information elements (-&amp;gt; 6.26).</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>gsm700_cap</Name>
                <BitLen>4</BitLen>
                <Comment>GSM 700 Associated Radio Capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_pow_class</Name>
            </ValuesLink>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"> UMTS 1.28 Mcps TDD Radio Access Technology; MS does supports UMTS TDD (1) or not (0) </XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>umts_tdd_128</Name>
                <BitLen>1</BitLen>
                <Version>REL99 OR TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>UMTS 1.28 Mcps TDD Radio Access Technology; MS does supports UMTS TDD (1) or not (0)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"> Network Support for GERAN Feature 1 Package ( Rel 4 ) </XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>geran_feat_pack_1</Name>
                <BitLen>1</BitLen>
                <Version>REL99 OR TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>Network Support for GERAN Feature 1 Package</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Extended DTM GPRS Multi Slot Sub-Class</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ext_dtm_g_ms_class</Name>
                <BitLen>2</BitLen>
                <Version>REL99 OR TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>Extended DTM GPRS Multi Slot Sub-Class</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"> Extended DTM EGPRS Multi Slot Sub-Class </XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ext_dtm_e_ms_class</Name>
                <BitLen>2</BitLen>
                <Version>REL99 OR TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>Extended DTM EGPRS Multi Slot Sub-Class</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"> This indicates whether the MS supports a feature or not respectively whether the value is set or not. </XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dummy_r4_ind</Name>
                <BitLen>1</BitLen>
                <Comment>Dummy R4 inclusion indicator; A dummy field to suppress R4 fields (esp.in MS RACAP)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>ccn_support</Name>
                <BitLen>1</BitLen>
                <Version>REL99</Version>
                <Comment>CCN is supported towards the corresponding cell</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ccn_supported</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="05" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Modulation based multislot class support</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>mod_ms_sup</Name>
                <BitLen>1</BitLen>
                <Version>REL99</Version>
                <Comment>Modulation based multislot class support</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">TDD_Indic0, information 0 indicator (1 bit): This field indicates if the TDD_CELL_INFORMATION parameter value ‘0000000000’ is a member of the set. Bit0 parameter value ‘0000000000’ is not a member of the set1 parameter value ‘0000000000’ is a member of the set</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tdd_indic0</Name>
                <BitLen>1</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>TDD_Indic0</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="09" Month="06" Year="2004"/>
                <Author>XGIRIDHA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">TDD_CELL_INFORMATION Field (q bit field) This field allows to compute a set of 9-bit-long TDD_CELL_INFORMATION parameters, re-using the Range 512 format compression algorithm. The formulas for decoding are given in the 'Range 512 format' sub-clause, 10.5.2.13.4, with w0=0.  The consecutive parameters of this field are concatenated, starting withw1, and then w2, w3… The total number of bits q of this field depends on the value of the parameter NR_OF_TDD_CELLS = m This is derived from function implementation in CCD. If m=0 and TDD_Indic0=0 or m is equal or greater than 21, this shall not be considered as an error;  the corresponding index in the 3G Neighbour Cell list shall be incremented by one. For each (9-bit-long) decoded Parameter, bits 1-7 are the Cell Parameter, bit 8 is the Sync Case and bit 9 is the Diversity bit. </XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tdd_ncell_data</Name>
                <BitLen>9</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>bits 1-7 are the Cell Parameter, bit 8 is the Sync Case and bit 9 is the Diversity bit. </Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="09" Month="06" Year="2004"/>
                <Author>XGIRIDHA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field indicates if the FDD_CELL_INFORMATION parameter value ‘0000000000’ is a member of the set. Bit0 parameter value ‘0000000000’ is not a member of the set1 parameter value ‘0000000000’ is a member of the set NOTE: This bit FDD_Indic0 is equivalent to the bit F0 bit in the frequency list information element (see sub-clause 10.5.2.13.3).</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>fdd_indic0</Name>
                <BitLen>1</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>FDD_Indic0</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="09" Month="06" Year="2004"/>
                <Author>XGIRIDHA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This field allows to compute a set of 10-bit-long FDD_CELL_INFORMATION parameters, re-using the Range 1024 format compression algorithm. The formulas for decoding are given in the 'Range 1024 format' sub-clause, 10.5.2.13.3.  The consecutive parameters of this field are concatenated, starting with w1, and then w2, w3… The total number of bits p of this field depends on the value of the parameter NR_OF_FDD_CELLS = n. (mapping fn.p(x) ) If n=0 and FDD_Indic0=0, this indicates the 3G Neighbour Cell list index for report on RSSI, see 3GPP TS 45.008.If n is equal or greater than 17, this shall not be considered as an error; the corresponding index in the 3G Neighbour Cell list shall be incremented by one.For each (10-bit-long) decoded Parameter, bits 1-9 are the Scrambling Code and bit 10 is the corresponding Diversity Parameter. </XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>fdd_ncell_data</Name>
                <BitLen>10</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>bits 1-9 are the Scrambling Code and bit 10 is the corresponding Diversity Parameter</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="09" Month="06" Year="2004"/>
                <Author>XGIRIDHA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>index_start_3g</Name>
                <BitLen>7</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Index Start 3G</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>abs_index_emr</Name>
                <BitLen>7</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Absolute Index start EMR</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.56 (3G Target Cell)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bw_fdd</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Bandwidth FDD</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.56 (3G Target Cell)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>bw_tdd</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Bandwidth TDD</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.1d (UTRAN Frequency List)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>fdd_arfcn</Name>
                <BitLen>14</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>FDD_ARFCN</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>fdd_arfcn_index</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>FDD ARFCN index</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference : [3GPP 04.18] section 10.5.2.1d (UTRAN Frequency List)</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tdd_arfcn</Name>
                <BitLen>14</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>TDD_ARFCN</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP 04.18] section 10.5.2.33b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tdd_arfcn_index</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>TDD ARFCN index</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="10" Month="12" Year="2002"/>
                <Author>JMA</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cdma2000_frequency_band </Name>
                <BitLen>5</BitLen>
                <Comment>cdma2000 frequency band </Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cdma2000_frequency</Name>
                <BitLen>11</BitLen>
                <Comment>cdma2000 frequency</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>number_cdma2000_cells</Name>
                <BitLen>5</BitLen>
                <Comment>number_cdma2000_cells</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>pilot_PN_offset</Name>
                <BitLen>9</BitLen>
                <Comment>Pilot PN offset</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>td_mode</Name>
                <BitLen>2</BitLen>
                <Comment>TD_MODE</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>td_power_level</Name>
                <BitLen>3</BitLen>
                <Comment>TD_POWER_LEVEL </Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>qof</Name>
                <BitLen>2</BitLen>
                <Comment>QOF</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>walsh_len_a</Name>
                <BitLen>3</BitLen>
                <Comment>WALSH_LEN_A</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>aux_pilot_walsh</Name>
                <BitLen>1</BitLen>
                <Comment>AUX_PILOT_WALSH</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>walsh_len_b</Name>
                <BitLen>3</BitLen>
                <Comment>WALSH_LEN_B </Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>aux_td_walsh</Name>
                <BitLen>1</BitLen>
                <Comment>AUX_TD_WALSH</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>aux_td_power_level</Name>
                <BitLen>2</BitLen>
                <Comment>AUX_TD_POWER_LEVEL</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>sr3_prim_pilot</Name>
                <BitLen>2</BitLen>
                <Comment>SR3_PRIM_PILOT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>sr3_pilot_power1</Name>
                <BitLen>3</BitLen>
                <Comment>SR3_PILOT_POWER1</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>sr3_pilot_power2</Name>
                <BitLen>3</BitLen>
                <Comment>SR3_PILOT_POWER2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>walsh_len_c</Name>
                <BitLen>3</BitLen>
                <Comment>WALSH_LEN_C</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>aux_walsh_len</Name>
                <BitLen>1</BitLen>
                <Comment>AUX_WALSH_LEN </Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>qof1</Name>
                <BitLen>2</BitLen>
                <Comment>QOF1</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>walsh_length1</Name>
                <BitLen>3</BitLen>
                <Comment>WALSH_LENGTH1</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>aux_pilot_walsh1</Name>
                <BitLen>1</BitLen>
                <Comment>AUX_PILOT_WALSH1</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>qof2</Name>
                <BitLen>2</BitLen>
                <Comment>QOF2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>walsh_length2</Name>
                <BitLen>3</BitLen>
                <Comment>WALSH_LENGTH2 </Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>aux_pilot_walsh2</Name>
                <BitLen>1</BitLen>
                <Comment>AUX_PILOT_WALSH2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>flag_3bit</Name>
                <BitLen>3</BitLen>
                <Comment>FLAG 3 bits</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="03" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [2] section 11.2.4</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>search_prio_3g</Name>
                <BitLen>1</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Search Prio 3G</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [2] section 11.2.23</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tdd_multirat_rep</Name>
                <BitLen>2</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>TDD Multirat Reporting</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [2] section 11.2.9b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cdma2000_multirat_rep</Name>
                <BitLen>2</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>CDMA2000 Multirat Reporting</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="11" Month="01" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [2] section 11.2.23</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>fdd_rep_quant</Name>
                <BitLen>1</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>FDD REP Quant</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [2] section 11.2.23</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>fdd_multi_rep</Name>
                <BitLen>2</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>FDD MULTI Reporting Struct</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [2] section 11.2.23</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>fdd_rep_offset</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>FDD Reporting Offset</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [2] section 11.2.23</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>fdd_rep_thres</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>FDD Reporting Threshold</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [2] section 11.2.23</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tdd_rep_offset</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>TDD Reporting Offset</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [2] section 11.2.9b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cdma2000_rep_offset</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>CDMA2000 Reporting Offset</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="11" Month="1" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [2] section 11.2.23</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>tdd_rep_thres</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>TDD Reporting Threshold</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="6" Month="12" Year="2002"/>
                <Author>CTN</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [2] section 11.2.9b</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>cdma2000_rep_thres</Name>
                <BitLen>3</BitLen>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>CDMA2000 Reporting Threshold</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="11" Month="1" Year="2004"/>
                <Author>HB</Author>
                <Comment>Initial version release 99</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [2] section 11.2.4</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>qsearch_c</Name>
                <BitLen>4</BitLen>
                <Comment>Qsearch C</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="15" Month="6" Year="2004"/>
                <Author>XGIRIDHA</Author>
                <Comment>Initial version </Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>flag_ra_cap2</Name>
                <BitLen>1</BitLen>
                <Version>!REL99</Version>
                <Comment>Valid flag for MS RA capability value part II; Second part of MS RA capability is available (1) or not (1)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="19" Month="04" Year="2006"/>
                <Author>Gopinath</Author>
                <Comment>R97 RAC</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>high_ms_cap</Name>
                <BitLen>2</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>High Multislot Capability</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>geran_iu_mod_cap</Name>
                <BitLen>1</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>GERAN Iu Mode Capabilities</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>geran_feat_pack_2</Name>
                <BitLen>1</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>GERAN Feature Package 2</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>gmsk_ms_pwr_prof</Name>
                <BitLen>2</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>GMSK Multislot Power Profile</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ms_pwr_profile</Name>
            </ValuesLink>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>psk8_ms_pwr_prof</Name>
                <BitLen>2</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>8-PSK Multislot Power Profile</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_ms_pwr_profile</Name>
            </ValuesLink>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dl_adv_rx_per</Name>
                <BitLen>2</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>Downlink Advanced Receiver Performance</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_dl_adv_rx_per</Name>
            </ValuesLink>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>dtm_enhance_cap</Name>
                <BitLen>1</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>DTM Enhancements Capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">rr_com</DocName>
                <Name>VAL_bool</Name>
            </ValuesLink>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reference: [3GPP_TS24.008] section 10.5.1.7</XHTMLElement>
                </DocElement>
            </Description>
            <MsgBasicElemDef>
                <Name>offset_required</Name>
                <BitLen>1</BitLen>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>Offset required</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
    </MsgBasicElementsSection>
    <ValuesSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all sets of values that are defined for the RR_COM AIM</XHTMLElement>
            </DocElement>
        </Description>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ab_type</Name>
                <Version>REL99</Version>
                <Comment>values for ab_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>AB_8_BIT</Alias>
                <Comment>8 bit access burst shall be used</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>AB_11_BIT</Alias>
                <Comment>11 bit access burst shall be used</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_acc_tech_typ</Name>
                <Comment>values for acc_tech_typ</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ACC_GSM_P</Alias>
                <Comment>GSM P</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ACC_GSM_E</Alias>
                <Comment>GSM E -note that GSM E covers GSM P</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>ACC_GSM_R</Alias>
                <Comment>GSM R - note that GSM R covers GSM E and GSM P</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>ACC_GSM_1800</Alias>
                <Comment>GSM 1800 (DCS)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>ACC_GSM_1900</Alias>
                <Comment>GSM 1900 (PCS)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>ACC_GSM_450</Alias>
                <Comment>GSM 450</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>ACC_GSM_480</Alias>
                <Comment>GSM 480</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>ACC_GSM_850</Alias>
                <Comment>GSM 850</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>ACC_CAP_SAME_AS_PRECED</Alias>
                <Version>REL99</Version>
                <Comment>When access capabilities of a band is same as it's previously included band.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias>ACC_INVALID</Alias>
                <Version>REL99</Version>
                <Comment>no valid access technology type present (this value isn?t defined in the specification)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>ACC_INVALID</Alias>
                <Version>!REL99</Version>
                <Comment>no valid access technology type present (this value isn?t defined in the specification)</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>unknown</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pow_class</Name>
                <Comment>values for pow_class</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>POWER_CLASS_1</Alias>
                <Comment>Power Class 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>POWER_CLASS_2</Alias>
                <Comment>Power Class 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>POWER_CLASS_3</Alias>
                <Comment>Power Class 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>POWER_CLASS_4</Alias>
                <Comment>Power Class 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>POWER_CLASS_5</Alias>
                <Comment>Power Class 5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias/>
                <Comment>Reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias/>
                <Comment>Reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="ALPHA">POWER_CLASS_2</Value>
                <Alias>MIN_CLASS_GSM</Alias>
                <Comment>minimal GSM power class</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="ALPHA">POWER_CLASS_5</Value>
                <Alias>MAX_CLASS_GSM</Alias>
                <Comment>maximal GSM power class</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="ALPHA">POWER_CLASS_1</Value>
                <Alias>MIN_CLASS_DCS</Alias>
                <Comment>minimal DCS power class</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="ALPHA">POWER_CLASS_3</Value>
                <Alias>MAX_CLASS_DCS</Alias>
                <Comment>maximal DCS power class</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="ALPHA">POWER_CLASS_1</Value>
                <Alias>MIN_CLASS_PCS</Alias>
                <Comment>minimal PCS power class</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="ALPHA">POWER_CLASS_3</Value>
                <Alias>MAX_CLASS_PCS</Alias>
                <Comment>maximal PCS power class</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="ALPHA">POWER_CLASS_5</Value>
                <Alias>CLASS_MIN_POW_GSM</Alias>
                <Comment>GSM power class with the lowest output power</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="ALPHA">POWER_CLASS_2</Value>
                <Alias>CLASS_MIN_POW_DCS</Alias>
                <Comment>DCS power class with the lowest output power</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="ALPHA">POWER_CLASS_2</Value>
                <Alias>CLASS_MIN_POW_PCS</Alias>
                <Comment>PCS power class with the lowest output power</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>IDX_PWRCLASS_900</Alias>
                <Comment>Index for use with rf_cap.rf_power.pow_class4[] array</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>IDX_PWRCLASS_1800</Alias>
                <Comment>Index for use with rf_cap.rf_power.pow_class4[] array</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>IDX_PWRCLASS_1900</Alias>
                <Comment>Index for use with rf_cap.rf_power.pow_class4[] array</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>IDX_PWRCLASS_850</Alias>
                <Comment>Index for use with rf_cap.rf_power.pow_class4[] array</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>IDX_PWRCLASS_400</Alias>
                <Comment>Index for use with rf_cap.rf_power.pow_class4[] array</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>IDX_PWRCLASS_700</Alias>
                <Version>REL99</Version>
                <Comment>Index for use with rf_cap.rf_power.pow_class4[] array</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Added GSM 700</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_bool</Name>
                <Comment>values for bool</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NO</Alias>
                <Comment>value is not set</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>YES</Alias>
                <Comment>value is set</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NOT_SUPPORTED</Alias>
                <Comment>feature not supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SUPPORTED</Alias>
                <Comment>feature supported</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_flag</Name>
                <Comment>values for flag</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>GRR_NO</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>GRR_YES</Alias>
                <Comment>present</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_bss_paging_coord</Name>
                <Version>REL99</Version>
                <Comment>values for bss_paging_coord</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CS_PG_NOT_SUPPORTED</Alias>
                <Comment>The cell does not support Circuit-Switched paging co-ordination</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CS_PG_SUPPORTED</Alias>
                <Comment>The cell supports Circuit-Switched paging co-ordination</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ctrl_ack_type</Name>
                <Comment>values for ctrl_ack_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>default format is four access bursts</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>default format is RLC/MAC control block.</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_dtm_g_ms_class</Name>
                <Comment>values for dtm_g_ms_class</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SUB_CLASS_1</Alias>
                <Comment>Sub-Class 1 supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SUB_CLASS_5</Alias>
                <Comment>Sub-Class 5 supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SUP_CLASS_9</Alias>
                <Comment>Sub-Class 9 supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias/>
                <Comment>Reserved</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_dtm_g_high_ms_class</Name>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>values for dtm_g_high_ms_class</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>Reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SUB_CLASS_31_OR_36</Alias>
                <Comment>Multislot class 31 or 36 supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SUB_CLASS_32_OR_37</Alias>
                <Comment>Multislot class 32 or 37 supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SUB_CLASS_33_OR_38</Alias>
                <Comment>Multislot class 33 or 38 supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SUB_CLASS_41</Alias>
                <Comment>Multislot class 41 supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SUB_CLASS_42</Alias>
                <Comment>Multislot class 42 supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>SUB_CLASS_43</Alias>
                <Comment>Multislot class 43 supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>SUB_CLASS_44</Alias>
                <Comment>Multislot class 44 supported</Comment>
            </ValuesItem>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_dtm_support</Name>
                <Version>REL99</Version>
                <Comment>values for dtm_support</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DTM_NOT_SUPPORTED</Alias>
                <Comment>The cell does not support DTM procedures.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DTM_SUPPORTED</Alias>
                <Comment>The cell supports DTM procedures.</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_egprs_packet_channel_request</Name>
                <Version>REL99</Version>
                <Comment>values for egprs_packet_channel_request</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EGPRS_PACKET_CHANNEL_REQUEST_MSG_SENT</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PACKET_CHANNEL_REQUEST_MSG_SENT</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_bands</Name>
                <Comment>values for bands</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>BAND_AUTO</Alias>
                <Comment>0b00000000: All bands shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>BAND_GSM_900</Alias>
                <Comment>0b00000001: GSM 900 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>BAND_DCS_1800</Alias>
                <Comment>0b00000010: DCS 1800 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>BAND_PCS_1900</Alias>
                <Comment>0b00000100: PCS 1900 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">08</Value>
                <Alias>BAND_E_GSM</Alias>
                <Comment>0b00001000: Extended GSM is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">10</Value>
                <Alias>BAND_GSM_850</Alias>
                <Comment>0b00010000: GSM 850 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">20</Value>
                <Alias>BAND_GSM_450</Alias>
                <Comment>0b00100000: GSM 450 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">40</Value>
                <Alias>BAND_GSM_480</Alias>
                <Comment>0b01000000: GSM 480 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">80</Value>
                <Alias>BAND_R_GSM</Alias>
                <Comment>0b10000000: R-GSM is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>BAND_DUAL</Alias>
                <Comment>0b00000011: GSM 900 and DCS 1800 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0B</Value>
                <Alias>BAND_DUAL_EXT</Alias>
                <Comment>0b00001011: GSM 900, E-GSM and DCS 1800 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">14</Value>
                <Alias>BAND_DUAL_US</Alias>
                <Comment>0b00010100: GSM 850 and PCS 1900 is supported, shall be scanned</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_egsm</Name>
                <Comment>values for egsm</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EGSM_NOT_SUPPORTED</Alias>
                <Comment>The mobile station does not support the extension band.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EGSM_SUPPORTED</Alias>
                <Comment>The mobile station does support the extension band (E-GSM or R-GSM).</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_freq_scroll</Name>
                <Version>REL99</Version>
                <Comment>values for freq_scroll</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SCROL_NO</Alias>
                <Comment>Frequency scrolling is not used</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SCROL_YES</Alias>
                <Comment>Frequency scrolling is used</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_gsm400_supp</Name>
                <Comment>values for gsm400_supp</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>reserved (if neither GSM 480 nor GSM 450 is supported the whole gsm400_struct is omitted)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>GSM480</Alias>
                <Comment>GSM 480 supported but GSM 450 not supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>GSM450</Alias>
                <Comment>GSM 450 supported but GSM 480 not supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>GSM450_480</Alias>
                <Comment>GSM 450 supported and GSM 480 supported</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pow_8psk_cap</Name>
                <Comment>values for pow_8psk_cap</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>Reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>POWER_CLASS_E1</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>POWER_CLASS_E2</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>POWER_CLASS_E3</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_mod_cap</Name>
                <Comment>values for mod_cap</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DL_ONLY_8PSK</Alias>
                <Comment>8-PSK supported for downlink reception only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>FULL_8PSK</Alias>
                <Comment>8-PSK supported for uplink transmission and downlink reception</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_mb_value</Name>
                <Comment>values for mb_value</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MB_NO_EUROPEAN_BAND</Alias>
                <Comment>0b000: neither GSM 900, E-GSM or DCS 1800 supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MB_GSM900</Alias>
                <Comment>0b001: GSM 900 is supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MB_EGSM</Alias>
                <Comment>0b010: E-GSM is supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>MB_DCS1800</Alias>
                <Comment>0b100: DCS 1800 is supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>MB_DUAL</Alias>
                <Comment>0b101: GSM 900 and DCS 1800 is supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>MB_DUAL_EXT</Alias>
                <Comment>0b110: E-GSM and DCS 1800 is supported</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ms_class</Name>
                <Comment>values for ms_class</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MSLOT_CLASS_1</Alias>
                <Comment>Multi Slot Class 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MSLOT_CLASS_2</Alias>
                <Comment>Multi Slot Class 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MSLOT_CLASS_3</Alias>
                <Comment>Multi Slot Class 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>MSLOT_CLASS_4</Alias>
                <Comment>Multi Slot Class 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>MSLOT_CLASS_5</Alias>
                <Comment>Multi Slot Class 5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>MSLOT_CLASS_6</Alias>
                <Comment>Multi Slot Class 6</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>MSLOT_CLASS_7</Alias>
                <Comment>Multi Slot Class 7</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>MSLOT_CLASS_8</Alias>
                <Comment>Multi Slot Class 8</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>MSLOT_CLASS_9</Alias>
                <Comment>Multi Slot Class 9</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>MSLOT_CLASS_10</Alias>
                <Comment>Multi Slot Class 10</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>MSLOT_CLASS_11</Alias>
                <Comment>Multi Slot Class 11</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>MSLOT_CLASS_12</Alias>
                <Comment>Multi Slot Class 12</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">13</Value>
                <Alias>MSLOT_CLASS_13</Alias>
                <Comment>Multi Slot Class 13</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias>MSLOT_CLASS_14</Alias>
                <Comment>Multi Slot Class 14</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>MSLOT_CLASS_15</Alias>
                <Comment>Multi Slot Class 15</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">16</Value>
                <Alias>MSLOT_CLASS_16</Alias>
                <Comment>Multi Slot Class 16</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">17</Value>
                <Alias>MSLOT_CLASS_17</Alias>
                <Comment>Multi Slot Class 17</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">18</Value>
                <Alias>MSLOT_CLASS_18</Alias>
                <Comment>Multi Slot Class 18</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">19</Value>
                <Alias>MSLOT_CLASS_19</Alias>
                <Comment>Multi Slot Class 19</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">20</Value>
                <Alias>MSLOT_CLASS_20</Alias>
                <Comment>Multi Slot Class 20 (not for HSCSD)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">21</Value>
                <Alias>MSLOT_CLASS_21</Alias>
                <Comment>Multi Slot Class 21 (not for HSCSD)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">22</Value>
                <Alias>MSLOT_CLASS_22</Alias>
                <Comment>Multi Slot Class 22 (not for HSCSD)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">23</Value>
                <Alias>MSLOT_CLASS_23</Alias>
                <Comment>Multi Slot Class 23 (not for HSCSD)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">24</Value>
                <Alias>MSLOT_CLASS_24</Alias>
                <Comment>Multi Slot Class 24 (not for HSCSD)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">25</Value>
                <Alias>MSLOT_CLASS_25</Alias>
                <Comment>Multi Slot Class 25 (not for HSCSD)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">26</Value>
                <Alias>MSLOT_CLASS_26</Alias>
                <Comment>Multi Slot Class 26 (not for HSCSD)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">27</Value>
                <Alias>MSLOT_CLASS_27</Alias>
                <Comment>Multi Slot Class 27 (not for HSCSD)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">28</Value>
                <Alias>MSLOT_CLASS_28</Alias>
                <Comment>Multi Slot Class 28 (not for HSCSD)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">29</Value>
                <Alias>MSLOT_CLASS_29</Alias>
                <Comment>Multi Slot Class 29 (not for HSCSD)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_nmo</Name>
                <Comment>values for nmo</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias/>
                <Comment>Network Mode 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias/>
                <Comment>Network Mode 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10</Value>
                <Alias/>
                <Comment>Network Mode 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pfc_feature_mode</Name>
                <Version>REL99</Version>
                <Comment>values for pfc_feature_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PFC_NOT_SUPPORTED</Alias>
                <Comment>The network does not support packet flow context procedures.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PFC_SUPPORTED</Alias>
                <Comment>The network supports packet flow context procedures.</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rep_priority</Name>
                <Version>REL99</Version>
                <Comment>values for rep_priority</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NORMAL_PRIO</Alias>
                <Comment>Normal reporting priority</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>HIGH_PRIO</Alias>
                <Comment>High reporting priority</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rf_pow_cap</Name>
                <Comment>values for rf_pow_cap</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>RF_CLASS_1</Alias>
                <Comment>class 1 for GSM 850, 900P+E, DCS 1800 and PCS 1900</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>RF_CLASS_2</Alias>
                <Comment>class 2 for GSM 850, 900P+E, DCS 1800 and PCS 1900</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>RF_CLASS_3</Alias>
                <Comment>class 3 for GSM 850, 900P+E, DCS 1800 and PCS 1900</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>RF_CLASS_4</Alias>
                <Comment>class 4 for GSM 850, 900P+E (reserved for DCS 1800 and PCS 1900)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>RF_CLASS_5</Alias>
                <Comment>class 5 for GSM 850, 900P+E (reserved for DCS 1800 and PCS 1900)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>RF_CLASS_IRRELEVANT</Alias>
                <Comment>irrelevant for this IE (multiband GSM MS)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rev_lev</Name>
                <Comment>values for rev_lev</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>REV_LEV_PHASE_1</Alias>
                <Comment>Reserved for GSM phase 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>REV_LEV_PHASE_2</Alias>
                <Comment>Used by GSM phase 2 mobile stations</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>REV_LEV_R99_SUPPORT</Alias>
                <Comment>Used by mobile stations supporting R99 or later versions</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Reserved by future use</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rev99</Name>
                <Version>REL99</Version>
                <Comment>values for rev99</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PHASE_1</Alias>
                <Comment>Release ?98 or older</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>RELEASE99</Alias>
                <Comment>Release ?99 onwards</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_single_band</Name>
                <Comment>values for single_band</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SINGLE_EGSM</Alias>
                <Comment>Extended GSM is supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SINGLE_GSM900</Alias>
                <Comment>GSM 900 is supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SINGLE_DCS1800</Alias>
                <Comment>DCS 1800 is supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SINGLE_GSM450</Alias>
                <Comment>GSM 450 is supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SINGLE_GSM480</Alias>
                <Comment>GSM 480 is supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SINGLE_GSM850</Alias>
                <Comment>GSM 850 is supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>SINGLE_PCS1900</Alias>
                <Comment>PCS 1900 is supported</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_sms_val</Name>
                <Comment>values for sms_val</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SM_1</Alias>
                <Comment>1/4  timeslot (~144 micro sec)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SM_2</Alias>
                <Comment>2/4 timeslot (~288 micro sec)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SM_3</Alias>
                <Comment>3/4 timeslot (~433 micro sec)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SM_4</Alias>
                <Comment>4/4 timeslot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SM_5</Alias>
                <Comment>5/4 timeslot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SM_6</Alias>
                <Comment>6/4 timeslot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>SM_7</Alias>
                <Comment>7/4 timeslot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>SM_8</Alias>
                <Comment>8/4 timeslot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>SM_9</Alias>
                <Comment>9/4 timeslot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>SM_10</Alias>
                <Comment>10/4 timeslot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>SM_11</Alias>
                <Comment>11/4 timeslot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>SM_12</Alias>
                <Comment>12/4 timeslot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>SM_13</Alias>
                <Comment>13/4 timeslot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">13</Value>
                <Alias>SM_14</Alias>
                <Comment>14/4 timeslot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias>SM_15</Alias>
                <Comment>15/4 timeslot</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>SM_16</Alias>
                <Comment>16/4 timeslot (~2307 micro sec)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ss_screen</Name>
                <Comment>values for ss_screen</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SS_SCREEN_DEFAULT</Alias>
                <Comment>default value of phase 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SS_SCREEN_PHASE_2</Alias>
                <Comment>capability of handling of ellipsis notation and phase 2 error handling</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>for future use (The network shall interpret these values the same as ?1?)</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ucs2_treat</Name>
                <Comment>values for ucs2_treat</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DEFAULT_PREF</Alias>
                <Comment>the ME has a preference for the default alphabet (defined in GSM 03.38) over UCS2.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NO_PREF</Alias>
                <Comment>the ME has no preference between the use of the default alphabet and the use of UCS2.</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rep_offset_900</Name>
                <Version>REL99</Version>
                <Comment>values for rep_offset_900</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ZERO_DB</Alias>
                <Comment>Apply an offset of 0 dB to the reported value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SIX_DB</Alias>
                <Comment>Apply an offset of 6 dB to the reported value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>TWELVE_DB</Alias>
                <Comment>Apply an offset of 12 dB to the reported value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>EIGHTEEN_DB</Alias>
                <Comment>Apply an offset of 18 dB to the reported value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>TWENTYFOUR_DB</Alias>
                <Comment>Apply an offset of 24 dB to the reported value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>THIRTY_DB</Alias>
                <Comment>Apply an offset of 30 dB to the reported value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>THIRTYSIX_DB</Alias>
                <Comment>Apply an offset of 36 dB to the reported value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>FORTYTWO_DB</Alias>
                <Comment>Apply an offset of 42 dB to the reported value</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_th_rep_900</Name>
                <Version>REL99</Version>
                <Comment>values for th_rep_900</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ZERO</Alias>
                <Comment>Apply priority reporting if the reported value is above 0 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SIX</Alias>
                <Comment>Apply priority reporting if the reported value is above 6 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>TWELVE</Alias>
                <Comment>Apply priority reporting if the reported value is above 12 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>EIGHTEEN</Alias>
                <Comment>Apply priority reporting if the reported value is above 18 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>TWENTYFOUR</Alias>
                <Comment>Apply priority reporting if the reported value is above 24 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>THIRTY</Alias>
                <Comment>Apply priority reporting if the reported value is above 30 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>THIRTYSIX</Alias>
                <Comment>Apply priority reporting if the reported value is above 36 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>INDEFINITELY</Alias>
                <Comment>Never apply priority reporting</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">CCN (NACC )Support  by Rel 4 Network</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ccn_active</Name>
                <Version>REL99</Version>
                <Comment>Values for ccn_active</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>The Cell has not enabled CCN procedure.(but if received on PMO/ PCCO then follow the one received on broadcast)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>The Cell has enabled CCN procedure.</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Extended Uplink TBF Support  by Rel 4 Network</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_nw_ext_ul_tbf</Name>
                <Version>REL99</Version>
                <Comment>Values for nw_ext_ul_tbf</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EXT_UL_TBF_NOT_SUPPORTED</Alias>
                <Comment>The network does not support Extended UL TBF procedures.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EXT_UL_TBF_SUPPORTED</Alias>
                <Comment>The network does support Extended UL TBF procedures.</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="01" Year="2004"/>
                <Author>x0abuali</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ccn_supported</Name>
                <Version>REL99</Version>
                <Comment>Values for ccn_supported</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CCN_SUPPORTED</Alias>
                <Comment>CCN is enabled towards the corresponding cell</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CCN_NOT_SUPPORTED</Alias>
                <Comment>CCN is disabled towards the corresponding cell</Comment>
            </ValuesItem>
            <History>
                <Date Day="12" Month="05" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ms_pwr_profile</Name>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>GMSK/8PSK Multislot Power Profile</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MS_PWR_PROF0</Alias>
                <Comment>MULTISLOT_POWER_PROFILE 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MS_PWR_PROF1</Alias>
                <Comment>MULTISLOT_POWER_PROFILE 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MS_PWR_PROF2</Alias>
                <Comment>MULTISLOT_POWER_PROFILE 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MS_PWR_PROF3</Alias>
                <Comment>MULTISLOT_POWER_PROFILE 3</Comment>
            </ValuesItem>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <DocLink DocType="OTHER">
                        <Name/>
                    </DocLink>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rep_acch_cap</Name>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>Indicates support of Repeated Downlink FACCH or Repeated SACCH</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>REP_DL_FACCH</Alias>
                <Comment>MS supports Repeated Downlink FACCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>REP_SACCH_DL_FACCH</Alias>
                <Comment>MS supports Repeated SACCH and Repeated Downlink FACCH</Comment>
            </ValuesItem>
            <History>
                <Date Day="20" Month="02" Year="2007"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_dl_adv_rx_per</Name>
                <Version>TI_PS_FF_REL99_AND_ABOVE</Version>
                <Comment>Values for dl_adv_rx_perf</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DL_ADVANC_RX_PERF_NOT_SUPPORT</Alias>
                <Comment>Downlink Advanced Receiver Performance not supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DL_ADVANC_RX_PERF_PHASE1_SUPPORT</Alias>
                <Comment>Downlink Advanced Receiver Performance – phase I supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>DL_ADVANC_RX_PERF_RESERVE_VALUE1</Alias>
                <Comment>If value is received by the network, they shall be interpreted as ‘01’.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>DL_ADVANC_RX_PERF_RESERVE_VALUE2</Alias>
                <Comment>If value is received by the network, they shall be interpreted as ‘01’.</Comment>
            </ValuesItem>
            <History>
                <Date Day="08" Month="06" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
    </ValuesSection>
</AIM>
