<?xml version="1.0" encoding="UTF-8"?>
<!-- edited with SAPE SAP Editor -->
<SAP xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="sap.xsd">
    <DocInfoSection>
        <DocName DocType="SAP">mph</DocName>
        <DocNum Number="109" Project="6148"/>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">The Protocol Stacks are used to define the functionality of the GSM protocols for interfaces. The GSM specifications are normative when used to describe the functionality of interfaces, but the stacks and the subdivision of protocol layers does not imply or restrict any implementation.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">The base of the Protocol Stack rests on the physical layer.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">The Data Link Layer (DL) is used to handle an acknowledged connection between mobile and base station. The LAPDm protocol is used.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">Radio Resource (RR) manages the resources of the air-interface. That means configuration of physical layer, cell selection and cell reselection, data transfer, RR-Connection handling.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">Mobility Management (MM) handles registration aspects for the mobile station. It detects changes of location areas and updates a mobile station in the new location area.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">Call Control (CC) provides the call functionality. This includes call establishment, call maintenance procedures like Hold, Retrieve or Modify, and call disconnection.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">Supplementary Services (SS) handles all call independent supplementary services like call forwarding or call barring.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">Short Message Services (SMS) is used for sending and receiving point-to-point short messages.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">The man machine interface (MMI) is the interface to the user. Normally it is connected with a keypad as input device and a display as output device.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">Between the several entities data interfaces are defined. These data interfaces are called Service Access Points (SAPs), indicating that an upper layer uses the services of a lower layer.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">The GSM specification do not set out any implementation of the Protocol Stack. The following diagrams show the implementation described in all these documents for the mobile station. All entities except the Man Machine Interface and Physical Layer are implemented as part of the Protocol Stack.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">Figure 1: Mobile-station protocol architecture</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This document describes the services offered by the physical layer to the radio resource management.</XHTMLElement>
            </DocElement>
        </Description>
        <DocHistory>
            <DocVersion Number="100" Year="97"/>
            <Date Day="26" Month="5" Year="1997"/>
            <Author>LE_et_al</Author>
            <DocStatus State="APPROVED"/>
            <Comment>Initial version.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="101" Year="97"/>
            <Date Day="20" Month="10" Year="1997"/>
            <Author>LE</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Changes for integration variant B, opcode direction bit changed.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="102" Year="97"/>
            <Date Day="19" Month="2" Year="1998"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add MODE_SYS_INFO_CHANGE.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="103" Year="97"/>
            <Date Day="28" Month="5" Year="1998"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add dummy parameter to avoid empty primitives.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="104" Year="97"/>
            <Date Day="15" Month="1" Year="1999"/>
            <Author>LE</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Removedunnecessary primitives.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="105" Year="97"/>
            <Date Day="18" Month="7" Year="2000"/>
            <Author>MPA</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add extensions for GPRS.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="106" Year="97"/>
            <Date Day="18" Month="7" Year="2001"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>PDCH Assignment, update references, use name Condat AG.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="107" Year="97"/>
            <Date Day="26" Month="10" Year="2001"/>
            <Author>SBK</Author>
            <DocStatus State="SUBMITTED"/>
            <Comment>Loads of changes to enhance clarity, preciseness etc. especially from the GTI point of view.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="200" Year="01"/>
            <Date Day="31" Month="10" Year="2001"/>
            <Author>SBK</Author>
            <DocStatus State="APPROVED"/>
            <Comment>Changes after review.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="201" Year="01"/>
            <Date Day="2" Month="11" Year="2001"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add Extended Measurmeent.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="202" Year="01"/>
            <Date Day="9" Month="4" Year="2002"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add GPRS Ext Measurement, re-format, change Date format.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="202" Year="01"/>
            <Date Day="4" Month="4" Year="2002"/>
            <Author>MSB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add Multiband Feature.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="203" Year="01"/>
            <Date Day="5" Month="5" Year="2002"/>
            <Author>MSB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>No comment.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="204" Year="01"/>
            <Date Day="29" Month="8" Year="2002"/>
            <Author>LG</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add E-OTD stuff. New parameter 'ch' at MPH_CHANNEL_MODE_REQ</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="205" Year="01"/>
            <Date Day="16" Month="9" Year="2002"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add Timing Advance in MPH_NCELL_POS_IND.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="206" Year="01"/>
            <Date Day="10" Month="12" Year="2002"/>
            <Author>VK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Change array size in MPH_EMO_MEAS_IND.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="207" Year="01"/>
            <Date Day="4" Month="2" Year="2003"/>
            <Author>LG</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>renamed components of cod_prop.</Comment>
        </DocHistory>
        <DocRef>
            <RefId>[1]</RefId>
            <RefTitle>GSM 01.04, Abbreviations and acronyms</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[2]</RefId>
            <RefTitle>GSM 03.41, Technical Realization of Short Message Service Cell Broadcast</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[3]</RefId>
            <RefTitle>GSM 04.03, MS-BSS Interface Channel Structures and Access Capabilities</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[4]</RefId>
            <RefTitle>GSM 04.07, Mobile Radio Interface Signalling Layer 3 General Aspects</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[5]</RefId>
            <RefTitle>GSM 04.08, Mobile Radio Interface Layer 3 Specification</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[6]</RefId>
            <RefTitle>GSM 04.12, Short Message Service Cell Broadcast Support on Mobile Radio Interface</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[7]</RefId>
            <RefTitle>GSM 04.14, Special conformance testing functions</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[8]</RefId>
            <RefTitle>GSM 05.01, Physical Layer on the Radio Path General Description</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[9]</RefId>
            <RefTitle>GSM 05.02, Multiplexing and Multiple Access on the Radio Path</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[10]</RefId>
            <RefTitle>GSM 05.05, Radio Transmission and Reception</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[11]</RefId>
            <RefTitle>GSM 05.08, Radio Sub-system Link Control</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[12]</RefId>
            <RefTitle>GSM 05.10, Radio Sub-system Synchronisation</RefTitle>
        </DocRef>
    </DocInfoSection>
    <ConstantsSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all constants that are defined for the MPH SAP</XHTMLElement>
            </DocElement>
        </Description>
        <Constant>
            <Alias>MAX_MA_CHANNELS</Alias>
            <Value ValueType="DEC">64</Value>
            <Comment>determines the (maximum) size of mobile allocation list; the list is delimited with 0xFFFF = NOT_PRESENT_16BIT (except if all entries are used)</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NEIGHBOURCELLS</Alias>
            <Value ValueType="DEC">33</Value>
            <Comment>determines the (maximum) size of neighbourcell list (maximal case is 32 neighbour cells and the serving cell); the list is delimited with 0xFFFF = NOT_PRESENT_16BIT (except if all entries are used)</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CHANNELS</Alias>
            <Value ValueType="DEC">100</Value>
            <Comment>used for power measurements (sum of a maximum of 25 GSM 900 / 850 channels and a maximum of 40 DCS 1800 / PCS 1900 channels)</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NCELL_EOTD_ALR</Alias>
            <Value ValueType="DEC">15</Value>
            <Comment>number of neighbour cells the layer 1 is able to perform EOTD measurements for</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NCELL_EOTD_RES</Alias>
            <Value ValueType="DEC">12</Value>
            <Comment>number of ncells returned</Comment>
        </Constant>
        <Constant>
            <Alias>XCOR_NO</Alias>
            <Value ValueType="DEC">18</Value>
            <Comment>number of cross correlation values</Comment>
        </Constant>
        <Constant>
            <Alias>STD_900</Alias>
            <Value ValueType="DEC">1</Value>
            <Comment>Frequency band GSM 900</Comment>
        </Constant>
        <Constant>
            <Alias>STD_EGSM</Alias>
            <Value ValueType="DEC">2</Value>
            <Comment>Frequency band extended GSM 900</Comment>
        </Constant>
        <Constant>
            <Alias>STD_1900</Alias>
            <Value ValueType="DEC">3</Value>
            <Comment>Frequency band PCS 1900 (US band)</Comment>
        </Constant>
        <Constant>
            <Alias>STD_1800</Alias>
            <Value ValueType="DEC">4</Value>
            <Comment>Frequency band DCS 1800</Comment>
        </Constant>
        <Constant>
            <Alias>STD_DUAL</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment>Dual frequency band GSM 900 and DCS 1800</Comment>
        </Constant>
        <Constant>
            <Alias>STD_DUAL_EGSM</Alias>
            <Value ValueType="DEC">6</Value>
            <Comment>Dual frequency band extended GSM 900 and DCS 1800</Comment>
        </Constant>
        <Constant>
            <Alias>STD_850</Alias>
            <Value ValueType="DEC">7</Value>
            <Comment>Frequency band GSM 850 (US band)</Comment>
        </Constant>
        <Constant>
            <Alias>STD_DUAL_US</Alias>
            <Value ValueType="DEC">8</Value>
            <Comment>Dual frequency band GSM 850 and PCS 1900 (US bands)</Comment>
        </Constant>
        <Constant>
            <Alias>STD_850_1800</Alias>
            <Value ValueType="DEC">9</Value>
            <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
            <Comment>Dual frequency band GSM 850 and DCS 1800</Comment>
        </Constant>
        <Constant>
            <Alias>STD_900_1900</Alias>
            <Value ValueType="DEC">10</Value>
            <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
            <Comment>Dual frequency band GSM 900 and PCS 1900</Comment>
        </Constant>
        <Constant>
            <Alias>STD_850_900_1800</Alias>
            <Value ValueType="DEC">11</Value>
            <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
            <Comment>Tri frequency band GSM 850, GSM 900 and DCS 1800</Comment>
        </Constant>
        <Constant>
            <Alias>STD_850_900_1900</Alias>
            <Value ValueType="DEC">12</Value>
            <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
            <Comment>Tri frequency band GSM 850, GSM 900 and PCS 1900</Comment>
        </Constant>
        <Constant>
            <Alias>US_BIT</Alias>
            <Value ValueType="HEX">8000</Value>
            <Comment>the most significant bit is set for channel numbers of the united states to differentiate them from european channel numbers</Comment>
        </Constant>
        <Constant>
            <Alias>STD_BIT_MASK</Alias>
            <Value ValueType="HEX">7800</Value>
            <Comment>bit mask (bits 11..14 in the range 0..15) for  discriminate the std value from arfcn;                                             std =((arfcn&amp;STD_BIT_MASK)&gt;&gt;STD_BIT_SHIFT)+1; value range range 1..16</Comment>
        </Constant>
        <Constant>
            <Alias>STD_BIT_SHIFT</Alias>
            <Value ValueType="DEC">11</Value>
            <Comment>bit mask to eleminate the channel numbers without the US_BIT and the std bits</Comment>
        </Constant>
        <Constant>
            <Alias>ARFCN_MASK</Alias>
            <Value ValueType="HEX">07FF</Value>
            <Comment>bit mask to eleminate the channel numbers without the US_BIT and the std bits</Comment>
        </Constant>
        <Constant>
            <Alias>EUROPEAN_FREQ_AREA</Alias>
            <Value ValueType="DEC">1</Value>
            <Comment>search frequencies from the american frequency bands at power request</Comment>
        </Constant>
        <Constant>
            <Alias>AMERICAN_FREQ_AREA</Alias>
            <Value ValueType="DEC">2</Value>
            <Comment>search frequencies from the europeanfrequency bands at power request</Comment>
        </Constant>
        <Constant>
            <Alias>ALL_FREQ_AREA</Alias>
            <Value ValueType="DEC">3</Value>
            <Comment>search frequencies from all frequency bands at power request</Comment>
        </Constant>
        <Constant>
            <Alias>NEXT_AMERICAN_AREA</Alias>
            <Value ValueType="HEX">80</Value>
            <Comment>search frequencies from the american frequency bands at next scan part</Comment>
        </Constant>
        <Constant>
            <Alias>LOW_CHANNEL_900</Alias>
            <Value ValueType="DEC">1</Value>
            <Comment>Low border channel of the GSM 900 band</Comment>
        </Constant>
        <Constant>
            <Alias>HIGH_CHANNEL_900</Alias>
            <Value ValueType="DEC">124</Value>
            <Comment>High border channel of the GSM 900 band</Comment>
        </Constant>
        <Constant>
            <Alias>LOW_CHANNEL_EGSM</Alias>
            <Value ValueType="DEC">975</Value>
            <Comment>Low border channel of the extended GSM 900 band</Comment>
        </Constant>
        <Constant>
            <Alias>HIGH_CHANNEL_EGSM</Alias>
            <Value ValueType="DEC">1024</Value>
            <Comment>High border channel of the extended GSM 900 band</Comment>
        </Constant>
        <Constant>
            <Alias>CHANNEL_0</Alias>
            <Value ValueType="DEC">0</Value>
            <Comment>Channel 0 of the extended GSM 900 band</Comment>
        </Constant>
        <Constant>
            <Alias>CHANNEL_0_INTERNAL</Alias>
            <Value ValueType="DEC">1024</Value>
            <Comment>Channel 0 of the extended GSM 900 band in internal representation</Comment>
        </Constant>
        <Constant>
            <Alias>LOW_CHANNEL_1900</Alias>
            <Value ValueType="DEC">512</Value>
            <Comment>Low border channel of the OCS 1900 band</Comment>
        </Constant>
        <Constant>
            <Alias>HIGH_CHANNEL_1900</Alias>
            <Value ValueType="DEC">810</Value>
            <Comment>High border channel of the OCS 1900 band</Comment>
        </Constant>
        <Constant>
            <Alias>LOW_CHANNEL_1800</Alias>
            <Value ValueType="DEC">512</Value>
            <Comment>Low border channel of the DCS 1800 band</Comment>
        </Constant>
        <Constant>
            <Alias>HIGH_CHANNEL_1800</Alias>
            <Value ValueType="DEC">885</Value>
            <Comment>High border channel of the DCS 1800 band</Comment>
        </Constant>
        <Constant>
            <Alias>LOW_CHANNEL_850</Alias>
            <Value ValueType="DEC">128</Value>
            <Comment>Low border channel of the GSM 850 band</Comment>
        </Constant>
        <Constant>
            <Alias>HIGH_CHANNEL_850</Alias>
            <Value ValueType="DEC">251</Value>
            <Comment>High border channel of the GSM 850 band</Comment>
        </Constant>
        <Constant>
            <Alias>LOW_CHANNEL_1900_INTERNAL</Alias>
            <Value ValueType="DEC">1024</Value>
            <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
            <Comment>Low border channel of the PCS 1900 band used in L1</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CARRIERS_GSM900</Alias>
            <Value ValueType="DEC">124</Value>
            <Comment>Maximally number of carriers for GSM 900</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CARRIERS_EGSM900</Alias>
            <Value ValueType="DEC">174</Value>
            <Comment>Maximally number of carriers for extended GSM 900</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CARRIERS_PCS1900</Alias>
            <Value ValueType="DEC">299</Value>
            <Comment>Maximally number of carriers for PCS 1900</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CARRIERS_DCS1800</Alias>
            <Value ValueType="DEC">374</Value>
            <Comment>Maximally number of carriers for DCS 1800</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CARRIERS_DUAL</Alias>
            <Value ValueType="DEC">498</Value>
            <Comment>Maximally number of carriers for dual band with GSM 900 and DCS 1800</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CARRIERS_DUAL_EGSM</Alias>
            <Value ValueType="DEC">548</Value>
            <Comment>Maximally number of carriers for dual band with extended GSM 900 and DCS 1800</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CARRIERS_GSM850</Alias>
            <Value ValueType="DEC">124</Value>
            <Comment>Maximally number of carriers for GSM 850</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CARRIERS_DUAL_US</Alias>
            <Value ValueType="DEC">423</Value>
            <Comment>Maximally number of carriers for dual band with GSM 850 and PCS 1900</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_EMO_CHANNELS</Alias>
            <Value ValueType="DEC">21</Value>
            <Comment>21 ARFCN for Extended Measurement Order (SACCH)</Comment>
        </Constant>
        <Constant>
            <Alias>RR_BA_HIGH</Alias>
            <Value ValueType="DEC">255</Value>
            <Comment>maximum BA_ID used by RR</Comment>
        </Constant>
        <Constant>
            <Alias>RR_BA_LOW</Alias>
            <Value ValueType="DEC">128</Value>
            <Comment>minimum BA_ID used by RR</Comment>
        </Constant>
        <Constant>
            <Alias>ALR_BA_HIGH</Alias>
            <Value ValueType="DEC">127</Value>
            <Comment>maximum BA_ID used by ALR</Comment>
        </Constant>
        <Constant>
            <Alias>ALR_BA_LOW</Alias>
            <Value ValueType="DEC">0</Value>
            <Comment>minimum BA_ID used by ALR</Comment>
        </Constant>
        <Constant>
            <Alias>KC_STRING_SIZE</Alias>
            <Value ValueType="DEC">16</Value>
            <Comment>Maximum KC string length</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_RACH_REQ</Alias>
            <Value ValueType="DEC">8</Value>
            <Comment>Maximum number of RACH Requests</Comment>
        </Constant>
        <Constant>
            <Alias>RR_ALR_MEAS_REPORT_SIZE</Alias>
            <Value ValueType="DEC">7</Value>
            <Comment>Measurement report size(1 serving cell and 6 nc)</Comment>
        </Constant>
        <Constant>
            <Alias>LIST_MAX_SIZE</Alias>
            <Value ValueType="DEC">128</Value>
            <Comment>maximum arfcns 128x8-1024 carriers</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_REGIONS</Alias>
            <Value ValueType="DEC">2</Value>
            <Comment>maximum regions European and American</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NUM_BANDS</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment>Maximum number of frequency bands</Comment>
        </Constant>
        <Constant>
            <Alias>LOWER_RXLEV_THRESHOLD</Alias>
            <Value ValueType="DEC">4</Value>
            <Comment>lower rxlevel thershold below this value cells are not selected</Comment>
        </Constant>
        <Constant>
            <Alias>LOWER_RXLEV_THRESHOLD_850</Alias>
            <Value ValueType="DEC">7</Value>
            <Comment>lower rxlevel thershold for GSM 850 band</Comment>
        </Constant>
        <Constant>
            <Alias>B_GSM_850</Alias>
            <Value ValueType="DEC">0</Value>
            <Comment>Band index for GSM 850 band threshold rxlevel</Comment>
        </Constant>
        <Constant>
            <Alias>B_GSM_900</Alias>
            <Value ValueType="DEC">1</Value>
            <Comment>Band index for GSM 900 band threshold rxlevel</Comment>
        </Constant>
        <Constant>
            <Alias>B_DCS_1800</Alias>
            <Value ValueType="DEC">2</Value>
            <Comment>Band index for DCS 1800 band threshold rxlevel</Comment>
        </Constant>
        <Constant>
            <Alias>B_PCS_1900</Alias>
            <Value ValueType="DEC">3</Value>
            <Comment>Band index for PCS 1900 band threshold rxlevel</Comment>
        </Constant>
        <Constant>
            <Alias>B_E_GSM</Alias>
            <Value ValueType="DEC">4</Value>
            <Comment>Band index for EGSM band threshold rxlevel</Comment>
        </Constant>
        <Constant>
            <Alias>FULL_SEARCH_MODE_ATTEMPTS</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment>Number of power measurement attempts for Full search mode</Comment>
        </Constant>
        <Constant>
            <Alias>NORMAL_SEARCH_MODE_ATTEMPTS</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment>Number of power measurement attempts for Normal search mode</Comment>
        </Constant>
        <Constant>
            <Alias>TIM_FULL_SEARCH_POWERMEAS_VAL</Alias>
            <Value ValueType="DEC">4000</Value>
            <Comment>Maximum amount of time for full search power measurement </Comment>
        </Constant>
        <Constant>
            <Alias>TIM_NORMAL_SEARCH_POWERMEAS_VAL</Alias>
            <Value ValueType="DEC">4000</Value>
            <Comment>Maximum amount of time for Normal search power measurement </Comment>
        </Constant>
        <Constant>
            <Alias>MIN_CHANNELS_PER_BAND</Alias>
            <Value ValueType="DEC">25</Value>
            <Comment>Minimum number of channels per band should be added in MPH_POWER_CNF</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CHANNELS_PER_BAND</Alias>
            <Value ValueType="DEC">30</Value>
            <Comment>Maximum number of channels per band should be added in MPH_POWER_CNF</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NUM_CELLS_IN_REPORT</Alias>
            <Value ValueType="DEC">32</Value>
            <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
            <Comment>Maximum number of cells reported by ALR.</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NUM_CELLS_IN_REPORT</Alias>
            <Value ValueType="DEC">6</Value>
            <Version>!REL99 OR !(TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
            <Comment>Constant element</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NUM_OF_RTD_VALUES</Alias>
            <Value ValueType="DEC">3</Value>
            <Version>REL99 AND TI_PS_FF_RTD</Version>
            <Comment>Maximum number of RTD values available for an neighbour cell arfcn</Comment>
        </Constant>
        <History>
            <Date Day="15" Month="5" Year="1996"/>
            <Author>MS</Author>
            <Comment>Initial</Comment>
        </History>
        <History>
            <Date Day="3" Month="9" Year="1997"/>
            <Author>VK</Author>
            <Comment>set MAX_NEIGHBOURCELLS to 124</Comment>
        </History>
        <History>
            <Date Day="17" Month="9" Year="1997"/>
            <Author>LE</Author>
            <Comment>adapted to maximum</Comment>
        </History>
        <History>
            <Date Day="13" Month="7" Year="1997"/>
            <Author>LE</Author>
            <Comment>Constants minimized</Comment>
        </History>
        <History>
            <Date Day="4" Month="1" Year="1999"/>
            <Author>LE</Author>
            <Comment>MAX_CHANNELS, MAX_SDU_LEN added</Comment>
        </History>
        <History>
            <Date Day="7" Month="9" Year="2000"/>
            <Author>DG</Author>
            <Comment>enhancement for tripleband: MAX_CHANNELS = 120</Comment>
        </History>
        <History>
            <Date Day="5" Month="4" Year="2001"/>
            <Author>MPA</Author>
            <Comment>add constants</Comment>
        </History>
        <History>
            <Date Day="28" Month="10" Year="2001"/>
            <Author>SBK</Author>
            <Comment>removed MAC_BBCH_CHANNELS (obsolete); added comments;</Comment>
        </History>
        <History>
            <Date Day="09" Month="12" Year="2004"/>
            <Author>khasim</Author>
            <Comment>Added constants for cell selection improvements</Comment>
        </History>
        <History>
            <Date Day="05" Month="01" Year="2007"/>
            <Author>xparapgu</Author>
            <Comment>Added MAX_NUM_CELLS_IN_REPORT.</Comment>
        </History>
    </ConstantsSection>
    <PrimitivesSection PrimIDType="BIT16" SAPid="23">
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all primitives that are defined for the MPH SAP</XHTMLElement>
            </DocElement>
        </Description>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_POWER_REQ is used to start power measurements (used for carrier detection purposes) in PL. The field strength of all channels shall be measured.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_POWER_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="21"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>pch_interrupt</Name>
                </ItemLink>
                <Comment>pch interrupt</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>freq_bands</Name>
                </ItemLink>
                <Comment>frequency bands; used since support of 'PCS 1900 channels'</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>search_mode</Name>
                </ItemLink>
                <Comment>Search mode </Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>lower_rxlevel_threshold</Name>
                </ItemLink>
                <Control>[MAX_NUM_BANDS]</Control>
                <Comment>Lower Rxlev Threshold</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>black_list</Name>
                </ItemLink>
                <Comment>List of Black Listed carriers</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>white_list</Name>
                </ItemLink>
                <Comment>List of carriers in White List</Comment>
            </PrimItem>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description</Comment>
            </History>
            <History>
                <Date Day="8" Month="4" Year="2002"/>
                <Author>VK</Author>
                <Comment>comment changed for freq_bands</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_POWER_CNF is used by PL to send the result of power measurements (used for carrier detection purposes) to RR. A list of channels in decreasing field strength order shall be built by PL and sent to RR.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_POWER_CNF</Name>
                <PrimID Direction="UPLINK" Number="7"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>num_of_chan</Name>
                </ItemLink>
                <Comment>Number of channels</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>num_of_white_list_chan</Name>
                </ItemLink>
                <Comment>Number of White list channels</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>[MAX_CHANNELS]</Control>
                <Comment>cell channel numbers</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rx_lev</Name>
                </ItemLink>
                <Control>[MAX_CHANNELS]</Control>
                <Comment>field strength</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>inactive_carrier_list</Name>
                </ItemLink>
                <Comment>List of inactive carriers</Comment>
            </PrimItem>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, editorial corrections on elements' long names</Comment>
            </History>
            <History>
                <Date Day="07" Month="12" Year="2004"/>
                <Author>khasim</Author>
                <Comment>Added new parameter num_of_white_list_chan</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_BSIC_REQ is used to start in the PL the search for the frequency correction burst and synchronisation burst on the given physical channel.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_BSIC_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="22"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_BSIC_CNF is sent by PL to RR after successful detection of the synchronisation burst (element cs = CS_NO_ERROR) or to indicate the inability to detect the synchronisation burst (element cs = CS_NO_BCCH_AVAIL) of the previously requested channel.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_BSIC_CNF</Name>
                <PrimID Direction="UPLINK" Number="8"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Comment>base station identification code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>cs</Name>
                </ItemLink>
                <Comment>cause / error code; The following causes can occur within this primitive: CS_NO_ERROR, CS_NO_BCCH_AVAIL</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, added possible cause values</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_UNITDATA_IND is used to send unacknowledged information received via the air interface to RR (e.g. BCCH messages).</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_UNITDATA_IND</Name>
                <PrimID Direction="UPLINK" Number="9"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>fn</Name>
                </ItemLink>
                <Comment>full frame number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>sdu</Name>
                </ItemLink>
                <Comment>service data unit</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="29" Month="8" Year="2000"/>
                <Author>MPA</Author>
                <Comment>added frame number</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, changed long name to"full frame number"</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_RANDOM_ACCESS_REQ is used in the mobile station to request sending of (multiple) random access bursts.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_RANDOM_ACCESS_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="23"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>send_mode</Name>
                </ItemLink>
                <Comment>RACH sending mode</Comment>
            </PrimItem>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_RANDOM_ACCESS_CNF is used in the mobile station to confirm sending of a (single) random access burst including the frame number in which it was sent.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_RANDOM_ACCESS_CNF</Name>
                <PrimID Direction="UPLINK" Number="10"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>frame_no</Name>
                </ItemLink>
                <Comment>reduced frame number</Comment>
            </PrimItem>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Corrected description, changed long name</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_IDLE_REQ is used by RR to request from PL that a configuration of the idle mode, a so-called IDLE configuration, is set and adhered to.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_IDLE_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="3"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>mod</Name>
                </ItemLink>
                <Comment>idle mode scenario; the following mod values can occur within this primitive: MODE_CELL_SELECTION, MODE_CELL_RESELECTION, MODE_SYS_INFO_CHANGE, MODE_PACKET_TRANSFER (GPRS only), MODE_CELL_CHANGE_ORDER (GPRS only)</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ext_bcch</Name>
                </ItemLink>
                <Comment>dummy; unused, reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>comb_ccch</Name>
                </ItemLink>
                <Comment>combined CCCH</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <Comment>timeslot</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>dlt</Name>
                </ItemLink>
                <Comment>downlink timeout</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>pg</Name>
                </ItemLink>
                <Comment>paging group</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>bs_ag_blocks_res</Name>
                </ItemLink>
                <Comment>AGCH blocks reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>bs_pa_mfrms</Name>
                </ItemLink>
                <Comment>multiframe period</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>power</Name>
                </ItemLink>
                <Comment>transmission power level</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ncc_permitted</Name>
                </ItemLink>
                <Comment>NCC permitted</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>reorg_only</Name>
                </ItemLink>
                <Comment>page mode override; for a GSM only terminal the value is always NORMAL_PGM</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>eotd_avail</Name>
                </ItemLink>
                <Comment>EOTD available</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>gprs_support</Name>
                </ItemLink>
                <Comment>Cell supports GPRS; (GPRS only)</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>si2quater_status</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Indicates status of SI-2quater in serving cell</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>si2quater_pos</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Indicates position of SI-2quater (Normal or Extended BCCH)</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>Idle Mode Scenario added, opcode direction bit changed</Comment>
            </History>
            <History>
                <Date Day="12" Month="5" Year="1998"/>
                <Author>LE</Author>
                <Comment>CBCH removed</Comment>
            </History>
            <History>
                <Date Day="13" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>page mode removed</Comment>
            </History>
            <History>
                <Date Day="4" Month="1" Year="1998"/>
                <Author>LE</Author>
                <Comment>ncc permitted bitmap added</Comment>
            </History>
            <History>
                <Date Day="29" Month="5" Year="2001"/>
                <Author>MPA</Author>
                <Comment>added reorg only</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, added possible values for mod, comment</Comment>
            </History>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Added parameters for EMR</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_MEASUREMENT_IND is sent to RR after measuring new values for serving or neighbour cells. It is used both in idle and dedicated mode.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_MEASUREMENT_IND</Name>
                <PrimID Direction="UPLINK" Number="1"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>channel number; refers to serving cell</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rx_lev_full</Name>
                </ItemLink>
                <Comment>received full field strength; refers to serving cell</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rx_lev_sub</Name>
                </ItemLink>
                <Comment>received sub field strength; refers to serving cell</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rx_qual_full</Name>
                </ItemLink>
                <Comment>received full quality; refers to serving cell</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rx_qual_sub</Name>
                </ItemLink>
                <Comment>received sub quality; refers to serving cell</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>dtx</Name>
                </ItemLink>
                <Comment>use of DTX; refers to serving cell</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>otd</Name>
                </ItemLink>
                <Comment>timing advance; refers to serving cell (short name otd, although misleading, is kept only for backwards compatibility reasons); used in GSM dedicated mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>valid</Name>
                </ItemLink>
                <Comment>valid flag; refers to both serving and neighbour cells, i.e. the entire report; set to valid except for first measurement indications after an update of the BA list</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>TDMA frame offset; used for  C2 calculation</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ncells</Name>
                </ItemLink>
                <Comment>neighbour cell measurement results; referring to neighbour cells</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>gprs_sync</Name>
                </ItemLink>
                <Comment>GPRS synchronisation results; referring to neighbour cells; for a GSM only terminal the value is always NORMAL_MEAS_REP</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rx_lev_full</Name>
                </ItemLink>
                <Alias>rxlev_val</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>RXLEV VAL on SACCH, valid only for EMR </Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>nbr_rcvd_blks</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Number of blocks received, valid only for EMR</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>mean_bep</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Mean BEP, valid only for EMR</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>cv_bep</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>CV BEP, valid only for EMR</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>scale_order</Name>
                </ItemLink>
                <Alias>scale_used</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Indicates the scale used. Valid values are 0(0dB) and 1(10dB), valid only for EMR</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>nc_index</Name>
                </ItemLink>
                <Control>[MAX_NUM_CELLS_IN_REPORT]</Control>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>One-One correspondence with info in ncells: assistance data for RR during EMR</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>bsic_seen</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>TRUE / FALSE</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>bcch_rxlev_of_sc</Name>
                </ItemLink>
                <Comment>rxlev of SC BCCH channel. Used in dedicated mode, to distinguish between rxlev of traffic channel and BCCH channel.</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>opcode direction bit changed</Comment>
            </History>
            <History>
                <Date Day="29" Month="5" Year="2001"/>
                <Author>MPA</Author>
                <Comment>added gprs_sync</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, added comments for elements</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_NEIGHBOURCELL_REQ is used to forward a list of neighbour cells to PL.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note: It is possible that different neighbour cell descriptions exists for idle and dedicated mode.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_NEIGHBOURCELL_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="4"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>multi_band</Name>
                </ItemLink>
                <Comment>multi-band report parameter; fed from SYSTEM INFORMATION 2ter's / 5ter's neighbour cell description 2 IE</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>[MAX_NEIGHBOURCELLS]</Control>
                <Comment>neighbour cell channel numbers; the list is delimited with 0xFFFF = NOT_PRESENT_16BIT (except if all entries are used)</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>sync_only</Name>
                </ItemLink>
                <Comment>GPRS synchronisation only; for a GSM only terminal the value is always NORMAL_BA</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>opcode direction bit changed</Comment>
            </History>
            <History>
                <Date Day="13" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Multiband Report Parameter added</Comment>
            </History>
            <History>
                <Date Day="29" Month="5" Year="2001"/>
                <Author>MPA</Author>
                <Comment>added sync_only</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, added comments for elements</Comment>
            </History>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Added EMR related parameters</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_DEDICATED_REQ is used by RR to request from PL that a configuration of the dedicated mode is set and adheredto.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Note: Potential validity of other elements than dedicated mode scenario, i.e. mod, of this primitive depends on the value of dedicated mode scenario / mod.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_DEDICATED_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="6"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>mod</Name>
                </ItemLink>
                <Comment>dedicated mode scenario; the following mod values can occur within this primitive: MODE_IMM_ASSIGN, MODE_CHAN_ASSIGN, MODE_ASYNC_HANDOVER, MODE_SYNC_HANDOVER, MODE_PRE_SYNC_HANDOVER, MODE_PSEUDO_SYNC_HANDOVER, MODE_SYS_INFO_CHANGE, MODE_PDCH_ASSIGN (GPRS only)</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>start</Name>
                </ItemLink>
                <Comment>starting time; validity can be indicated within the element by a valid flag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ch_type</Name>
                </ItemLink>
                <Comment>channel type after time</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ch_type2</Name>
                </ItemLink>
                <Comment>channel type before time; invalidity of the entire element including sub-elements can be indicated by a sub-element channel type ch being equal to 0xFF = NOT_PRESENT_8BIT</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>BCCH channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Comment>base station identification code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ho_param</Name>
                </ItemLink>
                <Comment>handover parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>tr_para</Name>
                </ItemLink>
                <Comment>transmission parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ciph</Name>
                </ItemLink>
                <Comment>ciphering parameters</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>amr_conf</Name>
                </ItemLink>
                <Comment>AMR configuration</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>dedicated mode scenario, bsic, ch_type2, ho_param added opcode direction bit changed</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, added comments for elements</Comment>
            </History>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>amr_conf for AMR added</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_DEDICATED_CNF is used to confirm the requested configuration of dedicated mode.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_DEDICATED_CNF</Name>
                <PrimID Direction="UPLINK" Number="2"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>dedi_res</Name>
                </ItemLink>
                <Comment>dedicated result</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>dedicated result added, opcode direction bit changed</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_DEDICATED_FAIL_REQ is used to go back to the old channel after failure during a channel assignment, handover or PDCH assignment procedure.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_DEDICATED_FAIL_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="7"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>opcode direction bit changed</Comment>
            </History>
            <History>
                <Date Day="28" Month="5" Year="1998"/>
                <Author>VK</Author>
                <Comment>add param</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_DEDICATED_FAIL_CNF is used to confirm the change back to the old channel after a failed channel assignment, handover or PDCH assignment procedure.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_DEDICATED_FAIL_CNF</Name>
                <PrimID Direction="UPLINK" Number="3"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>opcode direction bit changed</Comment>
            </History>
            <History>
                <Date Day="28" Month="5" Year="1998"/>
                <Author>VK</Author>
                <Comment>add param</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Corrected description</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_CIPHERING_REQ is used to forward changes in ciphering parameters to PL.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_CIPHERING_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="8"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ciph</Name>
                </ItemLink>
                <Comment>ciphering parameters</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>opcode direction bit changed</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_FREQ_REDEF_REQ is used to configure a new mobile allocation for frequency hopping after reception of a FREQUENCY REDEFINITION message.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_FREQ_REDEF_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="9"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>start</Name>
                </ItemLink>
                <Comment>starting time</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ch_type</Name>
                </ItemLink>
                <Comment>channel description</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>starting time added</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>channel description added, freq_red removed, opcode direction bit changed</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_CHANNEL_MODE_REQ is used to configure a new channel mode during the channel mode modify procedure.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_CHANNEL_MODE_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="10"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>mode</Name>
                </ItemLink>
                <Comment>channel mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ch</Name>
                </ItemLink>
                <Comment>channel type</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>amr_conf</Name>
                </ItemLink>
                <Comment>AMR configuration</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>opcode direction bit changed</Comment>
            </History>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>amr_conf for AMR added</Comment>
            </History>
            <History>
                <Date Day="5" Month="5" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Add parameter channel type</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_ERROR_IND is to inform RR about different failure situations such as downlink signalling or radio link failure.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_ERROR_IND</Name>
                <PrimID Direction="UPLINK" Number="4"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>cs</Name>
                </ItemLink>
                <Comment>cause; The following causes can occur within this primitive: CS_DOWN_LINK_FAIL, CS_RADIO_LINK_FAIL, CS_BCCH_READ_ERROR</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>opcode direction bit changed</Comment>
            </History>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>channel number added</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, added possible cause values</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_DEACTIVATE_REQ is used to request the deactivation of the PL, especially the RF output.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_DEACTIVATE_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="11"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>opcode direction bit changed</Comment>
            </History>
            <History>
                <Date Day="28" Month="5" Year="1998"/>
                <Author>VK</Author>
                <Comment>add param</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added requirement on PL to turn off RF output</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_CLASSMARK_REQ is used to configure the classmark of the mobile station.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_CLASSMARK_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="12"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>classmark</Name>
                </ItemLink>
                <Comment>classmark</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>opcode direction bit changed</Comment>
            </History>
            <History>
                <Date Day="12" Month="7" Year="2000"/>
                <Author>DG</Author>
                <Comment>element short name changed from class to classmark (Forum G23M / No 0057)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_TCH_LOOP_REQ  is used to close or to open a TCH loop in PL. This is used in association with the special conformance testing functions (internal test loops) of GSM 04.14.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_TCH_LOOP_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="17"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>tch_loop</Name>
                </ItemLink>
                <Comment>loop command</Comment>
            </PrimItem>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>opcode direction bit changed</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_DAI_REQ  is used to start or stop DAI testing in PL. This is used in association with the special conformance testing functions (activating and deactivating DAI tests) of GSM 04.14.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_DAI_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="18"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>device</Name>
                </ItemLink>
                <Comment>dai device</Comment>
            </PrimItem>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>opcode direction bit changed</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_CBCH_REQ is used to configure a cell broadcast channel.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_CBCH_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="19"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>cbch</Name>
                </ItemLink>
                <Comment>cell broadcast channel</Comment>
            </PrimItem>
            <History>
                <Date Day="12" Month="5" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_IDENTITY_REQ is used to forward mobile identities from RR to PL.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_IDENTITY_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="20"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>mid</Name>
                </ItemLink>
                <Comment>Mobile identities</Comment>
            </PrimItem>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_PAGING_IND is used to indicate a paging of the mobile station.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_PAGING_IND</Name>
                <PrimID Direction="UPLINK" Number="6"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>identity_type</Name>
                </ItemLink>
                <Comment>Identity type</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>channel_needed</Name>
                </ItemLink>
                <Comment>Channel needed</Comment>
            </PrimItem>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_MON_CTRL_REQ is used to start and stop, respectively, the monitoring of BCCH or CCCH.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_MON_CTRL_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="24"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>action</Name>
                </ItemLink>
                <Comment>Control action</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>si_to_read</Name>
                </ItemLink>
                <Comment>SI to read</Comment>
            </PrimItem>
            <History>
                <Date Day="18" Month="7" Year="2000"/>
                <Author>DG</Author>
                <Comment>GPRS support</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_SYNC_REQ is used to forward a synchronisation cause from RR to PL.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_SYNC_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="25"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>cs</Name>
                </ItemLink>
                <Comment>Cause; The following causes can occur within this primitive: CS_STOP_BCCH_READING, CS_STOP_PLMN_SEARCH, CS_STOP_PLMN_SEARCH_AND_DEACTIVATE, CS_CLEAN_SYS_INFO, CS_RXLEV_VAL_REQ (GPRS only)</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="1" Year="2001"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, added possible cause values</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2002"/>
                <Author>MPA</Author>
                <Comment>add CS_STOP_PLMN_SEARCH_AND_DEACTIVATE</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_SYNC_IND is used to indicate a synchronisation cause from PL to RR.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_SYNC_IND</Name>
                <PrimID Direction="UPLINK" Number="11"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>cs</Name>
                </ItemLink>
                <Comment>cause; The following causes can occur within this primitive: CS_SYS_INFO_1_NOT_NEEDED</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>Channel number</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="1" Year="2001"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, added possible cause values</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_MEAS_ORDER_CNF is used to indicate the measurement results due to the measurement order procedure from PL to RR.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_MEAS_ORDER_CNF</Name>
                <PrimID Direction="UPLINK" Number="12"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>no_of_ncells</Name>
                </ItemLink>
                <Comment>number of ncells</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>meas_results</Name>
                </ItemLink>
                <Control>[MAX_NEIGHBOURCELLS]</Control>
                <Comment>measurement results; the list is delimited with 0xFFFF = NOT_PRESENT_16BIT (except if all entries are used)</Comment>
            </PrimItem>
            <History>
                <Date Day="17" Month="5" Year="2001"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_EMO_REQ is used to start an Extended Measurement Order procedure according to GSM 04.08, section 3.4.1.3.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_EMO_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="5"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ba_id</Name>
                </ItemLink>
                <Comment>reference number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>[0..MAX_EMO_CHANNELS]</Control>
                <Comment>frequencies to be measured</Comment>
            </PrimItem>
            <History>
                <Date Day="2" Month="11" Year="2001"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_EMO_IND returns the result of the is used to start an Extended Measurement Order procedure according to GSM 04.08, section 3.4.1.3. . The result may also contain a measurement of the serving cell even if not requested.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_EMO_MEAS_IND</Name>
                <PrimID Direction="UPLINK" Number="5"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ba_id</Name>
                </ItemLink>
                <Comment>reference number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>dtx</Name>
                </ItemLink>
                <Comment>discontinuous transmission</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>meas_results</Name>
                </ItemLink>
                <Control>[0..MAX_EMO_CHANNELS+1]</Control>
                <Comment>measurement results</Comment>
            </PrimItem>
            <History>
                <Date Day="2" Month="11" Year="2001"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="6" Month="11" Year="2002"/>
                <Author>VK</Author>
                <Comment>Increase size of array meas_result.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">MPH_EXT_MEAS_REQ is used to start power measurements for the Extended Measurement procedure according GSM 05.08, section 10.1.5. The field strength of the specified channels shall be measured.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_EXT_MEAS_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="13"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>pch_interrupt</Name>
                </ItemLink>
                <Comment>pch interrupt</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>freq_bands</Name>
                </ItemLink>
                <Comment>frequency bands</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>num_of_chan</Name>
                </ItemLink>
                <Comment>Number of channels</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>[MAX_CHANNELS]</Control>
                <Comment>cell channel numbers</Comment>
            </PrimItem>
            <History>
                <Date Day="26" Month="3" Year="2002"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="4" Year="2002"/>
                <Author>VK</Author>
                <Comment>Add freq_bands</Comment>
            </History>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>VK</Author>
                <Comment>Add pch_interrupt</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">MPH_EXT_MEAS_CNF is used by PL to send the result of power measurements (used for the Extended Measurement procedure) to RR.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_EXT_MEAS_CNF</Name>
                <PrimID Direction="UPLINK" Number="13"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>num_of_chan</Name>
                </ItemLink>
                <Comment>Number of channels</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>num_of_white_list_chan</Name>
                </ItemLink>
                <Comment>Number of White list channels</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>[MAX_CHANNELS]</Control>
                <Comment>cell channel numbers</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rx_lev</Name>
                </ItemLink>
                <Control>[MAX_CHANNELS]</Control>
                <Comment>field strength</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>inactive_carrier_list</Name>
                </ItemLink>
                <Comment>List of inactive carriers</Comment>
            </PrimItem>
            <History>
                <Date Day="26" Month="3" Year="2002"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">MPH_NCELL_POS_REQ is used to request the measurement of enhanced observed time differences for a given list of  neighbour cells.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_NCELL_POS_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="14"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>req_id</Name>
                </ItemLink>
                <Comment>Request Ident</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ncell_eotd</Name>
                </ItemLink>
                <Control>[1..MAX_NCELL_EOTD_ALR]</Control>
                <Comment>Neighbour Cell List</Comment>
            </PrimItem>
            <History>
                <Date Day="29" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">MPH_NCELL_POS_IND is used to carry the resultsof measurement of enhanced observed time differences for a list of neighbour cells and the serving cell.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_NCELL_POS_IND</Name>
                <PrimID Direction="UPLINK" Number="14"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>req_id</Name>
                </ItemLink>
                <Comment>Request Ident</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>eotd_res</Name>
                </ItemLink>
                <Comment>EOTD Result</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ta</Name>
                </ItemLink>
                <Comment>Timing Advance</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>fn</Name>
                </ItemLink>
                <Comment>Frame Number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>eotd_sc_res</Name>
                </ItemLink>
                <Comment>EOTD SC Results</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>eotd_sc_res1</Name>
                </ItemLink>
                <Comment>EOTD SC Results</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>eotd_nc_res</Name>
                </ItemLink>
                <Control>[1.. MAX_NCELL_EOTD_RES]</Control>
                <Comment>EOTD NC Results</Comment>
            </PrimItem>
            <History>
                <Date Day="29" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="9" Year="2002"/>
                <Author>LG</Author>
                <Comment>eotd_res added</Comment>
            </History>
            <History>
                <Date Day="16" Month="9" Year="2002"/>
                <Author>VK</Author>
                <Comment>add 'ta'</Comment>
            </History>
            <History>
                <Date Day="19" Month="9" Year="2002"/>
                <Author>MPA</Author>
                <Comment>add fn</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The MPH_CLEAN_BUF_REQ is used to clean buffers in PL containing System Information messages.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_CLEAN_BUF_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="26"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>si_to_clean</Name>
                </ItemLink>
                <Comment>SI to clean</Comment>
            </PrimItem>
            <History>
                <Date Day="20" Month="5" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_STOP_DEDICATED_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="27"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy</Comment>
            </PrimItem>
            <History>
                <Date Day="23" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_STOP_DEDICATED_CNF</Name>
                <PrimID Direction="UPLINK" Number="15"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy</Comment>
            </PrimItem>
            <History>
                <Date Day="23" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_MEAS_REP_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="28"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>Meas req to ALR</Comment>
            </PrimItem>
            <History>
                <Date Day="16" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_MEAS_REP_CNF</Name>
                <PrimID Direction="UPLINK" Number="16"/>
                <PrimUsage>
                    <Sender>ALR</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>meas_rep</Name>
                </ItemLink>
                <Control>[RR_ALR_MEAS_REPORT_SIZE]</Control>
                <Comment>Primitive Item</Comment>
            </PrimItem>
            <History>
                <Date Day="17" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This is primitive is used by RR to convey enhanced measurement parameters to ALR. This can be used: a. When there is change in enhanced measurement parameters b. when neighbor cell list is already available and enhanced meas-urement parameters are received at different times c. when report type is changed from ‘enhanced’ to ‘normal’ or vice-versa</XHTMLElement>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_ENHPARA_UPDATE_REQ</Name>
                <PrimID Direction="DOWNLINK" Number="29"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>ALR</Receiver>
                </PrimUsage>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rep_type</Name>
                </ItemLink>
                <Comment>Report type :'Enhanced' or 'Normal'</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>enh_para_struct</Name>
                </ItemLink>
                <Alias>enh_para</Alias>
                <Comment>Parameters valid when report type is 'Enhanced'</Comment>
            </PrimItem>
            <History>
                <Date Day="10" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <DocElement>
                    <DocLink DocType="OTHER">
                        <Name/>
                    </DocLink>
                </DocElement>
            </Description>
            <PrimDef>
                <Name>MPH_INIT_RR_IND</Name>
                <PrimID Direction="UPLINK" Number="17"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>pclass_900</Name>
                </ItemLink>
                <Comment>Power Class GSM 900</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>pclass_850</Name>
                </ItemLink>
                <Comment>Power Class GSM 850</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>pclass_1800</Name>
                </ItemLink>
                <Comment>Power Class DCS 1800</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>pclass_1900</Name>
                </ItemLink>
                <Comment>Power Class PCS 1900</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>freq_bands</Name>
                </ItemLink>
                <Comment>Frequency bands</Comment>
            </PrimItem>
            <History>
                <Date Day="31" Month="05" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
    </PrimitivesSection>
    <PrimStructElementsSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">Parameters shall be part of the primitives described below and if applied the parameters shall contain the values specified here.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">Parameters shall be part of the primitives described below and if applied the parameters shall contain the values specified here.</XHTMLElement>
            </DocElement>
        </Description>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the use and the allocation of a cell broadcast channel.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>cbch</Name>
                <Comment>cell broadcast channel</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>stat</Name>
                </ItemLink>
                <Comment>CBCH status; binary state</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ch</Name>
                </ItemLink>
                <Comment>channel type</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <Comment>timeslot number</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <Comment>training sequence code</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>h</Name>
                </ItemLink>
                <Comment>hopping</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>channel number; valid only if h=0</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <Comment>mobile allocation index offset; valid only if h=1</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>hsn</Name>
                </ItemLink>
                <Comment>hopping sequence number; valid only if h=1</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ma</Name>
                </ItemLink>
                <Control>[MAX_MA_CHANNELS]</Control>
                <Comment>mobile allocation list; valid only if h=1; coding as arfcn field above; determines the (maximum) size of mobile allocation list; the list is delimited with 0xFFFF = NOT_PRESENT_16BIT (except if all entries are used)</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added comments at elements, added range for tsc</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Added references for 'tn' , 'arfcn' and 'state'.</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the results of neighbour cell measurements.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>ncells</Name>
                <Comment>neighbour cell measurement results</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>no_of_ncells</Name>
                </ItemLink>
                <Comment>number of neighbour cells; semantics as in 47</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>[MAX_NUM_CELLS_IN_REPORT]</Control>
                <Comment>channel number; semantics as in 4.1</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rx_lev</Name>
                </ItemLink>
                <Control>[MAX_NUM_CELLS_IN_REPORT]</Control>
                <Comment>received field strength; semantics as in 4.11</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Control>[MAX_NUM_CELLS_IN_REPORT]</Control>
                <Comment>base station identification code; semantics as in 4.13</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>time_alignmt</Name>
                </ItemLink>
                <Control>[MAX_NUM_CELLS_IN_REPORT]</Control>
                <Comment>timing alignment; refers to difference in time between serving and neighbour cell</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>frame_offset</Name>
                </ItemLink>
                <Control>[MAX_NUM_CELLS_IN_REPORT]</Control>
                <Comment>frame offset; refers to difference in time between serving and neighbour cell</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>otd expanded to USHORT</Comment>
            </History>
            <History>
                <Date Day="3" Month="12" Year="1999"/>
                <Author>LE</Author>
                <Comment>otd renamed to time_alignmt and frame_offset</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>added comments</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>added references for the first four members</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines a starting time in form of a reduced frame number. For the definition of the reduced frame number please refer to GSM 05.10.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>start</Name>
                <Comment>starting time</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>v_start</Name>
                </ItemLink>
                <Comment>starting time valid</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>t1</Name>
                </ItemLink>
                <Comment>frame number modulo 32</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>t2</Name>
                </ItemLink>
                <Comment>frame number modulo 26</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>t3</Name>
                </ItemLink>
                <Comment>frame number modulo 51</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>valid flag inserted</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Added references</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines a channel type configuration.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>ch_type</Name>
                <Comment>channel type configuration</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>ch_type2</Name>
                <Comment>channel type</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ch</Name>
                </ItemLink>
                <Comment>channel type</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <Comment>timeslot number</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <Comment>training sequence code</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>h</Name>
                </ItemLink>
                <Comment>hopping</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>channel number; valid only if h=0</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <Comment>mobile allocation index offset; valid only if h=1</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>hsn</Name>
                </ItemLink>
                <Comment>hopping sequence number; valid only if h=1</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ma</Name>
                </ItemLink>
                <Control>[MAX_MA_CHANNELS]</Control>
                <Comment>mobile allocation list; valid  only if h=1; coding as arfcn field above; determines the (maximum) size of mobile allocation list; the list is delimited with 0xFFFF = NOT_PRESENT_16BIT (except if all entries are used)</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>training sequence code added</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>comments aligned with ch. 4.10</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Added references</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the transmission parameters for the dedicated mode.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>tr_para</Name>
                <Comment>transmission parameter</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>power</Name>
                </ItemLink>
                <Comment>transmission power level</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>dtx</Name>
                </ItemLink>
                <Comment>discontinuous transmission</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rlt</Name>
                </ItemLink>
                <Comment>radio link timeout</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>tav</Name>
                </ItemLink>
                <Comment>timing advance</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>pwrc</Name>
                </ItemLink>
                <Comment>power control indicator</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>mode</Name>
                </ItemLink>
                <Comment>channel mode</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>mobile allocation removed</Comment>
            </History>
            <History>
                <Date Day="30" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>channel mode added</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>added reference for 'power' and 'dtx'</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the parameters needed for ciphering.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>ciph</Name>
                <Comment>ciphering parameters</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>stat</Name>
                </ItemLink>
                <Comment>Ciphering Status; binary state</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>algo</Name>
                </ItemLink>
                <Comment>Algorithm</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>kc</Name>
                </ItemLink>
                <Control>[KC_STRING_SIZE]</Control>
                <Comment>Kc value; the format in the GTI case is as on the SIM; the least significant bit of kc is the least significant bit of the eighth byte; the most significant bit of kc is the most significant bit of the first byte.</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="1" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>introduce STAT_CIPH_ON</Comment>
            </History>
            <History>
                <Date Day="31" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>added comment on Kc</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>added reference</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Encodes the adaptiv multirate configuration for the speech codec.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>amr_conf</Name>
                <Comment>Parameters for AMR</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>nscb</Name>
                </ItemLink>
                <Comment>noise suppression control bit</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>icmi</Name>
                </ItemLink>
                <Comment>initial code mode indicator</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>st_mode</Name>
                </ItemLink>
                <Comment>initial code mode</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>acs</Name>
                </ItemLink>
                <Comment>active codec set</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>v_cod_prop</Name>
                </ItemLink>
                <Comment>valid flag codec properties</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>c_cod_prop</Name>
                </ItemLink>
                <Comment>counter</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>cod_prop</Name>
                </ItemLink>
                <Control>[3]</Control>
                <Comment>codec properties</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter defines the codec properties.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>cod_prop</Name>
                <Comment>codec properties</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>codec_thr</Name>
                </ItemLink>
                <Comment>Codec threshold</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>codec_hyst</Name>
                </ItemLink>
                <Comment>Codec hysteresis</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="2" Year="2003"/>
                <Author>LG</Author>
                <Comment>renamed components</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the mobile station classmark part relevant for PL.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>classmark</Name>
                <Comment>classmark</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>pclass</Name>
                </ItemLink>
                <Comment>power class</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>pclass2</Name>
                </ItemLink>
                <Comment>power class 2</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>band removed, pclass2 added</Comment>
            </History>
            <History>
                <Date Day="12" Month="7" Year="2000"/>
                <Author>DG</Author>
                <Comment>definition short name changed from class to classmark (Forum G23M / No 0057)</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>made description more precise</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the handover parameter.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>ho_param</Name>
                <Comment>handover parameter</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ho_ref</Name>
                </ItemLink>
                <Comment>reference</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ho_pow</Name>
                </ItemLink>
                <Comment>transmission power level</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ho_acc_type</Name>
                </ItemLink>
                <Comment>access type</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ho_nci</Name>
                </ItemLink>
                <Comment>normal cell indication</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added ranges and semantics for some elements</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains mobile identities which are used by PL for paging detection.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>mid</Name>
                <Comment>Mobile identities</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>len_imsi</Name>
                </ItemLink>
                <Comment>Length of IMSI</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>imsi</Name>
                </ItemLink>
                <Control>[15]</Control>
                <Comment>IMSI digits</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>v_tmsi</Name>
                </ItemLink>
                <Comment>Valid TMSI flag</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>tmsi</Name>
                </ItemLink>
                <Comment>Binary TMSI representatino</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>v_ptmsi</Name>
                </ItemLink>
                <Comment>Valid PTMSI flag; can indicate"valid"only for the GPRS supporting terminal</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ptmsi</Name>
                </ItemLink>
                <Comment>Binary PTMSI representatino</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>v_ptmsi2</Name>
                </ItemLink>
                <Comment>Valid PTMSI flag; can indicate"valid"only for the GPRS supporting terminal</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ptmsi2</Name>
                </ItemLink>
                <Comment>Binary PTMSI representatino</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>MPA</Author>
                <Comment>GPRS support</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Clarified range of len_imsi</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines sending of RACH bursts. It contains the number of RACH bursts, the contents and thetime between two RACH bursts.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>send_mode</Name>
                <Comment>RACH sending mode</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>c</Name>
                </ItemLink>
                <Comment>dummy; unused, reserved</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>no</Name>
                </ItemLink>
                <Comment>number of RACH messages; this number includes re-transmissions and the first, initial RACH burst, i.e. no = M +1, where M is as defined in GSM 04.08's specification of the initiation of the immediate assignment procedure</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>delta</Name>
                </ItemLink>
                <Control>[MAX_RACH_REQ]</Control>
                <Comment>time in TDMA frames between bursts; delta[0]corresponds to the time between MPH_RANDOM_ACCESS_REQ and the first RACH burst, delta[1]to the time between the first and the 2nd RACH burst and so on</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rach</Name>
                </ItemLink>
                <Control>[MAX_RACH_REQ]</Control>
                <Comment>channel request content burst n; rach[0]corresponds to the contents of the first RACH burst, rach[1]to the 2nd and so on</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added comments, declared c parameter to be reserved</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the time a random burst was sent. Format of a reduced frame number. For the definition of the reduced frame number please refer to GSM 05.10.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>frame_no</Name>
                <Comment>reduced frame number</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>t1</Name>
                </ItemLink>
                <Comment>frame number modulo 32</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>t2</Name>
                </ItemLink>
                <Comment>frame number modulo 26</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>t3</Name>
                </ItemLink>
                <Comment>frame number modulo 51</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="31" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved comment,added values in line with 4.18</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Added references</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines a service data unit.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>sdu</Name>
                <Comment>Service Data Unit</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>l_buf</Name>
                </ItemLink>
                <Comment>length of content in bit</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>o_buf</Name>
                </ItemLink>
                <Comment>offset of content in bit</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>buf</Name>
                </ItemLink>
                <Control>[1]</Control>
                <Comment>buffer content; comment as in PH SAP</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the results of neighbour cell measurements.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">It is used for providing the fieldstrength of all neighbour cells.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>meas_results</Name>
                <Comment>neighbourcell measurement results</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rx_lev</Name>
                </ItemLink>
                <Comment>received field strength</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="16" Month="5" Year="2001"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="31" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added PCS arfcns</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Added references</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the results of E-OTD measurements of one cell.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>eotd_sc_res</Name>
                <Comment>EOTD SC Results at start of measurement</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>eotd_sc_res1</Name>
                <Comment>EOTD SC Results at stop of measurement</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>eotd_nc_res</Name>
                <Comment>EOTD NC Results</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>sb_flag</Name>
                </ItemLink>
                <Comment>Valid flag; named 'Data Valid' by cursor task</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Comment>base station identity code</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>eotd_crosscor</Name>
                </ItemLink>
                <Control>[XCOR_NO]</Control>
                <Comment>Cross correlation</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>d_eotd_nrj</Name>
                </ItemLink>
                <Comment>Sum of Amplitudes; named 'RSSI' by cursor task</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>time_tag</Name>
                </ItemLink>
                <Comment>Time tag; named 'Nominal Position' by cursor task</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="29" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="2" Year="2003"/>
                <Author>LG</Author>
                <Comment>eotd_crosscor length by symbol</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter describes a neighbour cell the MS shall synchronise to and shall get E-ODT measurements from.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>ncell_eotd</Name>
                <Comment>Parameters of a neighbour cell</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Comment>Bsic</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>mfrm_offset</Name>
                </ItemLink>
                <Comment>multiframe offset</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>otd_type</Name>
                </ItemLink>
                <Comment>otd type</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>exp_otd</Name>
                </ItemLink>
                <Comment>expected otd</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>uncertainty</Name>
                </ItemLink>
                <Comment>uncertainty of exp. otd</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rough_rtd</Name>
                </ItemLink>
                <Comment>rough rtd</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="29" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial.</Comment>
            </History>
            <History>
                <Date Day="3" Month="9" Year="2002"/>
                <Author>LG</Author>
                <Comment>renamed</Comment>
            </History>
            <History>
                <Date Day="18" Month="9" Year="2002"/>
                <Author>MPA</Author>
                <Comment>change to NW coding</Comment>
            </History>
            <History>
                <Date Day="19" Month="9" Year="2002"/>
                <Author>MPA</Author>
                <Comment>add BSIC</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This structure contains the measurement results ordered by the network.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>meas_rep</Name>
                <Comment>meas report to RR</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Comment>values for bsic</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rx_lev</Name>
                </ItemLink>
                <Comment>received field strength</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="17" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This is a element in "White List" and "Black List" structures.It stores a list frequencie</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>list</Name>
                <Comment>stores a list of frequencies</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>channels</Name>
                </ItemLink>
                <Control>[LIST_MAX_SIZE]</Control>
                <Comment>stores a list of frequencies</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="07" Month="12" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This is new element in the MPH_POWER_REQ primitive.Contains a separate  bit map of  Black Listed carries for Euro / American regions</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>black_list</Name>
                <Comment>Contains a separate  bit map of  Black Listed carries for Euro / American regions</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>list</Name>
                </ItemLink>
                <Control>[MAX_REGIONS]</Control>
                <Comment>Primitive structure element item</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="07" Month="12" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This is new element in the MPH_POWER_REQ primitive.Contains the bitmap of carriers present in the "White List"</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>white_list</Name>
                <Comment>contains the bitmap of carriers present in the "White List"</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>white_list_valid</Name>
                </ItemLink>
                <Comment>Indicates whether "White List" is valid or not</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>region</Name>
                </ItemLink>
                <Comment>Indicates whether "White List"belongs to European or American region</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>list</Name>
                </ItemLink>
                <Comment>stores a list of frequencies</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="07" Month="12" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>inactive_carrier_list</Name>
                <Comment>Contains the bitmap of inactive carriers in the current location</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>list</Name>
                </ItemLink>
                <Control>[MAX_REGIONS]</Control>
                <Comment>Bitmap of GSM channels</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="17" Month="01" Year="2005"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Primitive structure element item</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>enh_para_struct</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Enhanced measurement parameters</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>num_valid_cells</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>number of cells in the list below</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>enh_cell_list</Name>
                </ItemLink>
                <Control>[MAX_NEIGHBOURCELLS]</Control>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>List of enhanced cell information</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rep_rate</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reorting rate for low priority cells</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>inv_bsic_enabled</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Is invalid BSIC reporting enabled?</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>ncc_permitted</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>When Invalid BSIC reporting is enables, the NCC part that is permitted</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>multiband_rep</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Num cells in each Non serving band for reporting</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>servingband_rep</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Num cells in serving band for reporting</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>scale_order</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Scaling ordered by NW</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>enh_rep_data</Name>
                </ItemLink>
                <Control>[MAX_NUM_BANDS]</Control>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Info per band in the order:900,1800,400,1900,850</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author>x0059970</Author>
                <Comment>R99 PEMR feature</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Enhanced cell list that contains reporting priority associated with each cell.  The ARFCN information given here should be same as given in neighbor cell list. ARFCN is repeated here only to make the information complete.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>enh_cell_list</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Enhanced cell list</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>ARFCN of the cell</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>BSIC of the cell</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rep_priority</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting priority of this cell</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rtd</Name>
                </ItemLink>
                <Control>[0..MAX_NUM_OF_RTD_VALUES]</Control>
                <Version>REL99 AND TI_PS_FF_RTD</Version>
                <Comment>Primitive structure element item</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author>x0059970</Author>
                <Comment>R99 PEMR feature</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Data required while processing the neighbor cell measurements according to reporting priority.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>enh_rep_data</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Enhanced data for reporting</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rep_threshold</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting threshold</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mph</DocName>
                    <Name>rep_offset</Name>
                </ItemLink>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting offset</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author>x0059970</Author>
                <Comment>R99 PEMR feature</Comment>
            </History>
        </PrimStructElem>
    </PrimStructElementsSection>
    <PrimBasicElementsSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">Parameters shall be part of the primitives described below and if applied the parameters shall contain the values specified here.</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">Parameters shall be part of the primitives described below and if applied the parameters shall contain the values specified here.</XHTMLElement>
            </DocElement>
        </Description>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter identifies a channel number. Coding is inspired by the ARFCN as defined by GSM 05.05 but not identical in all cases of frequency band combinations.</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter identifies a channel number. Coding is inspired by the ARFCN as defined by GSM 05.05 but not identical in all cases of frequency band combinations.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>arfcn</Name>
                <Type>U16</Type>
                <Comment>channel number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_arfcn</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, added possible values for PCS1900 band</Comment>
            </History>
            <History>
                <Date Day="11" Month="2" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change values and comments for american frequencies</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter identifies a channel number. Coding is inspired by the ARFCN as defined by GSM 05.05 but not identical in all cases of frequency band combinations.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>ma</Name>
                <Type>U16</Type>
                <Comment>channel number in the mobile allocation list (used with frequency hopping)</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_arfcn</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, added possible values for PCS1900 band</Comment>
            </History>
            <History>
                <Date Day="11" Month="2" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change values and comments for american frequencies</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter is unused and reserved (for backwards compatibility reasons).</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>ext_bcch</Name>
                <Type>U8</Type>
                <Comment>unused, reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="31" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>declared as unused / reserved</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines whether it is a combined CCCH or not.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>comb_ccch</Name>
                <Type>U8</Type>
                <Comment>extended BCCH listening</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_comb_ccch</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the timeslot number.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>tn</Name>
                <Type>U8</Type>
                <Comment>timeslot number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_tn</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the initial value for the downlink signalling failure criterion (counter) to be applied by PL.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>dlt</Name>
                <Type>U8</Type>
                <Comment>downlink initial value</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_dlt</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, corrected lower bound of range</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the paging group of the mobile station. Values are in accordance with GSM 05.02.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>pg</Name>
                <Type>U8</Type>
                <Comment>paging group</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_pg</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the number of blocks reserved for access grant channels on the common control channel. Values are in accordance with GSM 05.02.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>bs_ag_blocks_res</Name>
                <Type>U8</Type>
                <Comment>blocks reserved for AGCH</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_bs_ag_blocks_res</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description, added range</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the number of multiframes for transmission of the same paging group. Values correspond to the system parameter BS-PA-MFRMS as coded in GSM 04.08.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>bs_pa_mfrms</Name>
                <Type>U8</Type>
                <Comment>Multiframe Period</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_bs_pa_mfrms</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added reference to GSM standard</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the maximum transmission power level to be used by the PL when the mobile station is accessing on a CCCH. Values correspond to the system parameter MS-TXPWR-MAX-CCH as coded in GSM 04.08 / 05.08.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>power</Name>
                <Type>U8</Type>
                <Comment>transmission power level</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_power</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Elaborated description</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the received field strength value as defined in GSM 05.08.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rx_lev</Name>
                <Type>U8</Type>
                <Comment>received field strength</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_rx_lev</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the received field strength value as defined in GSM 05.08.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rx_lev_full</Name>
                <Type>U8</Type>
                <Comment>received field strength</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the received field strength value as defined in GSM 05.08.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rx_lev_sub</Name>
                <Type>U8</Type>
                <Comment>received field strength</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the received quality as defined in GSM 05.08.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rx_qual_full</Name>
                <Type>U8</Type>
                <Comment>received quality</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_rx_qual_full</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the received quality as defined in GSM 05.08.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rx_qual_sub</Name>
                <Type>U8</Type>
                <Comment>received quality</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the base station identification code as defined in GSM 03.03. The lowest 3 bits represent the base station colour code (BCC), the next 3 bits represent the network colour code (NCC).</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>bsic</Name>
                <Type>U8</Type>
                <Comment>base station identification code</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_bsic</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Elaborated description</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies whether discontinuous transmission is used or not.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>dtx</Name>
                <Type>U8</Type>
                <Comment>discontinuous transmission</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_dtx</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Editorial improvements</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the timing advance (of the serving cell) in bit periods.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>otd</Name>
                <Type>U16</Type>
                <Comment>timing advance</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_otd</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>expanded to USHORT</Comment>
            </History>
            <History>
                <Date Day="31" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>added range</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the timing advance (of the serving cell) in bit periods.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>ta</Name>
                <Type>U8</Type>
                <Comment>timing advance</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_ta</Name>
            </ValuesLink>
            <History>
                <Date Day="16" Month="9" Year="2002"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the results of neighbour cell measurements.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>time_alignmt</Name>
                <Type>U32</Type>
                <Comment>timing alignment; refers to difference in time between serving and neighbour cell</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>otd expanded to USHORT</Comment>
            </History>
            <History>
                <Date Day="3" Month="12" Year="1999"/>
                <Author>LE</Author>
                <Comment>otd renamed to time_alignmt and frame_offset</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>added comments</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>added references for the first four members</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the results of neighbour cell measurements.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>frame_offset</Name>
                <Type>U32</Type>
                <Comment>frame offset; refers to difference in time between serving and neighbour cell</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>otd expanded to USHORT</Comment>
            </History>
            <History>
                <Date Day="3" Month="12" Year="1999"/>
                <Author>LE</Author>
                <Comment>otd renamed to time_alignmt and frame_offset</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>added comments</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>added references for the first four members</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines a starting time in form of a reduced frame number. For the definition of the reduced frame number please refer to GSM 05.10.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>v_start</Name>
                <Type>U8</Type>
                <Comment>starting time valid</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_v_start</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>valid flag inserted</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Added references</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies the type of channel.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>ch</Name>
                <Type>U8</Type>
                <Comment>channel type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_ch</Name>
            </ValuesLink>
            <History>
                <Date Day="2" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies the binary state of something.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>tsc</Name>
                <Type>U8</Type>
                <Comment>trainings sequence code</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_tsc</Name>
            </ValuesLink>
            <History>
                <Date Day="2" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies the use of frequency hopping or static rf channel.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>h</Name>
                <Type>U8</Type>
                <Comment>hopping</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_h</Name>
            </ValuesLink>
            <History>
                <Date Day="2" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies the mobile allocation index offset, coded as in GSM 04.08 / 05.02. Only used together with frequency hopping.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>maio</Name>
                <Type>U8</Type>
                <Comment>mobile allocation index offset</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_maio</Name>
            </ValuesLink>
            <History>
                <Date Day="2" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies the mobile allocation index offset, coded as in GSM 04.08 / 05.02. Only used together with frequency hopping.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>hsn</Name>
                <Type>U8</Type>
                <Comment>hopping sequence number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_hsn</Name>
            </ValuesLink>
            <History>
                <Date Day="2" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the transmission parameters for the dedicated mode.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rlt</Name>
                <Type>U8</Type>
                <Comment>radio link timeout</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_rlt</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>mobile allocation removed</Comment>
            </History>
            <History>
                <Date Day="30" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>channel mode added</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>added reference for 'power' and 'dtx'</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the transmission parameters for the dedicated mode.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>tav</Name>
                <Type>U8</Type>
                <Comment>timing advance</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_tav</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>mobile allocation removed</Comment>
            </History>
            <History>
                <Date Day="30" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>channel mode added</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>added reference for 'power' and 'dtx'</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the transmission parameters for the dedicated mode.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>pwrc</Name>
                <Type>U8</Type>
                <Comment>power control indicator</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_pwrc</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>mobile allocation removed</Comment>
            </History>
            <History>
                <Date Day="30" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>channel mode added</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>added reference for 'power' and 'dtx'</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the parameters needed for ciphering.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>algo</Name>
                <Type>U8</Type>
                <Comment>Algorithm</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_algo</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="1" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>introduce STAT_CIPH_ON</Comment>
            </History>
            <History>
                <Date Day="31" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>added comment on Kc</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>added reference</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the parameters needed for ciphering.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>kc</Name>
                <Type>U8</Type>
                <Comment>Kc value; the format in the GTI case is as on the SIM; the least significant bit of kc is the least significant bit of the eighth byte; the most significant bit of kc is the most significant bit of the first byte.</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="1" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>introduce STAT_CIPH_ON</Comment>
            </History>
            <History>
                <Date Day="31" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>added comment on Kc</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>added reference</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the idle ordedicated mode scenario in RR.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>mod</Name>
                <Type>U8</Type>
                <Comment>idle / dedicated mode scenario</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_mod</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="19" Month="2" Year="1998"/>
                <Author>VK</Author>
                <Comment>Add MODE_SYS_INFO_CHANGE</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="2001"/>
                <Author>VK</Author>
                <Comment>Add MODE_PDCH_ASSIGN</Comment>
            </History>
            <History>
                <Date Day="2" Month="8" Year="2001"/>
                <Author>VK</Author>
                <Comment>Add MODE_CELL_CHANGE_ORDER</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the used channel mode.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>mode</Name>
                <Type>U8</Type>
                <Comment>channel mode</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Corrected values to those used over the air interface, added 14.5</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Encodes the adaptiv multirate configuration for the speech codec.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>nscb</Name>
                <Type>U8</Type>
                <Comment>noise suppression control bit</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Encodes the adaptiv multirate configuration for the speech codec.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>icmi</Name>
                <Type>U8</Type>
                <Comment>initial code mode indicator</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Encodes the adaptiv multirate configuration for the speech codec.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>st_mode</Name>
                <Type>U8</Type>
                <Comment>initial code mode</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_st_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Encodes the adaptiv multirate configuration for the speech codec.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>acs</Name>
                <Type>U8</Type>
                <Comment>active codec set</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Encodes the adaptiv multirate configuration for the speech codec.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>v_cod_prop</Name>
                <Type>U8</Type>
                <Comment>valid flag codec properties</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Encodes the adaptiv multirate configuration for the speech codec.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>c_cod_prop</Name>
                <Type>U8</Type>
                <Comment>counter</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter defines the codec properties.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>codec_thr</Name>
                <Type>U8</Type>
                <Comment>Codec threshold</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="2" Year="2003"/>
                <Author>LG</Author>
                <Comment>renamed components</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The parameter defines the codec properties.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>codec_hyst</Name>
                <Type>U8</Type>
                <Comment>Codec hysteresis</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="2" Year="2003"/>
                <Author>LG</Author>
                <Comment>renamed components</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines a cause.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>cs</Name>
                <Type>U8</Type>
                <Comment>cause</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_cs</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="19" Month="9" Year="1997"/>
                <Author>LE</Author>
                <Comment>cause CS_BCCH_READ_ERROR added</Comment>
            </History>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>cause CS_NO_ERROR added</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2001"/>
                <Author>LE</Author>
                <Comment>new causes added</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2002"/>
                <Author>MPA</Author>
                <Comment>add CS_STOP_PLMN_SEARCH_AND_DEACTIVATE</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the mobile station classmark part relevant for PL.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>pclass</Name>
                <Type>U8</Type>
                <Comment>power class</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_pclass</Name>
            </ValuesLink>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>band removed, pclass2 added</Comment>
            </History>
            <History>
                <Date Day="12" Month="7" Year="2000"/>
                <Author>DG</Author>
                <Comment>definition short name changed from class to classmark (Forum G23M / No 0057)</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>made description more precise</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the mobile station classmark part relevant for PL.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>pclass2</Name>
                <Type>U8</Type>
                <Comment>power class 2</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="15" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>band removed, pclass2 added</Comment>
            </History>
            <History>
                <Date Day="12" Month="7" Year="2000"/>
                <Author>DG</Author>
                <Comment>definition short name changed from class to classmark (Forum G23M / No 0057)</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>made description more precise</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the number of TDMA frames between two measurement reports.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>fn_offset</Name>
                <Type>U16</Type>
                <Comment>TDMA Frame Offset</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the TCH loop command.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>tch_loop</Name>
                <Type>U8</Type>
                <Comment>TCH loop command</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_tch_loop</Name>
            </ValuesLink>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added values</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the result of configuration for a dedicated channel configuration.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>dedi_res</Name>
                <Type>U8</Type>
                <Comment>dedicated configuration result</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_dedi_res</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the device for DAI testing. Values are corresponding to the Tested Device IE of the TEST_INTERFACE message of GSM 04.14.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>device</Name>
                <Type>U8</Type>
                <Comment>DAI testing device</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_device</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the handover parameter.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>ho_ref</Name>
                <Type>U8</Type>
                <Comment>reference</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added ranges and semantics for some elements</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the handover parameter.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>ho_pow</Name>
                <Type>U8</Type>
                <Comment>transmission power level</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_ho_pow</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added ranges and semantics for some elements</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the handover parameter.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>ho_acc_type</Name>
                <Type>U8</Type>
                <Comment>access type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_ho_acc_type</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added ranges and semantics for some elements</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the handover parameter.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>ho_nci</Name>
                <Type>U8</Type>
                <Comment>normal cell indication</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_ho_nci</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added ranges and semantics for some elements</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter is supplied to avoid empty primitives.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>param</Name>
                <Type>U8</Type>
                <Comment>dummy parameter</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="28" Month="5" Year="1998"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines during dedicated mode whether a measurement report is valid or not. A value of 0 indicates not present / not valid, any other value indicates presence / validity.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>valid</Name>
                <Type>U8</Type>
                <Comment>valid flag</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="2" Month="6" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the multiband report mode for multiband mobile stations. Values are in accordance with GSM 04.08.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>multi_band</Name>
                <Type>U8</Type>
                <Comment>multiband report parameter</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_multi_band</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains mobile identities which are used by PL for paging detection.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>len_imsi</Name>
                <Type>U8</Type>
                <Comment>Length of IMSI</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_len_imsi</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>MPA</Author>
                <Comment>GPRS support</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Clarified range of len_imsi</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains mobile identities which are used by PL for paging detection.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>imsi</Name>
                <Type>U8</Type>
                <Comment>IMSI digits</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>MPA</Author>
                <Comment>GPRS support</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Clarified range of len_imsi</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains mobile identities which are used by PL for paging detection.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>v_tmsi</Name>
                <Type>U8</Type>
                <Comment>Valid TMSI flag</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>MPA</Author>
                <Comment>GPRS support</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Clarified range of len_imsi</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains mobile identities which are used by PL for paging detection.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>tmsi</Name>
                <Type>U32</Type>
                <Comment>Binary TMSI representatino</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>MPA</Author>
                <Comment>GPRS support</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Clarified range of len_imsi</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains mobile identities which are used by PL for paging detection.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>v_ptmsi</Name>
                <Type>U8</Type>
                <Comment>Valid PTMSI flag; can indicate"valid"only for the GPRS supporting terminal</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>MPA</Author>
                <Comment>GPRS support</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Clarified range of len_imsi</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains mobile identities which are used by PL for paging detection.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>ptmsi</Name>
                <Type>U32</Type>
                <Comment>Binary PTMSI representatino</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>MPA</Author>
                <Comment>GPRS support</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Clarified range of len_imsi</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains mobile identities which are used by PL for paging detection.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>v_ptmsi2</Name>
                <Type>U8</Type>
                <Comment>Valid PTMSI flag; can indicate"valid"only for the GPRS supporting terminal</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>MPA</Author>
                <Comment>GPRS support</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Clarified range of len_imsi</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains mobile identities which are used by PL for paging detection.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>ptmsi2</Name>
                <Type>U32</Type>
                <Comment>Binary PTMSI representatino</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>MPA</Author>
                <Comment>GPRS support</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Clarified range of len_imsi</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the type of identity recognised during paging.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>identity_type</Name>
                <Type>U8</Type>
                <Comment>Identity type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_identity_type</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>MPA</Author>
                <Comment>GPRS support</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the needed channel recognised during paging.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>channel_needed</Name>
                <Type>U8</Type>
                <Comment>Channel needed</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_channel_needed</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="10" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>MPA</Author>
                <Comment>GPRS support</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines whether power measurements shall be carried out with or without interrupting listening to the PCH.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>pch_interrupt</Name>
                <Type>U8</Type>
                <Comment>PCH Interrupt</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_pch_interrupt</Name>
            </ValuesLink>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines which frequency bands shall be measured. It is a bitmap indicating the frequency bands for which power measurements shall be carried out.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>freq_bands</Name>
                <Type>U8</Type>
                <Comment>Bitmap of frequency bands</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_freq_bands</Name>
            </ValuesLink>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Expansion of the range for frequency bands</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the number of detected channels during power measurements.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>num_of_chan</Name>
                <Type>U8</Type>
                <Comment>Number of detected channels</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines sending of RACH bursts. It contains the number of RACH bursts, the contents and the time between two RACH bursts.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>c</Name>
                <Type>U8</Type>
                <Comment>dummy; unused, reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added comments, declared c parameter to be reserved</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines sending of RACH bursts. It contains the number of RACH bursts, the contents and the time between two RACH bursts.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>no</Name>
                <Type>U8</Type>
                <Comment>number of RACH messages; this number includes re-transmissions and the first, initial RACH burst, i.e. no = M +1, where M is as defined in GSM 04.08's specification of the initiation of the immediate assignment procedure</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_no</Name>
            </ValuesLink>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added comments, declared c parameter to be reserved</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines sending of RACH bursts. It contains the number of RACH bursts, the contents and the time between two RACH bursts.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>delta</Name>
                <Type>U8</Type>
                <Comment>time in TDMA frames between bursts; delta[0]corresponds to the time between MPH_RANDOM_ACCESS_REQ and the first RACH burst, delta[1]to the time between the first and the 2nd RACH burst and so on</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added comments, declared c parameter to be reserved</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines sending of RACH bursts. It contains the number of RACH bursts, the contents and the time between two RACH bursts.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rach</Name>
                <Type>U8</Type>
                <Comment>channel request content burst n; rach[0]corresponds to the contents of the first RACH burst, rach[1]to the 2nd and so on</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Added comments, declared c parameter to be reserved</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the time a random burst was sent. Format of a reduced frame number. For the definition of the reduced frame number please refer to GSM 05.10.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>t1</Name>
                <Type>U8</Type>
                <Comment>reduced frame number modula 32</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_t1</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the time a random burst was sent. Format of a reduced frame number. For the definition of the reduced frame number please refer to GSM 05.10.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>t2</Name>
                <Type>U8</Type>
                <Comment>reduced frame number modula 26</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_t2</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the time a random burst was sent. Format of a reduced frame number. For the definition of the reduced frame number please refer to GSM 05.10.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>t3</Name>
                <Type>U8</Type>
                <Comment>reduced frame number modula 51</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_t3</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines a service data unit.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>l_buf</Name>
                <Type>U16</Type>
                <Comment>length of content in bit</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines a service data unit.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>o_buf</Name>
                <Type>U16</Type>
                <Comment>offset of content in bit</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines a service data unit.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>buf</Name>
                <Type>U8</Type>
                <Comment>buffer content; comment as in PH SAP</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains the NCC permitted bitmap of the System Information Messages. It is used for selecting accessible neighbour cells for cell reselection purposes. Values are in accordance with GSM 04.08, ch. 10.5.2.27.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>ncc_permitted</Name>
                <Type>U8</Type>
                <Comment>NCC permitted bitmap</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="1" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Elaborated description</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains the type of action.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>action</Name>
                <Type>U8</Type>
                <Comment>start or stop reading of BCCH resp. CCCH</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_action</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>DG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="5" Month="12" Year="2000"/>
                <Author>ID</Author>
                <Comment>Add stop all activities</Comment>
            </History>
            <History>
                <Date Day="30" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Removed stop all activities, elaborated comment</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter indicates which SI should be read.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>si_to_read</Name>
                <Type>U8</Type>
                <Comment>SI to read</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_si_to_read</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="7" Year="2000"/>
                <Author>DG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the frame number when a data block was received, i.e. when the data contained in MPH_UNITDATA_IND was received.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>fn</Name>
                <Type>U32</Type>
                <Comment>full frame number; format: absolute frame number</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="29" Month="8" Year="2000"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>SBK</Author>
                <Comment>Improved description and comment</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the number neighbour cells indicated in MPH_MEAS_ORDER_CNF.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>no_of_ncells</Name>
                <Type>U8</Type>
                <Comment>Number of ncells</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="8" Year="2001"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies if page mode reorganisation should be used and kept (i.e. ignore Page Mode IE in PAGING REQUEST messages) in the idle mode.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>reorg_only</Name>
                <Type>U8</Type>
                <Comment>specifies if reorg should be used</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_reorg_only</Name>
            </ValuesLink>
            <History>
                <Date Day="4" Month="8" Year="2001"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies whether the neighbour cell list provided, shall only be used for synchronisation. No measurements and BCCH reading shall be performed. This is used for GPRS when a PBCCH is available.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>sync_only</Name>
                <Type>U8</Type>
                <Comment>specifies if only sync is used</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_sync_only</Name>
            </ValuesLink>
            <History>
                <Date Day="4" Month="8" Year="2001"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies that the measurement report contains only synchronisation results.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>gprs_sync</Name>
                <Type>U8</Type>
                <Comment>specifies sync results</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_gprs_sync</Name>
            </ValuesLink>
            <History>
                <Date Day="4" Month="8" Year="2001"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter serves as a link bewteen the requested frequency list and measurement results. The values 0 thru 127 are used by procdures controlled at PL, the values 128 thru 255 are reserved for procedures in RR.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>ba_id</Name>
                <Type>U8</Type>
                <Comment>link frequency list and measurement report</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_ba_id</Name>
            </ValuesLink>
            <History>
                <Date Day="2" Month="11" Year="2001"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies the binary state of something.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>stat</Name>
                <Type>U8</Type>
                <Comment>status</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_stat</Name>
            </ValuesLink>
            <History>
                <Date Day="2" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains real and imaginary parts for m=p-4 to p+4 of an E-OTD measurement.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>eotd_crosscor</Name>
                <Type>S16</Type>
                <Comment>Cross correlation</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="29" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the success of an EOTD measurement.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>eotd_res</Name>
                <Type>U8</Type>
                <Comment>EOTD Result</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_eotd_res</Name>
            </ValuesLink>
            <History>
                <Date Day="3" Month="9" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter identifies the requests to measure E-OTD values. This IE is NOT_PRESENT_16BIT for a MPH_NCELL_POS_IND which was not triggered by a MPH_NCELL_POS_REQ. This IE is named 'call reference' by the cursor task that's why it is a USHORT.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>req_id</Name>
                <Type>U16</Type>
                <Comment>Request Identifier</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="29" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="9" Year="2002"/>
                <Author>MPA</Author>
                <Comment>change req_id</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains the energy computed by L1. This IE is named 'RSSI' by the cursor task.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>d_eotd_nrj</Name>
                <Type>U32</Type>
                <Comment>Sum of Amplitudes</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="29" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter contains time difference between the 1st serving cell SB an the neighbour cell SB. This IE is named 'Nominal Position' by the cursor task.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>time_tag</Name>
                <Type>U32</Type>
                <Comment>Time tag</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="29" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter indicates if SB has been demodulated or not.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>sb_flag</Name>
                <Type>U8</Type>
                <Comment>Valid flag</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="29" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies the offset in multiframes between the scell and</XHTMLElement>
                </DocElement>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">the specified cell.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>mfrm_offset</Name>
                <Type>U8</Type>
                <Comment>multiframe offset</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_mfrm_offset</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="9" Year="2002"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies the type of OTD data given by the network.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>otd_type</Name>
                <Type>U8</Type>
                <Comment>OTD type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_otd_type</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="9" Year="2002"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies the expected OTD given by the network.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>exp_otd</Name>
                <Type>U16</Type>
                <Comment>expectedOTD</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_exp_otd</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="9" Year="2002"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies the expected OTD given by the network.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>uncertainty</Name>
                <Type>U8</Type>
                <Comment>Uncertainty of expected OTD</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_uncertainty</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="9" Year="2002"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies the rough RTD given by the network.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rough_rtd</Name>
                <Type>U16</Type>
                <Comment>rough RTD</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_rough_rtd</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="9" Year="2002"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter specifies if EOTD measurements have to be made.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>eotd_avail</Name>
                <Type>U8</Type>
                <Comment>eotd avail</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_eotd_avail</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="9" Year="2002"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter defines the support of GPRS in the cell.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>gprs_support</Name>
                <Type>U8</Type>
                <Comment>GPRS</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_gprs_support</Name>
            </ValuesLink>
            <History>
                <Date Day="30" Month="8" Year="2002"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter indicates by a bit mask which SI buffers should be cleaned.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>si_to_clean</Name>
                <Type>U16</Type>
                <Comment>SI to clean</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_si_to_clean</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="5" Year="2003"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>cause</Name>
                <Type>U8</Type>
                <Comment>Meas report</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_cause</Name>
            </ValuesLink>
            <History>
                <Date Day="16" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>bcch_rxlev_of_sc</Name>
                <Type>U8</Type>
                <Comment>This is the rxlev of BCCH channel. Used only in dedicated mode</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="03" Month="12" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This is a element in the "White List" structure.Indicates whether "White List"belongs to European or American region</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>region</Name>
                <Type>U8</Type>
                <Comment>Indicates whether "White List"belongs to European or American region</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_region</Name>
            </ValuesLink>
            <History>
                <Date Day="07" Month="12" Year="2004"/>
                <Author>khasim</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This is new element in the primitive MPH_POWER_REQ.Identifies the search mode.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>search_mode</Name>
                <Type>U8</Type>
                <Comment>Basic Element</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_search_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="07" Month="12" Year="2004"/>
                <Author>khasim</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This is element in the "White List" structure.Indicates whether "White List" is valid or not</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>white_list_valid</Name>
                <Type>U8</Type>
                <Comment>Indicates whether "White List" is valid or not</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_whitelist_valid</Name>
            </ValuesLink>
            <History>
                <Date Day="07" Month="12" Year="2004"/>
                <Author>khasim</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This is a element in the List structure(Which stores the list of ARFCNS)</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>channels</Name>
                <Type>U8</Type>
                <Comment>Stores list of ARFCNS</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="07" Month="12" Year="2004"/>
                <Author>khasim</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This is new parameter in the MPH_POWER_CNF primitive.The number of "White List"carriers included in the list.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>num_of_white_list_chan</Name>
                <Type>U8</Type>
                <Comment>The number of "White List"carriers included in the list</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="07" Month="12" Year="2004"/>
                <Author>khasim</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This Parameter indicates the number of carriers to be removed from Black List</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>num_of_carriers</Name>
                <Type>U8</Type>
                <Comment>Number of carriers to be removed from the Black List</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="08" Month="12" Year="2004"/>
                <Author>RamPrakash</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>lower_rxlevel_threshold</Name>
                <Type>U8</Type>
                <Comment>lower rxlevel thershold for GSM channels</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="19" Month="01" Year="2005"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">SI-2quater configuration status</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>si2quater_status</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>SI-2quater configuration status</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>Val_si2quater_status</Name>
            </ValuesLink>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">SI-2quater position </XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>si2quater_pos</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>on N-BCCH or E-BCCH</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>Val_si2quater_pos</Name>
            </ValuesLink>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The number of correctly decoded blocks, as defined for RXLEV_VAL, (excluding all SID frames, RATSCCH, SACCH and FACCH blocks) that were completed during the measurement report period. As an exception, FACCH blocks shall be included in the case of signalling only mode.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>nbr_rcvd_blks</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Number of received blocks</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Mapped mean BEP value, as given in sec.8.2.5 of 5.08. In CS side no distinguish as to coding scheme is made.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>mean_bep</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>mapped value of mean BEP</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>Val_mean_bep</Name>
            </ValuesLink>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">CV BEP</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>cv_bep</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>CV BEP</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>Val_cv_bep</Name>
            </ValuesLink>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Indicates the corresponding GSM Neighbour cell index, in case reporting is by EMR. NOT_PRESENT_8BIT is the invalid value. If set as invalid value then it indicates that corresponding BSIC is invalid.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>nc_index</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>GSM Neighbour cell index /index to enhanced cell list</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Indicates if a GSM cell with invalid BSIC and allowed NCC part of the BSIC is one of the six strongest cells. </XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>bsic_seen</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Indicates if a GSM cell with invalid BSIC and allowed NCC part of the BSIC is one of the six strongest cells. </Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Member of enh_para_struct</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>num_valid_cells</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Indicates number of cells valid in cell list in enh para</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author>x0059970</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Member of enh_para_struct</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rep_rate</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting rate</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_rep_rate</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author>x0059970</Author>
                <Comment>R99 PEMR feature</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Member of enh_para_struct. Indicates whether Invalid BSIC reporting is enabled or not. Enabled, if the value is TRUE.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>inv_bsic_enabled</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Is Invalid BSIC reporting enabled?</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>Val_inv_bsic</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author>x0059970</Author>
                <Comment>R99 PEMR feature</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Member of enh_para_struct</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>multiband_rep</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Number of cells, in each non-serving cell band, to be reported </Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author>x0059970</Author>
                <Comment>R99 PEMR feature</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Member of enh_para_struct</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>servingband_rep</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Number of cells, in serving cell band, to be reported</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author>x0059970</Author>
                <Comment>R99 PEMR feature</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">The scale order given by network, to be used for scaling RXLEV values</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>scale_order</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Basic Element</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>Val_scale_ord</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author>x0059970</Author>
                <Comment>R99 PEMR feature</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Member of enh_para_struct</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rep_priority</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting priority of a cell</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>VAL_rep_priority</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">0,1 or more Real Time Difference values for each available neighbour cell arfcn.This is used for the neighbour cell synchronisation without acquiring the FB and SB of the neighbourcell. </XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rtd</Name>
                <Type>U16</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Real Time Difference value for all the neighbour cells </Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Member of enh_para_struct. Apply priority reporting if the reported value is above threshold for GSM frequency band or access technology/mode XXX (one or more), 0, 6, … , 36, infinity (never).Default value = always.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rep_threshold</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting threshold</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>Val_rep_threshold</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Member of enh_para_struct. Apply an offset to the reported value when prioritising the cells for reporting for GSM frequency band or access technology/mode XXX (one or more), 0, 6, … , 42 dB.Default value = 0 dB.</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rep_offset</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting offset</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>Val_rep_offset</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">0,1 or more Real Time Difference values for each available neighbour cell arfcn.This is used for the neighbour cell synchronisation without acquiring the FB and SB of the neighbourcell. </XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rtd</Name>
                <Type>U16</Type>
                <Version>REL99 AND TI_PS_FF_RTD</Version>
                <Comment>Real Time Difference value for all the neighbour cells </Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="19" Month="01" Year="2007"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Report type : Normal or Enhanced</XHTMLElement>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>rep_type</Name>
                <Type>U8</Type>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Report type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mph</DocName>
                <Name>Val_rep_type</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="10" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <DocLink DocType="OTHER">
                        <Name>This parameter defines the mobile station classmark part relevant for PL.</Name>
                    </DocLink>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>pclass_900</Name>
                <Type>U8</Type>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>Power Class GSM 900</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="04" Month="05" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <DocLink DocType="OTHER">
                        <Name>This parameter defines the mobile station classmark part relevant for PL.</Name>
                    </DocLink>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>pclass_850</Name>
                <Type>U8</Type>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>Power Class 850</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="04" Month="05" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <DocLink DocType="OTHER">
                        <Name>This parameter defines the mobile station classmark part relevant for PL.</Name>
                    </DocLink>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>pclass_1900</Name>
                <Type>U8</Type>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>Power Class 1900</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="04" Month="05" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <DocElement>
                    <DocLink DocType="OTHER">
                        <Name>This parameter defines the mobile station classmark part relevant for PL.</Name>
                    </DocLink>
                </DocElement>
            </Description>
            <PrimBasicElemDef>
                <Name>pclass_1800</Name>
                <Type>U8</Type>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>Power Class 1800</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="04" Month="05" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
    </PrimBasicElementsSection>
    <ValuesSection>
        <Description>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all sets of values that are defined for the MPH SAP</XHTMLElement>
            </DocElement>
            <DocElement>
                <XHTMLElement Type="TEXT_SECTION">This section contains all sets of values that are defined for the MPH SAP</XHTMLElement>
            </DocElement>
        </Description>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_arfcn</Name>
                <Comment>values for arfcn</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>E-GSM 900</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4096</Value>
                <Alias/>
                <Comment>E-GSM 900 (E-GSM mode, std=2)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12288</Value>
                <Alias/>
                <Comment>E-GSM 900 (Extended dual mode, std=6)</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>124</MaxValue>
                <Comment>GSM 900 without extension band</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>975</MinValue>
                <MaxValue>1023</MaxValue>
                <Comment>E-GSM 900</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>512</MinValue>
                <MaxValue>810</MaxValue>
                <Comment>DCS 1800 or PCS 1900 (without US_BIT)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>811</MinValue>
                <MaxValue>885</MaxValue>
                <Comment>DCS 1800</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>128</MinValue>
                <MaxValue>256</MaxValue>
                <Comment>GSM 850 without US_BIT</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>2048</MinValue>
                <MaxValue>2048</MaxValue>
                <Comment>GSM 900 without extension band (single mode, std=1)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>4097</MinValue>
                <MaxValue>4220</MaxValue>
                <Comment>GSM 900 (E-GSM mode, std=2)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>5071</MinValue>
                <MaxValue>5119</MaxValue>
                <Comment>E-GSM 900 (E-GSM mode, std=2)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>39424</MinValue>
                <MaxValue>39722</MaxValue>
                <Comment>PCS 1900 (US single mode, std=3)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>8704</MinValue>
                <MaxValue>9077</MaxValue>
                <Comment>DCS 1800 (single mode, std=4)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>10241</MinValue>
                <MaxValue>10364</MaxValue>
                <Comment>GSM 900 (Dual mode, std=5)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>10752</MinValue>
                <MaxValue>11125</MaxValue>
                <Comment>DCS 1800 (Dual mode, std=5)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>12288</MinValue>
                <MaxValue>12412</MaxValue>
                <Comment>GSM 900 (Extended dual mode, std=6)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>13263</MinValue>
                <MaxValue>13311</MaxValue>
                <Comment>E-GSM 900 (Extended dual mode, std=6)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>12800</MinValue>
                <MaxValue>13173</MaxValue>
                <Comment>DCS 1800 (Extended dual mode, std=6)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>47232</MinValue>
                <MaxValue>47355</MaxValue>
                <Comment>GSM 850 (US single mode, std=7)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>49280</MinValue>
                <MaxValue>49403</MaxValue>
                <Comment>GSM 850 (US dual mode, std=8)</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>49664</MinValue>
                <MaxValue>49962</MaxValue>
                <Comment>PCS 1900 (US dual mode, std=8)</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_comb_ccch</Name>
                <Comment>values for comb_ccch</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>COMB_CCCH_NOT_COMB</Alias>
                <Comment>CCCH not combined with SDCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>COMB_CCCH_COMB</Alias>
                <Comment>CCCH combined with SDCCH</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_tn</Name>
                <Comment>values for tn</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>timeslot number 0-7</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_dlt</Name>
                <Comment>values for dlt</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>10</MinValue>
                <MaxValue>45</MaxValue>
                <Comment>initial value</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pg</Name>
                <Comment>values for pg</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>80</MaxValue>
                <Comment>paging group number</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_bs_ag_blocks_res</Name>
                <Comment>values for bs_ag_blocks_res</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>number of blocks reserved for AGCH</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_bs_pa_mfrms</Name>
                <Comment>values for bs_pa_mfrms</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>2 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>3 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias/>
                <Comment>4 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias/>
                <Comment>5 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias/>
                <Comment>6 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias/>
                <Comment>7 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias/>
                <Comment>8 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias/>
                <Comment>9 Multiframe Periods</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_power</Name>
                <Comment>values for power</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>31</MaxValue>
                <Comment>transmission power level</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rx_lev</Name>
                <Comment>values for rx_lev</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>received field strength</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rx_qual_full</Name>
                <Comment>values for rx_qual_full</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>received quality</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_bsic</Name>
                <Comment>values for bsic</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">64</Value>
                <Alias>MPH_BSIC_UNKNOWN</Alias>
                <Comment>Cell is removed from list (GPRS)</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>base station identification code</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_dtx</Name>
                <Comment>values for dtx</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DTX_NOT_USED</Alias>
                <Comment>DTX is not used</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DTX_USED</Alias>
                <Comment>DTX is used</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_otd</Name>
                <Comment>values for otd</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>timing advance</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ta</Name>
                <Comment>values for ta</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>TA_NOT_AVAIL</Alias>
                <Comment>timing advance is not available in Idle Mode</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>timing advance</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_v_start</Name>
                <Comment>values for v_start</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>not valid</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>valid</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ch</Name>
                <Comment>values for ch</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CH_TCH_F</Alias>
                <Comment>TCH/F, FACCH Full Rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CH_TCH_H_1</Alias>
                <Comment>TCH/H(1), FACCH Half Rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CH_TCH_H_2</Alias>
                <Comment>TCH/H(2), FACCH Half Rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CH_SDCCH_4_0</Alias>
                <Comment>SDCCH/4(0)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>CH_SDCCH_4_1</Alias>
                <Comment>SDCCH/4(1)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>CH_SDCCH_4_2</Alias>
                <Comment>SDCCH/4(2)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>CH_SDCCH_4_3</Alias>
                <Comment>SDCCH/4(3)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>CH_SDCCH_8_0</Alias>
                <Comment>SDCCH/8(0)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>CH_SDCCH_8_1</Alias>
                <Comment>SDCCH/8(1)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>CH_SDCCH_8_2</Alias>
                <Comment>SDCCH/8(2)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>CH_SDCCH_8_3</Alias>
                <Comment>SDCCH/8(3)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>CH_SDCCH_8_4</Alias>
                <Comment>SDCCH/8(4)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">13</Value>
                <Alias>CH_SDCCH_8_5</Alias>
                <Comment>SDCCH/8(5)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias>CH_SDCCH_8_6</Alias>
                <Comment>SDCCH/8(6)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>CH_SDCCH_8_7</Alias>
                <Comment>SDCCH/8(7)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_tsc</Name>
                <Comment>values for tsc</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>training sequence code, coded as in GSM 04.08 / 05.02</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_h</Name>
                <Comment>values for h</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>H_NO</Alias>
                <Comment>no hopping</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>H_FREQ</Alias>
                <Comment>frequency hopping</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_maio</Name>
                <Comment>values for maio</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>mobile allocation index offset, coded as in GSM 04.08 / 05.02</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_hsn</Name>
                <Comment>values for hsn</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>hopping sequence number, coded as in GSM 04.08 / 05.02</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rlt</Name>
                <Comment>values for rlt</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>15</MaxValue>
                <Comment>code point allocation according to GSM 04.08, ch. 10.5.2.3a; mapping to values 4, 8, 12, ... 60, 64 has to be done by PL</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pwrc</Name>
                <Comment>values for pwrc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PWRC_NOT_SET</Alias>
                <Comment>PWRC is not set, exact meaning is defined in GSM 05.08</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PWRC_SET</Alias>
                <Comment>PWRC is set, exact meaning is defined in GSM 05.08</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_tav</Name>
                <Comment>values for tav</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>31</MaxValue>
                <Comment>timing advance, coding as in GSM 04.08, ch. 10.5.2.40, bit periods</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_algo</Name>
                <Comment>values for algo</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ALGO_A5_1</Alias>
                <Comment>A5/1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ALGO_A5_2</Alias>
                <Comment>A5/2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>ALGO_A5_3</Alias>
                <Comment>A5/3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>ALGO_A5_4</Alias>
                <Comment>A5/4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>ALGO_A5_5</Alias>
                <Comment>A5/5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>ALGO_A5_6</Alias>
                <Comment>A5/6</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>ALGO_A5_7</Alias>
                <Comment>A5/7</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_mod</Name>
                <Comment>values for mod</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MODE_CELL_SELECTION</Alias>
                <Comment>cell selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MODE_CELL_RESELECTION</Alias>
                <Comment>cell reselection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias/>
                <Comment>unused</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MODE_IMM_ASSIGN</Alias>
                <Comment>immediate assignment</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>MODE_CHAN_ASSIGN</Alias>
                <Comment>channel assignment</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>MODE_ASYNC_HANDOVER</Alias>
                <Comment>asynchronous handover</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>MODE_SYNC_HANDOVER</Alias>
                <Comment>synchronous handover</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>MODE_PRE_SYNC_HANDOVER</Alias>
                <Comment>pre synchronous handover</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>MODE_PSEUDO_SYNC_HANDOVER</Alias>
                <Comment>pseudo synchronous handover</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>MODE_SYS_INFO_CHANGE</Alias>
                <Comment>sys info has changed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>MODE_PACKET_TRANSFER</Alias>
                <Comment>enter packet transfer mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>MODE_PDCH_ASSIGN</Alias>
                <Comment>PDCH assignment</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>MODE_CELL_CHANGE_ORDER</Alias>
                <Comment>network controlled cell change</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">13</Value>
                <Alias>MODE_CELL_RESELECTION_SYNC_ONLY</Alias>
                <Comment>Sync only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias>MODE_CONFIG_PL</Alias>
                <Comment>Config idle mode params, but don't start processes in L1</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_mode</Name>
                <Comment>values for mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>MODE_SIG_ONLY</Alias>
                <Comment>signalling only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias>MODE_SPEECH_VER1</Alias>
                <Comment>speech (full rate or half rate), version 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100001</Value>
                <Alias>MODE_SPEECH_VER2</Alias>
                <Comment>speech (full rate or half rate), version 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01000001</Value>
                <Alias>MODE_SPEECH_VER3</Alias>
                <Comment>speech (full rate or half rate), version 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00001111</Value>
                <Alias>MODE_DATA_14_5</Alias>
                <Comment>data, 14.5 kbit/s radio interface rate, corresponds to 14.4 kbit/s user rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000011</Value>
                <Alias>MODE_DATA_12_0</Alias>
                <Comment>data, 12.0 kbit/s radio interface rate, corresponds to 9.6 kbit/s user rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00001011</Value>
                <Alias>MODE_DATA_6_0</Alias>
                <Comment>data, 6.0 kbit/s radio interface rate, corresponds to 4.8 kbit/s user rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00010011</Value>
                <Alias>MODE_DATA_3_6</Alias>
                <Comment>data, 3.6 kbit/s radio interface rate, corresponds to 2.4 kbit/s user rate</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_st_mode</Name>
                <Comment>values for st_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CODEC_MODE_1</Alias>
                <Comment>lowest codec mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CODEC_MODE_2</Alias>
                <Comment>second lowest mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CODEC_MODE_3</Alias>
                <Comment>third lowest mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CODEC_MODE_4</Alias>
                <Comment>highest mode</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_cs</Name>
                <Comment>values for cs</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CS_NO_BCCH_AVAIL</Alias>
                <Comment>no BCCH available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CS_DOWN_LINK_FAIL</Alias>
                <Comment>down link failure</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CS_RADIO_LINK_FAIL</Alias>
                <Comment>radio link failure</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CS_NO_HBCCH_AVAIL</Alias>
                <Comment>no HPLMN BCCH available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>CS_BCCH_READ_ERROR</Alias>
                <Comment>error during BCCH reading</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>CS_STOP_BCCH_READING</Alias>
                <Comment>stop BCCH reading</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>CS_STOP_PLMN_SEARCH</Alias>
                <Comment>Stop PLMN search</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>CS_CLEAN_SYS_INFO</Alias>
                <Comment>Clean System Information buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">13</Value>
                <Alias>CS_SYS_INFO_1_NOT_NEEDED</Alias>
                <Comment>System info 1 is not needed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias>CS_RXLEV_VAL_REQ</Alias>
                <Comment>Rxlev values are requested</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>CS_STOP_PLMN_SEARCH_AND_DEACTIVATE</Alias>
                <Comment>Stop PLMN search and enter sleep mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">16</Value>
                <Alias>CS_SCELL_IS_SYNCED</Alias>
                <Comment>Synchronization done</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">17</Value>
                <Alias>CS_START_PCCO</Alias>
                <Comment>start of packet cell change order and the cell is not in the BA list</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">18</Value>
                <Alias>CS_NC_SYNC_FAILED</Alias>
                <Comment>Lost synchronization with neighbour cell</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">19</Value>
                <Alias>CS_SYS_INFO_2BIS_SUPPORT_CHANGED</Alias>
                <Comment>Started/stopped broadcasting of SI2bis in idle</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">20</Value>
                <Alias>CS_SYS_INFO_2TER_SUPPORT_CHANGED</Alias>
                <Comment>Started/stopped broadcasting of SI2ter in idle</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>CS_NO_ERROR</Alias>
                <Comment>no error occurred</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pclass</Name>
                <Comment>values for pclass</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CLASS_1</Alias>
                <Comment>class 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CLASS_2</Alias>
                <Comment>class 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CLASS_3</Alias>
                <Comment>class 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CLASS_4</Alias>
                <Comment>class 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CLASS_5</Alias>
                <Comment>class 5</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_tch_loop</Name>
                <Comment>values for tch_loop</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">FF</Value>
                <Alias/>
                <Comment>NOT_PRESENT_8BIT, open TCH loop, valid OPEN_LOOP_CMD message has been received</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TCH_LOOP_A</Alias>
                <Comment>Internal test TCH loop command A</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>TCH_LOOP_B</Alias>
                <Comment>Internal test TCH loop command B</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>TCH_LOOP_C</Alias>
                <Comment>Internal test TCH loop command C</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>TCH_LOOP_D</Alias>
                <Comment>Internal test TCH loop command D</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>TCH_LOOP_E</Alias>
                <Comment>Internal test TCH loop command E</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>TCH_LOOP_F</Alias>
                <Comment>Internal test TCH loop command F</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>TCH_LOOP_I</Alias>
                <Comment>Internal test TCH loop command I</Comment>
            </ValuesItem>
            <ValuesRange ValueType="HEX">
                <MinValue>00</MinValue>
                <MaxValue>FE</MaxValue>
                <Comment>values correspond to GSM 04.14, sub-channel IE of the CLOSE_TCH_LOOP_CMD message</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_dedi_res</Name>
                <Comment>values fordedi_res</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DEDI_RES_OK</Alias>
                <Comment>success</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DEDI_RES_TIMEOUT</Alias>
                <Comment>timeout</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>DEDI_RES_TA_OUT_OF_RANGE</Alias>
                <Comment>timing advance out of range</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>DEDI_RES_CELL_NOT_SYNC</Alias>
                <Comment>cell not sync by ALR</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_device</Name>
                <Comment>values for device</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DAI_NO_TEST</Alias>
                <Comment>normal operation (no tested device via DAI)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DAI_SPEECH_DL</Alias>
                <Comment>test of speech decoder / DTX downlink</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>DAI_SPEECH_UL</Alias>
                <Comment>test of speech decoder / DTX uplink</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>DAI_AD_DA</Alias>
                <Comment>test of acoustic devicesand A/D and D/A</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ho_pow</Name>
                <Comment>values for ho_pow</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>31</MaxValue>
                <Comment>transmission power level; e.g. from a Power Command IE of a HANDOVER COMMAND</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ho_acc_type</Name>
                <Comment>values for ho_acc_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>sending of HANDOVER ACCESS is mandatory</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>sending of HANDOVER ACCESS is optional</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ho_nci</Name>
                <Comment>values for ho_nci</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NCI_TA_OUT_OF_RANGE_OK</Alias>
                <Comment>timing advance out of range allowed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NCI_TA_OUT_OF_RANGE_NOT_ALLOWED</Alias>
                <Comment>timing advance out of range not allowed</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_multi_band</Name>
                <Comment>values for multi_band</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MULTI_BAND_0</Alias>
                <Comment>normal operation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MULTI_BAND_1</Alias>
                <Comment>one cell of the non-serving cell band</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MULTI_BAND_2</Alias>
                <Comment>two cells of the non-serving cell band</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MULTI_BAND_3</Alias>
                <Comment>three cells of the non-serving cell band</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_len_imsi</Name>
                <Comment>values for len_imsi</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>indicates not valid</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>15</MaxValue>
                <Comment>indicates length of IMSI</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_identity_type</Name>
                <Comment>values for identity_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ID_IMSI</Alias>
                <Comment>Paged by IMSI</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>ID_TMSI</Alias>
                <Comment>Paged by TMSI</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>ID_PTMSI</Alias>
                <Comment>Paged by PTMSI</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_channel_needed</Name>
                <Comment>values for channel_needed</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CN_ANY</Alias>
                <Comment>Any channel</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CN_SDCCH</Alias>
                <Comment>SDCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CN_TCH_FULL</Alias>
                <Comment>TCH Full Rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CN_TCH_H_OR_F</Alias>
                <Comment>TCH Half Rate or Full Rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CN_PACKET</Alias>
                <Comment>Packet Channel (GPRS only)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_pch_interrupt</Name>
                <Comment>values for pch_interrupt</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NO_PCH_INTERRUPT</Alias>
                <Comment>Power measurements with PCH listening</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PCH_INTERRUPT</Alias>
                <Comment>Power measurements without PCH listening</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_freq_bands</Name>
                <Comment>values for freq_bands</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>BAND_AUTO</Alias>
                <Comment>0b00000000: All bands shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>BAND_GSM_900</Alias>
                <Comment>0b00000001: GSM 900 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>BAND_DCS_1800</Alias>
                <Comment>0b00000010: DCS 1800 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>BAND_PCS_1900</Alias>
                <Comment>0b00000100: PCS 1900 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">08</Value>
                <Alias>BAND_E_GSM</Alias>
                <Comment>0b00001000: Extended GSM is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">10</Value>
                <Alias>BAND_GSM_850</Alias>
                <Comment>0b00010000: GSM 850 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">20</Value>
                <Alias>BAND_GSM_450</Alias>
                <Comment>0b00100000: GSM 450 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">40</Value>
                <Alias>BAND_GSM_480</Alias>
                <Comment>0b01000000: GSM 480 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">80</Value>
                <Alias>BAND_R_GSM</Alias>
                <Comment>0b10000000: R-GSM is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>BAND_DUAL</Alias>
                <Comment>0b00000011: GSM 900 and DCS 1800 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0B</Value>
                <Alias>BAND_DUAL_EXT</Alias>
                <Comment>0b00001011: GSM 900, E-GSM and DCS 1800 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">14</Value>
                <Alias>BAND_DUAL_US</Alias>
                <Comment>0b00010100: GSM 850 and PCS 1900 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">12</Value>
                <Alias>BAND_850_1800</Alias>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>0b00010010: GSM 850 and DCS 1800 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0D</Value>
                <Alias>BAND_900_1900</Alias>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>0b00001101:  GSM 900, E-GSM and PCS 1900 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">1B</Value>
                <Alias>BAND_850_900_1800</Alias>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>0b00011011: GSM 850, GSM 900, E-GSM and DCS 1800 is supported, shall be scanned</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">1D</Value>
                <Alias>BAND_850_900_1900</Alias>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>0b00011101: GSM 850, GSM 900, E-GSM and PCS 1900 is supported, shall be scanned</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="05" Month="05" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Added BAND_850_1800, BAND_900_1900, BAND_850_900_1800 and BAND_850_900_1900</Comment>
            </History>
            <History>
                <Date Day="02" Month="07" Year="2008"/>
                <Author>x0083022</Author>
                <Comment>Added GSM_900 Band value to Bands: BAND_850_900_180, BAND_850_900_1900 and BAND_900_1900</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_no</Name>
                <Comment>values for no</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NO_STP_SND_CONT_SND</Alias>
                <Comment>stop sending of RACH bursts</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>8</MaxValue>
                <Comment>valid values for number of RACH bursts to be sent</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_t1</Name>
                <Comment>values for t1</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>31</MaxValue>
                <Comment>frame number modulo 32</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_t2</Name>
                <Comment>values for t2</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>25</MaxValue>
                <Comment>frame number modulo 26</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_t3</Name>
                <Comment>values for t3</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>50</MaxValue>
                <Comment>frame number modulo 51</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_action</Name>
                <Comment>values for action</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>START_MON_NBCCH</Alias>
                <Comment>start reading of BCCH, excluding ext BCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>START_MON_EBCCH</Alias>
                <Comment>start reading of ext BCCH, excluding BCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>STOP_MON_BCCH</Alias>
                <Comment>stop reading of BCCH, including both BCCH and ext BCCH (if previously requested)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>START_MON_CCCH</Alias>
                <Comment>start reading of CCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>STOP_MON_CCCH</Alias>
                <Comment>stop reading of CCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">05</Value>
                <Alias>LEAVING_PIM_PBCCH</Alias>
                <Comment>Leave PIM</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">06</Value>
                <Alias>LEAVING_PAM_PBCCH</Alias>
                <Comment>Leave PAM</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">07</Value>
                <Alias>LEAVING_PTM_PBCCH</Alias>
                <Comment>Leave PTM</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">08</Value>
                <Alias>ENTER_PTM_PBCCH</Alias>
                <Comment>Enter PTM</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">09</Value>
                <Alias>ENTER_PIM_PBCCH</Alias>
                <Comment>Enter PIM</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0A</Value>
                <Alias>ENTER_PTM_BCCH</Alias>
                <Comment>Enter PTM for BCCH</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_si_to_read</Name>
                <Comment>values for si_to_read</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>UNSPECIFIED_SI</Alias>
                <Comment>Update of unspecified SI message or SI messages</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>UPDATE_SI1</Alias>
                <Comment>Update of SI1 message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>UPDATE_SI2_SI2BIS_OR_SI2TER</Alias>
                <Comment>Update of SI2, SI2 bis or SI2 ter message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>UPDATE_SI3_SI4_SI7_OR_SI8</Alias>
                <Comment>Update of SI3, SI4, SI7 or SI8 message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>UPDATE_SI9</Alias>
                <Comment>Update of SI9 message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>COMPLETE_SI</Alias>
                <Comment>Read complete SI</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>UPDATE_SI13_GSM</Alias>
                <Comment>Read SI13 during GPRS activation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>UPDATE_SI2QUATER</Alias>
                <Comment>Request to update SI-2quater</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>UPDATE_SI2QUATER_AGAIN</Alias>
                <Comment>Request to update SI-2quater again as the prev si-2quater BA-IND was not correct</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>UPDATE_SI13</Alias>
                <Comment>Update SI13</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Updated for SI-2quater</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_reorg_only</Name>
                <Comment>values for reorg_only</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NORMAL_PGM</Alias>
                <Comment>ignore this parameter (and do not ignore Page Mode IE in PAGING REQUEST messages); used to switch off REORG_ONLY</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>REORG_ONLY</Alias>
                <Comment>set page mode to paging reorganisation</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_sync_only</Name>
                <Comment>values for sync_only</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NORMAL_BA</Alias>
                <Comment>normal GSM behaviour</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SYNC_LIST</Alias>
                <Comment>GPRS sync only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>RECONFIRM_SYNC_LIST</Alias>
                <Comment>Reconfirm Sync 10 sec timer for Pbcch Cells</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="01" Year="2006"/>
                <Author>xjohnrak</Author>
                <Comment>Added value RECONFIRM_SYNC_LIST</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_gprs_sync</Name>
                <Comment>values for gprs_sync</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NORMAL_MEAS_REP</Alias>
                <Comment>normal GSM behaviour</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SYNC_RESULTS</Alias>
                <Comment>GPRS sync only</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_ba_id</Name>
                <Comment>values for ba_id</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>127</MaxValue>
                <Comment>used by PL</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>128</MinValue>
                <MaxValue>255</MaxValue>
                <Comment>used by RR</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_stat</Name>
                <Comment>values for stat</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>STAT_INACT</Alias>
                <Comment>inactive</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>STAT_ACT</Alias>
                <Comment>active</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>STAT_CIPH_OFF</Alias>
                <Comment>ciphering off</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>STAT_CIPH_ON</Alias>
                <Comment>ciphering on</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_eotd_res</Name>
                <Comment>values for eotd_res</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EOTD_SUCC</Alias>
                <Comment>success</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EOTD_REF</Alias>
                <Comment>wrong reference BTS</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_mfrm_offset</Name>
                <Comment>values for mfrm_offset</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>51</MaxValue>
                <Comment>multiframes/ 51 is interpreted as 0</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_otd_type</Name>
                <Comment>values for otd_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ROUGH_OTD</Alias>
                <Comment>only roughOTD has been provided by the NW</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EXPECTED_OTD</Alias>
                <Comment>only expectedOTD has been provided by the NW</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>BOTH_OTD</Alias>
                <Comment>Both OTD type have been provided by the NW</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_exp_otd</Name>
                <Comment>values for exp_otd</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>1250</MaxValue>
                <Comment>The used resolution is 1 bits. This OTD value is the OTD value of TS0s (i.e. the difference in starting of TS0), not only the OTD between starts of bursts expected OTD between the scell and the specified cell. Note: 1250 is interpreted as 0</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_uncertainty</Name>
                <Comment>values for uncertainty</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>UNC_MAX_2BIT</Alias>
                <Comment>uncertainty in bits. 0 - 2 bits</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>UNC_MAX_4BIT</Alias>
                <Comment>uncertainty in bits. 3 - 4 bits</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>UNC_MAX_8BIT</Alias>
                <Comment>uncertainty in bits. 5 - 8 bits</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>UNC_MAX_12BIT</Alias>
                <Comment>uncertainty in bits. 9 - 12 bits</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>UNC_MAX_16BIT</Alias>
                <Comment>uncertainty in bits. 13 - 16 bits</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>UNC_MAX_22BIT</Alias>
                <Comment>uncertainty in bits. 17 - 22 bits</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>UNC_MAX_30BIT</Alias>
                <Comment>uncertainty in bits. 23 - 30 bits</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>UNC_GT_30BIT</Alias>
                <Comment>uncertainty in bits.  &gt; 30 bits</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rough_rtd</Name>
                <Comment>values for rough_rtd</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>roughRTD in bits (see expected OTD)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_eotd_avail</Name>
                <Comment>values for eotd_avail</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>EOTD is not available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>EOTD is available</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_gprs_support</Name>
                <Comment>values for gprs_support</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MPH_GPRS_PROCS_USED</Alias>
                <Comment>yes</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MPH_GPRS_PROCS_NOT_USED</Alias>
                <Comment>no</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_si_to_clean</Name>
                <Comment>values for si_to_clean</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">0001</Value>
                <Alias>IND_SI_1</Alias>
                <Comment>Clean SI 1 buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0002</Value>
                <Alias>IND_SI_2</Alias>
                <Comment>Clean SI 2 buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0004</Value>
                <Alias>IND_SI_2BIS</Alias>
                <Comment>Clean SI 2bis buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0008</Value>
                <Alias>IND_SI_2TER</Alias>
                <Comment>Clean SI 2ter buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0010</Value>
                <Alias>IND_SI_3</Alias>
                <Comment>Clean SI 3 buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0020</Value>
                <Alias>IND_SI_4</Alias>
                <Comment>Clean SI 4 buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0040</Value>
                <Alias>IND_SI_13</Alias>
                <Comment>Clean SI 13 buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0080</Value>
                <Alias>IND_SI_2QUATER</Alias>
                <Comment>Clean SI 2quater buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0100</Value>
                <Alias>IND_SI_5</Alias>
                <Comment>Clean SI 5 buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0200</Value>
                <Alias>IND_SI_5BIS</Alias>
                <Comment>Clean SI 5bis buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0400</Value>
                <Alias>IND_SI_5TER</Alias>
                <Comment>Clean SI 5ter buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0800</Value>
                <Alias>IND_SI_6</Alias>
                <Comment>Clean SI 6 buffer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">007F</Value>
                <Alias>IND_ALL_IDLE_SI</Alias>
                <Comment>Clean all SI of idle mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">000E</Value>
                <Alias>IND_ALL_IDLE_BA</Alias>
                <Comment>Clean all SI of idle mode BA list</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0F00</Value>
                <Alias>IND_ALL_DEDI_SI</Alias>
                <Comment>Clean all SI of dedicated  mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0700</Value>
                <Alias>IND_ALL_DEDI_BA</Alias>
                <Comment>Clean all SI of dedicated  mode BA list</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0F7F</Value>
                <Alias>IND_ALL_SI</Alias>
                <Comment>Clean all SI buffers</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Updated for SI-2quater. </Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION"/>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_cause</Name>
                <Comment>values for cause</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">0</Value>
                <Alias>NC_STOP_MEAS</Alias>
                <Comment>Stop the measurement</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">1</Value>
                <Alias>NC_START_MEAS</Alias>
                <Comment>Start Averaging the measurements</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">2</Value>
                <Alias>NC_REPORT_MEAS </Alias>
                <Comment>get the meas report from RR</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Indicates whether "White List"belongs to European or American region 0x00 European region,0x01 American region </XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_region</Name>
                <Comment>Indicates whether "White List"belongs to European or American region</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EUROPEAN_REGION</Alias>
                <Comment>Indicates European region</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>AMERICAN_REGION</Alias>
                <Comment>Indicates American region</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>BOTH_REGIONS</Alias>
                <Version>TI_PS_FF_QUAD_BAND_SUPPORT</Version>
                <Comment>Indicates both European and American region</Comment>
            </ValuesItem>
            <History>
                <Date Day="07" Month="12" Year="2004"/>
                <Author>khasim</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="06" Month="05" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Added both region</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Identifies the search mode. Can take four values 0x01   -  FAST_SEARCH_MODE,0x02   - NORMAL_SEARCH_MODE,0x03   -  FULL_SEARCH_MODE,0x04   -  BLACKLIST_SEARCH_MODE</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_search_mode</Name>
                <Comment>Identifies the search mode.</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>FULL_SEARCH_MODE</Alias>
                <Comment>Identifies "Full Search" mode, default mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>NORMAL_SEARCH_MODE</Alias>
                <Comment>Identifies "Normal Search" mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>FAST_SEARCH_MODE</Alias>
                <Comment>Identifies "Fast Search" mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>BLACK_LIST_SEARCH_MODE</Alias>
                <Comment>Identifies "Black List Search" mode</Comment>
            </ValuesItem>
            <History>
                <Date Day="07" Month="12" Year="2004"/>
                <Author>khasim</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Indicates whether "White List" is valid or not</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_whitelist_valid</Name>
                <Comment>Indicates whether "White List" is valid or not</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>WHITELIST_NOT_VALID</Alias>
                <Comment>not valid</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>WHITELIST_VALID</Alias>
                <Comment>valid</Comment>
            </ValuesItem>
            <History>
                <Date Day="07" Month="12" Year="2004"/>
                <Author>khasim</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">This parameter is used for measurements - SACCH rate reporting or Reduced reporting rate.</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rep_rate</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values for reporting rate</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>NORMAL_REP_RATE</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Normal(SACCH)reporting rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>REDUCED_REP_RATE</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reduced reporting rate</Comment>
            </ValuesItem>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author>x0059970</Author>
                <Comment>R99 PEMR feature</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Values for Invalid BSIC reporting.</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>Val_inv_bsic</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Invalid BSIC reporting</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>INV_BSIC_REPORTING_DISABLED</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Invalid BSIC reporting not enabled</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>INV_BSIC_REPORTING_ENABLED</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Invalid BSIC reporting enabled</Comment>
            </ValuesItem>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author>x0059970</Author>
                <Comment>R99 PEMR feature</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">SI-2quater status</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>Val_si2quater_status</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values for SI2QUATER Status</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SI2QUATER_ABSENT</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Not present/Not required</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SI2QUATER_CONFIGURE</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Has to be configured</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SI2QUATER_ACQ_PENDING</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Acquisition is pending.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SI2QUATER_ACQ_COMP</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Acquisition is complete</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SI2QUATER_ACQ_FULL_BCCH</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Acquisition is on going as part of full BCCH reading</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SI2QUATER_ACQ_WRONG_BAIND</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Acquired with wrong BA-IND</Comment>
            </ValuesItem>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">SI-2Quater Position</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>Val_si2quater_pos</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values for SI-2Quater Position</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SI2QUATER_ON_NBCCH</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>SI-2quater on NBCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SI2QUATER_ON_EBCCH</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>SI-2quater on EBCCH</Comment>
            </ValuesItem>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">values of Mean BEP</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>Val_mean_bep</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>values of Mean BEP</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>MEAN_BEP_0</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>MEAN_BEP_1</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>MEAN_BEP_2</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>MEAN_BEP_3</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>MEAN_BEP_4</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">05</Value>
                <Alias>MEAN_BEP_5</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">06</Value>
                <Alias>MEAN_BEP_6</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">07</Value>
                <Alias>MEAN_BEP_7</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">08</Value>
                <Alias>MEAN_BEP_8</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">09</Value>
                <Alias>MEAN_BEP_9</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0a</Value>
                <Alias>MEAN_BEP_10</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0b</Value>
                <Alias>MEAN_BEP_11</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0c</Value>
                <Alias>MEAN_BEP_12</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0d</Value>
                <Alias>MEAN_BEP_13</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0e</Value>
                <Alias>MEAN_BEP_14</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0f</Value>
                <Alias>MEAN_BEP_15</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">10</Value>
                <Alias>MEAN_BEP_16</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">11</Value>
                <Alias>MEAN_BEP_17</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">12</Value>
                <Alias>MEAN_BEP_18</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">13</Value>
                <Alias>MEAN_BEP_19</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">14</Value>
                <Alias>MEAN_BEP_20</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">15</Value>
                <Alias>MEAN_BEP_21</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">16</Value>
                <Alias>MEAN_BEP_22</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">17</Value>
                <Alias>MEAN_BEP_23</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">18</Value>
                <Alias>MEAN_BEP_24</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">19</Value>
                <Alias>MEAN_BEP_25</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">1a</Value>
                <Alias>MEAN_BEP_26</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">1b</Value>
                <Alias>MEAN_BEP_27</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">1c</Value>
                <Alias>MEAN_BEP_28</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">1d</Value>
                <Alias>MEAN_BEP_29</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">1e</Value>
                <Alias>MEAN_BEP_30</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">1f</Value>
                <Alias>MEAN_BEP_31</Alias>
                <Comment>mapped value</Comment>
            </ValuesItem>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Values of CV BEP </XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>Val_cv_bep</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values of CV BEP</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CV_BEP_0</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values Item</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CV_BEP_1</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values Item</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CV_BEP_2</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values Item</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CV_BEP_3</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values Item</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CV_BEP_4</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values Item</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>CV_BEP_5</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values Item</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>CV_BEP_6</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values Item</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>CV_BEP_7</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values Item</Comment>
            </ValuesItem>
            <History>
                <Date Day="05" Month="01" Year="2007"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Scaling order values as indicated by NW </XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>Val_scale_ord</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>scale order</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>SCALE_0dB</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Scaling by 0dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>SCALE_10dB</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Scaling by 10dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>SCALE_AUTO</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Automatic scaling</Comment>
            </ValuesItem>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Reporitng priority as received in air message</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>VAL_rep_priority</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values for reporting priority</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>REP_PRIOR_NORM</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Normal reporting priority</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>REP_PRIOR_HIGH</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>High reporting priority</Comment>
            </ValuesItem>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Values for Reporting thresholds- Enumerated.</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>Val_rep_threshold</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Reporting thresholds</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>REP_THRESHOLD_0</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>0 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>REP_THRESHOLD_6</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>6 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>REP_THRESHOLD_12</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>12 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>REP_THRESHOLD_18</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>18 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>REP_THRESHOLD_24</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>24 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">05</Value>
                <Alias>REP_THRESHOLD_30</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>30 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">06</Value>
                <Alias>REP_THRESHOLD_36</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>36 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">07</Value>
                <Alias>REP_THRESHOLD_INF</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Report Never</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">ff</Value>
                <Alias>REP_THRESHOLD_NONE</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Report Always, default value</Comment>
            </ValuesItem>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Values for reporting offset</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>Val_rep_offset</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Values for reporting offset</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>REP_OFFSET_0</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>0dB (Default)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>REP_OFFSET_6</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>6 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>REP_OFFSET_12</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>12 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>REP_OFFSET_18</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>18 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>REP_OFFSET_24</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>24 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">05</Value>
                <Alias>REP_OFFSET_30</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>30 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">06</Value>
                <Alias>REP_OFFSET_36</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>36 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">07</Value>
                <Alias>REP_OFFSET_42</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>42 dB</Comment>
            </ValuesItem>
            <History>
                <Date Day="25" Month="10" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <DocElement>
                    <XHTMLElement Type="TEXT_SECTION">Report type for measurement reporting</XHTMLElement>
                </DocElement>
            </Description>
            <ValuesDef>
                <Name>Val_rep_type</Name>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>report type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">0</Value>
                <Alias>REP_TYPE_ENH</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Report type is 'Enhanced'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">1</Value>
                <Alias>REP_TYPE_NORM</Alias>
                <Version>REL99 AND (TI_PS_FF_EMR OR TI_PS_FF_RTD)</Version>
                <Comment>Report type is 'Normal'</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="10" Year="2006"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
    </ValuesSection>
</SAP>