<?xml version="1.0" encoding="UTF-8"?>
<!-- edited with SAPE SAP Editor -->
<SAP xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="sap.xsd">
    <DocInfoSection>
        <DocName DocType="SAP">em</DocName>
        <DocNum Number="129" Project="8304"/>
        <Description>
            <Section>The Protocol Stacks are used to define the functionality of the GSM protocols for interfaces. The GSM specifications are normative when used to describe the functionality of interfaces, but the stacks and the subdivision of protocol layers does not imply or restrict any implementation.</Section>
            <Section>The base of the Protocol Stack rests on the physical layer.</Section>
            <Section>The Data Link Layer (DL) is used to handle an acknowledged connection between mobile and base station. The LAPDm protocol is used.</Section>
            <Section>Radio Resource (RR) manages the resources of the air-interface. That means configuration of physical layer, cell selection and cell reselection, data transfer, RR-Connection handling.</Section>
            <Section>Mobility Management (MM) handles registration aspects for the mobile station. It detects changes of location areas and updates a mobile station in the new location area.</Section>
            <Section>Call Control (CC) provides the call functionality. This includes call establishment, call maintenance procedures like Hold, Retrieve or Modify, and call disconnection.</Section>
            <Section>Supplementary Services (SS) handles all call independent supplementary services like call forwarding or call barring.</Section>
            <Section>Short Message Services (SMS) is used for sending and receiving point-to-point short messages. Additionally the reception of cell broadcast short messages is included.</Section>
            <Section>The man machine interface (MMI) is the interface to the user. Normally it is connected with a keypad as input device and a display as output device.</Section>
            <Section>Between the several entities data interfaces are defined. These data interfaces are called Service Access Points (SAPs), indicating that an upper layer uses the services of a lower layer.</Section>
            <Section>The GSM specification do not set out any implementation of the Protocol Stack. The following diagrams show the implementation described in all these documents for the mobile station. All entities except the Man Machine Interface and Physical Layer are implemented as part of the Protocol Stack.</Section>
            <Section>Figure 1: Mobile-station protocol architecture</Section>
            <Section>This document describes the monitoring services offered by radio resource and TI++ for the Condat RT.</Section>
        </Description>
        <DocHistory>
            <DocVersion Number="100" Year="96"/>
            <Date Day="15" Month="7" Year="1998"/>
            <Author>Stefan</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Lemke et al Initial</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="101" Year="96"/>
            <Date Day="11" Month="8" Year="1998"/>
            <Author>Volker</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Klann Swap comment for Hopping Flag, introduce v_plmn in T_plmn</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="102" Year="96"/>
            <Date Day="1" Month="6" Year="2001"/>
            <Author>Oliver</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Thoenissen Update for the Engineering Mode</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="103" Year="96"/>
            <Date Day="25" Month="2" Year="2002"/>
            <Author>Oliver</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Thoenissen v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
        </DocHistory>
        <DocRef>
            <RefId>[2]</RefId>
            <RefTitle>GSM 2.82, Call Forwarding Supplementary Services - Stage 1 ETS 300 515, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[3]</RefId>
            <RefTitle>GSM 2.83, Call Waiting and Call Hold Supplementary Services - Stage 1 ETS 300 516, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[4]</RefId>
            <RefTitle>GSM 2.84, Multi Party Supplementary Services - Stage 1 ETS 300 517, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[5]</RefId>
            <RefTitle>GSM 2.85, Closed User Group Supplementary Services - Stage 1 ETS 300 518, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[6]</RefId>
            <RefTitle>GSM 2.86, Advice of Charge Supplementary Services - Stage 1 ETS 300 519, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[7]</RefId>
            <RefTitle>GSM 2.88, Call Barring Supplementary Services - Stage 1 ETS 300 520, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[8]</RefId>
            <RefTitle>GSM 3.14, Support of Dual Tone Multi Frequency Signalling via the GSM System ETS 300 532, ETSI, April 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[9]</RefId>
            <RefTitle>GSM 3.40, Technical Realization of the Short Message Service Point-to-Point ETS 300 536, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[10]</RefId>
            <RefTitle>GSM 3.41, Technical Realization of Short Message Service Cell Broadcast ETS 300 537, ETSI, June 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[11]</RefId>
            <RefTitle>GSM 3.81, Line Identification Supplementary Services - Stage 2 ETS 300 542, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[12]</RefId>
            <RefTitle>GSM 3.82, Call Forwarding Supplementary Services - Stage 2 ETS 300 543, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[13]</RefId>
            <RefTitle>GSM 3.83, Call Waiting and Call Hold Supplementary Services - Stage 2 ETS 300 544, ETSI, November 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[14]</RefId>
            <RefTitle>GSM 3.84, Multi Party Supplementary Services - Stage 2 ETS 300 545, ETSI, November 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[15]</RefId>
            <RefTitle>GSM 3.85, Closed User Group Supplementary Services - Stage 2 ETS 300 546, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[16]</RefId>
            <RefTitle>GSM 3.86, Advice of Charge Supplementary Services - Stage 2 ETS 300 547, ETSI, March 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[17]</RefId>
            <RefTitle>GSM 3.88, Call Barring Supplementary Services - Stage 2 ETS 300 548, ETSI, November 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[18]</RefId>
            <RefTitle>GSM 4.01, MS-BSS Interface General Aspects and Principles ETS 300 550, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[18a]</RefId>
            <RefTitle>GSM 4.03, MS-BSS Interface Channel Structures and Access Capabilities ETS 300 552, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[19]</RefId>
            <RefTitle>GSM 4.05, Data Link Layer General Aspects ETS 300 554, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[20]</RefId>
            <RefTitle>GSM 4.06, MS-BSS Interface Data Link Layer Specification ETS 300 555, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[21]</RefId>
            <RefTitle>GSM 4.07, Mobile Radio Interface Signalling Layer 3 General Aspects ETS 300 556, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[22]</RefId>
            <RefTitle>GSM 4.08, Mobile Radio Interface Layer 3 Specification ETS 300 557, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[23]</RefId>
            <RefTitle>GSM 4.10, Mobile Radio Interface Layer 3 Supplementary Services Specification  General Aspects ETS 300 558, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[24]</RefId>
            <RefTitle>GSM 4.11, Point-to-Point Short Message Service Support on Mobile Radio Interface ETS 300 559, ETSI, October 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[25]</RefId>
            <RefTitle>GSM 4.12, Short Message Service Cell Broadcast Support on Mobile Radio Interface ETS 300 560, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[26]</RefId>
            <RefTitle>GSM 4.80, Mobile Radio Interface Supplementary Services Specification Formats and Coding ETS 300 564, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[27]</RefId>
            <RefTitle>GSM 4.81, Line Identification Supplementary Services - Stage 3 ETS 300 565, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[28]</RefId>
            <RefTitle>GSM 4.82, Call Forwarding Supplementary Services - Stage 3 ETS 300 566, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[29]</RefId>
            <RefTitle>GSM 4.83, Call Waiting and Call Hold Supplementary Services - Stage 3 ETS 300 567, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[30]</RefId>
            <RefTitle>GSM 4.84, Multi Party Supplementary Services - Stage 3 ETS 300 568, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[31]</RefId>
            <RefTitle>GSM 4.85, Closed User Group Supplementary Services - Stage 3 ETS 300 569, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[32]</RefId>
            <RefTitle>GSM 4.86, Advice of Charge Supplementary Services - Stage 3 ETS 300 570, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[33]</RefId>
            <RefTitle>GSM 4.88, Call Barring Supplementary Services - Stage 3 ETS 300 571, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[34]</RefId>
            <RefTitle>GSM 5.01, Physical Layer on the Radio Path General Description ETS 300 573, ETSI, October 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[35]</RefId>
            <RefTitle>GSM 5.02, Multiplexing and Multiple Access on the Radio Path ETS 300 574, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[36]</RefId>
            <RefTitle>GSM 5.08, Radio Sub-system Link Control ETS 300 578, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[37]</RefId>
            <RefTitle>GSM 5.10, Radio Sub-system Synchronisation ETS 300 579, ETSI, October 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[38]</RefId>
            <RefTitle>Service Access Point MMREG 6147.100.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[39]</RefId>
            <RefTitle>Service Access Point MNCC 6147.101.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[40]</RefId>
            <RefTitle>Service Access Point MNSS 6147.102.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[41]</RefId>
            <RefTitle>Service Access Point MNSMS 6147.103.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[42]</RefId>
            <RefTitle>Service Access Point MMCC 6147.104.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[43]</RefId>
            <RefTitle>Service Access Point MMSS 6147.105.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[44]</RefId>
            <RefTitle>Service Access Point MMSMS 6147.106.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[45]</RefId>
            <RefTitle>Service Access Point RR 6147.107.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[46]</RefId>
            <RefTitle>Service Access Point SIM 6147.108.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[47]</RefId>
            <RefTitle>Service Access Point MPH 6147.109.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[48]</RefId>
            <RefTitle>Service Access Point DL 6147.110.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[49]</RefId>
            <RefTitle>Service Access Point MDL 6147.111.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[50]</RefId>
            <RefTitle>Service Access Point PH 6147.112.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[51]</RefId>
            <RefTitle>Service Access Point MMI 6147.113.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[52]</RefId>
            <RefTitle>Message Sequence Charts CC 6147.200.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[53]</RefId>
            <RefTitle>Message Sequence Charts SS 6147.201.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[54]</RefId>
            <RefTitle>Message Sequence Charts SMS 6147.202.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[55]</RefId>
            <RefTitle>Message Sequence Charts MM 6147.203.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[56]</RefId>
            <RefTitle>Message Sequence Charts RR 6147.204.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[57]</RefId>
            <RefTitle>Message Sequence Charts DL 6147.205.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[58]</RefId>
            <RefTitle>Users Guide 6147.300.96.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[59]</RefId>
            <RefTitle>Test Specification CC 6147.400.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[60]</RefId>
            <RefTitle>Test Specification SS 6147.401.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[61]</RefId>
            <RefTitle>Test Specification SMS 6147.402.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[62]</RefId>
            <RefTitle>Test Specification MM 6147.403.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[63]</RefId>
            <RefTitle>Test Specification RR 6147.404.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[64]</RefId>
            <RefTitle>Test Specification DL 6147.405.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[65]</RefId>
            <RefTitle>Test Specification CCD 6147.406.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[66]</RefId>
            <RefTitle>SDL Specification CC 6147.500.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[67]</RefId>
            <RefTitle>SDL Specification SS 6147.501.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[68]</RefId>
            <RefTitle>SDL Specification SMS 6147.502.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[69]</RefId>
            <RefTitle>SDL Specification MM 6147.503.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[70]</RefId>
            <RefTitle>SDL Specification RR 6147.504.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[71]</RefId>
            <RefTitle>SDL Specification DL 6147.505.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[72]</RefId>
            <RefTitle>Message Specification CC 6147.600.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[73]</RefId>
            <RefTitle>Message Specification SS 6147.601.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[74]</RefId>
            <RefTitle>Message Specification SMS 6147.602.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[75]</RefId>
            <RefTitle>Message Specification MM 6147.603.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[76]</RefId>
            <RefTitle>Message Specification RR 6147.604.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[77]</RefId>
            <RefTitle>Message Specification DL 6147.605.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[78]</RefId>
            <RefTitle>Technical Documentation CC 6147.700.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[79]</RefId>
            <RefTitle>Technical Documentation SS 6147.701.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[80]</RefId>
            <RefTitle>Technical Documentation SMS 6147.702.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[81]</RefId>
            <RefTitle>Technical Documentation MM 6147.703.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[82]</RefId>
            <RefTitle>Technical Documentation RR 6147.704.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[83]</RefId>
            <RefTitle>Technical Documentation DL 6147.705.97.100; Condat GmbH</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[84]</RefId>
            <RefTitle>Technical Documentation CCD 6147.706.97.100; Condat GmbH</RefTitle>
        </DocRef>
    </DocInfoSection>
    <ConstantsSection>
        <Description>
            <Section>This section contains all constants that are defined for the EM SAP</Section>
        </Description>
        <Constant>
            <Alias>MAX_SDU_LEN</Alias>
            <Value ValueType="DEC">1</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_PDP_CTXT</Alias>
            <Value ValueType="DEC">2</Value>
            <Comment>MAX number of PDP contexts supported</Comment>
        </Constant>
        <History>
            <Date Day="19" Month="9" Year="2001"/>
            <Author>OT</Author>
            <Comment>Initial</Comment>
        </History>
    </ConstantsSection>
    <PrimitivesSection PrimIDType="BIT16" SAPid="62">
        <Description>
            <Section>This section contains all primitives that are defined for the EM SAP</Section>
        </Description>
        <Primitive>
            <Description>
                <Section>The EM_SC_INFO_REQ is used to request the serving cell infrastructure data as specified in 8443.601.01.002 from RR.</Section>
                <Section>It is send by ACI_EM.</Section>
            </Description>
            <PrimDef>
                <Name>EM_SC_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="0"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SC_INFO_CNF is used to send the requested cell infrastructure data from RR to EM.</Section>
                <Section>It is send by RR.</Section>
            </Description>
            <PrimDef>
                <Name>EM_SC_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="0"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>Channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c1</Name>
                </ItemLink>
                <Comment>Path loss criterion</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c2</Name>
                </ItemLink>
                <Comment>Cell reselection criterion</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rxlev</Name>
                </ItemLink>
                <Comment>Received field strength</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Comment>Base station ID code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>dsc</Name>
                </ItemLink>
                <Comment>Downlink signalling counter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>txlev</Name>
                </ItemLink>
                <Comment>Transmit power level</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <Comment>Timeslot number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rlt</Name>
                </ItemLink>
                <Comment>Radio link timeout counter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tav</Name>
                </ItemLink>
                <Comment>Timing advance</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rxlev_f</Name>
                </ItemLink>
                <Comment>Received field strength full</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rxlev_s</Name>
                </ItemLink>
                <Comment>Received field strength sub</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rxqual_f</Name>
                </ItemLink>
                <Comment>Received quality full</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rxqual_s</Name>
                </ItemLink>
                <Comment>Received quality sub</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>lac</Name>
                </ItemLink>
                <Comment>Location area code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cba</Name>
                </ItemLink>
                <Comment>Cell bar access</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cbq</Name>
                </ItemLink>
                <Comment>Cell bar qualifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cell_id</Name>
                </ItemLink>
                <Comment>Cell Identity</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cell_type_ind</Name>
                </ItemLink>
                <Comment>Cell type indicator</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>vocoder</Name>
                </ItemLink>
                <Comment>vocoder type</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SC_GPRS_INFO_REQ is used to request the serving cell GPRS infrastructure data as specified in 8443.601.01.002 from RR.</Section>
                <Section>It is send by ACI_EM.</Section>
            </Description>
            <PrimDef>
                <Name>EM_SC_GPRS_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="1"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SC_GPRS_INFO_CNF is used to send the requested GPRS cell infrastructure data from RR to EM.</Section>
                <Section>It is send by RR.</Section>
            </Description>
            <PrimDef>
                <Name>EM_SC_GPRS_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="1"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>gmm_state</Name>
                </ItemLink>
                <Comment>GPRS state</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <Comment>PCCCH_Timeslot</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>nmo</Name>
                </ItemLink>
                <Comment>Network Mode of Operation</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>net_ctrl</Name>
                </ItemLink>
                <Comment>Network control</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cba</Name>
                </ItemLink>
                <Comment>Cell bar access</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rac</Name>
                </ItemLink>
                <Comment>Routing area code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tav</Name>
                </ItemLink>
                <Comment>Timing advance</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>dsc</Name>
                </ItemLink>
                <Comment>Downlink signalling counter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c31</Name>
                </ItemLink>
                <Comment>Cell reselection criterion c32</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c32</Name>
                </ItemLink>
                <Comment>Cell reselection criterion c32</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>nco</Name>
                </ItemLink>
                <Comment>Network controlled order</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_NC_INFO_REQ is used to request the neighbour cell infrastructure data as specified in 8443.601.01.002 from RR.</Section>
                <Section>It is send by ACI_EM.</Section>
            </Description>
            <PrimDef>
                <Name>EM_NC_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="2"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SC_INFO_CNF is used to send the requested cell infrastructure data from RR to EM.</Section>
                <Section>It is send by RR.</Section>
            </Description>
            <PrimDef>
                <Name>EM_NC_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="2"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>no_ncells</Name>
                </ItemLink>
                <Comment>Number of neighbour cells</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>arfcn_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>BCCH channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c1_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Path loss criterion C1</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c2_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Reselection criterion C2</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rxlev_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Received field strength</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bsic_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Base station ID code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cell_id_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Cell ID</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>lac_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Location area code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>frame_offset</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Frame offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>time_alignmt</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Time alignment</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cba_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Cell bar access</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cbq_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Cell bar qualifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cell_type_ind</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>cell type indicator</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rac</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>routing area code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>temp_offset</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>temporary offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cell_resel_offset</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Cell reselect offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rxlev_acc_min</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>RXLEV_ACCESS_MIN</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_LOC_PAG_INFO_REQ is used to request location and paging parameter of the plmn as specified in 8443.601.01.002 from RR.</Section>
                <Section>It is send by ACI_EM.</Section>
            </Description>
            <PrimDef>
                <Name>EM_LOC_PAG_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="3"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_LOC_PAG_INFO_CNF is used to send the requested cell infrastructure data from RR to EM.</Section>
                <Section>It is send by RR.</Section>
            </Description>
            <PrimDef>
                <Name>EM_LOC_PAG_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="3"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bs_pa_mfrms</Name>
                </ItemLink>
                <Comment>Paging repeat period</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>t3212</Name>
                </ItemLink>
                <Comment>Periodic location updating interval</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>mcc</Name>
                </ItemLink>
                <Control>[3]</Control>
                <Comment>Mobile Country Code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>mnc</Name>
                </ItemLink>
                <Control>[3]</Control>
                <Comment>Mobile Network Code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tmsi</Name>
                </ItemLink>
                <Comment>Temporary Mobile Subscriber Identity</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_PLMN_INFO_REQ is used to request PLMN information data from RR to EM.</Section>
                <Section>It is send by RR.</Section>
            </Description>
            <PrimDef>
                <Name>EM_PLMN_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="4"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_RR_PLMN_INFO_CNF is used to send the requested PLMN information data from RR to EM.</Section>
                <Section>It is send by RR.</Section>
            </Description>
            <PrimDef>
                <Name>EM_PLMN_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="4"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>no_creq_max</Name>
                </ItemLink>
                <Comment>Max. no of retries for channel requests</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>reest_flag</Name>
                </ItemLink>
                <Comment>Re-establishment flag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>txpwr_max</Name>
                </ItemLink>
                <Comment>MS TXPWR MAX CCCH</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rxlev_min</Name>
                </ItemLink>
                <Comment>Rxlev access min</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rel_cause</Name>
                </ItemLink>
                <Comment>Release cause</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_CIP_HOP_DTX_INFO_REQ is used to request cipher, hopping and dtx infrastructure data from RR to EM.</Section>
                <Section>It is send by RR.</Section>
            </Description>
            <PrimDef>
                <Name>EM_CIP_HOP_DTX_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="5"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_CIP_HOP_DTX_INFO_CNF is used to send the requested cell infrastructure data from RR to EM.</Section>
                <Section>It is send by RR.</Section>
            </Description>
            <PrimDef>
                <Name>EM_CIP_HOP_DTX_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="5"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ciph_stat</Name>
                </ItemLink>
                <Comment>Cipher status</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>hop</Name>
                </ItemLink>
                <Comment>Hopping configuration</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>ARFCN, valid if hop = 0</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>hsn</Name>
                </ItemLink>
                <Comment>HSN, valid if hop = 1</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>dtx_stat</Name>
                </ItemLink>
                <Comment>DTX status</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_start</Name>
                </ItemLink>
                <Comment>Starting time valid or not</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>hop_chn</Name>
                </ItemLink>
                <Comment>Hopping channels</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>hop_chn2</Name>
                </ItemLink>
                <Comment>Hopping channels</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_POWER_INFO_REQ is used to request classmark information data from RR to EM.</Section>
                <Section>It is send by RR.</Section>
            </Description>
            <PrimDef>
                <Name>EM_POWER_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="6"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_POWER_INFO_CNF is used to send the requested classmark information data from RR to EM.</Section>
                <Section>It is send by RR.</Section>
            </Description>
            <PrimDef>
                <Name>EM_POWER_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="6"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>classm2</Name>
                </ItemLink>
                <Comment>Classmark 2</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>classm3</Name>
                </ItemLink>
                <Comment>Classmark 3</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_IDENTITY_INFO_REQ is used to request mobile data identity parameters from MM to EM.</Section>
                <Section>It is send by EM.</Section>
            </Description>
            <PrimDef>
                <Name>EM_IDENTITY_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="7"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_IDENTITY_INFO_CNF is used to to send the request mobile data identity parameters from MM to EM.</Section>
                <Section>It is send by MM.</Section>
            </Description>
            <PrimDef>
                <Name>EM_IDENTITY_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="7"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>em_imeisv</Name>
                </ItemLink>
                <Comment>IMEISV</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>em_imsi</Name>
                </ItemLink>
                <Comment>IMSI</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tmsi</Name>
                </ItemLink>
                <Comment>tmsi</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SW_VERSION_INFO_REQ is used to request software version information for the involved entities.</Section>
                <Section>It is send by EM.</Section>
            </Description>
            <PrimDef>
                <Name>EM_SW_VERSION_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="8"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SW_VERSION_INFO_CNF is used to send the requested software version information for the involved entities.</Section>
                <Section>It is send by MM.</Section>
            </Description>
            <PrimDef>
                <Name>EM_SW_VERSION_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="8"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_mmi</Name>
                </ItemLink>
                <Comment>Version MMI (SMI/ACI/MFW)</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_sim</Name>
                </ItemLink>
                <Comment>Version SIM</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_cc</Name>
                </ItemLink>
                <Comment>Version CC</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_ss</Name>
                </ItemLink>
                <Comment>Version SS</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_sms</Name>
                </ItemLink>
                <Comment>Version SMS</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_mm</Name>
                </ItemLink>
                <Comment>Version MM</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_rr</Name>
                </ItemLink>
                <Comment>Version RR</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_dl</Name>
                </ItemLink>
                <Comment>Version DL</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_l1</Name>
                </ItemLink>
                <Comment>Version Layer 1 (ALR)</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_COUNTER_IDLE_IND is used to send the downlink failure counter values to Condat EM.</Section>
            </Description>
            <PrimDef>
                <Name>EM_COUNTER_IDLE_IND</Name>
                <PrimID Direction="DOWNLINK" Number="9"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>max_dlt</Name>
                </ItemLink>
                <Comment>Maximum Downlink Counter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>act_dlt</Name>
                </ItemLink>
                <Comment>Actual Downlink Counter</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial, copied from SAP MON</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_COUNTER_DEDI_IND is used to send the radiolink timeout counter values to Condat EM.</Section>
            </Description>
            <PrimDef>
                <Name>EM_COUNTER_DEDI_IND</Name>
                <PrimID Direction="DOWNLINK" Number="10"/>
                <PrimUsage>
                    <Sender>PL</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>max_rlt</Name>
                </ItemLink>
                <Comment>Maximum Radiolink Timeout Counter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>act_rlt</Name>
                </ItemLink>
                <Comment>Actual Radiolink Timeout Counter</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial, copied from SAP MON</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SS_EVENT_REQ is used to send the information bits for the supplementary services.</Section>
            </Description>
            <PrimDef>
                <Name>EM_L1_EVENT_REQ</Name>
                <PrimID Direction="UPLINK" Number="9"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bitmask_l1_h</Name>
                </ItemLink>
                <Comment>Information bits high</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bitmask_l1_l</Name>
                </ItemLink>
                <Comment>Information bits low</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SS_EVENT_REQ is used to send the information bits for the supplementary services.</Section>
            </Description>
            <PrimDef>
                <Name>EM_DL_EVENT_REQ</Name>
                <PrimID Direction="UPLINK" Number="10"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>DL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bitmask_dl</Name>
                </ItemLink>
                <Comment>Information bits</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SS_EVENT_REQ is used to send the information bits for the supplementary services.</Section>
            </Description>
            <PrimDef>
                <Name>EM_RR_EVENT_REQ</Name>
                <PrimID Direction="UPLINK" Number="11"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bitmask_rr_h</Name>
                </ItemLink>
                <Comment>Information bits high</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bitmask_rr_l</Name>
                </ItemLink>
                <Comment>Information bits low</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SS_EVENT_REQ is used to send the information bits for the supplementary services.</Section>
            </Description>
            <PrimDef>
                <Name>EM_MM_EVENT_REQ</Name>
                <PrimID Direction="UPLINK" Number="12"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>MM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bitmask_mm</Name>
                </ItemLink>
                <Comment>Information bits</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SS_EVENT_REQ is used to send the information bits for the supplementary services.</Section>
            </Description>
            <PrimDef>
                <Name>EM_CC_EVENT_REQ</Name>
                <PrimID Direction="UPLINK" Number="13"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bitmask_cc_h</Name>
                </ItemLink>
                <Comment>Information bits high</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bitmask_cc_l</Name>
                </ItemLink>
                <Comment>Information bits low</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SS_EVENT_REQ is used to send the information bits for the supplementary services.</Section>
            </Description>
            <PrimDef>
                <Name>EM_SS_EVENT_REQ</Name>
                <PrimID Direction="UPLINK" Number="14"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>SS</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bitmask_ss</Name>
                </ItemLink>
                <Comment>Information bits</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SS_EVENT_REQ is used to send the information bits for the supplementary services.</Section>
            </Description>
            <PrimDef>
                <Name>EM_SMS_EVENT_REQ</Name>
                <PrimID Direction="UPLINK" Number="15"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>SMS</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bitmask_sms_h</Name>
                </ItemLink>
                <Comment>Information bits high</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bitmask_sms_l</Name>
                </ItemLink>
                <Comment>Information bits low</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_SS_EVENT_REQ is used to send the information bits for the supplementary services.</Section>
            </Description>
            <PrimDef>
                <Name>EM_SIM_EVENT_REQ</Name>
                <PrimID Direction="UPLINK" Number="16"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>SIM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>bitmask_sim</Name>
                </ItemLink>
                <Comment>Information bits</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_DATA_IND is used to signal occurrence of the first requested event.</Section>
            </Description>
            <PrimDef>
                <Name>EM_DATA_IND</Name>
                <PrimID Direction="DOWNLINK" Number="11"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>entity</Name>
                </ItemLink>
                <Comment>Entity information</Comment>
            </PrimItem>
            <History>
                <Date Day="19" Month="9" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_FMM_SC_INFO_REQ is used to request the data RR-SC data for the microtec's fmM1251 program.</Section>
            </Description>
            <PrimDef>
                <Name>EM_FMM_SC_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="18"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="27" Month="10" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_FMM_SC_INFO_CNF is used to send the requested data for the microtec's fmM1251 program.</Section>
                <Section>First, it will only be send via AT-Commands. Later a Primitive is send directly to fmM1251, because it will be the only calling function.</Section>
            </Description>
            <PrimDef>
                <Name>EM_FMM_SC_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="18"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>Channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c1</Name>
                </ItemLink>
                <Comment>Path loss criterion</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c2</Name>
                </ItemLink>
                <Comment>Cell reselection criterion</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rac</Name>
                </ItemLink>
                <Comment>Routing area code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>hyst</Name>
                </ItemLink>
                <Comment>C2/C32 hysteresis value</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c32</Name>
                </ItemLink>
                <Comment>Cell reselection criterion c32</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>gprs_prio_class</Name>
                </ItemLink>
                <Comment>GPRS Priority Class</Comment>
            </PrimItem>
            <History>
                <Date Day="27" Month="10" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_FMM_GPRS_INFO_REQ is used to request the data GRR-SC data for the microtec's fmM1251 program.</Section>
            </Description>
            <PrimDef>
                <Name>EM_FMM_SC_GPRS_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="19"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>GRR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="27" Month="10" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_FMM_SC_GPRS_INFO_CNF is used to send the requested GPRS cell infrastructure data from GRR to EM.</Section>
                <Section>It is send by GRR.</Section>
            </Description>
            <PrimDef>
                <Name>EM_FMM_SC_GPRS_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="19"/>
                <PrimUsage>
                    <Sender>GRR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c31_hyst</Name>
                </ItemLink>
                <Comment>C31 Hysteresis Flag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ra_re_hyst</Name>
                </ItemLink>
                <Comment>RAC hysteresis</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>nco</Name>
                </ItemLink>
                <Comment>Network Controlled resel. Order</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_FMM_NC_INFO_REQ is used to request the data RR-SC data for the microtec's fmM1251 program.</Section>
            </Description>
            <PrimDef>
                <Name>EM_FMM_NC_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="20"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="27" Month="10" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_FMM_NC_INFO_CNF is used to send the requested data for the microtec's fmM1251 program.</Section>
                <Section>First, it will only be send via AT-Commands. Later a Primitive is send directly to fmM1251, because it will be the only calling function.</Section>
            </Description>
            <PrimDef>
                <Name>EM_FMM_NC_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="20"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>no_ncells</Name>
                </ItemLink>
                <Comment>Number of neighbour cells</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>arfcn_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>BCCH channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c2_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Reselection criterion C2</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rac_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>Routing Area Code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c31_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>C31 Measurement</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c32_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>C32 Measurement</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>gprs_prio_class_nc</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>GPRS Priority Class</Comment>
            </PrimItem>
            <History>
                <Date Day="27" Month="10" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_FMM_RLC_TRANS_INFO_REQ is used by microtec's fmM1251 to get data about the status of the RLC - Blocks.</Section>
            </Description>
            <PrimDef>
                <Name>EM_FMM_RLC_TRANS_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="21"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>GRLC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="12" Month="12" Year="1954"/>
                <Author>doc2xml</Author>
                <Comment>no history in source document</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_FMM_RLC_TRANS_INFO_CNF is used for microtec's fmM1251. The Primitive sends data about RLC - Blocks.</Section>
            </Description>
            <PrimDef>
                <Name>EM_FMM_RLC_TRANS_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="21"/>
                <PrimUsage>
                    <Sender>GRLC</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rlc_num_retrans</Name>
                </ItemLink>
                <Comment>RLC Blocks retransmitted</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rlc_num_trans</Name>
                </ItemLink>
                <Comment>RLC Blocks successfull transmitted</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rlc_pdu_cnt</Name>
                </ItemLink>
                <Comment>PDU Counter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rlc_start_fn</Name>
                </ItemLink>
                <Comment>Start Frame Number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rlc_end_fn</Name>
                </ItemLink>
                <Comment>End Frame Number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rlc_tbc</Name>
                </ItemLink>
                <Comment>Number of rlc data blocks during the tbf, which is requested to send</Comment>
            </PrimItem>
            <History>
                <Date Day="3" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_FMM_RESELECTION_START_IND is used to send data to the microtec's fmM1251 program.</Section>
                <Section>It will be used to indicate a starting  change of the serving cell.</Section>
            </Description>
            <PrimDef>
                <Name>EM_FMM_RESELECTION_START_IND</Name>
                <PrimID Direction="DOWNLINK" Number="12"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>Channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rac</Name>
                </ItemLink>
                <Comment>Routing area code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>res_type</Name>
                </ItemLink>
                <Comment>Reselection Type</Comment>
            </PrimItem>
            <History>
                <Date Day="3" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_FMM_RESELECTION_END_IND is used to send data to microtec's fmM1251 program.</Section>
                <Section>It will be used to indicate a successful change of the serving cell.</Section>
            </Description>
            <PrimDef>
                <Name>EM_FMM_RESELECTION_END_IND</Name>
                <PrimID Direction="DOWNLINK" Number="13"/>
                <PrimUsage>
                    <Sender>RR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Comment>Channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rac</Name>
                </ItemLink>
                <Comment>Routing area code</Comment>
            </PrimItem>
            <History>
                <Date Day="3" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_FMM_TBF_INFO_REQ is used to request data for microtec's fmM1251 program.</Section>
                <Section>It will be used get certain TBF data parameter.</Section>
            </Description>
            <PrimDef>
                <Name>EM_FMM_TBF_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="22"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>GRR</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Data bitmask</Comment>
            </PrimItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_FMM_TBF_CNF is used to send data to microtec's fmM1251 program.</Section>
                <Section>It will be used to provide actual TBF data.</Section>
            </Description>
            <PrimDef>
                <Name>EM_FMM_TBF_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="22"/>
                <PrimUsage>
                    <Sender>GRR</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tbf_trans_type</Name>
                </ItemLink>
                <Comment>TBF transfer type</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tbf_num_ults</Name>
                </ItemLink>
                <Comment>Number of UL-Timeslots</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tbf_num_rlc</Name>
                </ItemLink>
                <Comment>Uplink RLC-Blocks</Comment>
            </PrimItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_PCO_TRACE_REQ is used to request data from the EM and trace this data at the PCO. It is a one-time-reaction from the protocol stack.</Section>
            </Description>
            <PrimDef>
                <Name>EM_PCO_TRACE_REQ</Name>
                <PrimID Direction="UPLINK" Number="17"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>RR, GRR, GMM, GRLC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>pco_bitmap</Name>
                </ItemLink>
                <Comment>bitmap for requested EM information</Comment>
            </PrimItem>
            <History>
                <Date Day="10" Month="12" Year="2003"/>
                <Author>MA2</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_GRLC_INFO_REQ is used to request the RLC/MAC data for the Engineering Window Mode Tool (EMW)</Section>
            </Description>
            <PrimDef>
                <Name>EM_GRLC_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="24"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>GRLC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Primitive Item</Comment>
            </PrimItem>
            <History>
                <Date Day="19" Month="01" Year="2004"/>
                <Author>ZL</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_GRLC_INFO_CNF is used to send the RLC/MAC data for the Engineering Window Mode Tool (EMW)</Section>
            </Description>
            <PrimDef>
                <Name>EM_GRLC_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="24"/>
                <PrimUsage>
                    <Sender>GRLC</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>grlc_state</Name>
                </ItemLink>
                <Comment>grlc state</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tbf_mod</Name>
                </ItemLink>
                <Comment>tbf state</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ul_tbf_par</Name>
                </ItemLink>
                <Comment>ul tbf parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>dl_tbf_par</Name>
                </ItemLink>
                <Comment>dl tbf parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="19" Month="01" Year="2004"/>
                <Author>zl</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_GMM_INFO_REQ is used to request the GMM data for the Engineering Window Mode Tool (EMW)</Section>
            </Description>
            <PrimDef>
                <Name>EM_GMM_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="23"/>
                <PrimUsage>
                    <Sender>EM</Sender>
                    <Receiver>GMM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Primitive Item</Comment>
            </PrimItem>
            <History>
                <Date Day="20" Month="01" Year="2004"/>
                <Author>zl/ans</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The EM_GMM_INFO_CNF is used to send the GMM data for the Engineering Window Mode Tool (EMW)</Section>
            </Description>
            <PrimDef>
                <Name>EM_GMM_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="23"/>
                <PrimUsage>
                    <Sender>GMM</Sender>
                    <Receiver>EM</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ready_state</Name>
                </ItemLink>
                <Comment>ready-standby state</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ciphering_algorithm</Name>
                </ItemLink>
                <Comment>Primitive Item</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tlli</Name>
                </ItemLink>
                <Comment>Primitive Item</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ptmsi</Name>
                </ItemLink>
                <Comment>Primitive Item</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ptmsi_sig</Name>
                </ItemLink>
                <Comment>Primitive Item</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ready_timer</Name>
                </ItemLink>
                <Comment>Primitive Item</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>t3312</Name>
                </ItemLink>
                <Comment>Primitive Item</Comment>
            </PrimItem>
            <History>
                <Date Day="20" Month="01" Year="2004"/>
                <Author>zl/ans</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>EM_AMR_INFO_REQ is used to request AMR configuration data for the engineering window mopde tool</Section>
            </Description>
            <PrimDef>
                <Name>EM_AMR_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="25"/>
                <PrimUsage>
                    <Sender/>
                    <Receiver/>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>data</Name>
                </ItemLink>
                <Comment>Primitive Item</Comment>
            </PrimItem>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author>Gopinath</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>EM_AMR_INFO_CNF is used to send AMR configuration data to Engineering window mode tool</Section>
            </Description>
            <PrimDef>
                <Name>EM_AMR_INFO_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="25"/>
                <PrimUsage>
                    <Sender/>
                    <Receiver/>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>amr_vocoder</Name>
                </ItemLink>
                <Comment>AMR vocoder type</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>amr_icmi</Name>
                </ItemLink>
                <Comment>Initial codec mode indicator</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>amr_icm</Name>
                </ItemLink>
                <Comment>Index into ACS</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>amr_acs</Name>
                </ItemLink>
                <Comment>Active codec set</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>amr_first_codec</Name>
                </ItemLink>
                <Comment>Highest bit rate codec mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>amr_nr_modes</Name>
                </ItemLink>
                <Comment>Number of modes in ACS</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>amr_cod_prop</Name>
                </ItemLink>
                <Control>[3]</Control>
                <Comment>codec mode properties</Comment>
            </PrimItem>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author>Gopinath</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
    </PrimitivesSection>
    <PrimStructElementsSection>
        <Description>
            <Section>Parameters shall be part of the primitives described below and if applied the parameters shall contain the values specified here. These values are selected to correspond element values used in the air interface protocol.</Section>
        </Description>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the network control (GPRS).</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>net_ctrl</Name>
                <Comment>Network control</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>spgc_ccch_sup</Name>
                </ItemLink>
                <Comment>SPLIT_PG_CYCLE_SUPPORT: whether it is supported or not - should be BOOL, but BOOL is not valid in SAP</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>priority_access_thr</Name>
                </ItemLink>
                <Comment>packet access to the network according to priority level</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the international mobile equipment identity.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>em_imeisv</Name>
                <Comment>IMEISV</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>em_imsi</Name>
                <Comment>IMSI</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ident_type</Name>
                </ItemLink>
                <Comment>Type of identity</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>odd_even</Name>
                </ItemLink>
                <Comment>Odd/ Even indication</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_ident_dig</Name>
                </ItemLink>
                <Comment>valid-flag</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>c_ident_dig</Name>
                </ItemLink>
                <Comment>counter</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ident_dig</Name>
                </ItemLink>
                <Control>[16]</Control>
                <Comment>Identity digit</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the frequency hopping channels.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>hop_chn</Name>
                <Comment>frequency hopping channel list after time</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <Comment>Mobile allocation index offset</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>nr_arfcns</Name>
                </ItemLink>
                <Comment>Number of hopping channels</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ma</Name>
                </ItemLink>
                <Control>[65]</Control>
                <Comment>MA list after time</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>classm2</Name>
                <Comment>Classmark 2</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rev_lev</Name>
                </ItemLink>
                <Comment>rev_lev</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>es_ind</Name>
                </ItemLink>
                <Comment>es_ind</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>a5_1</Name>
                </ItemLink>
                <Comment>a5_1</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>rf_pow_cap</Name>
                </ItemLink>
                <Comment>rf_pow_cap</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ps_cap</Name>
                </ItemLink>
                <Comment>ps_cap</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ss_screen</Name>
                </ItemLink>
                <Comment>ss_screen</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>sm_cap</Name>
                </ItemLink>
                <Comment>sm_cap</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>freq_cap</Name>
                </ItemLink>
                <Comment>freq_cap</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>class_3</Name>
                </ItemLink>
                <Comment>class_3</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cmsp</Name>
                </ItemLink>
                <Comment>cmsp</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>a5_3</Name>
                </ItemLink>
                <Comment>a5_3</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>a5_2</Name>
                </ItemLink>
                <Comment>a5_2</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>classm3</Name>
                <Comment>Classmark 3</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>mb_sub</Name>
                </ItemLink>
                <Comment>mb_sub</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>a5_7</Name>
                </ItemLink>
                <Comment>a5_7</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>a5_6</Name>
                </ItemLink>
                <Comment>a5_6</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>a5_5</Name>
                </ItemLink>
                <Comment>a5_5</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>a5_4</Name>
                </ItemLink>
                <Comment>a5_4</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_radio_cap_2</Name>
                </ItemLink>
                <Comment>v_radio_cap_2</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>radio_cap_2</Name>
                </ItemLink>
                <Comment>radio_cap_2</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_radio_cap_1</Name>
                </ItemLink>
                <Comment>v_radio_cap_1</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>radio_cap_1</Name>
                </ItemLink>
                <Comment>radio_cap_1</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_r_support</Name>
                </ItemLink>
                <Comment>v_r_support</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>r_support</Name>
                </ItemLink>
                <Comment>r_support</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_m_s_class</Name>
                </ItemLink>
                <Comment>v_m_s_class</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>m_s_class</Name>
                </ItemLink>
                <Comment>m_s_class</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ucs2_treat</Name>
                </ItemLink>
                <Comment>ucs2_treat</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ext_meas_cap</Name>
                </ItemLink>
                <Comment>ext_meas_cap</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>v_meas_cap</Name>
                </ItemLink>
                <Comment>v_meas_cap</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>meas_cap</Name>
                </ItemLink>
                <Comment>T_meas_cap</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the classmark3 meas_cap.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>meas_cap</Name>
                <Comment>meas_cap</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>sw_time</Name>
                </ItemLink>
                <Comment>sw_time</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>sws_time</Name>
                </ItemLink>
                <Comment>sws_time</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>dummy1</Name>
                </ItemLink>
                <Comment>dummy1</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>dummy2</Name>
                </ItemLink>
                <Comment>dummy2</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>dummy1 &amp; dummy2 added.</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>It defines some features of rlc/mac for ul tbf</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>ul_tbf_par</Name>
                <Comment>ul tbf parameter</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tfi</Name>
                </ItemLink>
                <Comment>tfi</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>mac_mod</Name>
                </ItemLink>
                <Comment>allocation type</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ul_nb_block</Name>
                </ItemLink>
                <Comment>Number of blocks to be sent for uplink</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cv</Name>
                </ItemLink>
                <Comment>countdown value</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>cs</Name>
                </ItemLink>
                <Comment>coding scheme</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="19" Month="01" Year="2004"/>
                <Author>zl</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section/>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>dl_tbf_par</Name>
                <Comment>dl tbf parameters</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>tfi</Name>
                </ItemLink>
                <Comment>temporary flow identifier</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>mac_mod</Name>
                </ItemLink>
                <Comment>allocation type</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="19" Month="01" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section/>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>t3312</Name>
                <Comment>Structured Element</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>t3312_deactivated</Name>
                </ItemLink>
                <Comment>Primitive structure element item</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>t3312_val</Name>
                </ItemLink>
                <Comment>Primitive structure element item</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>Parameters for multirate speech field</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>amr_cod_prop</Name>
                <Comment>Parameters for multirate speech field</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>amr_codec_thr</Name>
                </ItemLink>
                <Comment>Primitive structure element item</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>amr_codec_hyst</Name>
                </ItemLink>
                <Comment>Primitive structure element item</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="03" Month="08" Year="2004"/>
                <Author>Gopinath</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>Frequency channel hopping list before time</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>hop_chn2</Name>
                <Comment>Frequency channel hopping list before time</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <Comment>Mobile allocation index offset</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>nr_arfcns</Name>
                </ItemLink>
                <Comment>Number of hopping channels</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">em</DocName>
                    <Name>ma</Name>
                </ItemLink>
                <Control>[65]</Control>
                <Comment>Hopping channel list</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="04" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
    </PrimStructElementsSection>
    <PrimBasicElementsSection>
        <Description>
            <Section>Parameters shall be part of the primitives described below and if applied the parameters shall contain the values specified here. These values are selected to correspond element values used in the air interface protocol.</Section>
        </Description>
        <PrimBasicElem>
            <Description>
                <Section>The parameter identifies a channel number.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>arfcn</Name>
                <Type>U16</Type>
                <Comment>channel number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_arfcn</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter identifies a channel number.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>arfcn_nc</Name>
                <Type>U16</Type>
                <Comment>channel number</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the timeslot number.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tn</Name>
                <Type>U8</Type>
                <Comment>timeslot number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_tn</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the transmit power level used by the physical layer according to GSM 5.08.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>txlev</Name>
                <Type>U8</Type>
                <Comment>Power Level</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_txlev</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="6" Month="6" Year="2001"/>
                <Author>OT</Author>
                <Comment>short name changed</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the transmit power level used by the physical layer according to GSM 5.08.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>txpwr_max</Name>
                <Type>U8</Type>
                <Comment>Max power level in a cell</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_txlev</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="6" Month="6" Year="2001"/>
                <Author>OT</Author>
                <Comment>short name changed</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the received field strength value.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev</Name>
                <Type>U8</Type>
                <Comment>received field strength</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_rxlev</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>rxlev_nc, rxlev_full, rxlev_sub added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the received field strength value.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev_nc</Name>
                <Type>U8</Type>
                <Comment>received field strength neighbour cell</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>rxlev_nc, rxlev_full, rxlev_sub added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the received field strength value.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev_f</Name>
                <Type>U8</Type>
                <Comment>received field strength</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>rxlev_nc, rxlev_full, rxlev_sub added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the received field strength value.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev_s</Name>
                <Type>U8</Type>
                <Comment>received field strength</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>rxlev_nc, rxlev_full, rxlev_sub added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the received field strength value.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev_min</Name>
                <Type>U8</Type>
                <Comment>min. rxlev to access the cell</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>rxlev_nc, rxlev_full, rxlev_sub added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the received quality.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxqual_f</Name>
                <Type>U8</Type>
                <Comment>received quality</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_rxqual_f</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="2" Year="2000"/>
                <Author>LE</Author>
                <Comment>unused rx_qual removed</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the received quality.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxqual_s</Name>
                <Type>U8</Type>
                <Comment>received quality</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="2" Year="2000"/>
                <Author>LE</Author>
                <Comment>unused rx_qual removed</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the base station identification code.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bsic</Name>
                <Type>U8</Type>
                <Comment>base station ID code</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_bsic</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the base station identification code.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bsic_nc</Name>
                <Type>U8</Type>
                <Comment>base station ID code neighbour cell</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the timing advance receveived with dedicated mode SI's in quarter bit periods.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tav</Name>
                <Type>U8</Type>
                <Comment>timing advance</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="6" Month="6" Year="2001"/>
                <Author>OT</Author>
                <Comment>unused tav_nc removed</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the frame offset.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>frame_offset</Name>
                <Type>U32</Type>
                <Comment>frame offset</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the time alignment.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>time_alignmt</Name>
                <Type>U32</Type>
                <Comment>time alignment</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines the Cell Identity of the serving cell</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>cell_id</Name>
                <Type>U16</Type>
                <Comment>cell identity SC</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="01" Month="03" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the cell identity.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>cell_id_nc</Name>
                <Type>U16</Type>
                <Comment>cell identity neighbour cell</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the location area code.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>lac</Name>
                <Type>U16</Type>
                <Comment>location area code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the location area code.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>lac_nc</Name>
                <Type>U16</Type>
                <Comment>location area code neighbour cells</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the path loss criterion C1 and the cell reselection criterion C2/C31/C32.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c1</Name>
                <Type>S16</Type>
                <Comment>path loss criterion C1</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>GPRS parameter added (C31 &amp; C32)</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the path loss criterion C1 and the cell reselection criterion C2/C31/C32.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c2</Name>
                <Type>S16</Type>
                <Comment>reselection criterion C2</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>GPRS parameter added (C31 &amp; C32)</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the path loss criterion C1 and the cell reselection criterion C2/C31/C32.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c1_nc</Name>
                <Type>S16</Type>
                <Comment>path loss criterion C1 neighbour cells</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>GPRS parameter added (C31 &amp; C32)</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the path loss criterion C1 and the cell reselection criterion C2/C31/C32.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c2_nc</Name>
                <Type>S16</Type>
                <Comment>reselection criterion C2 neighbour cells</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>GPRS parameter added (C31 &amp; C32)</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the path loss criterion C1 and the cell reselection criterion C2/C31/C32.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c31</Name>
                <Type>S16</Type>
                <Comment>reselection criterion C31 (GPRS)</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>GPRS parameter added (C31 &amp; C32)</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the path loss criterion C1 and the cell reselection criterion C2/C31/C32.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c32</Name>
                <Type>S16</Type>
                <Comment>reselection criterion C32 (GPRS)</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>GPRS parameter added (C31 &amp; C32)</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the path loss criterion C1 and the cell reselection criterion C2/C31/C32.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c31_nc</Name>
                <Type>S16</Type>
                <Comment>reselection criterion C31 (GPRS) neighbour cells</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>GPRS parameter added (C31 &amp; C32)</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the path loss criterion C1 and the cell reselection criterion C2/C31/C32.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c32_nc</Name>
                <Type>S16</Type>
                <Comment>reselection criterion C32 (GPRS) neighbour cells</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>GPRS parameter added (C31 &amp; C32)</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the actual downlink timeout value.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dsc</Name>
                <Type>U8</Type>
                <Comment>actual downlink signalling counter</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="6" Month="6" Year="2001"/>
                <Author>OT</Author>
                <Comment>short name changed</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the actual or maximum of radiolink timeout value.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rlt</Name>
                <Type>U8</Type>
                <Comment>actual radiolink timeout counter</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the cell bar access.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>cba</Name>
                <Type>U8</Type>
                <Comment>cell bar access</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the cell bar access.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>cba_nc</Name>
                <Type>U8</Type>
                <Comment>cell bar access neighbour cells</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the cell bar qualifier.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>cbq</Name>
                <Type>U8</Type>
                <Comment>cell bar  qualifier</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the cell bar qualifier.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>cbq_nc</Name>
                <Type>U8</Type>
                <Comment>cell bar qualifier neighbour cells</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the network mode of operation  (GPRS).</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>nmo</Name>
                <Type>U8</Type>
                <Comment>network mode of operation</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the network control (GPRS).</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>spgc_ccch_sup</Name>
                <Type>U8</Type>
                <Comment>SPLIT_PG_CYCLE_SUPPORT: whether it is supported or not - should be BOOL, but BOOL is not valid in SAP</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the network control (GPRS).</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>priority_access_thr</Name>
                <Type>U8</Type>
                <Comment>packet access to the network according to priority level</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the routing area code (GPRS).</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rac</Name>
                <Type>U8</Type>
                <Comment>routing area code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the routing area code (GPRS).</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rac_nc</Name>
                <Type>U8</Type>
                <Comment>routing area code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of neighbour cells.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>no_ncells</Name>
                <Type>U8</Type>
                <Comment>no of neighbour cells</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="6" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the timer for the periodic location update.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>t3212</Name>
                <Type>U8</Type>
                <Comment>Timer T3212</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_t3212</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the international mobile equipment identity.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ident_type</Name>
                <Type>U8</Type>
                <Comment>Type of identity</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the international mobile equipment identity.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>odd_even</Name>
                <Type>U8</Type>
                <Comment>Odd/ Even indication</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the international mobile equipment identity.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_ident_dig</Name>
                <Type>U8</Type>
                <Comment>valid-flag</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the international mobile equipment identity.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c_ident_dig</Name>
                <Type>U8</Type>
                <Comment>counter</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the international mobile equipment identity.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ident_dig</Name>
                <Type>U8</Type>
                <Comment>Identity digit</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the temporary international mobile subscriber identity.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tmsi</Name>
                <Type>U32</Type>
                <Comment>binary representation TMSI</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the MCC. MCC is defined as BCD digits. The delimiter is 0xF.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>mcc</Name>
                <Type>U8</Type>
                <Comment>mobile country code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the MNC. MNC is defined as BCD digits. The delimiter is 0xF.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>mnc</Name>
                <Type>U8</Type>
                <Comment>mobile network code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Max. no of retries for channel requests.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>no_creq_max</Name>
                <Type>U8</Type>
                <Comment>mobile country code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the ciphering information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ciph_stat</Name>
                <Type>U8</Type>
                <Comment>Cipher status</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the frequency hopping channels.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ma</Name>
                <Type>U16</Type>
                <Comment>MA list after time</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the frequency hopping channels.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ma2</Name>
                <Type>U16</Type>
                <Comment>MA list before  time</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the frequency hopping channels.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_start</Name>
                <Type>U8</Type>
                <Comment>starting time valid</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_v_start</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the frequency hopping information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>hsn</Name>
                <Type>U8</Type>
                <Comment>Hopping sequence number</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the cipher, hopping and dtx information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dtx_stat</Name>
                <Type>U8</Type>
                <Comment>DTX status</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_dtx_stat</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rev_lev</Name>
                <Type>U8</Type>
                <Comment>rev_lev</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>es_ind</Name>
                <Type>U8</Type>
                <Comment>es_ind</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>a5_1</Name>
                <Type>U8</Type>
                <Comment>a5_1</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rf_pow_cap</Name>
                <Type>U8</Type>
                <Comment>rf_pow_cap</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ps_cap</Name>
                <Type>U8</Type>
                <Comment>ps_cap</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ss_screen</Name>
                <Type>U8</Type>
                <Comment>ss_screen</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>sm_cap</Name>
                <Type>U8</Type>
                <Comment>sm_cap</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>freq_cap</Name>
                <Type>U8</Type>
                <Comment>freq_cap</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>class_3</Name>
                <Type>U8</Type>
                <Comment>class_3</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>cmsp</Name>
                <Type>U8</Type>
                <Comment>cmsp</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>a5_3</Name>
                <Type>U8</Type>
                <Comment>a5_3</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>a5_2</Name>
                <Type>U8</Type>
                <Comment>a5_2</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>mb_sub</Name>
                <Type>U8</Type>
                <Comment>mb_sub</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>a5_7</Name>
                <Type>U8</Type>
                <Comment>a5_7</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>a5_6</Name>
                <Type>U8</Type>
                <Comment>a5_6</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>a5_5</Name>
                <Type>U8</Type>
                <Comment>a5_5</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>a5_4</Name>
                <Type>U8</Type>
                <Comment>a5_4</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_radio_cap_2</Name>
                <Type>U8</Type>
                <Comment>v_radio_cap_2</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>radio_cap_2</Name>
                <Type>U8</Type>
                <Comment>radio_cap_2</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_radio_cap_1</Name>
                <Type>U8</Type>
                <Comment>v_radio_cap_1</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>radio_cap_1</Name>
                <Type>U8</Type>
                <Comment>radio_cap_1</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_r_support</Name>
                <Type>U8</Type>
                <Comment>v_r_support</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>r_support</Name>
                <Type>U8</Type>
                <Comment>r_support</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_m_s_class</Name>
                <Type>U8</Type>
                <Comment>v_m_s_class</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>m_s_class</Name>
                <Type>U8</Type>
                <Comment>m_s_class</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ucs2_treat</Name>
                <Type>U8</Type>
                <Comment>ucs2_treat</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ext_meas_cap</Name>
                <Type>U8</Type>
                <Comment>ext_meas_cap</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark2 information.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_meas_cap</Name>
                <Type>U8</Type>
                <Comment>v_meas_cap</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>v_ucs2_treat &amp; v_ext_meas_cap removed.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark3 meas_cap.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>sw_time</Name>
                <Type>U8</Type>
                <Comment>sw_time</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>dummy1 &amp; dummy2 added.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark3 meas_cap.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>sws_time</Name>
                <Type>U8</Type>
                <Comment>sws_time</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>dummy1 &amp; dummy2 added.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark3 meas_cap.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dummy1</Name>
                <Type>U8</Type>
                <Comment>dummy1</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>dummy1 &amp; dummy2 added.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the classmark3 meas_cap.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dummy2</Name>
                <Type>U8</Type>
                <Comment>dummy2</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>dummy1 &amp; dummy2 added.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the software version for the corresponding entities.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_mmi</Name>
                <Type>U16</Type>
                <Comment>not implemented yet</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the software version for the corresponding entities.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_sim</Name>
                <Type>U16</Type>
                <Comment>not implemented yet</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the software version for the corresponding entities.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_cc</Name>
                <Type>U16</Type>
                <Comment>not implemented yet</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the software version for the corresponding entities.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_ss</Name>
                <Type>U16</Type>
                <Comment>not implemented yet</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the software version for the corresponding entities.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_sms</Name>
                <Type>U16</Type>
                <Comment>not implemented yet</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the software version for the corresponding entities.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_mm</Name>
                <Type>U16</Type>
                <Comment>not implemented yet</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the software version for the corresponding entities.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_rr</Name>
                <Type>U16</Type>
                <Comment>not implemented yet</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the software version for the corresponding entities.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_dl</Name>
                <Type>U16</Type>
                <Comment>not implemented yet</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the software version for the corresponding entities.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>v_l1</Name>
                <Type>U16</Type>
                <Comment>not implemented yet</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the release cause.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rel_cause</Name>
                <Type>U16</Type>
                <Comment>release cause</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of multiframes for transmission of the same paging group.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bs_pa_mfrms</Name>
                <Type>U8</Type>
                <Comment>Multiframe Period</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_bs_pa_mfrms</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines a bitmask for the requested data. It is only used to prevent unnecessary usage of primitives.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>data</Name>
                <Type>U16</Type>
                <Comment>requested data</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the reestablishment flag.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>reest_flag</Name>
                <Type>U8</Type>
                <Comment>Re-establishment flag</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the actual or maximum of downlink timeout value.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>max_dlt</Name>
                <Type>U8</Type>
                <Comment>maximum downlink timeout counter</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial, copied from SAP MON</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the actual or maximum of downlink timeout value.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>act_dlt</Name>
                <Type>U8</Type>
                <Comment>actual downlink timeout counter</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial, copied from SAP MON</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the actual or maximum of radiolink timeout value.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>max_rlt</Name>
                <Type>U8</Type>
                <Comment>maximum radiolink timeout counter</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial, copied from SAP MON</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the actual or maximum of radiolink timeout value.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>act_rlt</Name>
                <Type>U8</Type>
                <Comment>actual radiolink timeout counter</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial, copied from SAP MON</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The actual bits are set according the requested event information for ALR.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmask_l1_h</Name>
                <Type>U16</Type>
                <Comment>bitmask for L1 higher bits</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The actual bits are set according the requested event information for ALR.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmask_l1_l</Name>
                <Type>U32</Type>
                <Comment>bitmask for L1 lower bits</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The actual bits are set according the requested event information for Data Link Layer.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmask_dl</Name>
                <Type>U16</Type>
                <Comment>bitmask for DL</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The actual bits are set according the requested event information for Radio Resource Management.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmask_rr_h</Name>
                <Type>U16</Type>
                <Comment>bitmask for RR higher bits</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The actual bits are set according the requested event information for Radio Resource Management.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmask_rr_l</Name>
                <Type>U32</Type>
                <Comment>bitmask for RR lower bits</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The actual bits are set according the requested event information for Mobility Management.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmask_mm</Name>
                <Type>U32</Type>
                <Comment>bitmask for MM</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The actual bits are set according the requested event information for Call Control.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmask_cc_h</Name>
                <Type>U32</Type>
                <Comment>bitmask for CC higher bits</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The actual bits are set according the requested event information for Call Control.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmask_cc_l</Name>
                <Type>U32</Type>
                <Comment>bitmask for CC lower bits</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The actual bits are set according the requested event information for ALR.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmask_ss</Name>
                <Type>U16</Type>
                <Comment>bitmask for SS</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The actual bits are set according the requested event information for Short Message Service.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmask_sms_h</Name>
                <Type>U32</Type>
                <Comment>bitmask for SMS higher bits</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The actual bits are set according the requested event information for Short Message Service.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmask_sms_l</Name>
                <Type>U32</Type>
                <Comment>bitmask for SMS lower bits</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The actual bits are set according the requested event information for SIM</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bitmask_sim</Name>
                <Type>U32</Type>
                <Comment>bitmask for SIM</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Defines the entity the data indication is coming from.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>entity</Name>
                <Type>U8</Type>
                <Comment>Entity name</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_entity</Name>
            </ValuesLink>
            <History>
                <Date Day="27" Month="8" Year="2001"/>
                <Author>OT</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>According to the BITMAP EM data is shown as PCO-Trace or not.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>pco_bitmap</Name>
                <Type>U32</Type>
                <Comment>EM-Data output to PCO according to bitmap</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_pco_bitmap</Name>
            </ValuesLink>
            <History>
                <Date Day="09" Month="03" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The usage of this information is defined in TS GSM 05.08.</Section>
                <Section>Reference : [GSM_04.08] section (Cell Selection Parameters)</Section>
                <Section>Used for Microtec.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>hyst</Name>
                <Type>U8</Type>
                <Comment>C2 / C32 Hysteresis</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_hyst</Name>
            </ValuesLink>
            <History>
                <Date Day="21" Month="10" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The GPRS_PRIORITY_CLASS field contains the binary representation of the HCS priority for the cell.</Section>
                <Section>Used for Microtec.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>gprs_prio_class</Name>
                <Type>U8</Type>
                <Comment>GPRS_PRIORITY_CLASS</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_gprs_prio_class</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="15" Month="4" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add c-macro value</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The GPRS_PRIORITY_CLASS field contains the binary representation of the HCS priority for the cell.</Section>
                <Section>Used for Microtec.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>gprs_prio_class_nc</Name>
                <Type>U8</Type>
                <Comment>GPRS_PRIORITY_CLASS</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_gprs_prio_class</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="15" Month="4" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add c-macro value</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The C31_HYST field indicates if set to 1 that the GPRS_RESELECT_HYSTERESIS shall be applied to the C31 criterion.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c31_hyst</Name>
                <Type>U8</Type>
                <Comment>C31_HYST</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="10" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The RA_RESELECT_HYSTERESIS field indicates in both STANDBY and READY state the additional hysteresis which applies when selecting a cell in a new Routing Area. If this field is not present, the default value is GPRS_CELL_RESELECT_HYSTERESIS. The value is to interpret as value*2 dB .</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ra_re_hyst</Name>
                <Type>U8</Type>
                <Comment>RAC_HYSTERESIS</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="27" Month="10" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The RESELECTION_TYPE field indicates the reason in a case of cell reselection. We will see, if it is possible to get all the requested cause.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>res_type</Name>
                <Type>U8</Type>
                <Comment>Reselection Type</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="3" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The TBF transfer type indicates weather the connection is UL, DL or bidirectional.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tbf_trans_type</Name>
                <Type>U8</Type>
                <Comment>TBF unique ID</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_tbf_trans_type</Name>
            </ValuesLink>
            <History>
                <Date Day="3" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field shows the number of used timeslots.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tbf_num_ults</Name>
                <Type>U8</Type>
                <Comment>number of assigned Timeslots</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="3" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field shows the number of granted uplink RLC blocks.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tbf_num_rlc</Name>
                <Type>U16</Type>
                <Comment>number of granted uplink RLC blocks</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="3" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field shows Information about the Network Controlled reselection Order.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>nco</Name>
                <Type>U8</Type>
                <Comment>Network Controlled reselection Order</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_nco</Name>
            </ValuesLink>
            <History>
                <Date Day="3" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field shows the number of RLC Block, which have been retransmitted.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rlc_num_retrans</Name>
                <Type>U8</Type>
                <Comment>Info about the number of retransmitted RLCs</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field shows the number of RLC blocks, which have been transmitted without the retransmitted.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rlc_num_trans</Name>
                <Type>U16</Type>
                <Comment>Info about the number of transmitted RLCs</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field shows the number of the current PDU to transmit.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rlc_pdu_cnt</Name>
                <Type>U8</Type>
                <Comment>Info about the number of transmitted RLCs</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field shows the Frame number of the first frame.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rlc_start_fn</Name>
                <Type>U32</Type>
                <Comment>Info about the number of transmitted RLCs</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This field shows the Frame number of the last frame.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rlc_end_fn</Name>
                <Type>U32</Type>
                <Comment>Info about the number of transmitted RLCs</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>AM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>ul_nb_block</Name>
                <Type>U16</Type>
                <Comment>Number of blocks to be sent for uplink</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="19" Month="01" Year="2004"/>
                <Author>zl</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>grlc_state</Name>
                <Type>U8</Type>
                <Comment>grlc state</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_grlc_state</Name>
            </ValuesLink>
            <History>
                <Date Day="19" Month="01" Year="2004"/>
                <Author>zl</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>countdown value in uplink tbf</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>cv</Name>
                <Type>U8</Type>
                <Comment>countdown value</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="19" Month="01" Year="2004"/>
                <Author>zl</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>cs</Name>
                <Type>U8</Type>
                <Comment>Basic Element</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_cs</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="01" Year="2004"/>
                <Author>zl</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>ready-standby state</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ready_state</Name>
                <Type>U8</Type>
                <Comment>ready-standby state</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="20" Month="01" Year="2004"/>
                <Author>zl/ans</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>tlli</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tlli</Name>
                <Type>U32</Type>
                <Comment>tlli</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="20" Month="01" Year="2004"/>
                <Author>zl/ans</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>ptmsi</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ptmsi</Name>
                <Type>U32</Type>
                <Comment>ptmsi</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="20" Month="01" Year="2004"/>
                <Author>zl/ans</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>ptmsi signature </Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ptmsi_sig</Name>
                <Type>U32</Type>
                <Comment>ptmsi signature</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="20" Month="01" Year="2004"/>
                <Author>zl/ans</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>ready timer T3314</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ready_timer</Name>
                <Type>U32</Type>
                <Comment>ready timer T3314</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="20" Month="01" Year="2004"/>
                <Author>zl/ans</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>ciphering algorithm</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ciphering_algorithm</Name>
                <Type>U8</Type>
                <Comment>ciphering algorithm</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="20" Month="01" Year="2004"/>
                <Author>zl/ans</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>tbf_mod</Name>
                <Type>U8</Type>
                <Comment>Basic Element</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="22" Month="01" Year="2004"/>
                <Author>zl</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>mac_mod</Name>
                <Type>U8</Type>
                <Comment>Basic Element</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="22" Month="01" Year="2004"/>
                <Author>zl</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>tfi</Name>
                <Type>U8</Type>
                <Comment>Basic Element</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="22" Month="01" Year="2004"/>
                <Author>zl</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>gmm_state</Name>
                <Type>U8</Type>
                <Comment>codes the GPRS state</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="02" Month="03" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This filed show the number of rlc data blocks during the tbf, which is requested to send</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rlc_tbc</Name>
                <Type>U16</Type>
                <Comment>Number of rlc data blocks during the tbf, which is requested to send</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="10" Month="09" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>cell_type_ind</Name>
                <Type>U8</Type>
                <Comment>Indicates the cell type GSM/GPRS</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_cell_type_ind</Name>
            </ValuesLink>
            <History>
                <Date Day="29" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>cell_resel_offset</Name>
                <Type>U8</Type>
                <Comment>stores cell reselect offset</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_cell_resel_offset</Name>
            </ValuesLink>
            <History>
                <Date Day="29" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>temp_offset</Name>
                <Type>U8</Type>
                <Comment>Stores temporary offset</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_temp_offset</Name>
            </ValuesLink>
            <History>
                <Date Day="29" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev_acc_min</Name>
                <Type>U8</Type>
                <Comment>stores RXLEV_ACCESS_MIN</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_rxlev_acc_min</Name>
            </ValuesLink>
            <History>
                <Date Day="29" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>vocoder</Name>
                <Type>U8</Type>
                <Comment>Vocoder type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_vocoder</Name>
            </ValuesLink>
            <History>
                <Date Day="30" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>t3312_deactivated</Name>
                <Type>U8</Type>
                <Comment>Periodic RAU timer state</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_t3312_state</Name>
            </ValuesLink>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Periodic RAU timer value</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>t3312_val</Name>
                <Type>U32</Type>
                <Comment>Periodic RAU timer value in seconds</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section> AMR vocoder type </Section>
            </Description>
            <PrimBasicElemDef>
                <Name>amr_vocoder</Name>
                <Type>U8</Type>
                <Comment>AMR vocoder type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_amr_voc</Name>
            </ValuesLink>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section> AMR initial codec mode indicator </Section>
            </Description>
            <PrimBasicElemDef>
                <Name>amr_icmi</Name>
                <Type>U8</Type>
                <Comment>AMR initial codec mode indicator</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_amr_icmi</Name>
            </ValuesLink>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author>Gopinath</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>AMR initial codec mode</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>amr_icm</Name>
                <Type>U8</Type>
                <Comment>AMR initial codec mode(index in the ACS)</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author>Gopinath</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section> AMR active codec set </Section>
            </Description>
            <PrimBasicElemDef>
                <Name>amr_acs</Name>
                <Type>U8</Type>
                <Comment>AMR active codec set</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author>Gopinath</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Number of AMR codec modes in ACS</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>amr_nr_modes</Name>
                <Type>U8</Type>
                <Comment>Number of AMR codec modes</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author>Gopinath</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Lower thresholds for switching between mode j and j-1. Range 0-63, steps of 0.5db</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>amr_codec_thr</Name>
                <Type>U8</Type>
                <Comment>Lower thresholds for switching between mode j and j-1</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="03" Month="08" Year="2004"/>
                <Author>Gopinath</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Hysteresis values to obtain the higher thresholds for switching between mode j and j+1. Range 0-15 in steps of 0.5db</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>amr_codec_hyst</Name>
                <Type>U8</Type>
                <Comment>Hysteresis values to obtain the higher thresholds for switching between mode j and j+1</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="03" Month="08" Year="2004"/>
                <Author>Gopinath</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Highest bit rate AMR codec mode</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>amr_first_codec</Name>
                <Type>U8</Type>
                <Comment>Highest bit rate AMR codec mode</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_amr_first_cod</Name>
            </ValuesLink>
            <History>
                <Date Day="03" Month="08" Year="2004"/>
                <Author>Gopinath</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Mobile allocation index offset(0- 63)</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>maio</Name>
                <Type>U8</Type>
                <Comment>Mobile allocation index offset</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="04" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Number of arfcns in hopping list</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>nr_arfcns</Name>
                <Type>U8</Type>
                <Comment>Number of arfcns in hopping list</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="04" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Hopping valid or not flag</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>hop</Name>
                <Type>U8</Type>
                <Comment>Hopping valid or not flag</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">em</DocName>
                <Name>VAL_hop</Name>
            </ValuesLink>
            <History>
                <Date Day="04" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
    </PrimBasicElementsSection>
    <ValuesSection>
        <Description>
            <Section>This section contains all sets of values that are defined for the EM SAP</Section>
        </Description>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_arfcn</Name>
                <Comment>values for arfcn</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">FFFF</Value>
                <Alias/>
                <Comment>not present</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>124</MaxValue>
                <Comment>GSM 900 without extension band</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>124</MaxValue>
                <Comment>GSM 900 with extension band</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>975</MinValue>
                <MaxValue>1023</MaxValue>
                <Comment>GSM 900 with extension band</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>512</MinValue>
                <MaxValue>1023</MaxValue>
                <Comment>DCS 1800</Comment>
            </ValuesRange>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tn</Name>
                <Comment>values for tn</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>timeslot number 0-7</Comment>
            </ValuesRange>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_txlev</Name>
                <Comment>values for txlev</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>31</MaxValue>
                <Comment>power level</Comment>
            </ValuesRange>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_rxlev</Name>
                <Comment>values for rxlev</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>received field strength</Comment>
            </ValuesRange>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_rxqual_f</Name>
                <Comment>values for rxqual_f</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>received quality</Comment>
            </ValuesRange>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bsic</Name>
                <Comment>values for bsic</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">FF</Value>
                <Alias/>
                <Comment>not present</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>base station identification code</Comment>
            </ValuesRange>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_t3212</Name>
                <Comment>values for t3212</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>255</MaxValue>
                <Comment>value times 6minutes</Comment>
            </ValuesRange>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_v_start</Name>
                <Comment>values for v_start</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>no starting time</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>with starting time</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_dtx_stat</Name>
                <Comment>values for dtx_stat</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>without dtx</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>with dtx</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bs_pa_mfrms</Name>
                <Comment>values for bs_pa_mfrms</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>2 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>3 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias/>
                <Comment>4 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias/>
                <Comment>5 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias/>
                <Comment>6 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias/>
                <Comment>7 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias/>
                <Comment>8 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias/>
                <Comment>9 Multiframe Periods</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_entity</Name>
                <Comment>values for entity</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EM_L1</Alias>
                <Comment>L1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>EM_DL</Alias>
                <Comment>DL</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>EM_RR</Alias>
                <Comment>RR</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>EM_MM</Alias>
                <Comment>MM</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>EM_CC</Alias>
                <Comment>CC</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>EM_SS</Alias>
                <Comment>SS</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>EM_SMS</Alias>
                <Comment>SMS</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>EM_SIM</Alias>
                <Comment>SIM</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This values are used to set the RR entity to trace EM-Data at the PCO or disable that trace</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pco_bitmap</Name>
                <Comment>values for tracing the EM</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">0001</Value>
                <Alias>EM_PCO_SC_INFO</Alias>
                <Comment>request RR SC information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0002</Value>
                <Alias>EM_PCO_GPRS_INFO</Alias>
                <Comment>request GPRS SC information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0004</Value>
                <Alias>EM_PCO_NC_INFO</Alias>
                <Comment>request RR NC information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0008</Value>
                <Alias>EM_PCO_LOC_PAG_INFO</Alias>
                <Comment>request RR Location and Paging information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0010</Value>
                <Alias>EM_PCO_PLMN_INFO</Alias>
                <Comment>request RR PLMN information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0020</Value>
                <Alias>EM_PCO_CIPH_HOP_DTX_INFO</Alias>
                <Comment>request RR Ciphering Hopping and DTX information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0040</Value>
                <Alias>EM_PCO_POWER_INFO</Alias>
                <Comment>request RR Power (Classmark) information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0080</Value>
                <Alias>EM_PCO_IDENTITY_INFO</Alias>
                <Comment>request RR Identity information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0100</Value>
                <Alias>EM_PCO_SW_VERSION_INFO</Alias>
                <Comment>request SW Version information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0200</Value>
                <Alias>EM_PCO_GMM_INFO</Alias>
                <Comment>request GMM information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0400</Value>
                <Alias>EM_PCO_GRLC_INFO</Alias>
                <Comment>request GRLC information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0800</Value>
                <Alias>EM_PCO_AMR_INFO</Alias>
                <Comment>request AMR information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">1000</Value>
                <Alias>EM_PCO_PDP_INFO</Alias>
                <Comment>request PDP information</Comment>
            </ValuesItem>
            <History>
                <Date Day="09" Month="03" Year="2004"/>
                <Author>AM2</Author>
                <Comment>new EMW</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_hyst</Name>
                <Comment>values for hyst</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CELL_HYST_0_DB</Alias>
                <Comment>0 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CELL_HYST_2_DB</Alias>
                <Comment>2 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CELL_HYST_4_DB</Alias>
                <Comment>4 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CELL_HYST_6_DB</Alias>
                <Comment>6 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CELL_HYST_8_DB</Alias>
                <Comment>8 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>CELL_HYST_10_DB</Alias>
                <Comment>10 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>CELL_HYST_12_DB</Alias>
                <Comment>12 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>CELL_HYST_14_DB</Alias>
                <Comment>14 dB RXLEV hysteresis for LA re-selection</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_gprs_prio_class</Name>
                <Comment>values for gprs_prio_class</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">FF</Value>
                <Alias>GPRS_PRIORITY_CLASS_INVALID</Alias>
                <Comment>This value is used to indicate the absence of this parameter</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tbf_trans_type</Name>
                <Comment>values for tbf_trans_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>EM_TBF_TYPE_NULL</Alias>
                <Comment>No GPRS data transfer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>EM_TBF_TYPE_SB</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>EM_TBF_TYPE_FA</Alias>
                <Comment>Fixed Allocation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>EM_TBF_TYPE_DA</Alias>
                <Comment>Dynamic Allocation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>EM_TBF_TYPE_DL</Alias>
                <Comment>DL</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">05</Value>
                <Alias>EM_TBF_TYPE_DL_AND_DA</Alias>
                <Comment>DL + Dynamic Allocation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">06</Value>
                <Alias>EM_TBF_TYPE_DL_AND_FA</Alias>
                <Comment>DL + Fixed Allocation</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_nco</Name>
                <Comment>values for nco</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>FMM_NC0</Alias>
                <Comment>NC0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>FMM_NC1</Alias>
                <Comment>NC1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>FMM_NC2</Alias>
                <Comment>NC2, network controlled</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>FMM_RESET</Alias>
                <Comment>BCCH based reselection order</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>FMM_EMPTY</Alias>
                <Comment>undefined</Comment>
            </ValuesItem>
            <History>
                <Date Day="16" Month="12" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>indicates the state of grlc</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_grlc_state</Name>
                <Comment>indicates the state of grlc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>ACCESS_DISABLED</Alias>
                <Comment>access disabled       </Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>PIM</Alias>
                <Comment>Packet idle mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>PAM</Alias>
                <Comment>Packet access mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>PTM</Alias>
                <Comment>Packet transfer mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>WAIT_4_PIM</Alias>
                <Comment>wait for PIM</Comment>
            </ValuesItem>
            <History>
                <Date Day="20" Month="01" Year="2004"/>
                <Author>zl</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section/>
            </Description>
            <ValuesDef>
                <Name>VAL_cs</Name>
                <Comment>Values of coding scheme</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>CS_MODE_1</Alias>
                <Comment>Values Item</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>CS_MODE_2</Alias>
                <Comment>Values Item</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>CS_MODE_3</Alias>
                <Comment>Values Item</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>CS_MODE_4</Alias>
                <Comment>Values Item</Comment>
            </ValuesItem>
            <History>
                <Date Day="20" Month="01" Year="2004"/>
                <Author>zl</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>Indicates whether the cell type is GSM/GPRS</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_cell_type_ind</Name>
                <Comment>Value for indicating cell type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EM_CELL_NA</Alias>
                <Comment>Cell type is not available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EM_CELL_GSM</Alias>
                <Comment>Cell supports GSM only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>EM_CELL_GPRS</Alias>
                <Comment>Cell supports GSM and GPRS</Comment>
            </ValuesItem>
            <History>
                <Date Day="29" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section/>
            </Description>
            <ValuesDef>
                <Name>VAL_cell_resel_offset</Name>
                <Comment>Values for cell reselect offset</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>0   126 dB,2 dB steps, i.e. 0 = 0 dB, 1 = 2 dB, etc.</Comment>
            </ValuesRange>
            <History>
                <Date Day="29" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section/>
            </Description>
            <ValuesDef>
                <Name>VAL_temp_offset</Name>
                <Comment>Values for temporary offset</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>0   60 dB, 10 dB steps i.e. 0 = 0 dB,1 = 10 dB, etc. and 7 = infinity</Comment>
            </ValuesRange>
            <History>
                <Date Day="29" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section/>
            </Description>
            <ValuesDef>
                <Name>VAL_rxlev_acc_min</Name>
                <Comment>Values for RXLEV_ACCESS_MIN</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>Values Range</Comment>
            </ValuesRange>
            <History>
                <Date Day="29" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section/>
            </Description>
            <ValuesDef>
                <Name>VAL_vocoder</Name>
                <Comment>Values for vocoder type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>EM_VOC_SIG</Alias>
                <Comment>Signalling only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias>EM_VOC_SPEECH</Alias>
                <Comment>Speech</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100001</Value>
                <Alias>EM_VOC_EFR</Alias>
                <Comment>Enhanced full rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01000001</Value>
                <Alias>EM_VOC_AMR</Alias>
                <Comment>Adaptive multi rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00001111</Value>
                <Alias>EM_VOC_14_4</Alias>
                <Comment>User data rate of 14.4 kbps </Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000011</Value>
                <Alias>EM_VOC_9_6</Alias>
                <Comment>User data rate of 9.6kbps/12kbps radio interface rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00001011</Value>
                <Alias>EM_VOC_4_8</Alias>
                <Comment>User data rate of 4.8kbps/6kbps radio interface rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00010011</Value>
                <Alias>EM_VOC_2_4</Alias>
                <Comment>User data rate of 2.4kbps/3.6 radio interface rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11111111</Value>
                <Alias>EM_VOC_NA</Alias>
                <Comment>Not applicable in this state</Comment>
            </ValuesItem>
            <History>
                <Date Day="30" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section/>
            </Description>
            <ValuesDef>
                <Name>VAL_t3312_state</Name>
                <Comment>Periodic RAU timer</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EM_T3312_ACTIVE</Alias>
                <Comment>Periodic RAU timer is active</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EM_T3312_DEACTIVE</Alias>
                <Comment>Periodic RAU timer is de active</Comment>
            </ValuesItem>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section/>
            </Description>
            <ValuesDef>
                <Name>VAL_amr_voc</Name>
                <Comment>AMR vocoder type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EM_AFS</Alias>
                <Comment>AMR full rate speech</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>EM_AH0</Alias>
                <Comment>AMR half speech on sub channel 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>EM_AH1</Alias>
                <Comment>AMR half rate speech on sub channel 1</Comment>
            </ValuesItem>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>AMR initial codec mode indicator</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_amr_icmi</Name>
                <Comment>AMR initial codec mode indicator</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EM_AMR_ICMI_IMP</Alias>
                <Comment>The initial codec mode is defined by the implicit rule provided in 3GPP TS 05.09</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EM_AMR_ICMI_SMF</Alias>
                <Comment>The initial codec mode is defined by the Start Mode field</Comment>
            </ValuesItem>
            <History>
                <Date Day="02" Month="08" Year="2004"/>
                <Author>Gopinath</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>First codec (biggest transfer rate) in kbits per second</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_amr_first_cod</Name>
                <Comment>First codec (biggest transfer rate) in kbits per second</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EM_AMR_MODE_4_75</Alias>
                <Comment>4.75 kbps codec bit rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EM_AMR_MODE_5_15</Alias>
                <Comment>5.15 kbps codec bit rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>EM_AMR_MODE_5_9</Alias>
                <Comment>5.9 kbps codec bit rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>EM_AMR_MODE_6_7</Alias>
                <Comment>6.7 kbps codec bit rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>EM_AMR_MODE_7_4</Alias>
                <Comment>7.4 kbps codec bit rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>EM_AMR_MODE_7_95</Alias>
                <Comment>7.95 kbps codec bit rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>EM_AMR_MODE_10_2</Alias>
                <Comment>10.2 kbps codec bit rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>EM_AMR_MODE_12_2</Alias>
                <Comment>12.2 kbps codec bit rate</Comment>
            </ValuesItem>
            <History>
                <Date Day="03" Month="08" Year="2004"/>
                <Author>Gopinath</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>Hopping valid or not</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_hop</Name>
                <Comment>Hopping valid or not</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EM_HOP_NO</Alias>
                <Comment>Hopping is not present</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EM_HOP</Alias>
                <Comment>Hopping used</Comment>
            </ValuesItem>
            <History>
                <Date Day="04" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
    </ValuesSection>
</SAP>
