<?xml version="1.0" encoding="UTF-8"?>
<!-- edited with SAPE SAP Editor -->
<AIM xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="aim.xsd">
    <DocInfoSection>
        <DocName DocType="AIM">grr</DocName>
        <DocNum Number="601" Project="8441"/>
        <Description>
            <Section>The Protocol Stacks are used to define the functionality of the GSM protocols for interfaces. The GSM specifications are normative when used to describe the functionality of interfaces, but the stacks and the subdivision of protocol layers does not imply or restrict any implementation.</Section>
            <Section>The protocol stack for GPRS consists of several entities. Each entity has one ore more service access points, over which the entity provides a service for the upper entity.</Section>
            <Section>Figure 1-1: Architecture of the GSM/GPRS protocol stack</Section>
            <Section>The information units passed via the SAPs are called primitives and consists of an operation code and several parameters. See the Users Guide for details.</Section>
            <Section>The entities of the GPRS protocol stack are:</Section>
            <Section>1.1 GRR (RLC/MAC) - Radio Link Control/Medium Access Control</Section>
            <Section>This layer contains two functions: The Radio Link Control function provides a radio-solution-dependent reliable link. The Medium Access Control function controls the access signalling (request and grant) procedures for the radio channel, and the mapping of LLC frames onto the GSM physical channel.</Section>
            <Section>1.2 LLC - Logical Link Control</Section>
            <Section>The LLC entity provides multiple highly reliable logical links for asynchronous data transfer between the MS and the network. It supports variable-length information frames, acknowledged and unacknowledged data transfer, flow and sequence control, error detection and recovery, notification of unrecoverable errors, user identity confidentiality, and ciphering of user and signaling data.</Section>
            <Section>1.3 GMM - GPRS Mobility Management</Section>
            <Section>The GMM entity provides procedures for the mobility of the MS, such as informing the network of its present location, and user identity confidentiality. It manages the GMM context (attach, detach, routing area updating), supports security functions such as authentication of user and MS, controls ciphering of data, and initiates the response to paging messages.</Section>
            <Section>1.4 SM - Session Management</Section>
            <Section>The main function of the session management (SM) is to support PDP context handling of the user terminal. Session Management activates, modifies and deletes the contexts for packet data protocols (PDP). Session Management services are provided at the SMREG-SAP and the SNSM-SAP for anonymous and non-anonymous access. The non-anonymous and anonymous access procedures for PDP context activation and PDP context deactivation are available at the SMREG-SAP. In addition there exists a PDP context modification for non-anonymous PDP contexts.</Section>
            <Section>1.5 SNDCP - Subnetwork Dependant Convergence Protocol</Section>
            <Section>SNDCP carries out all functions related to transfer of Network layer Protocol Data Units (N-PDUs) over GPRS in a transparent way. SNDCP helps to improve channel efficiency by means of compression techniques. The set of protocol entities above SNDCP consists of commonly used network protocols. They all use the same SNDCP entity, which then performs multiplexing of data coming from different sources to be sent using the service provided by the LLC layer.</Section>
            <Section>1.6 GACI - GPRS Application Control Interface</Section>
            <Section>The GACI is the GPRS extension of the ACI. It is specified in GSM 07.07 and 07.60. It is responsible for processing of the GPRS related AT Commands to setup, activate and deactivate the PDP context parameter. It also provides functionality for the interworking between GMM/SM/SNDCP and a packet oriented protocol like PPP.</Section>
            <Section>1.7 USART - Universal Synchronous Asynchronous Receiver Transmitter Driver</Section>
            <Section>The USART is a hardware component that facilitates a connection between the mobile station and terminal equipment (e.g. a PC). This interface uses some of the circuits described in V.24.</Section>
            <Section>The data exchange provided by this unit is serial and asynchronous (synchronous communication is not in the scope of this document). A driver that uses interrupts to manage a circular buffer for the sending and receiving direction is necessary in order to use this component in the GPRS. The driver has to be able to perform flow control.</Section>
            <Section>1.8 TOM - Tunnelling of Messages</Section>
            <Section>The TOM entity is present if and only if HS136 is supported (the feature flag FF_HS136 is enabled).</Section>
            <Section>The main function of TOM is to tunnel non-GSM signalling messages between the MS and the SGSN. The only non-GSM signalling which is currently supported by TOM is for the EGPRS-136 system (according to TIA/EIA-136-376). Data transfer in both uplink and downlink direction is possible. Two different priorities (high, low) of signalling data transfer are supported. TOM uses the unacknowledged mode of LLC and the acknowledged mode of GRR (RLC/MAC).</Section>
        </Description>
        <DocHistory>
            <DocVersion Number="001" Year="99"/>
            <Date Day="14" Month="6" Year="1999"/>
            <Author>Stefan_Liepolt</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Initial</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="002" Year="99"/>
            <Date Day="23" Month="7" Year="1999"/>
            <Author>Stefan_Liepolt</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>consider GSM 0460d640</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="003" Year="99"/>
            <Date Day="4" Month="8" Year="1999"/>
            <Author>Stefan_Liepolt</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>replace CSN1_0 with flag</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="004" Year="99"/>
            <Date Day="7" Month="9" Year="1999"/>
            <Author>Ilker_Demirel</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>N_AVG_I is mandatory</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="005" Year="99"/>
            <Date Day="4" Month="10" Year="1999"/>
            <Author>Ilker_Demirel</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Changes is PSI2 message in PCCCH description and change of the structure sizes Cell_Alloc_Size, RFL_Size...</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="006" Year="99"/>
            <Date Day="10" Month="1" Year="2000"/>
            <Author>Stefan_Liepolt</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>consider GSM 0460d650</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="007" Year="99"/>
            <Date Day="12" Month="7" Year="2000"/>
            <Author>Thomas_Rozycki</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>TBF Starting Time Absolute redefined</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="008" Year="99"/>
            <Date Day="14" Month="9" Year="2000"/>
            <Author>Stefan_Kornprobst</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Editorial: removed problem of wrong section numbers to pass xGen100; removed obsolete SI 13 and fn</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="009" Year="99"/>
            <Date Day="18" Month="10" Year="2000"/>
            <Author>Ilker_Demirel</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Review of PSI3, 3BIS, 4, 5 messages. Set S_PADDING as optional. Set in the ctrl field for S_PADDING (22). Set presence bit to O instead of C.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="010" Year="00"/>
            <Date Day="30" Month="11" Year="2000"/>
            <Author>Bernd_Saborrosch</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>T_ALG_W changed to T_AVG_W, Ctrl-field for Power Control Parameters and Global Packet Timing Advance updated.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="011" Year="00"/>
            <Date Day="13" Month="12" Year="2000"/>
            <Author>Bernd_Saborrosch</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Changes in "Constant" section applied. Old structures nc_meas_par_psi5 and nc_meas_par rearranged.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="012" Year="00"/>
            <Date Day="13" Month="8" Year="2001"/>
            <Author>Harald_Mommer</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>3-digit-MNC</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="013" Year="00"/>
            <Date Day="15" Month="4" Year="2000"/>
            <Author>Bernd_Saborrosch</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add c-macro values for individual parameter..</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="014" Year="02"/>
            <Date Day="19" Month="4" Year="2002"/>
            <Author>MSB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Rename "tlli" to "tlli_value".  Link to Radio Access Capability</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="015" Year="02"/>
            <Date Day="23" Month="5" Year="2002"/>
            <Author>Bernd_Saborrosch</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add c-macro value for EXT_REPORTING_PERIOD.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="016" Year="03"/>
            <Date Day="30" Month="9" Year="2003"/>
            <Author>Bernd_Saborrosch</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>S_PADDING_0 is used instead of S_PADDING.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="017" Year="03"/>
            <Date Day="27" Month="10" Year="2003"/>
            <Author>Bernd_Saborrosch</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add RFL_NUMBER_4_DL_CTRL_MSG_MAX.</Comment>
        </DocHistory>
        <DocRef>
            <RefId>[1]</RefId>
            <RefTitle>GSM 05.02 version 8.0.0 Release 1999Digital cellular telecommunications system (Phase 2+);Multiplexing and multiple access on the radio path</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[2]</RefId>
            <RefTitle>GSM 04.60 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);General Packet Radio Service (GPRS);Mobile Station (MS) - Base Station System (BSS) interface;Radio Link Control/ Medium Access Control (RLC/MAC) protocol</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[3]</RefId>
            <RefTitle>GSM 04.08 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);Mobile radio interface layer 3 specification</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[4]</RefId>
            <RefTitle>GSM 03.64 version 6.1.0 Release 1997Digital cellular telecommunications system (Phase 2+);General Packet Radio Service (GPRS);Overall description of the GPRS radio interface; Stage 2</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[5]</RefId>
            <RefTitle>GSM 03.60 version 6.3.1 Release 1997Digital cellular telecommunications system (Phase 2+);General Packet Radio Service (GPRS);Service description; Stage 2</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[6]</RefId>
            <RefTitle>GSM 04.07 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);Mobile radio interface signalling layer 3; General aspects</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[7]</RefId>
            <RefTitle>GSM 04.64 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);General Packet Radio Service (GPRS);Mobile Station - Serving GPRS Support Node (MS-SGSN)Logical Link Control (LLC) layer specification</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[8]</RefId>
            <RefTitle>GSM 05.08 version 6.4.0 Release 1997Digital cellular telecommunications system (Phase 2+);Radio subsystem link control</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[9]</RefId>
            <RefTitle>GSM 05.10 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);Radio subsystem synchronization</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[10]</RefId>
            <RefTitle>GSM 03.20 TS 100 929: July 1998 (GSM 03.20 version 6.0.1)Security related network functions, ETSI</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[11]</RefId>
            <RefTitle>Draft GSM 03.22: August 1998 (GSM 03.22 version 6.1.0)Functions related to Mobile Station (MS) in idle mode and group receive mode, ETSI</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[12]</RefId>
            <RefTitle>GSM 04.65 V6.3.0: Subnetwork Dependant Convergence Protocol ETSI, March 1999</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[13]</RefId>
            <RefTitle>ITU-T V42bis ITU-T, Recommendation V.42 bis 1990</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[14]</RefId>
            <RefTitle>GSM 09.60 GPRS Tunneling Protocol (GTP) across the Gn and Gp Interface</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[15]</RefId>
            <RefTitle>RFC 1661 IETF STD 51 July 1994The Point-to-Point Protocol (PPP)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[16]</RefId>
            <RefTitle>RFC 1662 IETF STD 51 July 1994PPP in HDLC-like Framing</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[17]</RefId>
            <RefTitle>RFC 1570 January 1994PPP LCP Extensions</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[18]</RefId>
            <RefTitle>RFC 1989 August 1996PPP Link Quality Monitoring</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[19]</RefId>
            <RefTitle>RFC 1332 May 1992The PPP Internet Protocol Control Protocol (IPCP)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[20]</RefId>
            <RefTitle>RFC 1877 December 1995PPP IPCP Extensions for Name Server Addresses</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[21]</RefId>
            <RefTitle>RFC 2153 May 1997PPP Vendor Extensions</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[22]</RefId>
            <RefTitle>RFC 1334 October 1992PPP Authentication Protocols (for Password Authentication Protocol only)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[23]</RefId>
            <RefTitle>RFC 1994 August 1996PPP Challenge Handshake Authentication Protocol (CHAP)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[24]</RefId>
            <RefTitle>TIA/EIA-136-370Packet-Data Services - Enhanced General Packet Radio for TIA/EIA-136 (EGPRS-136) - Overview, Telecommunications Industry Association</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[25]</RefId>
            <RefTitle>TIA/EIA-136-376Packet-Data Services - EGPRS-136 Mobility Management, Telecommunications Industry Association</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[26]</RefId>
            <RefTitle>TIA/EIA-136-972Packet-Data Services - Stage 2 Description, Telecommunications Industry Association</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[MSG_RR_COM]</RefId>
            <RefTitle>GRR, Air Interface Message Specification, 8441.601.02.014, Condat AG</RefTitle>
        </DocRef>
    </DocInfoSection>
    <ConstantsSection>
        <Description>
            <Section>This section contains all constants that are defined for the GRR AIM</Section>
        </Description>
        <Constant>
            <Alias>MAX_REJECT</Alias>
            <Value ValueType="DEC">4</Value>
            <Comment>There is no reference in 0460 for that value. Assumption M. The maximum value for M == MAX_RETRANS is 4</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NCELL_REST</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment>MAX_NCELL -1 = 5</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CHAN_IMEAS</Alias>
            <Value ValueType="DEC">32</Value>
            <Comment>Total number  of channels for interference measurements</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CHAN_EXT</Alias>
            <Value ValueType="DEC">64</Value>
            <Comment>Max number of channels for extended Measurements</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CHAN_NC</Alias>
            <Value ValueType="DEC">64</Value>
            <Comment>Max number of channels for network controlled cell re-selection</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_RFL_NUM_LIST</Alias>
            <Value ValueType="DEC">16</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_ARFCN_LIST</Alias>
            <Value ValueType="DEC">64</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_NH_PCCCH_CARRIER</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_PCCCH_DES</Alias>
            <Value ValueType="DEC">16</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_M_NH_PCCCH_C</Alias>
            <Value ValueType="DEC">2</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_M_H_PCCCH_C</Alias>
            <Value ValueType="DEC">16</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_NCMP_S1</Alias>
            <Value ValueType="DEC">8</Value>
            <Comment>this is maximum because the length indicator is a 3 bit value</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_XMR_S1</Alias>
            <Value ValueType="DEC">32</Value>
            <Comment>this is maximum because the length indicator is a 5 bit value</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CELL_ALLOC</Alias>
            <Value ValueType="DEC">4</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_GPRS_MS_ALLOC</Alias>
            <Value ValueType="DEC">7</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_RFL_IN_PSI</Alias>
            <Value ValueType="DEC">4</Value>
            <Comment>"_IN_PSI" because of same name in RR air messages</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NCELL_PAR2</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_REP_PAGE_INFO</Alias>
            <Value ValueType="DEC">4</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_RFREQ</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment>Max removed frequencies in NC Meas.</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_AFREQ</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment>Max added frequencies in NC Meas.</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_LIST_AFREQ</Alias>
            <Value ValueType="DEC">2</Value>
            <Comment>Max number of added frequency lists</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_MSG_TYPE</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment>used in PACKET PSI STATUS</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NCELL_PARA</Alias>
            <Value ValueType="DEC">6</Value>
            <Comment>see PSI3</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NCELL_PAR2_S1</Alias>
            <Value ValueType="DEC">2</Value>
            <Comment>see PSI3bis</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NCELL_PAR2_S2</Alias>
            <Value ValueType="DEC">2</Value>
            <Comment>see PSI3bis</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NCELL_PAR2_DES</Alias>
            <Value ValueType="DEC">2</Value>
            <Comment>see PSI3bis</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NH_PCCCH_C</Alias>
            <Value ValueType="DEC">16</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_FREQ_DIFF_CS_PAR</Alias>
            <Value ValueType="DEC">8</Value>
            <Comment>Maximum number of frequency difference and Cell Selection parameters structure. See PSI3 description</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NCELL_IN_PSI3BIS</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment>Maximum number  of neighbor cell parmeters in PSI3BIS message. Calculation is based on, that this structure can contain at least 31 bits and the an RLC/MAC control block has a size of up to 22 bytes.</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NCELL2_IN_PSI3BIS</Alias>
            <Value ValueType="DEC">3</Value>
            <Comment>Maximum number  of  neighbor cell parameters 2 in PSI3BIS message. This structure can contain at least 45 bits.</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_BASIC_CELL_IN_NCELL2</Alias>
            <Value ValueType="DEC">3</Value>
            <Comment>See PSI3BIS</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_REMAINING_CELL_IN_NCELL2</Alias>
            <Value ValueType="DEC">18</Value>
            <Comment>See PSI3BIS</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NEIGHBOR_PARAMETER_SET_IN_NCELL2</Alias>
            <Value ValueType="DEC">4</Value>
            <Comment>See PSI3BIS</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_NR_OF_NCELL</Alias>
            <Value ValueType="DEC">32</Value>
            <Comment>See PSI3</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CHAN_LIST</Alias>
            <Value ValueType="DEC">7</Value>
            <Comment>See PSI4</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_EXT_FREQ_LIST</Alias>
            <Value ValueType="DEC">7</Value>
            <Comment>See PSI5</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_EXT_FREQ_LIST_ELEM</Alias>
            <Value ValueType="DEC">32</Value>
            <Comment>SeePSI5</Comment>
        </Constant>
        <History>
            <Date Day="21" Month="5" Year="1999"/>
            <Author>SL</Author>
            <Comment>Initial</Comment>
        </History>
        <History>
            <Date Day="23" Month="7" Year="1999"/>
            <Author>SL</Author>
            <Comment>consider GSM 0460d640</Comment>
        </History>
        <History>
            <Date Day="4" Month="10" Year="1999"/>
            <Author>ID</Author>
            <Comment>MAX_NH_PCCCH_C added</Comment>
        </History>
        <History>
            <Date Day="12" Month="10" Year="1999"/>
            <Author>ID</Author>
            <Comment>MAX_NCELL_PARA is set to 6</Comment>
        </History>
        <History>
            <Date Day="10" Month="1" Year="2000"/>
            <Author>SL</Author>
            <Comment>MAX_CHAN_IMEAS_REST is set to 32</Comment>
        </History>
        <History>
            <Date Day="25" Month="9" Year="2000"/>
            <Author>ID</Author>
            <Comment>Maximum number of structures for PSI3 and PSI3BIS changed</Comment>
        </History>
        <History>
            <Date Day="12" Month="10" Year="2000"/>
            <Author>ID</Author>
            <Comment>Maximum number of structures for PSI4 and PSI5 changed.</Comment>
        </History>
        <History>
            <Date Day="12" Month="10" Year="2000"/>
            <Author>ID</Author>
            <Comment>MAX_CHAN_IMEAS_REST changed to MAX_CHAN_IMEAS and set to 32</Comment>
        </History>
        <History>
            <Date Day="12" Month="10" Year="2000"/>
            <Author>ID</Author>
            <Comment>MAX_CHAN_EXT added. Max number of channels for Extended Meas.</Comment>
        </History>
        <History>
            <Date Day="13" Month="12" Year="2000"/>
            <Author>SAB</Author>
            <Comment>MAX_CHAN_NC added. Max number of channels for Extended Meas  increased.</Comment>
        </History>
        <History>
            <Date Day="16" Month="1" Year="2001"/>
            <Author>ID</Author>
            <Comment>MAX_RFL_NUM_LIST set to 15; MAX_ARFCN_LIST set 64. Both are used  in GPRS Mobile Allocation</Comment>
        </History>
        <History>
            <Date Day="21" Month="2" Year="2001"/>
            <Author>SAB</Author>
            <Comment>MAX_FREQ_LISTS removed, rename MAX_LIST_AF to MAX_LIST AFREQ,   change sequence of constants</Comment>
        </History>
    </ConstantsSection>
    <MessagesSection>
        <Description>
            <Section>This section contains all messages that are defined for the GRR AIM</Section>
        </Description>
        <Message>
            <Description>
                <Section>This message is sent on the PCCCH or PACCH by the network to the mobile station to indicate that the network has rejected the MSs access request. This message may contain fields addressing more than one mobile station. This Message is defined in [2] 11.2.1</Section>
            </Description>
            <MsgDef>
                <Name>d_access_rej</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">100001</MsgID>
                <Comment>Packet Access Reject</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>Page Mode</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>reject</Name>
                </ItemLink>
                <SpecRef>11.2.1</SpecRef>
                <Comment>Reject Structure</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>add_reject</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_REJECT]</TypeModifier>
                </Control>
                <SpecRef>11.2.1</SpecRef>
                <Comment>Additional Reject Structure</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PCCCH by the network to the mobile station to notify the mobile station that it is being placed in queue. The message allocates a Temporary Queuing Identity to the mobile station. This Message is defined in [2] 11.2.15 .</Section>
            </Description>
            <MsgDef>
                <Name>d_queuing_not</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">000110</MsgID>
                <Comment>Packet Queuing Notification</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>111</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef/>
                <Comment>spare</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>req_ref_p</Name>
                </ItemLink>
                <SpecRef>12.11</SpecRef>
                <Comment>Packet Request Reference</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tqi</Name>
                </ItemLink>
                <SpecRef>12.17</SpecRef>
                <Comment>TQI</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PACCH by the mobile station to the network to request a change in the uplink resources assigned. This Message is defined in [2] 11.2.16 .</Section>
            </Description>
            <MsgDef>
                <Name>u_resource_req</Name>
                <MsgID Direction="UPLINK" IDType="BIN">000101</MsgID>
                <Comment>Packet Resource Request</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>access_type</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.16</SpecRef>
                <Comment>Access Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>glob_tfi</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>12.10</SpecRef>
                <Comment>Global TFI</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tlli_value</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>12.16</SpecRef>
                <Comment>TLLI</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">rr_com</DocName>
                    <Name>ra_cap</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>see [22]</SpecRef>
                <Comment>MS Radio Access Capability</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>chan_req_des</Name>
                </ItemLink>
                <SpecRef>12.7</SpecRef>
                <Comment>Channel Request Description</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ma_ch_mark</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.16</SpecRef>
                <Comment>MA_CHANGE_MARK</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>c_value</Name>
                </ItemLink>
                <SpecRef>11.2.6</SpecRef>
                <Comment>C_VALUE</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>signvar</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.6</SpecRef>
                <Comment>SIGN_VAR</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilev</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>I_LEVEL Structure</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
            <History>
                <Date Day="17" Month="10" Year="2000"/>
                <Author>ID</Author>
                <Comment>Spare bits added</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="19" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>ref for MS Radio Access Capability changed. (Use link to rr_com.doc)</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PCCCH or PACCH by the network to the mobile station to assign uplink resources. The mobile station may be addressed by TFI, TQI, or Packet Request Reference depending upon the procedure used. A mobile allocation or reference frequency list received as part of this assignment message shall be valid until new assignment is received or each TBF of the MS are terminated. This Message is defined in [2] 11.2.29 .</Section>
            </Description>
            <MsgDef>
                <Name>d_ul_assign</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">001010</MsgID>
                <Comment>Packet Uplink Assignment</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>Page Mode</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pers_lev</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.14</SpecRef>
                <Comment>PERSISTENCE_LEVEL</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>add3</Name>
                </ItemLink>
                <SpecRef>11.2.20</SpecRef>
                <Comment>Address Information3</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef/>
                <Comment>spare</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>chan_coding_cmd</Name>
                </ItemLink>
                <SpecRef>11.2.29</SpecRef>
                <Comment>CHANNEL_CODING_COMMAND</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tlli_chan_coding</Name>
                </ItemLink>
                <SpecRef>12.16</SpecRef>
                <Comment>TLLI_BLOCK_CHANNEL_CODING</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pta</Name>
                </ItemLink>
                <SpecRef>12.12</SpecRef>
                <Comment>Packet Timing Advance</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.8</SpecRef>
                <Comment>Frequency Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Flag</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>Flag2</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dyn_alloc_p</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0 AND flag2=1</Condition>
                </Control>
                <SpecRef>11.2.29</SpecRef>
                <Comment>Dynamic Allocation</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>sin_alloc</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND flag2=0</Condition>
                </Control>
                <SpecRef>11.2.29</SpecRef>
                <Comment>Single Block Allocation</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>f_alloc_ul</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND flag2=1</Condition>
                </Control>
                <SpecRef>11.2.29</SpecRef>
                <Comment>Fixed Allocation Uplink Assignment</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="11" Month="12" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Rename dyn_alloc to dyn_alloc_p to resolve name equality with RR   structure.</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PCCCH or PACCH by the network to the mobile station to assign downlink resources to the mobile station. For a mobile station assigned to operate in the fixed allocation MAC mode, the network may assign regularly repeating intervals during which the mobile station shall measure neighbor cell power levels. A mobile allocation or reference frequency list received as part of this assignment message shall be valid until a new assignment is received or each TBF of the MS are terminated. This Message is defined in [2] 11.2.7 .</Section>
            </Description>
            <MsgDef>
                <Name>d_dl_assign</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">000010</MsgID>
                <Comment>Packet Downlink Assignment</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pers_lev</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.14</SpecRef>
                <Comment>PERSISTENCE_LEVEL</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>add1</Name>
                </ItemLink>
                <SpecRef>11.2.4</SpecRef>
                <Comment>Address Information1</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>11.2.4</SpecRef>
                <Comment>spare</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>mac_mode</Name>
                </ItemLink>
                <SpecRef>11.2.7</SpecRef>
                <Comment>MAC_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rlc_mode</Name>
                </ItemLink>
                <SpecRef>11.2.7</SpecRef>
                <Comment>RLC_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ctrl_ack</Name>
                </ItemLink>
                <SpecRef>11.2.7</SpecRef>
                <Comment>CONTROL_ACK</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ts_alloc</Name>
                </ItemLink>
                <SpecRef>12.18</SpecRef>
                <Comment>TIMESLOT_ALLOCATION</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pta</Name>
                </ItemLink>
                <SpecRef>12.12</SpecRef>
                <Comment>Packet Timing Advance</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bts_pwr_ctrl</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.29</SpecRef>
                <Comment>BTS_PWR_CTRL</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.8</SpecRef>
                <Comment>Frequency Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dl_tfi_assign</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.15.</SpecRef>
                <Comment>DOWNLINK_TFI_ASSIGNMENT</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pwr_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.13</SpecRef>
                <Comment>Power Control Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tbf_s_time</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.7</SpecRef>
                <Comment>TBF_STARTING_TIME</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>meas_map</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.7</SpecRef>
                <Comment>Measurement Mapping</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PACCH by the network to the mobile station to initiate release of an uplink TBF. This Message is defined in [2] 11.2.26 .</Section>
            </Description>
            <MsgDef>
                <Name>d_tbf_release</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">001000</MsgID>
                <Comment>Packet TBF Release</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef/>
                <Comment>spare</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>glob_tfi</Name>
                </ItemLink>
                <SpecRef>12.10</SpecRef>
                <Comment>Global TFI</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ul_release</Name>
                </ItemLink>
                <SpecRef>11.2.26</SpecRef>
                <Comment>UPLINK_RELEASE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dl_release</Name>
                </ItemLink>
                <SpecRef>11.2.26</SpecRef>
                <Comment>DOWNLINK_RELEASE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rel_cause</Name>
                </ItemLink>
                <SpecRef>11.2.26</SpecRef>
                <Comment>TBF Release Cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>spare bits reduced from .00 to .0</Comment>
            </History>
            <History>
                <Date Day="2" Month="10" Year="2001"/>
                <Author>CAN</Author>
                <Comment>TBF Release Cause len corrected</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PCCCH by the network to up to four mobile stations to trigger channel access by these for either TBF or RR connection establishment. It may also be sent on PACCH to a mobile station in packet transfer mode to indicate page request for RR connection establishment. The mobile stations are identified either by IMSI, TMSI or P-TMSI. Depending on the method used to identify the mobile station, 1 - 4 mobile stations can be addressed in the message. This Message is defined in [2] 11.2.10 .</Section>
            </Description>
            <MsgDef>
                <Name>d_paging_req</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">100010</MsgID>
                <Comment>Packet Paging Request</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pers_lev</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.14</SpecRef>
                <Comment>PERSISTENCE_LEVEL</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nln</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.10</SpecRef>
                <Comment>NLN</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rep_page_info</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_REP_PAGE_INFO]</TypeModifier>
                </Control>
                <SpecRef>11.2.10</SpecRef>
                <Comment>Repeated Page info</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PACCH from the mobile station to the network to indicate the status of downlink RLC data blocks received and to report the channel quality of the downlink. The mobile station may optionally initiate an uplink TBF or request a temporary suspension of the downlink TBF. This Message is defined in [2] 11.2.6 .</Section>
            </Description>
            <MsgDef>
                <Name>u_dl_ack</Name>
                <MsgID Direction="UPLINK" IDType="BIN">000010</MsgID>
                <Comment>Packet Downlink Ack/Nack</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dl_tfi</Name>
                </ItemLink>
                <SpecRef>12.15</SpecRef>
                <Comment>DOWNLINK_TFI</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ack_nack_des</Name>
                </ItemLink>
                <SpecRef>12.3</SpecRef>
                <Comment>Ack/Nack Description</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>chan_req_des</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.7</SpecRef>
                <Comment>Channel Request Description</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>chan_qual_rep</Name>
                </ItemLink>
                <SpecRef>11.2.6</SpecRef>
                <Comment>Channel Quality Report</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PACCH by the network to the mobile station indicate the status of the received RLC data blocks. This message may also update the timing advance and power control parameters. A fixed allocation mobile station may also be assigned uplink resources. This Message is defined in [2] 11.2.28 .</Section>
            </Description>
            <MsgDef>
                <Name>d_ul_ack</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">001001</MsgID>
                <Comment>Packet Uplink Ack/Nack</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <SpecRef/>
                <Comment>spare</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ul_tfi</Name>
                </ItemLink>
                <SpecRef>12.15</SpecRef>
                <Comment>UPLINK_TFI</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef/>
                <Comment>spare</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>chan_coding_cmd</Name>
                </ItemLink>
                <SpecRef>11.2.28</SpecRef>
                <Comment>CHANNEL_CODING_COMMAND</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ack_nack_des</Name>
                </ItemLink>
                <SpecRef>12.3</SpecRef>
                <Comment>Ack/Nack Description</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cr_tlli</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.16</SpecRef>
                <Comment>CONTENTION_RESOLUTION_TLLI :</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pta</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.12</SpecRef>
                <Comment>Packet Timing Advance</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pwr_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.13</SpecRef>
                <Comment>Power Control Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ext_bits</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.26</SpecRef>
                <Comment>Extension Structure</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>f_alloc_ack</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.28</SpecRef>
                <Comment>Fixed Allocation Uplink Ack/Nack</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Rename exten to ext_bits.</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network on the PBCCH or PACCH giving information for Cell selection, for control of the PRACH, for description of the control channel(s) and optional global power control parameters. This Message is defined in [2] 11.2.18 .</Section>
            </Description>
            <MsgDef>
                <Name>psi_1</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">110001</MsgID>
                <Comment>Packet System Information Type 1</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pbcch_change_ma</Name>
                </ItemLink>
                <SpecRef>11.2.18</SpecRef>
                <Comment>PBCCH_CHANGE_MARK</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi_change_field</Name>
                </ItemLink>
                <SpecRef>11.2.18</SpecRef>
                <Comment>PSI_CHANGE_FIELD</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi1_rep_per</Name>
                </ItemLink>
                <SpecRef>11.2.18</SpecRef>
                <Comment>PSI1_REPEAT_PERIOD</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi_cnt_lr</Name>
                </ItemLink>
                <SpecRef>11.2.18</SpecRef>
                <Comment>PSI_COUNT_LR</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi_cnt_hr</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.18</SpecRef>
                <Comment>PSI_COUNT_HR</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>meas_order</Name>
                </ItemLink>
                <SpecRef>11.2.18</SpecRef>
                <Comment>MEASUREMENT_ORDER</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_cell_opt</Name>
                </ItemLink>
                <SpecRef>12.24</SpecRef>
                <Comment>GPRS Cell Options</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>prach_ctrl_par</Name>
                </ItemLink>
                <SpecRef>12.14</SpecRef>
                <Comment>PRACH Control Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pccch_org_par</Name>
                </ItemLink>
                <SpecRef>12.25</SpecRef>
                <Comment>PCCCH Organization Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>g_pwr_par</Name>
                </ItemLink>
                <SpecRef>12.9</SpecRef>
                <Comment>Global Power Control Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi_status_ind</Name>
                </ItemLink>
                <SpecRef>11.2.18</SpecRef>
                <Comment>PSI_STATUS_IND</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Rename gprs_opt to gprs_cell_opt.</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network on PBCCH and PACCH giving information of reference frequency lists, cell allocation, GPRS mobile allocations and PCCCH descriptions being used in the cell. PSI2 also contains Non-GPRS cell options applicable for non-packet access. This Message is defined in [2] 11.2.19 .</Section>
            </Description>
            <MsgDef>
                <Name>psi_2</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">110010</MsgID>
                <Comment>Packet System Information Type 2</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi2_cm</Name>
                </ItemLink>
                <SpecRef>11.2.19</SpecRef>
                <Comment>PSI2_CHANGE_MARK</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi2_ind</Name>
                </ItemLink>
                <SpecRef>11.2.19</SpecRef>
                <Comment>PSI2_INDEX</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi2_cnt</Name>
                </ItemLink>
                <SpecRef>11.2.19</SpecRef>
                <Comment>PSI2_COUNT</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cell_id</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.21</SpecRef>
                <Comment>Cell Identification</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>non_gprs_opt</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.27</SpecRef>
                <Comment>Non GPRS Cell Options</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rfl</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_RFL_IN_PSI]</TypeModifier>
                </Control>
                <SpecRef>11.2.19</SpecRef>
                <Comment>Reference Frequency Lists</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cell_alloc</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_CELL_ALLOC]</TypeModifier>
                </Control>
                <SpecRef>11.2.19</SpecRef>
                <Comment>Cell Allocation</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_ms_alloc</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_GPRS_MS_ALLOC]</TypeModifier>
                </Control>
                <SpecRef>11.2.19</SpecRef>
                <Comment>GPRS Mobile Allocations</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pccch_des</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_PCCCH_DES]</TypeModifier>
                </Control>
                <SpecRef>11.2.19</SpecRef>
                <Comment>PCCCH Description</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network on the PBCCH or PACCH giving information of the BCCH allocation (BA_GPRS) in the neighbour cells and cell selection parameters for serving cell and non-serving cells. This Message is defined in [2] 11.2.20</Section>
            </Description>
            <MsgDef>
                <Name>psi_3</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">110011</MsgID>
                <Comment>Packet System Information Type 3</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi3_cm</Name>
                </ItemLink>
                <SpecRef>11.2.20</SpecRef>
                <Comment>PSI3_CHANGE_MARK</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi3bis_cnt</Name>
                </ItemLink>
                <SpecRef>11.2.20</SpecRef>
                <Comment>PSI3_BIS_COUNT</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>scell_par</Name>
                </ItemLink>
                <SpecRef>11.2.20</SpecRef>
                <Comment>Serving Cell parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gen_cell_par</Name>
                </ItemLink>
                <SpecRef>11.2.20</SpecRef>
                <Comment>General Cell Selection parameter</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ncell_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_NCELL_PARA]</TypeModifier>
                </Control>
                <SpecRef>11.2.20</SpecRef>
                <Comment>Neighbour Cell parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This optional message is sent by the network on the PBCCH and PACCH giving information of the BCCH allocation in the neighbour cells and cell selection parameters for non-serving cells. If all information does not fit into one PSI3bis message, the PSI3bis message can be repeated. This Message is defined in [2] 11.2.21 .</Section>
            </Description>
            <MsgDef>
                <Name>psi_3_bis</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">110100</MsgID>
                <Comment>Packet System Information Type 3 bis</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi3_cm</Name>
                </ItemLink>
                <SpecRef>11.2.21</SpecRef>
                <Comment>PSI3_CHANGE_MARK</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi3bis_ind</Name>
                </ItemLink>
                <SpecRef>11.2.21</SpecRef>
                <Comment>PSI3_BIS_INDEX</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi3bis_cnt</Name>
                </ItemLink>
                <SpecRef>11.2.21</SpecRef>
                <Comment>PSI3_BIS_COUNT</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ncell_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_NCELL_IN_PSI3BIS]</TypeModifier>
                </Control>
                <SpecRef>11.2.20</SpecRef>
                <Comment>Neigbour cell parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ncell_par2</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_NCELL2_IN_PSI3BIS]</TypeModifier>
                </Control>
                <SpecRef>11.2.21</SpecRef>
                <Comment>Neighbour Cell parameters 2</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="25" Month="9" Year="2000"/>
                <Author>ID</Author>
                <Comment>MAX_NCELL_PAR2</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag, ncell_par2 is optional and of type CSN1_S1</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is optionally sent by the network on the PBCCH and PACCH giving information directing the mobile station to make measurements on a list of serving cell PDCHs, during the idle frame of those PDCHs. This Message is defined in [2] 11.2.22 .</Section>
            </Description>
            <MsgDef>
                <Name>psi_4</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">110101</MsgID>
                <Comment>Packet System Information Type 4</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi4_cm</Name>
                </ItemLink>
                <SpecRef>11.2.22</SpecRef>
                <Comment>PSI4_CHANGE_MARK</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi4_ind</Name>
                </ItemLink>
                <SpecRef>11.2.22</SpecRef>
                <Comment>PSI4_INDEX</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi4_cnt</Name>
                </ItemLink>
                <SpecRef>11.2.22</SpecRef>
                <Comment>PSI4_COUNT</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>chan_list_imeas</Name>
                </ItemLink>
                <SpecRef>11.2.22</SpecRef>
                <Comment>Channel List for Interference measurements</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="10" Year="2000"/>
                <Author>ID</Author>
                <Comment>change psi3_cm to psi4_cm</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This optional message is sent by the network on the PBCCH giving information for measurement reporting and network controlled cell reselection. If all information does not fit into one message, the remaining information will be sent in other instances of the PSI5 message. The message is sent on PBCCH only if so indicated in PSI1. This Message is defined in [2] 11.2.23 .</Section>
            </Description>
            <MsgDef>
                <Name>psi_5</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">110110</MsgID>
                <Comment>Packet System Information Type 5</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi5_cm</Name>
                </ItemLink>
                <SpecRef>11.2.23</SpecRef>
                <Comment>PSI5_CHANGE_MARK</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi5_ind</Name>
                </ItemLink>
                <SpecRef>11.2.23</SpecRef>
                <Comment>PSI5_INDEX</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi5_cnt</Name>
                </ItemLink>
                <SpecRef>11.2.23</SpecRef>
                <Comment>PSI5_COUNT</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nc_meas_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.23</SpecRef>
                <Comment>NC Measurement Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>xmeas_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.23</SpecRef>
                <Comment>EXT Measurement Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="14" Month="12" Year="2000"/>
                <Author>SAB</Author>
                <Comment>nc_meas_par_psi5 changed to nc_meas_par</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message may be broadcast by the network on the PACCH. The message provides the mobile station with GPRS cell specific access-related information. The information in this message shall be the same as provided in the SI13 message on BCCH. This Message is defined in [2] 11.2.25 .</Section>
            </Description>
            <MsgDef>
                <Name>psi_13</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">110111</MsgID>
                <Comment>Packet System Information Type 13</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bcch_change_ma</Name>
                </ItemLink>
                <SpecRef>11.2.25</SpecRef>
                <Comment>BCCH_CHANGE_MARK</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>si_change_ma</Name>
                </ItemLink>
                <SpecRef>11.2.25</SpecRef>
                <Comment>SI_CHANGE_FIELD</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>si13_cm_gprs_alloc</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>SI13_CHANGE_MARK and GPRS Alloc</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>_</SpecRef>
                <Comment>Flag</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pbcch_n_pres</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>11.2.25</SpecRef>
                <Comment>PBCCH not present in cell structure</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi1_pbcch_info</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>11.2.25</SpecRef>
                <Comment>PSI1 and PBCCH info</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="14" Month="10" Year="1999"/>
                <Author>ID</Author>
                <Comment>flag values changed</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PACCH from the mobile station to the network. The message is formatted as either an RLC/MAC control block or as 4 access bursts. The System Information parameter CONTROL_ACK_TYPE indicates which format the mobile station shall use. This Message is defined in [2] 11.2.2 .</Section>
            </Description>
            <MsgDef>
                <Name>u_ctrl_ack</Name>
                <MsgID Direction="UPLINK" IDType="BIN">000001</MsgID>
                <Comment>Packet Control Acknowledgement</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tlli_value</Name>
                </ItemLink>
                <SpecRef>12.16</SpecRef>
                <Comment>TLLI</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pctrl_ack</Name>
                </ItemLink>
                <SpecRef>11.2.2</SpecRef>
                <Comment>P_CTRL_ACK</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PACCH from the mobile station to the network to indicate that a commanded cell change order has failed. This Message is defined in [2] 11.2.3 .</Section>
            </Description>
            <MsgDef>
                <Name>u_cell_chan_failure</Name>
                <MsgID Direction="UPLINK" IDType="BIN">000000</MsgID>
                <Comment>Packet Cell Change Failure</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tlli_value</Name>
                </ItemLink>
                <SpecRef>12.16</SpecRef>
                <Comment>TLLI</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <SpecRef>11.2.3</SpecRef>
                <Comment>ARFCN</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <SpecRef>11.2.3</SpecRef>
                <Comment>BSIC</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>failure_cause</Name>
                </ItemLink>
                <SpecRef>11.2.3</SpecRef>
                <Comment>CAUSE</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="8" Month="11" Year="2002"/>
                <Author>ZL</Author>
                <Comment>failure cause bit length from 8 to 4 bits.</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PCCCH or PACCH by the network to the mobile station to command the mobile station to leave the current cell and change to a new cell. This Message is defined in [2] 11.2.4 .</Section>
            </Description>
            <MsgDef>
                <Name>d_cell_chan_order</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">000001</MsgID>
                <Comment>Packet Cell Change Order</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>add1</Name>
                </ItemLink>
                <SpecRef>11.2.4</SpecRef>
                <Comment>Address Information1</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>11.2.4</SpecRef>
                <Comment>spare</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>im_rel</Name>
                </ItemLink>
                <SpecRef>11.2.4</SpecRef>
                <Comment>IMMEDIATE_REL</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <SpecRef>11.2.4</SpecRef>
                <Comment>ARFCN</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <SpecRef>11.2.4</SpecRef>
                <Comment>BSIC</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nc_meas_par_list</Name>
                </ItemLink>
                <SpecRef>11.2.9b</SpecRef>
                <Comment>NC Measurement Parameters Including Frequency List</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>some changes due to GSM 0460d650</Comment>
            </History>
            <History>
                <Date Day="14" Month="12" Year="2000"/>
                <Author>SAB</Author>
                <Comment>nc_meas_par changed to nc_meas_par_list</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PCCCH or PACCH by the network to the mobile station as a fill message with PAGE_MODE or with no content. This Message is defined in [2] 11.2.8 .</Section>
            </Description>
            <MsgDef>
                <Name>d_dl_dummy</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">100101</MsgID>
                <Comment>Packet Downlink Dummy Control Block</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pers_lev</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.14</SpecRef>
                <Comment>PERSISTENCE_LEVEL</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PCCCH or PACCH from the mobile station to the network when the mobile station has no other block to transmit. This Message is defined in [2] 11.2.8b</Section>
            </Description>
            <MsgDef>
                <Name>u_ul_dummy</Name>
                <MsgID Direction="UPLINK" IDType="BIN">000011</MsgID>
                <Comment>Packet Uplink Dummy Control Block</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tlli_value</Name>
                </ItemLink>
                <SpecRef>12.16</SpecRef>
                <Comment>TLLI</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent either on the PACCH if in packet transfer mode or on an assigned block on a PDTCH, from the mobile station to the network to report measurement results. The message may contain measurement results from the Network Control measurements or from the Extended measurements, but not both simultaneously. More than one message may be required depending on the number of measurements to report. This Message is defined in [2] 11.2.9 .</Section>
            </Description>
            <MsgDef>
                <Name>u_meas_report</Name>
                <MsgID Direction="UPLINK" IDType="BIN">000100</MsgID>
                <Comment>Packet Measurement Report</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tlli_value</Name>
                </ItemLink>
                <SpecRef>12.16</SpecRef>
                <Comment>TLLI</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi5_cm</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.9</SpecRef>
                <Comment>PSI5_CHANGE_MARK</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nc_meas_rep</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>11.2.9</SpecRef>
                <Comment>NC Measurement Report</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>xmeas_rep</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>11.2.9</SpecRef>
                <Comment>EXT Measurement Report</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PCCCH or PACCH by the network to a mobile station giving information for NC- and EXT measurement reporting and network controlled cell reselection. If all information does not fit into one message, the remaining information will be sent in other instances of the Packet Measurement Order message. This Message is defined in [2] 11.2.9b</Section>
            </Description>
            <MsgDef>
                <Name>d_meas_order</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">000011</MsgID>
                <Comment>Packet Measurement Order</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>add1</Name>
                </ItemLink>
                <SpecRef>11.2.4</SpecRef>
                <Comment>Address Information1</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pmo_index</Name>
                </ItemLink>
                <SpecRef>11.2.9b</SpecRef>
                <Comment>PMO_INDEX</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pmo_cnt</Name>
                </ItemLink>
                <SpecRef>11.2.9b</SpecRef>
                <Comment>PMO_COUNT</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nc_meas_par_list</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.9b</SpecRef>
                <Comment>NC Measurement Parameters Including Frequency List</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>xmeas_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.9b</SpecRef>
                <Comment>EXT Measurement Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="14" Month="12" Year="2000"/>
                <Author>SAB</Author>
                <Comment>nc_meas_par changed to nc_meas_par_list</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This Message is defined in [2] 11.2.9.</Section>
            </Description>
            <MsgDef>
                <Name>u_ms_tbf_status</Name>
                <MsgID Direction="UPLINK" IDType="BIN">000110</MsgID>
                <Comment>Packet Mobile TBF Status</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>glob_tfi</Name>
                </ItemLink>
                <SpecRef>12.10</SpecRef>
                <Comment>Global TFI</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tbf_cause</Name>
                </ItemLink>
                <SpecRef>11.2.9</SpecRef>
                <Comment>TBF_CAUSE</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type2</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>STATUS_MSG_TYPE</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on PACCH by the network to all mobile stations within the cell that are assigned to the corresponding PDCH, to notify mobile stations that one or more PDCHs will be immediately released and become unavailable for packet data traffic. This Message is defined in [2] 11.2.11 .</Section>
            </Description>
            <MsgDef>
                <Name>d_pdch_release</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">100011</MsgID>
                <Comment>Packet PDCH Release</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>11</SpecRef>
                <Comment>Flag</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ts_available</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>11.2.11</SpecRef>
                <Comment>Timeslots Available</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="20" Month="11" Year="2001"/>
                <Author>CAN</Author>
                <Comment>page mode added, ts_a adapted</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PCCCH or PACCH by the network to the mobile station to solicit four PACKET CONTROL ACKNOWLEDGEMENT messages of access burst format from the mobile station. This Message is defined in [2] 11.2.12 .</Section>
            </Description>
            <MsgDef>
                <Name>d_polling_req</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">000100</MsgID>
                <Comment>Packet Polling Request</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>add2</Name>
                </ItemLink>
                <SpecRef>11.2.12</SpecRef>
                <Comment>Address Information2</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ctrl_ack_type</Name>
                </ItemLink>
                <SpecRef>11.2.12</SpecRef>
                <Comment>CONTROL_ACK_TYPE</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on PACCH by the network to the mobile station in order to update the mobile station timing advance or power control parameters. This Message is defined in [2] 11.2.13 .</Section>
            </Description>
            <MsgDef>
                <Name>d_ctrl_pwr_ta</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">000101</MsgID>
                <Comment>Packet Power Control/Timing Advance</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>add3</Name>
                </ItemLink>
                <SpecRef>11.2.13</SpecRef>
                <Comment>Address Information3</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef/>
                <Comment>spare</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>g_pwr_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.9</SpecRef>
                <Comment>Global Power Control Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Flag2</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gpta</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0 OR flag=1 AND flag2=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Global Packet Timing Advance</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pwr_par</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0 OR flag=1 AND flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Power Control Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
            <History>
                <Date Day="30" Month="11" Year="2000"/>
                <Author>SAB</Author>
                <Comment>Ctrl-field for Power Control Parameters and Global Packet Timing   Advance updated</Comment>
            </History>
            <History>
                <Date Day="29" Month="11" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>swapped Power Control Parameters and Global Packet Timing Advance.</Comment>
            </History>
            <History>
                <Date Day="22" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Change sequence of AND and OR operator in control field of parameter gpta and pwr_par due to CCD constraints.</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PCCCH by the network to all mobile stations within the cell to update the PRACH parameters in between Packet System Information messages containing PRACH parameters. This Message is defined in [2] 11.2.14.</Section>
            </Description>
            <MsgDef>
                <Name>d_prach_par</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">100100</MsgID>
                <Comment>Packet PRACH Parameters</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>prach_ctrl_par</Name>
                </ItemLink>
                <SpecRef>12.14</SpecRef>
                <Comment>PRACH Control Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This Message is defined in [2] 11.2.17 .</Section>
            </Description>
            <MsgDef>
                <Name>u_psi_status_msg</Name>
                <MsgID Direction="UPLINK" IDType="BIN">000111</MsgID>
                <Comment>Packet PSI Status Message</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>glob_tfi</Name>
                </ItemLink>
                <SpecRef>12.10</SpecRef>
                <Comment>Global TFI</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pbcch_change_ma</Name>
                </ItemLink>
                <SpecRef>11.2.18</SpecRef>
                <Comment>PBCCH_CHANGE_MARK</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>received_psi</Name>
                </ItemLink>
                <SpecRef>11.2.17</SpecRef>
                <Comment>Received PSI</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>unknown_psi</Name>
                </ItemLink>
                <SpecRef>11.2.17</SpecRef>
                <Comment>Unknown PSI</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent on the PACCH by the network to the mobile station to assign uplink and/or downlink resources. A mobile allocation or reference frequency list received as part of this assignment message shall be valid until a new assignment is received or each TBF of the MS are terminated. This Message is defined in [2] 11.2.31 .</Section>
            </Description>
            <MsgDef>
                <Name>d_ts_reconfig</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">000111</MsgID>
                <Comment>Packet Timeslot Reconfigure</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>11.2.0.1</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <SpecRef>12.20</SpecRef>
                <Comment>PAGE_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef/>
                <Comment>spare</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>glob_tfi</Name>
                </ItemLink>
                <SpecRef>12.10</SpecRef>
                <Comment>GLOBAL_TFI</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef/>
                <Comment>spare</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>chan_coding_cmd</Name>
                </ItemLink>
                <SpecRef>11.2.31</SpecRef>
                <Comment>CHANNEL_CODING_COMMAND</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gpta</Name>
                </ItemLink>
                <SpecRef>12.12</SpecRef>
                <Comment>Packet Timing Advance</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dl_rlc_mode</Name>
                </ItemLink>
                <SpecRef>11.2.31</SpecRef>
                <Comment>DOWNLINK_RLC_MODE</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ctrl_ack</Name>
                </ItemLink>
                <SpecRef>11.2.31</SpecRef>
                <Comment>CONTROL_ACK</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dl_tfi</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>5</SpecRef>
                <Comment>Downlink TFI</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ul_tfi</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>5</SpecRef>
                <Comment>Uplink TFI</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dl_tn_alloc</Name>
                </ItemLink>
                <SpecRef>12.18</SpecRef>
                <Comment>DOWNLINK_TIMESLOT_ALLOCATION</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>12.8</SpecRef>
                <Comment>Frequency Parameters</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dyn_alloc_ts</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>11.2.31</SpecRef>
                <Comment>Dynamic Allocation</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>f_alloc_re</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>11.2.31</SpecRef>
                <Comment>Fixed allocation Reconfigure</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <Spare>
                    <Pattern>00101011</Pattern>
                    <BitLen>8</BitLen>
                </Spare>
                <Type>S_PADDING_0</Type>
                <Control>
                    <CmdSequence>22</CmdSequence>
                </Control>
                <SpecRef>see [21]</SpecRef>
                <Comment>Spare Padding</Comment>
            </MsgItem>
            <History>
                <Date Day="21" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
            <History>
                <Date Day="11" Month="12" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Rename dyn_alloc to dyn_alloc_p to resolve name equality with RR   structure.</Comment>
            </History>
            <History>
                <Date Day="25" Month="8" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>Downlink TFI before Uplink TFI.</Comment>
            </History>
            <History>
                <Date Day="5" Month="11" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>IE dyn_alloc is different from IE in Packet UL Assignment.</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2003"/>
                <Author>SAB</Author>
                <Comment>S_PADDING_0 is used instead of S_PADDING</Comment>
            </History>
        </Message>
    </MessagesSection>
    <MsgStructElementsSection>
        <Description>
            <Section>This section contains all structured elements that are defined for the GRR AIM</Section>
        </Description>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in the Message Packet Access Reject and is defined in [2] 11.2.1 .</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>reject</Name>
                <Comment>Reject Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>add_reject</Name>
                <Comment>Additional Reject Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tlli_value</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TLLI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>req_ref_tfi</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Packet Request Ref. or Global TFI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>wait</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Wait Structure</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in the structure Reject .</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>wait</Name>
                <Comment>Wait Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ind</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>WAIT_INDICATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>waitsize</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>WAIT INDICATIONSIZE</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Packet Request Ref. or Global TFI is implemented to structure messages according to the CSN1 concept.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>req_ref_tfi</Name>
                <Comment>Packet Request Ref. or Global TFI</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>req_ref_p</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Packet Request Ref.</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>glob_tfi</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Global TFI</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.4</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>add1</Name>
                <Comment>Address Information1</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>glob_tfi</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Global TFI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <Control>
                    <Condition>flag = 1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tlli_value</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TLLI</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.12</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>add2</Name>
                <Comment>Address Information2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>glob_tfi</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Global TFI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Flag2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tlli_value</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1 AND flag2 = 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TLLI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <Control>
                    <Condition>flag = 1 AND flag2 = 1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tqi</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1 AND flag2 = 1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TQI</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.12</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>add3</Name>
                <Comment>Address Information3</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>glob_tfi</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Global TFI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Flag2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tlli_value</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1 AND flag2 = 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TLLI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag3</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1 AND flag2 = 1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Flag3</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tqi</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1 AND flag2 = 1 AND flag3 = 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TQI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>req_ref_p</Name>
                </ItemLink>
                <Control>
                    <Condition>flag = 1 AND flag2 = 1 AND flag3 = 1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Packet Request Ref.</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.29</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>bts_pwr_ctrl</Name>
                <Comment>BTS_PWR_CTRL</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>p0</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BTS_PWR_CTRL_P0</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BTS_PWR_CTRL_MODE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pr_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PR_MODE</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>PR_MODE added</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.17</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>received_psi</Name>
                <Comment>Received PSI</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi_des</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_MSG_TYPE]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>PSI Description</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>add_msg_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Addional Message Type</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.17</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>psi_des</Name>
                <Comment>PSI Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Message Type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psix_cm</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PSIX_CHANGE_MARK</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psix_cnt</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>PSIX_COUNT</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>inst_bitmap</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[psix_cnt+1..16]</TypeModifier>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Instance Bitmap</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>add_msg_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Addional Message Type</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Increase bit-len of psix_cnt to 4.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.17</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>unknown_psi</Name>
                <Comment>Unkown PSI</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_MSG_TYPE]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Message Type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>add_msg_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Addional Message Type</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the Packet Request Reference information element is to provide the information field sent in the Packet Channel Request and the frame number, FN modulo 42432, in which the Packet Channel Request was received. This information element is defined in [2] 12.11.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>req_ref_p</Name>
                <Comment>Packet Request Reference</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>access_info</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RANDOM_ACCESS_INFORMATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>fn_mod</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>FRAME_NUMBER</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="13" Month="7" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Frame Number Field redefined</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Global TFI (Temporary Flow Identifier) information element contains either an uplink TFI or a downlink TFI. The uplink or downlink TFI identifies a single Temporary Block Flow. The definition is in [2] 12.10 .</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>glob_tfi</Name>
                <Comment>Global TFI</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>glob_tfi_assign</Name>
                <Comment>GLOBAL_TFI_ASSIGNMENT</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ul_tfi</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Uplink TFI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dl_tfi</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Downlink TFI</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Channel Request Description information element is sent by the mobile station to the network to request uplink resources an is defined in 12.7 .</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_req_des</Name>
                <Comment>Channel Request Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>peak_thr_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PEAK_THROUGHPUT_CLASS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>radio_prio</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RADIO_PRIORITY</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rlc_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RLC_MODE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>llc_pdu_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>LLC_ PDU_TYPE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rlc_octet_cnt</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RLC_OCTET_COUNT</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Global Packet Timing Advance field describes the timing advance mode and timing advance value assigned to the mobile station for uplink and/or downlink.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gpta</Name>
                <Comment>Global Packet Timing Advance</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ta_value</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>TIMING_ADVANCE_VALUE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ul_ta_index</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>UPLINK_TA_INDEX</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ul_ta_tn</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>UPLINK_TA_TIMESLOT</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dl_ta_index</Name>
                </ItemLink>
                <Control>
                    <Condition>flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>DOWNLINK_TA_INDEX</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dl_ta_tn</Name>
                </ItemLink>
                <Control>
                    <Condition>flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>DOWNLINK_TA_TIMESLOT</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Packet Timing Advance field describes the timing advance mode and timing advance value assigned to the mobile station for uplink or downlink.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pta</Name>
                <Comment>Packet Timing Advance</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ta_value</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>TIMING_ADVANCE_VALUE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ta_index_tn</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef/>
                <Comment>TA index and timeslot structure</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="03" Month="02" Year="2005"/>
                <Author>xparapgu</Author>
                <Comment>AIM optimization</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Frequency Parameters information element defines frequency parameters and a training sequence code (TSC), which may be allocated to a mobile station to define its channel configuration. All timeslots in the channel configuration of the mobile station shall use the same frequency parameters and training sequence code. The frequency parameters may consist of an ARFCN, defining a non-hopping radio frequency channel. The indirect encoding, the direct encoding 1 and the direct encoding 2 defines a hopping radio frequency channel.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>freq_par</Name>
                <Comment>Frequency Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Training Sequence Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0 AND flag2=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>ARFCN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>indi_encod</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0 AND flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Indirect encoding</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>di_encod1</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND flag2=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Direct encoding 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>di_encod2</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Direct encoding 2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in Frequency Parameters.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>indi_encod</Name>
                <Comment>Indirect Encoding</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MAIO</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ma_num</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MA_NUMBER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>chamge_ma_sub</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Change Mark Sub Structure</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in Indirect Encoding.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chamge_ma_sub</Name>
                <Comment>Change Mark Sub Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cm1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CHANGE_MARK_1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cm2</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>CHANGE_MARK_2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in Frequency Parameters.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>di_encod1</Name>
                <Comment>Direct Encoding 1</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MAIO</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_ms_alloc_ie</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Mobile Allocation IE</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in Frequency Parameters.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>di_encod2</Name>
                <Comment>Direct Encoding 2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MAIO</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>hsn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>HSN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>len_ma_list</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Length of MA Frequency List contents</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ma_list</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[len_ma_list +3..19]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>MA Frequency List contents</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in the message Packet Uplink Assignment.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>f_alloc_ul</Name>
                <Comment>Fixed Allocation Uplink Assignment</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ul_tfi_assign</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>UPLINK_TFI_ASSIGNMENT</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>final_alloc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>FINAL_ALLOCATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dl_ctrl_ts</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DOWNLINK_CONTROL_TIMESLOT</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bts_pwr_ctrl</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>BTS_PWR_CTRL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ts_alloc</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TIMESLOT_ALLOCATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pwr_par</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Power Control Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>half_dupelx</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>HALF_DUPLEX_MODE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tbf_s_time</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TBF_STARTING_TIME</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>block_struct</Name>
                </ItemLink>
                <Control>
                    <Condition>flag2=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Block Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>alloc_map</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..127]</TypeModifier>
                    <Condition>flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>ALLOCATION_BITMAP</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in 'Fixed Allocation Uplink Assignment' and 'FA Sub2'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>block_struct</Name>
                <Comment>Blocks Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bl_o_bl_per</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BLOCKS_OR_BLOCK_PERIODS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>a_map_len</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ALLOCATION_BITMAP_LENGTH</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>alloc_map</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[a_map_len..127]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>ALLOCATION_BITMAP</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in the 'Packet Uplink Ack/Nack' message.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>f_alloc_ack</Name>
                <Comment>Fixed Allocation Uplink Ack/Nack</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>final_alloc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>FINAL_ALLOCATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ts_overr</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TS_OVERRIDE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>fa_s2</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>FA Sub2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in Fixed Allocation Uplink Ack/Nack.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>fa_s2</Name>
                <Comment>FA Sub2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tbf_s_time</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TBF_STARTING_TIME</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ts_alloc</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>TIMESLOT_ALLOCATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>block_struct</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Block Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>alloc_map</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..127]</TypeModifier>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>ALLOCATION_BITMAP</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>spare added</Comment>
            </History>
            <History>
                <Date Day="19" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>supplement bit len and pres at spare bit</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This fixed allocation is included in the message 'Packet Timeslot Reconfigure'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>f_alloc_re</Name>
                <Comment>Fixed Allocation Reconfigure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ul_ts_alloc</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>UPLINK_TIMESLOT_ALLOCATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pwr_par</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Power Control Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>final_alloc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>FINAL_ALLOCATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dl_ctrl_ts</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DOWNLINK_CONTROL_TIMESLOT</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bts_pwr_ctrl</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>BTS_PWR_CTRL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>meas_map</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Measurement Mapping</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tbf_s_time</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TBF_STARTING_TIME</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>block_struct</Name>
                </ItemLink>
                <Control>
                    <Condition>flag2=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Block Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>alloc_map</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..127]</TypeModifier>
                    <Condition>flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>ALLOCATION_BITMAP</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Power Control parameters information element contains parameters the mobile station shall use to determine its TX power level.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pwr_par</Name>
                <Comment>Power Control Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Alpha</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gamma_tn</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[8]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>GAMMA Array</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Global Power Control Parameters information element contains parameters the mobile station shall use to determine its TX power level.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>g_pwr_par</Name>
                <Comment>Global Power Control Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ALPHA</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>t_avg_w</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T_AVG_W</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>t_avg_t</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T_AVG_T</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pb</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PB</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pc_meas_chan</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PC_MEAS_CHAN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>imeas_chan_list</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>INT_MEAS_CHANNEL_LIST_AVAIL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>n_avg_i</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>N_AVG_I</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="7" Month="9" Year="1999"/>
                <Author>ID</Author>
                <Comment>N_AVG_I is mandatory</Comment>
            </History>
            <History>
                <Date Day="30" Month="11" Year="2000"/>
                <Author>SAB</Author>
                <Comment>T_ALG_W changed to T_AVG_W</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This field is encoded as the Starting Frame Number Description IE. Depending on the value of the REL_OR_ABS_FN field indicated in this message, the length of this field will be 13 bits</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>tbf_s_time</Name>
                <Comment>TBF Starting Time</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>meas_start_grr</Name>
                <Comment>MEASUREMENT_STARTING_TIME</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rel</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TBF Starting Time Relative</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>abs</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TBF Starting Time Absolute</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="12" Month="7" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>TBF Starting Time Absolute redefined [GSM_04.60] section 10.5.2.38</Comment>
            </History>
            <History>
                <Date Day="13" Month="7" Year="2001"/>
                <Author>ID</Author>
                <Comment>rename meas_start to meas_start_grr</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This Structure summarises the IE for measurement mapping.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>meas_map</Name>
                <Comment>Measurement Mapping</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>meas_start_grr</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MEASUREMENT_STARTING_TIME</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>meas_inter</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MEASUREMENT_INTERVAL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>meas_bitmap</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MEASUREMENT_BITMAP</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="13" Month="7" Year="2001"/>
                <Author>ID</Author>
                <Comment>rename meas_start to meas_start_grr</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Repeated Page info structure is repeated as many times as required to fulfil the number of wanted paged mobiles. If the Paging Request Message is used with only P-TMSIs or TMSIs, the field can be repeated up to four times within one message. If the Paging Request Message is used with only IMSIs, the field can be repeated up to two times within one message.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rep_page_info</Name>
                <Comment>Repeated Page info</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rep_page_s1</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Repeated Page info Sub 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rep_page_s2</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Repeated Page info Sub 2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in 'Repeated Page info'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rep_page_s1</Name>
                <Comment>Repeated Page info Sub1</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ptmsi</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>PTMSI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ms_id</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile_identity</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in 'Repeated Page info'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rep_page_s2</Name>
                <Comment>Repeated Page info Sub 2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tmsi_field</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>TMSI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ms_id</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile_identity</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>chan_need</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CHANNEL_NEEDED</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>emlpp_prio</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>eMLPP_PRIORITY</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Channel Quality Report is included in 'Packet Downlink Ack/Nack'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_qual_rep</Name>
                <Comment>Channel Quality Report</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>c_value</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>C_VALUE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rxqual</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RXQUAL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>signvar</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SIGN_VAR</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilev</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL Structure</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The GPRS Cell Options information element is used to control a set of cell options related to GPRS.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_cell_opt</Name>
                <Comment>GPRS Cell Options</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nmo</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NMO</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>t3168</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T3168</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>t3192</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T3192</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>drx_t_max</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DRX_TIMER_MAX</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ab_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ACCESS_BURST_TYPE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ctrl_ack_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CONTROL_ACK_TYPE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bs_cv_max</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BS_CV_MAX</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pan_struct</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>PAN Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ext_bits</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Extension Structure</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Rename exten to ext_bits, pan to pan_struct and gprs_opt to    gprs_cell_opt.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure contain parameter for handling of counter N3102 during Packet Data Transfer. At each cell reselection the mobile station shall set the counter N3102 to the value defined by the optional broadcast parameter PAN_MAX. Whenever the mobile station receives a Packet Ack/Nack that allows the advancement of V(S), the mobile station shall increment N3102 by the broadcast value PAN_INC, however N3102 shall never exceed the value PAN_MAX. Each time T3182 expires the mobile station shall decrement N3102 by the broadcast value PAN_DEC. When N3102 ??0 is reached, the mobile station shall perform an abnormal release with cell re-selection.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pan_struct</Name>
                <Comment>PAN Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dec</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PAN_DEC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>inc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PAN_INC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pmax</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PAN_MAX</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Rename pan to pan_struct.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Extension Bits information element is used to provide a generalised means for possible future extension within a message. This information element is variable length and contains the length indicator and spare bits.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ext_bits</Name>
                <Comment>Extensions Bits IE</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ext_len</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>extension length</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>spare_ext</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[ext_len+1..64]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>spare bit extensions IE</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Set bit-len of spare_ext to 1, remove point (.) from ctrl field of    spare_ext, add 1 to ext_len in ctrl field of spare_ext, rename exten to   ext_bits.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the PRACH Control Parameters information element is to provide parameters used to control the PRACH utilisation.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>prach_ctrl_par</Name>
                <Comment>PRACH Control Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ac_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ACC_CONTR_CLASS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>max_retrans</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[4]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>MAX_RETRANS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>s_prach</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment/>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tx_int</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TX_INT</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pers_lev</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>PERSISTENCE_LEVEL</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The PCCCH Organization Parameters information element is used to control the organisation of PCCCHs present in the cell. This information element contains general PCCCH organisation parameters.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pccch_org_par</Name>
                <Comment>PCCCH Organization Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bs_pcc_rel</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BS_PCC_REL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bs_pbcch_blks</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BS_PBCCH_BLKS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bs_pag_blks</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BS_PAG_BLKS_RES</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bs_prach_blks</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BS_PRACH_BLKS</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in 'Packet System Information Type 2'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cell_id</Name>
                <Comment>Cell Identification</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>loc_area_ident</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Location Area Identification IE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rac</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RAC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cell_id_ie</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Cell Identity IE</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the Location Area Identification information element is to provide an unambiguous identification of location areas within the area covered by the GSM system.</Section>
                <Section>Reference : [11] section 10.5.1.3 .</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>loc_area_ident</Name>
                <Comment>Location Area Identification</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>mcc</Name>
                </ItemLink>
                <Type>BCD_NOFILL</Type>
                <Control>
                    <TypeModifier>[3]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Country Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>mnc</Name>
                </ItemLink>
                <Type>BCD_MNC</Type>
                <Control>
                    <TypeModifier>[2..3]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Mobile Network Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>lac</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Location Area Code</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>copy from RR</Comment>
            </History>
            <History>
                <Date Day="13" Month="8" Year="2001"/>
                <Author>HM</Author>
                <Comment>3-digit-MNC</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Non GPRS Cell Options IE is used to provide mobile stations operating in mode A or B with a repeated subset of BCCH information required for entering dedicated, group receive or group transmit mode.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>non_gprs_opt</Name>
                <Comment>Non GPRS Cell Options</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>att</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ATT</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>t3212</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>T3212</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>neci</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NECI</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pwcr</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PWRC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>dtx</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DTX</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rl_timeout</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RADIO-LINK-TIMEOUT</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bs_ag_blks_res</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BS_AG_BLKS_RES</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ccch_conf</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CCCH-CONF</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bs_pa_mfrms</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BS-PA-MFRMS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>max_retrans</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MAX-RETRANS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tx_integer</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TX-INTEGER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ec</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>txpwr_max_cch</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MS-TXPDR-MAX-CCCH</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ext_bits</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Extension Bits IE</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Rename exten to ext_bits.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This construction is the representation of the reference frequency lists provided in an instance of the PSI2 message. An RFL_NUMBER field preceding each reference frequency list (RFL) identifies the RFL.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rfl</Name>
                <Comment>Reference Frequency Lists</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rfl_num</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RFL_NUMBER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rfl_cont_len</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Length of RFL contents</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rfl_cont</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[rfl_cont_len+3..19]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>RFL contents</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This construction is a list specifying the referenced set of reference frequency lists for this information element. If the list is not included, this information element refers to the cell allocation defined for the cell.</Section>
                <Section>The number of radio frequency channels included in the referenced set of reference frequency lists or the referenced cell allocation (excluding any duplication of radio frequency channels) is denoted NF. The radio frequency channels shall be arranged by the receiver of this information element in the order of ascending ARFCN, except for ARFCN = 0, if included, which shall be put last. Each radio frequency channel shall then be assigned an ARFCN_INDEX value, ranging from zero, for the first radio frequency channel, to NF-1, for the last radio frequency channel in the ordered set.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rfl_num_list</Name>
                <Comment>Reference Frequency Lists</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rfl_num</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RFL_NUMBER</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the Frequency List information element is to provide the list of the absolute radio frequency channel numbers used in a frequency hopping sequence.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>rfl_cont</Name>
                <Comment>Frequency List</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flist</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Frequency List Contents</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="2" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This construction is a representation of the cell allocation (CA) defined for the cell. The set of radio frequency channels contained in the referenced RFLs in this construction defines the cell allocation.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cell_alloc</Name>
                <Comment>Cell Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rfl_num</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RFL_Number</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This construction is the representation of the GPRS mobile allocations provided in an instance of the PSI2 message. An MA_NUMBER field preceding each GPRS mobile allocation identifies the GPRS mobile allocation. The receiver shall disregard a GPRS mobile allocation provided in this message that is identified by MA_NUMBER = 14 or 15.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_ms_alloc</Name>
                <Comment>GPRS Mobile Allocations</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ma_num</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MA_NUMBER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_ms_alloc_ie</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Mobile Allocation IE</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Mark gprs_ms_alloc_ie as mandatory</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Decrease lower limit of gprs_ms_alloc_ie bit len from 17 to 13</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The GPRS Mobile Allocation information element defines a set of radio frequency channels and a hopping sequence number (HSN), which may be allocated to a mobile station to define its channel configuration.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_ms_alloc_ie</Name>
                <Comment>GPRS Mobile Allocations IE</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>hsn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>HSN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rfl_num_list</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_RFL_NUM_LIST]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>RFL number list</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ma_struct</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>MA Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>arfcn_index_list</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_ARFCN_LIST]</TypeModifier>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>ARFCN index list</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_S1 replaced with flag</Comment>
            </History>
            <History>
                <Date Day="17" Month="1" Year="2001"/>
                <Author>ID</Author>
                <Comment>SAB Change control field of rfl_num_list and arfcn_list: begin with 0 etc. Define arrays with variable length</Comment>
            </History>
            <History>
                <Date Day="26" Month="1" Year="2001"/>
                <Author>ID</Author>
                <Comment>Change arfcn_list to arfcn_index_list</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The MA structure is included in GPRS Mobile Allocations IE.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ma_struct</Name>
                <Comment>MA Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ma_len</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MA_LENGTH</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ma_map</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[ma_len+1..64]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>MA_BITMAP</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="16" Month="1" Year="2001"/>
                <Author>ID</Author>
                <Comment>SAB Remove point (.) from ctrl field of ma_map, add 1 to ma_len in ctrl field of ma_map</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This list is included in GPRS Mobile Allocations IE.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>arfcn_index_list</Name>
                <Comment>ARFCN Index List Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>arfcn_index</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ARFCN index</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="1" Year="2001"/>
                <Author>ID</Author>
                <Comment>Change structure name to arfcn_index_list</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This construction is a representation of the timeslots carrying PCCCH in the cell and their frequency configurations. The preceding training sequence code (TSC) shall be used for each timeslot carrying PCCCH.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pccch_des</Name>
                <Comment>PCCCH Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TSC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nh_pccch_c</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_NH_PCCCH_C]</TypeModifier>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Non-hopping PCCCH carriers</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ma_h_s1</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>MA_NUMBER and Hopping PCCCH carriers</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
            <History>
                <Date Day="4" Month="10" Year="1999"/>
                <Author>ID</Author>
                <Comment>MAX_NH_PCCCH_C added</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.25</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pbcch_des</Name>
                <Comment>PBCCH Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pb</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PB</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TSC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TIMESLOT_NUMBER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Flag2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND flag2=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>ARFCN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>MAIO</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="22" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in '5.60'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>h_pccch_c</Name>
                <Comment>Hopping PCCCH Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MAIO</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ts_alloc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TIMESLOT_ALLOCATION</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in '5.56'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nh_pccch_c</Name>
                <Comment>Non Hopping PCCCH Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ARFCN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ts_alloc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TIMESLOT_ALLOCATION</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in '5.56'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ma_h_s1</Name>
                <Comment>Hopping PCCCH Description and MA_NUMBER</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ma_num</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MA_NUMBER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>h_pccch_c</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_M_H_PCCCH_C]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Hopping PCCCH carriers</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Serving Cell parameters are included in the message PSI3 4.12.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>scell_par</Name>
                <Comment>Serving Cell parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cell_ba</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CELL_BAR_ACCESS_2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>exc_acc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EXC_ACC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_rxlev_access_min</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_RXLEV_ACCESS_MIN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>txpwr_max_cch</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_MS_TXPWR_MAX_CCH</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>hcs_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>HCS Serving Cell parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>multi_band_rep</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MULTIBAND_REPORTING</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The General Cell Selection parameter are included in the message 'Packet System Information Type 3'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gen_cell_par</Name>
                <Comment>General Cell Selection parameter</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_c_hyst</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_CELL_RESELECT_HYSTERESIS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>c31_hyst</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>C31_HYST</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>c32_qual</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>C32_QUAL:</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ra_retry</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RANDOM_ACCESS_RETRY</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>t_resel</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>T_RESEL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ra_re_hyst</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>RA_RESELECT_HYSTERESIS</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="10" Year="2000"/>
                <Author>ID</Author>
                <Comment>Change c51_hyst to c31_hyst</Comment>
            </History>
            <History>
                <Date Day="9" Month="9" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Change short name of parameter RANDOM_ACCESS_RETRY</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Neighbour cell parameters (BA-GPRS) are used to specify one or several groups of neighbouring cells and their corresponding cell selection parameters. Preferably cells with several common cell selection parameters can be grouped together. If PSI3 is not sufficient to specify the cell selection parameters of all neighbouring cells, the remaining frequency groups are specified in PSI3bis.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ncell_par</Name>
                <Comment>Neighbour Cell parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>start_freq</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>START_FREQUENCY</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BSIC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cs_par</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Cell selection parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>n_rest</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NR_OF_REMAINING_CELLS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_diff_len</Name>
                </ItemLink>
                <Control>
                    <CmdSequence>KEEP,1</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>FREQ_DIFF_LENGTH</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ncell_par_rest</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[n_rest..MAX_FREQ_DIFF_CS_PAR]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Neighbour Cell parameters Rest</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="11" Year="2000"/>
                <Author>GSP</Author>
                <Comment>ctrl of ncell_par_rest starts not with 0 but with n_rest</Comment>
            </History>
            <History>
                <Date Day="11" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Neighbour Cell Parameters Rest includes a bit field with variable length</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>ncell_par_rest_dl0 through ncell_par_rest_dl7 replaced by an array of   ncell_par_rest, freq_diff_len is stored in CCD register</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Extract BSIC from cell selection parameter.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in Neighbour Cell parameters, Neighbour Cell parameters, List of added Frequency, Neighbour Cell parameters Rest and List of added Frequency Sub.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cs_par</Name>
                <Comment>Cell selection parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cell_ba</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CELL_BAR_ACCESS_2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>exc_acc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EXC_ACC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>same_ra_scell</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SAME_RA_AS_SERVING_CELL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cs_par_s1</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Cell selection parameters Sub 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cs_par_s2</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Cell selection parameters Sub 2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_resel_off</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_RESELECT_OFFSET</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>hcs_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>HCS parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>si13_pbcch</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>SI13_PBCCH_LOCATION</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove BSIC from Cell Selection Parameters</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included Cell Selection Parameters.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si13_pbcch</Name>
                <Comment>SI13_PBCCH_LOCATION structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>si13_loc</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>SI13_LOCATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>si13_pbcch_s1</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>SI13_PBCCH_LOCATION Sub 1</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure contains parameter for hierarchical cell structures (HCS).</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>hcs_par</Name>
                <Comment>HCS Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_prio_class</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_PRIORITY_CLASS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_hcs_thr</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_HCS_THR</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Correction of typing error (gprs_hsc_thr to gprs_hcs_thr)</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included SI13_PBCCH_LOCATION structure</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si13_pbcch_s1</Name>
                <Comment>SI13_PBCCH_LOCATION sub1</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pbcch_loc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PBCCH_LOCATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi1_rep_per</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PSI1_REPEAT_PERIOD</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This is a sub-structure of Cell Selection .</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cs_par_s1</Name>
                <Comment>Cell Selection Parameters Sub 1</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_rxlev_access_min</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_RXLEV_ACCESS_MIN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>txpwr_max_cch</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_MS_TXPWR_MAX_CCH</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This is a sub-structure of Cell Selection .</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cs_par_s2</Name>
                <Comment>Cell selection parameters Sub 2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_temp_offset</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_TEMPORARY_OFFSET</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_penalty_time</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_PENALTY_TIME</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.21</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ncell_par2</Name>
                <Comment>Neighbour Cell parameters 2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>generation</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GENERATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ncell_par2_des</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_BASIC_CELL_IN_NCELL2]</TypeModifier>
                    <Condition>generation=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Neighbour Cell parameters 2 Description</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ncell_par2_set</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[(TAKE,2)+1..MAX_NEIGHBOR_PARAMETER_SET_IN_NCELL2]</TypeModifier>
                    <Condition>generation=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Neighbour Cell parameters 2 Parameter Set</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>New CCD command TAKE is used, type of ncell_par2_des is changed</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.21</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ncell_par2_des</Name>
                <Comment>Neighbour Cell parameters 2 Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ncell_par2_s1</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_REMAINING_CELL_IN_NCELL2]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Neighbour Cell parameters 2 Description Sub 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>para_ptr</Name>
                </ItemLink>
                <Control>
                    <CmdSequence>MAX,2</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>CELL_PARAMS_POINTER</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>New CCD command MAX is used, type of ncell_par2_s1 is changed</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.21</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ncell_par2_s1</Name>
                <Comment>Neighbour Cell parameters 2 Description Sub 1</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>start_freq</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>START_FREQUENCY</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>same_ra_scell</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SAME_RA_AS_SERVING_CELL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cell_ba</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CELL_BAR_ACCESS_2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bcc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BTS Colour Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>n_r_cells</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NR_OF_REMAINING_CELLS2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_diff_len</Name>
                </ItemLink>
                <Control>
                    <Condition>n_r_cells # 0</Condition>
                    <CmdSequence>KEEP,1</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>FREQ_DIFF_LENGTH</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ncell_par2_s2</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..MAX_NCELL_PAR2_S2]</TypeModifier>
                    <Condition>n_r_cells # 0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Neighbour Cell parameters 2 Description Sub 2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Neighbour Cell Parameters 2 Description Sub 2 includes a bit field with variable length</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>ncell_par2_s2_dl0 through ncell_par2_s2_dl7 replaced by an array of   ncell_par2_s2, freq_diff_len is stored in CCD register</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.21</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ncell_par2_set</Name>
                <Comment>Neighbour Cell parameters 2 Parameter Set</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ncc</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Network Colour Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>exc_acc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EXC_ACC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_rxlev_access_min</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_RXLEV_ACCESS_MIN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>txpwr_max_cch</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_MS_TXPWR_MAX_CCH</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_prio_class</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_PRIORITY_CLASS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_hcs_thr</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_HCS_THR</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>si13_pbcch</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>SI13_PBCCH_LOCATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_temp_offset</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_TEMPORARY_OFFSET</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_penalty_time</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_PENALTY_TIME</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_resel_off</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS_RESELECT_OFFSET</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="10" Year="2000"/>
                <Author>ID</Author>
                <Comment>SI13_PBCCH_LOCATION added</Comment>
            </History>
            <History>
                <Date Day="3" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Correction of typing error (gprs_hsc_thr to gprs_hcs_thr)</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in the message Packet System Information Type 4.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_list_imeas</Name>
                <Comment>Channel List for Interference measurements</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>chan_group</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Channel group structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>chan_list2</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0..MAX_CHAN_LIST]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Channel list structure</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="10" Year="2000"/>
                <Author>ID</Author>
                <Comment>MAX_CHAN_LIST added. One instance can have max. 22 Bytes. Therefore MAX_CHAN_LIST= 7. One Channel List have min 20 bits.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in Channel List for Interference measurements.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_list2</Name>
                <Comment>Channel List Structure 2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>chan_group</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Channel group structure</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in Channel List Structure 2.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_group</Name>
                <Comment>Channel group structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>arfcn</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>ARFCN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ma_num_maio</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>MA_NUMBER and MAIO</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ts_alloc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TIMESLOT_ALLOCATION</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in the 'Channel group structure'</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ma_num_maio</Name>
                <Comment>MA_NUMBER and MAIO</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ma_num</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MA_NUMBER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>MAIO</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in the messages 'Packet Cell Change Order' and 'Packet Measurement Order'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nc_meas_par_list</Name>
                <Comment>NC Measurement Parameters Including Frequency List</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nc_meas_par</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NC Measurement Parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nc_freq_list</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>NC_FREQUENCY_LIST</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="14" Month="12" Year="2000"/>
                <Author>SAB</Author>
                <Comment>Structure renamed</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Parameter nc_meas_par set to mandatory, nc_freq_list is no longer an   array</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in the message 'Packet System Information Type 5' and the structure 'NC Measurement Parameters Including Frequency List'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nc_meas_par</Name>
                <Comment>NC Measurement Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ctrl_order</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NETWORK_CONTROL_ORDER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nc_meas_per</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>NC Measurement Periods</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="14" Month="12" Year="2000"/>
                <Author>SAB</Author>
                <Comment>Structure renamed</Comment>
            </History>
            <History>
                <Date Day="09" Month="02" Year="2005"/>
                <Author>xparapgu</Author>
                <Comment>AIM optimization</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in 'NC Measurement Parameters Including Frequency List'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nc_freq_list</Name>
                <Comment>NC_FREQUENCY_LIST</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>list_rf</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>List of removed Frequency</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>list_af</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[1..MAX_LIST_AFREQ]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>List of added Frequency</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Rename MAX_LIST_AF to MAX_LIST_AFREQ, the number of lists of   added frequencies is now variable, rename nc_s1 to list_rf</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in 'NC_FREQUENCY_LIST'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>list_rf</Name>
                <Comment>List of removed Frequency</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>num_rfreq</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NR_OF_REMOVED_FREQ</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rfreq_index</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[num_rfreq+1.. MAX_RFREQ]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>REMOVED_FREQ_INDEX</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>rfreq_index set to mandatory, rename the whole element</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in 'NC_FREQUENCY_LIST'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>list_af</Name>
                <Comment>List of added Frequency</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>start_freq</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>START_FREQUENCY</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BSIC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cs_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Cell selection parameters</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nr_freq</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NR_OF_FREQUENCY</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_diff_len</Name>
                </ItemLink>
                <Control>
                    <CmdSequence>KEEP,1</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>FREQ_DIFF_LENGTH</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>afreq_s</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[nr_freq..MAX_AFREQ]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>List of added Frequency Sub</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>afreq_s_dl0 through afreq_s_dl7 replaced by an array of afreq_s,   freq_diff_len is stored in CCD register, replace cs_par_t1 by cs_par</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The 'EXT measurement parameters struct' contains the EXT Measurement Order, the EXT parameters and one or more EXT Frequency List structs. The EXT Frequency List struct is a frequency list which contains frequencies to be measured</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>xmeas_par</Name>
                <Comment>EXT Measurement Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>xmeas_order</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EXT_MEASUREMENT_ORDER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>em1</Name>
                </ItemLink>
                <Control>
                    <Condition>xmeas_order=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Ext. Measurement Struct</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d650</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Replace flag and flag2 by xmeas_order.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure contains parameter for ext. measurement.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>em1</Name>
                <Comment>EXT Measurement Struct</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>xrep_type</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>EXT_REPORTING_TYPE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ncc_permitted</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND xrep_type=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>NCC_PERMITTED</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND xrep_type=2</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Flag2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>int_freq</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1 AND xrep_type=2 AND flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>INT_FREQUENCY</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>xrep_per</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>EXT_REPORTING_PERIOD</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>xfreq_list</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EXT FREQUENCY LIST</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>xfreq_list2</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <Control>
                    <TypeModifier>[0.. MAX_EXT_FREQ_LIST]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>EXT FREQUENCY LIST</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="10" Year="2000"/>
                <Author>ID</Author>
                <Comment>MAX_EXT_FREQ_LIST added. MAX_EXT_FREQ_LIST=7. One instance of PSI5 can have maximum 22 bytes, therefore there can be up to 8 (MAX_EXT_FREQ_LIST + xfreq_list) extended frequency lists.</Comment>
            </History>
            <History>
                <Date Day="13" Month="10" Year="2000"/>
                <Author>ID</Author>
                <Comment>Flag_2bit value exchanged in NCC_PERMITED and flag4</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Delete spare bit.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Replace flag_2bit by xrep_type, replace flag4 by flag2.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in the 'EXT Measurement Struct'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>xfreq_list</Name>
                <Comment>EXT FREQUENCY LIST</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>xfreq_list2</Name>
                <Comment>EXT FREQUENCY LIST</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>start_freq</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>START_FREQUENCY</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nr_freq</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NR_OF_FREQUENCY</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_diff_len</Name>
                </ItemLink>
                <Control>
                    <CmdSequence>KEEP,1</CmdSequence>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>FREQ_DIFF_LENGTH</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_diff_struct</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[nr_freq..MAX_EXT_FREQ_LIST_ELEM]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>FREQ_DIFF_STRUCT</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>FREQ_DIFF expanded to FREQ_DIFF_1 through FREQ_DIFF_7, definition of a   bit field with variable length.</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>FREQ_DIFF_1 through FREQ_DIFF_7 replaced by an array of    FREQ_DIFF_STRUCT, freq_diff_len is stored in CCD register</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in the message Packet System Information Type 13.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>si13_cm_gprs_alloc</Name>
                <Comment>SI13_CHANGE_MARK and GPRS Alloc</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>si13_cm</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SI13_CHANGE_MARK</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_ms_alloc_ie</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Mobile Allocation IE</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="2" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>SI13 only contains MA IE, not MA</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in Packet System Information Type 13 if PBCCH is not present in the cell.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pbcch_n_pres</Name>
                <Comment>PBCCH not present in cell structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rac</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RAC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>spgc_ccch_sup</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SPGC_CCCH_SUP</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>prio_acc_thr</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PRIORITY_ACCESS_THR</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ctrl_order</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NETWORK_CONTROL_ORDER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gprs_cell_opt</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Cell Options</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi13_pwr_par</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS Power Control Parameters</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Rename gprs_opt to gprs_cell_opt.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Global Power Control Parameters information element contains parameters the mobile station shall use to determine its TX power level.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>psi13_pwr_par</Name>
                <Comment>PSI13 Power Control Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ALPHA</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>t_avg_w</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T_AVG_W</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>t_avg_t</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T_AVG_T</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pc_meas_chan</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PC_MEAS_CHAN</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>n_avg_i</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>N_AVG_I</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="11" Year="2000"/>
                <Author>SAB</Author>
                <Comment>T_ALG_W changed to T_AVG_W</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The structure is included in the message 'Packet Measurement Report'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nc_meas_rep</Name>
                <Comment>NC Measurement Report</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nc_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NC_MODE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rxlev_scell</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RXLEV_SERVING_CELL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>i_scell</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>INTERFERENCE_SERVING_CELL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>num_nc_meas</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NUMBER_OF_NC_MEASUREMENTS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>nc_meas_s1</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[num_nc_meas..MAX_NCMP_S1]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>NC Measurement Report Sub1</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This struct is a sub structure of 'NC Measurement Report'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nc_meas_s1</Name>
                <Comment>NC Measurement Report Sub1</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_n</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>FREQUENCY_N</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>BSIC_N</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rxlev_n</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RXLEV_N</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is a sub structure of 'Packet Measurement Report'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>xmeas_rep</Name>
                <Comment>EXT Measurement Report</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>xrep_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>EXT_REPORTING_TYPE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilev_abs</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL Absolute Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>num_meas</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NUMBER_OF_MEASUREMENTS</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ext_mp_s1</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[num_meas..MAX_XMR_S1]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>EXT Measurement Report Sub1</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Replace ilev by ilev_abs due to different bit length needed</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in 'Packet Downlink Ack/Nack' and 'Packet Resource Request'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ilev</Name>
                <Comment>I_LEVEL Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilev0</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_TN0</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilev1</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_TN1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilev2</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_TN2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilev3</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_TN3</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilev4</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_TN4</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilev5</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_TN5</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilev6</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_TN6</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilev7</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_TN7</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in 'EXT Measurement Report'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ilev_abs</Name>
                <Comment>I_LEVEL Absolute Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilevabs0</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_ABS_TN0</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilevabs1</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_ABS_TN1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilevabs2</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_ABS_TN2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilevabs3</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_ABS_TN3</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilevabs4</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_ABS_TN4</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilevabs5</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_ABS_TN5</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilevabs6</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_ABS_TN6</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ilevabs7</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>I_LEVEL_ABS_TN7</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This is a sub structure of 'EXT Measurement Report'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ext_mp_s1</Name>
                <Comment>EXT Measurement Report Sub1</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_n</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>FREQUENCY_N</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>BSIC_N</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rxlev_n</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>RXLEV_N</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This information element contains parameters necessary to define the radio resources of a Single Block allocation. For example for sending of a PACKET RESOURCE REQUEST message in a two phase access or a Measurement report.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>sin_alloc</Name>
                <Comment>Single Block Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TIMESLOT_NUMBER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>alf_gam</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>ALPHA and GAMMA</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bts_pwr_ctrl</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>BTS_PWR_CTRL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tbf_s_time</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>TBF_STARTING_TIME</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="7" Month="12" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>ALPHA added</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This information element contains parameters necessary to define the radio resources of a dynamic allocation or an extended dynamic allocation.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>dyn_alloc_p</Name>
                <Comment>Dynamic Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>xdyn_alloc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Extended Dynamic Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>flag2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>p0</Name>
                </ItemLink>
                <Control>
                    <Condition>flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>BTS_PWR_CTRL_P0</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pr_mode</Name>
                </ItemLink>
                <Control>
                    <Condition>flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>PR_MODE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>usf_grant</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>USF_GRANULARITY</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ul_tfi_assign</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>UPLINK_TFI_ASSIGNMENT</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rlc_db_granted</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>RLC_DATA_BLOCKS_GRANTED</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tbf_s_time</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>TBF_STARTING_TIME</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tn_alloc</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[8]</TypeModifier>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Timeslot Allocation Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tn_alloc_pwr</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Timeslot Allocation with Power Control Parameters</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="8" Year="1999"/>
                <Author>SL</Author>
                <Comment>CSN1_0 replaced with flag</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>PR_MODE,flag2 added</Comment>
            </History>
            <History>
                <Date Day="11" Month="12" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Define usf and gamma tables as arrays.</Comment>
            </History>
            <History>
                <Date Day="11" Month="12" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Rename dyn_alloc to dyn_alloc_p to resolve name equality with RR   structure.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This message is included in Dynamic Allocation.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>tn_alloc</Name>
                <Comment>Timeslot Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>usf</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>USF_TN</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="12" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Define usf table as array.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This message is included in Dynamic Allocation.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>tn_alloc_pwr</Name>
                <Comment>Timeslot Allocation with Power Control Parameters</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ALPHA</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>usf_array</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[8]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>USF and GAMMA Array</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="12" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Define usf and gamma tables as arrays.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This message is included in Dynamic Allocation.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>usf_g</Name>
                <Comment>USF_TN and GAMMA_TN</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>usf</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>USF</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gamma</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GAMMA</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="12" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Define usf and gamma tables as arrays.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The PERISTENCE_LEVEL field indicates the values of the access persistence level P(i) for each Radio Priority i (i = 1..4) where Radio Priority 1 represents the highest Radio Priority of an LLC PDU to be transmitted.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pers_lev</Name>
                <Comment>Persistence Level Structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>plev</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[4]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Persistence Level Radio Prio 1</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The Ack/Nack Description information element contains the RLC parameters used to acknowledge or negatively acknowledge a group of RLC data blocks.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ack_nack_des</Name>
                <Comment>Ack/Nack Description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>f_ack_ind</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>FINAL_ACK_INDICATION</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ssn</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>STARTING_SEQUENCE_NUMBER</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rbb</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[64]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>RECEIVED_BLOCK_BITMAP</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the Mobile Identity information element is to provide either the international mobile subscriber identity, IMSI, the temporary mobile subscriber identity, TMSI, the international mobile equipment identity, IMEI or the international mobile equipment identity together with the software version number, IMEISV.</Section>
                <Section>Reference : [11] section 10.5.1.4</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ms_id</Name>
                <Comment>Mobile Identity</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ms_id_len</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Length of Mobile Identity</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ident_digit</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[ms_id_len..15]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>value part</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>tmsi added</Comment>
            </History>
            <History>
                <Date Day="9" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="11" Month="9" Year="2001"/>
                <Author>ID</Author>
                <Comment>add value part</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the Starting Time information element is to provide the start TDMA frame number, FN modulo 42432.</Section>
                <Section>Reference : [GSM_04.08] section 10.5.2.38</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>abs</Name>
                <Comment>TBF Starting Time Absolute</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>fn_mod</Name>
                <Comment>FRAME_NUMBER</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>t1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T1'</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>t3</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T3</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>t2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>T2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="7" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The GAMMA Array provides an individiual GAMMA value for each timeslot.</Section>
                <Section>Reference : [GSM_04.60] section 12.13</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gamma_tn</Name>
                <Comment>Gamma Array</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gamma</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>GAMMA_TN</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="12" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This message is included in Dynamic Allocation.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>usf_array</Name>
                <Comment>USF and GAMMA Array</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>usf_g</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>USF_TN and GAMMA_TN</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="12" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Define usf and gamma tables as arrays.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This message is included in Dynamic Allocation.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>alf_gam</Name>
                <Comment>ALPHA and GAMMA</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>alpha</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>AlPHA</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>gamma</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GAMMA</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="12" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Define usf and gamma tables as arrays.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The FREQ_DIFF_STRUCT is used to define a FREQ_DIFF field with variable bit length.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>freq_diff_struct</Name>
                <Comment>FREQ_DIFF_STRUCT</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_diff</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[.(TAKE,1)+1..8]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>FREQ_DIFF</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in 'Neighbour Cell parameters'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ncell_par_rest</Name>
                <Comment>Neighbour Cell parameters Rest</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_diff_struct</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>FREQ_DIFF_STRUCT</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BSIC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cs_par</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Cell selection parameters</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [2] 11.2.21</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ncell_par2_s2</Name>
                <Comment>Neighbour Cell parameters 2 Description Sub 2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_diff_struct</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>FREQ_DIFF_STRUCT</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>same_ra_scell</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SAME_RA_AS_SERVING_CELL</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cell_ba</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CELL_BAR_ACCESS_2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bcc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BTS Colour Code</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure is included in 'List of added Frequency'.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>afreq_s</Name>
                <Comment>List of added Frequency Sub</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>freq_diff_struct</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>FREQ_DIFF_STRUCT</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>BSIC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>cs_par</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>Cell selection parameters</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This information element contains parameters necessary to define the radio resources of a dynamic allocation or an extended dynamic allocation.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>dyn_alloc_ts</Name>
                <Comment>Dynamic Allocation</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>xdyn_alloc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Extended Dynamic Allocation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>flag2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>p0</Name>
                </ItemLink>
                <Control>
                    <Condition>flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>BTS_PWR_CTRL_P0</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pr_mode</Name>
                </ItemLink>
                <Control>
                    <Condition>flag2=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>PR_MODE</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>usf_grant</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>USF_GRANULARITY</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rlc_db_granted</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>RLC_DATA_BLOCKS_GRANTED</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tbf_s_time</Name>
                </ItemLink>
                <Type>CSN1_S1</Type>
                <SpecRef>-</SpecRef>
                <Comment>TBF_STARTING_TIME</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>flag</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Flag</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tn_alloc</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[8]</TypeModifier>
                    <Condition>flag=0</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Timeslot Allocation Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>tn_alloc_pwr</Name>
                </ItemLink>
                <Control>
                    <Condition>flag=1</Condition>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Timeslot Allocation with Power Control Parameters</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="5" Month="11" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>IE dyn_alloc is different from IE in Packet UL Assignment.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section/>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ta_index_tn</Name>
                <Comment>TA index and timeslot structure</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ta_index</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>TA_INDEX</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>ta_tn</Name>
                </ItemLink>
                <SpecRef/>
                <Comment>TA_TIMESLOT</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="03" Month="02" Year="2005"/>
                <Author>xparapgu</Author>
                <Comment>AIM optimization</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section/>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>psi1_pbcch_info</Name>
                <Comment>PSI1 and PBCCH info</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>psi1_rep_per</Name>
                </ItemLink>
                <SpecRef>11.2.25</SpecRef>
                <Comment>PSI1_REPEAT_PERIOD</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>pbcch_des</Name>
                </ItemLink>
                <SpecRef>11.2.25</SpecRef>
                <Comment>PBCCH Description</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="03" Month="02" Year="2005"/>
                <Author>xparapgu</Author>
                <Comment>AIM optimization</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This structure contains the values for measurement periods used in NC Measurements.</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nc_meas_per</Name>
                <Comment>NC Measurement Periods</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>non_drx_per</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NC_NON_DRX_PERIOD</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rep_per_i</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NC_REPORTING_PERIOD_I</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">grr</DocName>
                    <Name>rep_per_t</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NC_REPORTING_PERIOD_T</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="09" Month="02" Year="2005"/>
                <Author>xparapgu</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
    </MsgStructElementsSection>
    <MsgBasicElementsSection>
        <Description>
            <Section>This section contains all basic elements that are defined for the GRR AIM</Section>
        </Description>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ps</Name>
                <BitLen>1</BitLen>
                <Comment>Pseudo Synchronisation capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_1</Name>
                <BitLen>1</BitLen>
                <Comment>A5/1</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_2</Name>
                <BitLen>1</BitLen>
                <Comment>A5/2</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_3</Name>
                <BitLen>1</BitLen>
                <Comment>A5/3</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_4</Name>
                <BitLen>1</BitLen>
                <Comment>A5/4</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_5</Name>
                <BitLen>1</BitLen>
                <Comment>A5/5</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_6</Name>
                <BitLen>1</BitLen>
                <Comment>A5/6</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>a5_7</Name>
                <BitLen>1</BitLen>
                <Comment>A5/7</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>vgcs</Name>
                <BitLen>1</BitLen>
                <Comment>Voice Group Call Service</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>vbs</Name>
                <BitLen>1</BitLen>
                <Comment>Voice Broadcast Service</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>es_ind</Name>
                <BitLen>1</BitLen>
                <Comment>Early Classmark Sending</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_edac</Name>
                <BitLen>1</BitLen>
                <Comment>GPRS Extended Dynamic Allocation Capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>final_alloc</Name>
                <BitLen>1</BitLen>
                <Comment>FINAL_ALLOCATION</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>half_dupelx</Name>
                <BitLen>1</BitLen>
                <Comment>HALF_DUPLEX_MODE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>same_ra_scell</Name>
                <BitLen>1</BitLen>
                <Comment>SAME_RA_AS_SERVING_CELL</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>repeat_alloc</Name>
                <BitLen>1</BitLen>
                <Comment>REPEAT_ALLOCATION</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>si15_ind</Name>
                <BitLen>1</BitLen>
                <Comment>SI15_IND</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>flag</Name>
                <BitLen>1</BitLen>
                <Comment>Flag</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>flag2</Name>
                <BitLen>1</BitLen>
                <Comment>Flag2</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>flag3</Name>
                <BitLen>1</BitLen>
                <Comment>Flag3</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>inst_bitmap</Name>
                <BitLen>1</BitLen>
                <Comment>Instance Bitmap Element</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ul_release</Name>
                <BitLen>1</BitLen>
                <Comment>UPLINK_RELEASE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dl_release</Name>
                <BitLen>1</BitLen>
                <Comment>DOWNLINK_RELEASE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>[22] GSM 04.08 section 10.5..5.12a (MS Radio access capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>flag_grr_ra_cap_2</Name>
                <BitLen>1</BitLen>
                <Comment>Valid flag for MS RA capability value part II</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ps</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>flag4 added</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Change bit to inst_bitmap.</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove flag4.</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2001"/>
                <Author>ROZ</Author>
                <Comment>MS RA Capabilities</Comment>
            </History>
            <History>
                <Date Day="9" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add flag_grr_ra_cap_2</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This IE is in [2] 11.2.0.1 defined.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>msg_type</Name>
                <BitLen>6</BitLen>
                <Comment>Message Type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_msg_type</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This IE is in [2] 11.2.0.1 defined.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>msg_type2</Name>
                <BitLen>6</BitLen>
                <Comment>Message Type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_msg_type</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The PAGE_MODE field controls the action of the mobile station belonging to the paging subgroup corresponding to the paging sub channel.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>page_mode</Name>
                <BitLen>2</BitLen>
                <Comment>Page Mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_page_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The Temporary Queuing Identifier (TQI) field identifies a mobile station during the queuing procedure. The contents of this field are operator defined.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>tqi</Name>
                <BitLen>16</BitLen>
                <Comment>TQI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the reason for requesting the access. It shall be included only in response to a single block assignment.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>access_type</Name>
                <BitLen>2</BitLen>
                <Comment>Access Type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_access_type</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The Temporary Logical Link Identity (TLLI) is associated with the GPRS subscriber.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>tlli_value</Name>
                <BitLen>32</BitLen>
                <Comment>TLLI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The Temporary Logical Link Identity (TLLI) is associated with the GPRS subscriber.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cr_tlli</Name>
                <BitLen>32</BitLen>
                <Comment>CONTENTION_RESOLUTION_TLLI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the mobile station's stored MA_CHANGE_MARK for the current cell. If the mobile station does not have a valid MA_CHANGE_MARK for the current cell, the mobile station shall omit this field. The coding of this field is network dependent. This IE is described in [2]11.2.16</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ma_ch_mark</Name>
                <BitLen>2</BitLen>
                <Comment>MA_CHANGE_MARK</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the mobile station's stored MA_CHANGE_MARK for the current cell. If the mobile station does not have a valid MA_CHANGE_MARK for the current cell, the mobile station shall omit this field. The coding of this field is network dependent. This IE is described in [2]11.2.16</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cm1</Name>
                <BitLen>2</BitLen>
                <Comment>CHANGE_MARK_1</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the mobile station's stored MA_CHANGE_MARK for the current cell. If the mobile station does not have a valid MA_CHANGE_MARK for the current cell, the mobile station shall omit this field. The coding of this field is network dependent. This IE is described in [2]11.2.16</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cm2</Name>
                <BitLen>2</BitLen>
                <Comment>CHANGE_MARK_2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the mobile station's stored MA_CHANGE_MARK for the current cell. If the mobile station does not have a valid MA_CHANGE_MARK for the current cell, the mobile station shall omit this field. The coding of this field is network dependent. This IE is described in [2]11.2.16</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi2_cm</Name>
                <BitLen>2</BitLen>
                <Comment>PSI2_CHANGE_MARK</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the mobile station's stored MA_CHANGE_MARK for the current cell. If the mobile station does not have a valid MA_CHANGE_MARK for the current cell, the mobile station shall omit this field. The coding of this field is network dependent. This IE is described in [2]11.2.16</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi3_cm</Name>
                <BitLen>2</BitLen>
                <Comment>PSI3_CHANGE_MARK</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the mobile station's stored MA_CHANGE_MARK for the current cell. If the mobile station does not have a valid MA_CHANGE_MARK for the current cell, the mobile station shall omit this field. The coding of this field is network dependent. This IE is described in [2]11.2.16</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi4_cm</Name>
                <BitLen>2</BitLen>
                <Comment>PSI4_CHANGE_MARK</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the mobile station's stored MA_CHANGE_MARK for the current cell. If the mobile station does not have a valid MA_CHANGE_MARK for the current cell, the mobile station shall omit this field. The coding of this field is network dependent. This IE is described in [2]11.2.16</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi5_cm</Name>
                <BitLen>2</BitLen>
                <Comment>PSI5_CHANGE_MARK</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the mobile station's stored MA_CHANGE_MARK for the current cell. If the mobile station does not have a valid MA_CHANGE_MARK for the current cell, the mobile station shall omit this field. The coding of this field is network dependent. This IE is described in [2]11.2.16</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>si13_cm</Name>
                <BitLen>2</BitLen>
                <Comment>SI13_CHANGE_MARK</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the mobile station's stored MA_CHANGE_MARK for the current cell. If the mobile station does not have a valid MA_CHANGE_MARK for the current cell, the mobile station shall omit this field. The coding of this field is network dependent. This IE is described in [2]11.2.16</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psix_cm</Name>
                <BitLen>2</BitLen>
                <Comment>PSIX_CHANGE_MARK</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the value of the C parameter calculated by the mobile station (see GSM 05.08). This field is encoded as the binary representation of the C parameter value defined in GSM 05.08.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>c_value</Name>
                <BitLen>6</BitLen>
                <Comment>C_VALUE</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the RXQUAL parameter field calculated by the mobile station (see GSM 05.08). This field is encoded as defined in GSM 04.08.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rxqual</Name>
                <BitLen>3</BitLen>
                <Comment>RXQUAL</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the signal variance parameter SIGN_VAR calculated by the mobile station (see</Section>
                <Section>GSM 05.08). The SIGN_VAR is    &gt;(value*0,25)dB 2 to ((value+1)*0,25) dB 2 and 0b111111 means &gt; 15,75 dB 2</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>signvar</Name>
                <BitLen>6</BitLen>
                <Comment>SIGN_VAR</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the ??value calculated on timeslots 0 through 7, respectively. The ??value is defined in GSM 05.08. These fields are transferred only when the mobile station is in packet transfer mode. These fields are encoded relative to C_VALUE as defined for the mapping defined in GSM 05.08 for interference level (I_LEVEL).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilev0</Name>
                <BitLen>4</BitLen>
                <Comment>I_LEVEL_TNO</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the ??value calculated on timeslots 0 through 7, respectively. The ??value is defined in GSM 05.08. These fields are transferred only when the mobile station is in packet transfer mode. These fields are encoded relative to C_VALUE as defined for the mapping defined in GSM 05.08 for interference level (I_LEVEL).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilev1</Name>
                <BitLen>4</BitLen>
                <Comment>I_LEVEL_TN1</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the ??value calculated on timeslots 0 through 7, respectively. The ??value is defined in GSM 05.08. These fields are transferred only when the mobile station is in packet transfer mode. These fields are encoded relative to C_VALUE as defined for the mapping defined in GSM 05.08 for interference level (I_LEVEL).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilev2</Name>
                <BitLen>4</BitLen>
                <Comment>I_LEVEL_TN2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the ??value calculated on timeslots 0 through 7, respectively. The ??value is defined in GSM 05.08. These fields are transferred only when the mobile station is in packet transfer mode. These fields are encoded relative to C_VALUE as defined for the mapping defined in GSM 05.08 for interference level (I_LEVEL).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilev3</Name>
                <BitLen>4</BitLen>
                <Comment>I_LEVEL_TN3</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the ??value calculated on timeslots 0 through 7, respectively. The ??value is defined in GSM 05.08. These fields are transferred only when the mobile station is in packet transfer mode. These fields are encoded relative to C_VALUE as defined for the mapping defined in GSM 05.08 for interference level (I_LEVEL).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilev4</Name>
                <BitLen>4</BitLen>
                <Comment>I_LEVEL_TN4</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the ??value calculated on timeslots 0 through 7, respectively. The ??value is defined in GSM 05.08. These fields are transferred only when the mobile station is in packet transfer mode. These fields are encoded relative to C_VALUE as defined for the mapping defined in GSM 05.08 for interference level (I_LEVEL).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilev5</Name>
                <BitLen>4</BitLen>
                <Comment>I_LEVEL_TN5</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the ??value calculated on timeslots 0 through 7, respectively. The ??value is defined in GSM 05.08. These fields are transferred only when the mobile station is in packet transfer mode. These fields are encoded relative to C_VALUE as defined for the mapping defined in GSM 05.08 for interference level (I_LEVEL).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilev6</Name>
                <BitLen>4</BitLen>
                <Comment>I_LEVEL_TN6</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the ??value calculated on timeslots 0 through 7, respectively. The ??value is defined in GSM 05.08. These fields are transferred only when the mobile station is in packet transfer mode. These fields are encoded relative to C_VALUE as defined for the mapping defined in GSM 05.08 for interference level (I_LEVEL).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilev7</Name>
                <BitLen>4</BitLen>
                <Comment>I_LEVEL_TN7</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the I_LEVEL value measured on timeslot 0 through 7, respectively for the frequency specified either in the Packet Measurement Order or in the PSI5 message. The fields are transferred if the data is available and each field is encoded as the binary representation of the I_LEVEL value defined in GSM 05.08. Range 0 to 63.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilevabs0</Name>
                <BitLen>6</BitLen>
                <Comment>I_LEVEL_ABS_TNO</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the I_LEVEL value measured on timeslot 0 through 7, respectively for the frequency specified either in the Packet Measurement Order or in the PSI5 message. The fields are transferred if the data is available and each field is encoded as the binary representation of the I_LEVEL value defined in GSM 05.08. Range 0 to 63.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilevabs1</Name>
                <BitLen>6</BitLen>
                <Comment>I_LEVEL_ABS_TN1</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the I_LEVEL value measured on timeslot 0 through 7, respectively for the frequency specified either in the Packet Measurement Order or in the PSI5 message. The fields are transferred if the data is available and each field is encoded as the binary representation of the I_LEVEL value defined in GSM 05.08. Range 0 to 63.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilevabs2</Name>
                <BitLen>6</BitLen>
                <Comment>I_LEVEL_ABS_TN2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the I_LEVEL value measured on timeslot 0 through 7, respectively for the frequency specified either in the Packet Measurement Order or in the PSI5 message. The fields are transferred if the data is available and each field is encoded as the binary representation of the I_LEVEL value defined in GSM 05.08. Range 0 to 63.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilevabs3</Name>
                <BitLen>6</BitLen>
                <Comment>I_LEVEL_ABS_TN3</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the I_LEVEL value measured on timeslot 0 through 7, respectively for the frequency specified either in the Packet Measurement Order or in the PSI5 message. The fields are transferred if the data is available and each field is encoded as the binary representation of the I_LEVEL value defined in GSM 05.08. Range 0 to 63.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilevabs4</Name>
                <BitLen>6</BitLen>
                <Comment>I_LEVEL_ABS_TN4</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the I_LEVEL value measured on timeslot 0 through 7, respectively for the frequency specified either in the Packet Measurement Order or in the PSI5 message. The fields are transferred if the data is available and each field is encoded as the binary representation of the I_LEVEL value defined in GSM 05.08. Range 0 to 63.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilevabs5</Name>
                <BitLen>6</BitLen>
                <Comment>I_LEVEL_ABS_TN5</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the I_LEVEL value measured on timeslot 0 through 7, respectively for the frequency specified either in the Packet Measurement Order or in the PSI5 message. The fields are transferred if the data is available and each field is encoded as the binary representation of the I_LEVEL value defined in GSM 05.08. Range 0 to 63.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilevabs6</Name>
                <BitLen>6</BitLen>
                <Comment>I_LEVEL_ABS_TN6</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields contain the I_LEVEL value measured on timeslot 0 through 7, respectively for the frequency specified either in the Packet Measurement Order or in the PSI5 message. The fields are transferred if the data is available and each field is encoded as the binary representation of the I_LEVEL value defined in GSM 05.08. Range 0 to 63.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ilevabs7</Name>
                <BitLen>6</BitLen>
                <Comment>I_LEVEL_ABS_TN7</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The Channel Coding Indicator field indicates the channel coding scheme that the mobile station shall use when transmitting on the uplink.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_coding_cmd</Name>
                <BitLen>2</BitLen>
                <Comment>CHANNEL_CODING_COMMAND</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_chan_coding_cmd</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the channel coding command that the mobile station shall use for any RLC data block containing a TLLI field in the RLC data block header.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>tlli_chan_coding</Name>
                <BitLen>1</BitLen>
                <Comment>TLLI_BLOCK_CHANNEL_CODING</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_tlli_chan_coding</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This information field indicates the medium access method to be used during the TBF.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>mac_mode</Name>
                <BitLen>2</BitLen>
                <Comment>MAC_MODE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_mac_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the RLC mode of the requested TBF.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rlc_mode</Name>
                <BitLen>1</BitLen>
                <Comment>RLC_MODE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_rlc_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the RLC mode of the requested TBF.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dl_rlc_mode</Name>
                <BitLen>1</BitLen>
                <Comment>DOWNLINK_RLC_MODE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_rlc_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field shall be set to '1' if the network establishes a new downlink TBF for the mobile station whose timer T3192 is running. Otherwise this field shall be set to '0'.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ctrl_ack</Name>
                <BitLen>1</BitLen>
                <Comment>CONTROL_ACK</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains acknowledgement information for the group of RLC/MAC control blocks that make up an RLC/MAC control message. The mobile station shall set the CTRL_ACK field to indicate which segments of an RLC/MAC control message have been received by the time of transmission of the PACKET CONTROL ACKNOWLEDGEMENT message.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pctrl_ack</Name>
                <BitLen>2</BitLen>
                <Comment>P_CONTROL_ACK</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_pctrl_ack</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The Temporary Flow Identifier (TFI) uniquely identifies either a single uplink Temporary Block Flow (TBF) or a single downlink Temporary Block Flow (TBF).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dl_tfi_assign</Name>
                <BitLen>5</BitLen>
                <Comment>DOWNLINK_TFI_ASSIGNMENT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The Temporary Flow Identifier (TFI) uniquely identifies either a single uplink Temporary Block Flow (TBF) or a single downlink Temporary Block Flow (TBF).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ul_tfi_assign</Name>
                <BitLen>5</BitLen>
                <Comment>UPLINK_TFI_ASSIGNMENT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The Temporary Flow Identifier (TFI) uniquely identifies either a single uplink Temporary Block Flow (TBF) or a single downlink Temporary Block Flow (TBF).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ul_tfi</Name>
                <BitLen>5</BitLen>
                <Comment>Uplink TFI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The Temporary Flow Identifier (TFI) uniquely identifies either a single uplink Temporary Block Flow (TBF) or a single downlink Temporary Block Flow (TBF).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dl_tfi</Name>
                <BitLen>5</BitLen>
                <Comment>Downlink TFI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the reason for the release of the TBF.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rel_cause</Name>
                <BitLen>4</BitLen>
                <Comment>TBF Release Cause</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_rel_cause</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="2" Month="10" Year="2001"/>
                <Author>CAN</Author>
                <Comment>bit len corrected</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Notification List Number - This field may only be present if the message contains at least one page request for an RR connection establishment. The field is coded as defined in the P1 Rest Octets information element in GSM 04.08.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>nln</Name>
                <BitLen>2</BitLen>
                <Comment>NLN</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The PBCCH_CHANGE_MARK field is a 3 bit counter incremented with one each time information has been changed in one or more of the broadcast PSI2-PSIn messages on PBCCH (n&gt;2).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pbcch_change_ma</Name>
                <BitLen>3</BitLen>
                <Comment>PBCCH_CHANGE_MARK</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The PSI_CHANGE_FIELD is a 4 bit value reflecting which PSI message or group of instantiated PSI message was most recent updated when the PBCCH_CHANGE_MARK was last incremented. If more than one PSI message or group of instantiated PSI message were changed at the same time, the PSI_CHANGE_FIELD indicates unspecified updates.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi_change_field</Name>
                <BitLen>4</BitLen>
                <Comment>PSI_CHANGE_FIELD</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_psi_change_field</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The MEASUREMENT ORDER field indicates if set = 0 that the mobile station is in control of the cell re-selection in both packet idle mode and packet transfer mode (= NC0 in GSM 05.08) and that the mobile station shall not send any measurement reports to the network (= NC0 and = EM0 in GSM 05.08). It also indicates that the Optional PSI5 message is not broadcast. If set = 1 the mobile station shall send measurement reports for cell re-selection and/or for extended measurements to the network. Further cell re-selection and measurement details are included in the PSI5 message.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>meas_order</Name>
                <BitLen>1</BitLen>
                <Comment>MEASUREMENT_ORDER</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The PSI1_REPEAT_PERIOD field indicates the PSI1 repeat period.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi1_rep_per</Name>
                <BitLen>4</BitLen>
                <Comment>PSI1_REPEAT_PERIOD</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The PSI_COUNT_LR field is a 6 bit value indicating the number of different Packet System Information messages that are mapped onto the PBCCH with low repetition rate.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi_cnt_lr</Name>
                <BitLen>6</BitLen>
                <Comment>PSI_COUNT_LR</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The PSI_COUNT_HR is a 4 bit value indicating the number of different Packet System Information messages that are mapped onto the PBCCH with high repetition rate. The value does not include PSI1, but can include any selected message and all instance of that message. If PSI_COUNT_HR is not included in PSI1, the default value of PSI_COUNT_HR = 0</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi_cnt_hr</Name>
                <BitLen>4</BitLen>
                <Comment>PSI_COUNT_HR</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields are the binary representation of the PSI index.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi2_ind</Name>
                <BitLen>3</BitLen>
                <Comment>PSI2_INDEX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields are the binary representation of the PSI index.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi4_ind</Name>
                <BitLen>3</BitLen>
                <Comment>PSI4_INDEX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields are the binary representation of the PSI index.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi5_ind</Name>
                <BitLen>3</BitLen>
                <Comment>PSI5_INDEX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields are the binary representation of the PSI count</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi2_cnt</Name>
                <BitLen>3</BitLen>
                <Comment>PSI2_COUNT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove psix_cnt.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields are the binary representation of the PSI count</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi4_cnt</Name>
                <BitLen>3</BitLen>
                <Comment>PSI4_COUNT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove psix_cnt.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields are the binary representation of the PSI count</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi5_cnt</Name>
                <BitLen>3</BitLen>
                <Comment>PSI5_COUNT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Remove psix_cnt.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is coded as the binary representation of the PSI3 bis index (in the PSI3 bis message) for the last (highest indexed) individual PSI3 bis message. # This field is 3 or 4 bit long. There is a ambiguous definition in 04.60.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi3bis_cnt</Name>
                <BitLen>4</BitLen>
                <Comment>PSI3_BIS_COUNT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field represents the PSI3_BIS_INDEX.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi3bis_ind</Name>
                <BitLen>4</BitLen>
                <Comment>PSI3_BIS_INDEX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the status of the information on BCCH. The value of this field shall be changed each time the information on BCCH, except for the contents of the SI-13 message, is changed.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bcch_change_ma</Name>
                <BitLen>3</BitLen>
                <Comment>BCCH_CHANGE_MARK</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary representation of which information was changed at the last indication in</Section>
                <Section>BCCH_CHANGE_MARK.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>si_change_ma</Name>
                <BitLen>4</BitLen>
                <Comment>SI_CHANGE_FIELD</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_si_change_ma</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is encoded as the ARFCN defined in GSM 04.08.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>arfcn</Name>
                <BitLen>10</BitLen>
                <Comment>ARFCN</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is encoded as the ARFCN defined in GSM 04.08.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>start_freq</Name>
                <BitLen>10</BitLen>
                <Comment>START_FREQUENCY</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The BSIC field is coded as the "Base Station Identity Code". One BSIC for each carrier in</Section>
                <Section>BA(GPRS) is defined.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bsic</Name>
                <BitLen>6</BitLen>
                <Comment>BSIC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The BSIC field is coded as the "Base Station Identity Code". One BSIC for each carrier in</Section>
                <Section>BA(GPRS) is defined.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bsic2</Name>
                <BitLen>6</BitLen>
                <Comment>BSIC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the cause of the cell change order failure on the target cell.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>failure_cause</Name>
                <BitLen>4</BitLen>
                <Comment>Packet Cell Change Failure Cause</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_failure_cause</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="11" Year="2002"/>
                <Author>ZL</Author>
                <Comment>failure cause bit length from 8 to 4 bits.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The NETWORK_CONTROL_ORDER field contains the network control order that the mobile station shall apply in the new cell. If NC1 or NC2 applies, the NC parameters (excluding the NC frequency list) to be applied in the new cell may be included in the PACKET CELL CHANGE ORDER message or may have been received in a previous PACKET MEASUREMENT ORDER. Otherwise the broadcast message in the new cell shall apply.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ctrl_order</Name>
                <BitLen>2</BitLen>
                <Comment>NETWORK_CONTROL_ORDER</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ctrl_order</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add c-macro definitions</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The purpose of the PMO_INDEX field and the PMO_COUNT field is to indicate the number of individual messages within the sequence of Packet Measurement Order messages and to assign an index to identify each one of them. The PMO_INDEX field is binary coded, range: 0 to 7, and provides an index to identify the individual Packet Measurement Order message. The PMO_COUNT field provides the PMO_INDEX value for the last (highest indexed) message in the sequence of Packet Measurement Order messages. A measurement order shall not be effected by the mobile station until all instances of a Packet Measurement Order message is received.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pmo_index</Name>
                <BitLen>3</BitLen>
                <Comment>PMO_INDEX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>See 6.38.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pmo_cnt</Name>
                <BitLen>3</BitLen>
                <Comment>PMO_COUNT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This information field indicates the timeslots assigned for GPRS use on the current MAIO or ARFCN. If this field is not present, the timeslot on which the message was sent is the timeslot being released. Bit 8 indicates the status of timeslot 0, bit 7 indicates the status of timeslot 1, etc.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ts_available</Name>
                <BitLen>8</BitLen>
                <Comment>Timeslots Available</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This is the ALPHA Power control parameter field.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>alpha</Name>
                <BitLen>4</BitLen>
                <Comment>Alpha</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_alpha</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The GAMMA_TN0..7 fields are the binary representation of the parameter ?CH for MS output power control in units of 2 dB, see GSM 05.08. GAMMA_TN0 contains the gamma value for timeslot number 0, GAMMA_TN1 contains the gamma value for timeslot number 1, etc. If this information element is also used to determine the timeslot allocation for an uplink TBF, for each timeslot, the presence of the GAMMA value indicates that the timeslot is assigned, and the absence of the GAMMA value indicates that the timeslot is not assigned (see subclause 12.18).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gamma</Name>
                <BitLen>5</BitLen>
                <Comment>GAMMA_TN</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The T_AVG_W parameter is a signal strength filter period for power control in packet idle mode.</Section>
                <Section>2 (k/2) / 6 multiframes, k = 0, 1, 2, ... 25. All other values are reserved.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>t_avg_w</Name>
                <BitLen>5</BitLen>
                <Comment>T_AVG_W</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="11" Year="2000"/>
                <Author>SAB</Author>
                <Comment>T_ALG_W changed to T_AVG_W</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The T_AVG_T parameter is a signal strength filter period for power control in packet transfer mode. 2 (k/2) / 6 multiframes, k = 0,1,2,...,25; All other values are reserved.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>t_avg_t</Name>
                <BitLen>5</BitLen>
                <Comment>T_AVG_T</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The Pb parameter is a power reduction value used by the BTS on PBCCH blocks, relative to the output power used on BCCH.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pb</Name>
                <BitLen>4</BitLen>
                <Comment>PB</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_pb</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The PC_MEAS_CHAN parameter indicates where the mobile station shall measure the received power level on the downlink for the purpose of the uplink power control.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pc_meas_chan</Name>
                <BitLen>1</BitLen>
                <Comment>PC_MEAS_CHAN</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_pc_meas_chan</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Indicates if the optional PSI4 message is broadcast. If broadcast it contains the Channel List for interference measurements.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>imeas_chan_list</Name>
                <BitLen>1</BitLen>
                <Comment>INT_MEAS_CHANNEL_LIST_AVAIL</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_imeas_chan_list</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The N_AVG_I parameter is an interfering signal strength filter constant for power control 2 (k/2), k=0,1,..,15 .</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>n_avg_i</Name>
                <BitLen>4</BitLen>
                <Comment>N_AVG_I</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The Measurement Interval field indicates the number of block periods from the start of one assigned measurement period to the beginning of the next measurement period. The value have to be interpreted in the following way: make measurements during every (value+1) block period</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>meas_inter</Name>
                <BitLen>5</BitLen>
                <Comment>MEASUREMENT_INTERVAL</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This information field indicates the timeslots assigned for use during measurement periods. The field as a bitmap where each bit corresponds with a timeslot number. Bit 1 corresponds to TS0; Bit 2 to TS1... A 0 means the MS shall receive downlink data during this timeslot, an 1 the MS shall make measurements during the timeslot.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>meas_bitmap</Name>
                <BitLen>8</BitLen>
                <Comment>MEASUREMENT_BITMAP</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>PTMSI (32 bit field) The Packet Temporary Mobile Station Identity (PTMSI) is defined in GSM 03.03.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ptmsi</Name>
                <BitLen>32</BitLen>
                <Comment>PTMSI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>PTMSI (32 bit field) The Packet Temporary Mobile Station Identity (PTMSI) is defined in GSM 03.03.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>tmsi_field</Name>
                <BitLen>32</BitLen>
                <Comment>TMSI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The channel needed field indicates which type of channel is needed for the mobile station for the transaction linked to the paging procedure.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_need</Name>
                <BitLen>2</BitLen>
                <Comment>CHANNEL_NEEDED</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_chan_need</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The optional eMLPP_PRIORITY field relates to Mobile Station Identity i(i = 1,2,3,4) and may only be present when the page relates to a paging request to trigger RR connection establishment.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>emlpp_prio</Name>
                <BitLen>3</BitLen>
                <Comment>eMLPP_PRIORITY</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>If the TIMING_ADVANCE_VALUE field is present, the mobile station shall use the value contained therein after time defined in GSM 05.10. If the TIMING_ADVANCE_VALUE field is not present the mobile station shall not change its timing advance value.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ta_value</Name>
                <BitLen>6</BitLen>
                <Comment>TIMING_ADVANCE_VALUE</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>If the TIMING_ADVANCE_INDEX and TIMING_ADVANCE_TIMESLOT_NUMBER fields are present the mobile station shall immediately begin operation of the Continuous Timing Advance procedure. If these two fields are not present the mobile station shall stop operation of the Continuous Timing Advance procedure. This information field is encoded as a binary representation of the Timing Advance Index defined in GSM 05.02.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ul_ta_index</Name>
                <BitLen>4</BitLen>
                <Comment>UPLINK_TA_INDEX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>ta_index without ul or dl removed</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>If the TIMING_ADVANCE_INDEX and TIMING_ADVANCE_TIMESLOT_NUMBER fields are present the mobile station shall immediately begin operation of the Continuous Timing Advance procedure. If these two fields are not present the mobile station shall stop operation of the Continuous Timing Advance procedure. This information field is encoded as a binary representation of the Timing Advance Index defined in GSM 05.02.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dl_ta_index</Name>
                <BitLen>4</BitLen>
                <Comment>DOWNLINK_TA_INDEX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>ta_index without ul or dl removed</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>If the TIMING_ADVANCE_INDEX and TIMING_ADVANCE_TIMESLOT_NUMBER fields are present the mobile station shall immediately begin operation of the Continuous Timing Advance procedure. If these two fields are not present the mobile station shall stop operation of the Continuous Timing Advance procedure. This information field is encoded as a binary representation of the Timing Advance Index defined in GSM 05.02.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ta_index</Name>
                <BitLen>4</BitLen>
                <Comment>TA_INDEX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>ta_index without ul or dl removed</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the timeslot assigned for Continuous Timing Advance operation on the PTCCH.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ta_tn</Name>
                <BitLen>3</BitLen>
                <Comment>TIMING_ADVANCE_TIMESLOT_NUMBER</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the timeslot assigned for Continuous Timing Advance operation on the PTCCH.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>tn</Name>
                <BitLen>3</BitLen>
                <Comment>TIMESLOT_NUMBER</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the timeslot assigned for Continuous Timing Advance operation on the PTCCH.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ul_ta_tn</Name>
                <BitLen>3</BitLen>
                <Comment>UPLINK_TA_TIMESLOT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the timeslot assigned for Continuous Timing Advance operation on the PTCCH.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dl_ta_tn</Name>
                <BitLen>3</BitLen>
                <Comment>DOWNLINK_TA_TIMESLOT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary representation of the Network Mode of Operation, see GSM 03.60.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>nmo</Name>
                <BitLen>2</BitLen>
                <Comment>NMO</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_nmo</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary representation of the timeout value of timer T3168. Range: 0 to 7. The timeout value is given as the binary value plus one in units of 500 millisecond.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>t3168</Name>
                <BitLen>3</BitLen>
                <Comment>T3168</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary representation of the timeout value of timer T3192. Range: 0 to 7. The timeout value is given as the binary value plus one in units of 500 millisecond.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>t3192</Name>
                <BitLen>3</BitLen>
                <Comment>T3192</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary representation of the parameter DRX_TIMER_MAX. Range: 0 to 7. The parameter value is given as two taken to the power of the binary value minus one (2 (bv - 1) in units of 1 second. The binary value zero indicates that non-DRX mode is not supported in the cell. (E.g. the parameter takes the values: 'not supported', 1 s, 2 s, 4 s, .. 64 s.)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>drx_t_max</Name>
                <BitLen>3</BitLen>
                <Comment>DRX_TIMER_MAX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The ACCESS_BURST_TYPE field indicates if 8 or 11 bit access burst shall be used on PRACH and in the PACKET CONTROL ACKNOWLEDGMENT message when the format is four access bursts.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ab_type</Name>
                <BitLen>1</BitLen>
                <Comment>Access Burst Type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ab_type</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary representation of the default format of the PACKET CONTROL ACKNOWLEDGMENT message.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ctrl_ack_type</Name>
                <BitLen>1</BitLen>
                <Comment>CONTROL_ACK_TYPE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ctrl_ack_type</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>CV - countdown value</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bs_cv_max</Name>
                <BitLen>4</BitLen>
                <Comment>BS_CV_MAX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>See PAN structure.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dec</Name>
                <BitLen>3</BitLen>
                <Comment>PAN_DEC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>See PAN structure.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>inc</Name>
                <BitLen>3</BitLen>
                <Comment>PAN_INC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>See PAN structure'.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pmax</Name>
                <BitLen>3</BitLen>
                <Comment>PAN_MAX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The length of the extension.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ext_len</Name>
                <BitLen>6</BitLen>
                <Comment>Extension Length</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>That field will be defined during future extension.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>spare_ext</Name>
                <BitLen>1</BitLen>
                <Comment>Extension Spare Bits</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Set bit-len of spare_ext to 1.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Number of slots to spread transmission of the random access.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>tx_int</Name>
                <BitLen>4</BitLen>
                <Comment>TX_INT</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_tx_int</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>S is a parameter used for calculation of the minimum number of slots between two successive Channel request.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>s_prach</Name>
                <BitLen>4</BitLen>
                <Comment>S (PRACH Parameter)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_s_prach</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Indicates for each Radio Priority level 1 to 4 the maximum number of retransmissions allowed. Radio Priority 1 represents the highest priority. The field is coded with two bits per Radio Priority.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>max_retrans</Name>
                <BitLen>2</BitLen>
                <Comment>MAX_RETRANS</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_max_retrans</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Access Control Class N (bit 1-16) (see octet 3 and 4 of the RACH Control Parameters IE in GSM 04.08) . For a mobile station with Access Control Class =N access is not barred if the Access Control Class N bit is coded with a "0"; N = 0, 1,....9,11,...,15. Bit 11= the EC bit is the Emergency Call Allowed coded as specified in GSM 04.08.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ac_class</Name>
                <BitLen>16</BitLen>
                <Comment>ACC_CONTR_CLASS</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This is an unformatted 11 bit field. If the System Information parameter Access Burst Type indicates 11 bit access bursts are to be used, all 11 bits of this field are valid. Otherwise, only bits 8 through 1 are valid and bits 11 through 9 shall be set to '0'.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>access_info</Name>
                <BitLen>11</BitLen>
                <Comment>Random Access Information</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the peak throughput class for the PD. context of the LLC PDU that caused the Channel Request Description IE to be transmitted. The field is coded as the binary representation of the Peak Throughput Class specified in GSM 03.60.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>peak_thr_class</Name>
                <BitLen>4</BitLen>
                <Comment>PEAK_THROUGHPUT_CLASS</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the Radio Priority of the requested TBF.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>radio_prio</Name>
                <BitLen>2</BitLen>
                <Comment>RADIO_PRIORITY</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_radio_prio</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the type of the first LLC PDU to be transmitted over the requested uplink TBF.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>llc_pdu_type</Name>
                <BitLen>1</BitLen>
                <Comment>LLC_PDU_TYPE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_llc_pdu_type</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The RLC_OCTET_COUNT field indicates the number of LLC data octets, plus the number of RLC data block length octets, that the mobile station wishes to transfer. The value '0' shall be interpreted as a request for an open ended TBF by the mobile station. All other values shall be interpreted as a request for a close ended TBF.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rlc_octet_cnt</Name>
                <BitLen>16</BitLen>
                <Comment>RLC_OCTET_COUNT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary representation of the training sequence code.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>tsc</Name>
                <BitLen>3</BitLen>
                <Comment>Training Sequence Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary representation of the mobile allocation index offset (MAIO).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>maio</Name>
                <BitLen>6</BitLen>
                <Comment>MAIO</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary representation of the mobile allocation index offset (MAIO).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rfreq_index</Name>
                <BitLen>6</BitLen>
                <Comment>REMOVED_FREQ_INDEX</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary reference to a GPRS mobile allocation received in either the PSI2 information, the SI13/PSI13 information or a previous assignment message.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ma_num</Name>
                <BitLen>4</BitLen>
                <Comment>MA_NUMBER</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary representation of the hopping sequence number.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>hsn</Name>
                <BitLen>6</BitLen>
                <Comment>HSN</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the length of the field MA Frequency List contents</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>len_ma_list</Name>
                <BitLen>4</BitLen>
                <Comment>Length of MA Frequency List contents</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This variable length octet string is the representation of a set of radio frequency channels defining a GPRS mobile allocation. The encoding of the octet string is defined by the value part of the type 4 information element Frequency List, defined in GSM 04.08.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ma_list</Name>
                <BitLen>8</BitLen>
                <Comment>MA Frequency List contents</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The BS_PCC_REL field indicates if set = 1 that the last PDCH carrying PCCCH and PBCCH will be released shortly. All mobile stations on PCCCH shall then as soon as this information has been received return to CCCH and there obey the information sent on BCCH as specified in GSM 04.08. If the field is set = 0, no channel release is pending.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bs_pcc_rel</Name>
                <BitLen>1</BitLen>
                <Comment>BS_PCC_REL</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The BS_PBCCH_BLKS field indicates the number of blocks allocated to the PBCCH in the multiframe.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bs_pbcch_blks</Name>
                <BitLen>2</BitLen>
                <Comment>BS_PBCCH_BLKS</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_bs_pbcch_blks</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The BS_PRACH_BLKS field indicates the number of blocks reserved in a fixed way to the PRACH channel on any PDCH carrying PCCCH and PBCCH(Only for 52 type PCCCH)(See GSM 05.02). The field is optional and if not included it shall be interpreted as no Block reserved for PRACH.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bs_prach_blks</Name>
                <BitLen>4</BitLen>
                <Comment>BS_PRACH_BLKS</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_bs_prach_blks</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The BS_PAG_BLKS_RES field indicates the number of blocks on each PDCH carrying the PCCCH per multiframe where neither packet paging nor PBCCH should appear. This number corresponds therefore to the number of blocks reserved for PAGCH in the 51 frame multiframe case and to the number of blocks reserved for PAGCH, PDTCH and PACCH for the 52 frames multiframe case. (See GSM 05.02). The field is optional and if not included it shall be interpreted as the default value of 0 blocks reserved for PAGCH, PDTCH and PACCH.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bs_pag_blks</Name>
                <BitLen>4</BitLen>
                <Comment>BS_PAG_BLKS_RES</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The TIMESLOT_ALLOCATION field indicates the timeslots for use during a TBF or the timeslots carrying a PCCCH.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ul_ts_alloc</Name>
                <BitLen>8</BitLen>
                <Comment>UPLINK_TIMESLOT_ALLOCATION</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The TIMESLOT_ALLOCATION field indicates the timeslots for use during a TBF or the timeslots carrying a PCCCH.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ts_alloc</Name>
                <BitLen>8</BitLen>
                <Comment>TIMESLOT_ALLOCATION</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The TIMESLOT_ALLOCATION field indicates the timeslots for use during a TBF or the timeslots carrying a PCCCH.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dl_tn_alloc</Name>
                <BitLen>8</BitLen>
                <Comment>DOWNLINK_TIMESLOT_ALLOCATION</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This information field indicates the downlink timeslot that mobile station operating in fixed allocation mode shall monitor for downlink PACCH.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dl_ctrl_ts</Name>
                <BitLen>3</BitLen>
                <Comment>DOWNLINK_CONTROL_TIMESLOT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The ALLOCATION_BITMAP represents uplink radio blocks, each bit representing one radio block or an entire block period. Each bit indicates whether the mobile station is permitted to transmit during the corresponding uplink radio block or radio block period.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>alloc_map</Name>
                <BitLen>1</BitLen>
                <Comment>ALLOCATION_BITMAP</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field combines the CELL_BAR_ACCESS and CELL_BAR_QUALIFY parameters and indicates the status for cell reselection, see GSM 05.08.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cell_ba</Name>
                <BitLen>1</BitLen>
                <Comment>CELL_BAR_ACCESS_2</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_cell_ba</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>GPRS_RESELECT_OFFSET is used by the mobile station to apply a positive or negative offset and a hysteresis to the GPRS cell reselection criterion. Default value is 0 dB. If the field is omitted from the message, the default value shall be used by the mobile station.</Section>
                <Section>For value 0- 10 the GPRS_RESELECT_OFFSET is = -52 dB + (value *4dB) .</Section>
                <Section>For value 11- 22 the GPRS_RESELECT_OFFSET is = -12 dB + ( (value-10) *2dB) .</Section>
                <Section>For value 23- 31 the GPRS_RESELECT_OFFSET is = +12 dB + ( (value-22) *4dB) .</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_resel_off</Name>
                <BitLen>5</BitLen>
                <Comment>GPRS_RESELECT_OFFSET</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_gprs_resel_off</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add default value</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The SI13_LOCATION field, if present, indicates the logical channel where the SYSTEM INFORMATION TYPE 13 is broadcast.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>si13_loc</Name>
                <BitLen>1</BitLen>
                <Comment>SI13_LOCATION</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_si13_loc</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The PBCCH_LOCATION field, if present, indicates the location of the PBCCH on the BCCH carrier (see GSM 05.02).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pbcch_loc</Name>
                <BitLen>2</BitLen>
                <Comment>PBCCH_LOCATION</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_pbcch_loc</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The GPRS_PRIORITY_CLASS field contains the binary representation of the HCS priority for the cell.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_prio_class</Name>
                <BitLen>3</BitLen>
                <Comment>GPRS_PRIORITY_CLASS</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_gprs_prio_class</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="15" Month="4" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add c-macro value</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The is the HCS signal strength threshold. The value is (-110 dB + value * 2).</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_hcs_thr</Name>
                <BitLen>5</BitLen>
                <Comment>GPRS_HCS_THR</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_gprs_hcs_thr</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="1" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Correction of typing error (gprs_hsc_thr to gprs_hcs_thr)</Comment>
            </History>
            <History>
                <Date Day="15" Month="4" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add c-macro value</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The GPRS_RXLEV_ACCESS_MIN field is coded as the binary representation of the "RXLEV_ACCESS_MIN" defined in GSM 05.08. It is the minimum received level at the mobile station required for access to the system.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_rxlev_access_min</Name>
                <BitLen>6</BitLen>
                <Comment>GPRS_RXLEV_ACCESS_MIN</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_gprs_rxlev_access_min</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add c-macro value</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The GPRS_MS_TXPWR_MAX_CCH field is coded as the binary representation of the 'power control level' in GSM 05.05 corresponding to the maximum TX power level a mobile station may use when accessing on a packet control channel.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>txpwr_max_cch</Name>
                <BitLen>5</BitLen>
                <Comment>GPRS_MS_TXPWR_MAX_CCH</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_txpwr_max_cch</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add c-macro value</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The GPRS_TEMPORARY_OFFSET field indicates the negative offset to C32 that the mobile station shall use for duration of GPRS_PENALTY_TIME. It is used by the mobile station as part of its calculation of C32 for the cell reselection process.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_temp_offset</Name>
                <BitLen>3</BitLen>
                <Comment>GPRS_TEMPORARY_OFFSET</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_gprs_temp_offset</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add c-macro value</Comment>
            </History>
            <History>
                <Date Day="2" Month="8" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add c-macro value</Comment>
            </History>
            <History>
                <Date Day="23" Month="4" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add c_macro value</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The GPRS_PENALTY_TIME defines the length of time for which GPRS_TEMPORARY_OFFSET is active. GPRS_PENALTY_TIME = (Value+1)* 10 seconds</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_penalty_time</Name>
                <BitLen>5</BitLen>
                <Comment>GPRS_PENALTY_TIME</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_gprs_penalty_time</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add c-macro value</Comment>
            </History>
            <History>
                <Date Day="2" Month="8" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add c-macro value</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The Wait Indication field indicates the time the mobile station shall wait before attempting another channel request. If this field is present the cause value is "Wait". If this field is not present, the cause value is "Read System Information". This field is coded as the binary representation of the T3172 timeout value in seconds.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ind</Name>
                <BitLen>8</BitLen>
                <Comment>Wait Indication</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the units of the WAIT_INDICATION field.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>waitsize</Name>
                <BitLen>1</BitLen>
                <Comment>Wait Indication Size</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_waitsize</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This specifies the number of bits in the ALLOCATION_BITMAP.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>a_map_len</Name>
                <BitLen>7</BitLen>
                <Comment>ALLOCATION_BITMAP_LENGTH</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This indicates if the ALLOCATION_BITMAP is to be interpreted as blocks or block periods.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bl_o_bl_per</Name>
                <BitLen>1</BitLen>
                <Comment>BLOCKS_OR_BLOCK_PERIODS</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_bl_o_bl_per</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This information field indicates which the timeslots whose allocation should be overridden. The override applies for one repeated allocation. Bit 8 indicates the status of timeslot 0, bit 7 indicates the status of timeslot 1, etc. The MS shall ignore any bit in the TS_OVERRIDE field whose corresponding bit in the previous timeslot allocation for the uplink TBF is set to '0'.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ts_overr</Name>
                <BitLen>8</BitLen>
                <Comment>TS_OVERRIDE</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The TBF Starting Time field contains a starting time that indicates the frame number during which the assigned TBF may start.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rel</Name>
                <BitLen>13</BitLen>
                <Comment>TBF Starting Time Relative</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="7" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>TBF Starting Time Absolute redefined [GSM_04.60] section 10.5.2.38</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [11] section 10.5.1.3 (Location Area Identification)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>mcc</Name>
                <BitLen>4</BitLen>
                <Comment>Mobile Country Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [11] section 10.5.1.3 (Location Area Identification)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>mnc</Name>
                <BitLen>4</BitLen>
                <Comment>Mobile Network Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [11]section 10.5.1.3 (Location Area Identification)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>lac</Name>
                <BitLen>16</BitLen>
                <Comment>Location Area Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary representation of the Routing Area Code.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rac</Name>
                <BitLen>8</BitLen>
                <Comment>RAC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The purpose of the Cell Identity information element is to identify a cell within a location area.</Section>
                <Section>Reference : [11]section 10.5.1.1 (Cell Identity)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cell_id_ie</Name>
                <BitLen>16</BitLen>
                <Comment>Cell identity</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1997"/>
                <Author>LE</Author>
                <Comment>length of cell identity is 16 bit</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [11] section 10.5.2.11 (Control Channel Description)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>att</Name>
                <BitLen>1</BitLen>
                <Comment>Attach / detach allowed</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_att</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [11] section 10.5.2.11 (Control Channel Description)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>t3212</Name>
                <BitLen>8</BitLen>
                <Comment>T 3212 time-out value</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Half rate support.</Section>
                <Section>Reference : [11] section 10.5.2.4 (Cell Selection Parameters)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>neci</Name>
                <BitLen>1</BitLen>
                <Comment>Half rate support</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_neci</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [11] section 10.5.2.3 (Cell Options (BCCH))</Section>
                <Section>[11] section 10.5.2.3a (Cell Options (SACCH))</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pwcr</Name>
                <BitLen>1</BitLen>
                <Comment>Power Control</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_pwcr</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [11] section 10.5.2.3 (Cell Options (BCCH))</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dtx</Name>
                <BitLen>2</BitLen>
                <Comment>Discontinuous Transmission (BCCH)</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_dtx</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The precise meaning of RADIO-LINK-TIMEOUT parameter can be found in Technical</Section>
                <Section>Specification GSM 05.08.</Section>
                <Section>Reference : [11]section 10.5.2.3 (Cell Options (BCCH))</Section>
                <Section>[11]section 10.5.2.3a (Cell Options (SACCH))</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rl_timeout</Name>
                <BitLen>4</BitLen>
                <Comment>Radio Link Timeout</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Content of a frequency list</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>flist</Name>
                <BitLen>8</BitLen>
                <Comment>Frequency List Contents</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="8" Month="2" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Copy from RR</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary identification of an RFL provided in this message or the binary reference to such.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rfl_num</Name>
                <BitLen>4</BitLen>
                <Comment>RFL_NUMBER</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_rfl_num</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="27" Month="10" Year="2003"/>
                <Author>SAB</Author>
                <Comment>Add RFL_NUMBER_4_DL_CTRL_MSG_MAX</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the length of Radio Frequency List.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rfl_cont_len</Name>
                <BitLen>4</BitLen>
                <Comment>Length of RFL contents</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field contains the length of MA_BITMAP.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ma_len</Name>
                <BitLen>6</BitLen>
                <Comment>MA_LENGTH</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is a bitmap representing the radio frequency channels belonging to the GPRS mobile allocation. The number of bit positions in MA_BITMAP shall equal NF. The first bit position in MA_BITMAP corresponds to ARFCN_INDEX = NF-1, the last position corresponds to ARFCN_INDEX = 0.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ma_map</Name>
                <BitLen>1</BitLen>
                <Comment>MA_BITMAP</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="16" Month="1" Year="2001"/>
                <Author>ID</Author>
                <Comment>Set bit-len to 1.</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Delete comment.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is included ARFCN Index List Structure.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>arfcn_index</Name>
                <BitLen>6</BitLen>
                <Comment>ARFCN index</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The GPRS_CELL_RESELECT_HYSTERESIS field indicates the Additional Hysteresis which applies in Ready state for cells in same RA. The value is to interpret as value*2dB .</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_c_hyst</Name>
                <BitLen>3</BitLen>
                <Comment>GPRS_CELL_RESELECT_HYSTERESIS</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The C31_HYST field indicates if set to 1 that the GPRS_RESELECT_HYSTERESIS shall be applied to the C31 criterion.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>c31_hyst</Name>
                <BitLen>1</BitLen>
                <Comment>C31_HYST</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>C32_QUAL is a flag indicating an exception rule for GPRS_RESELECT_OFFSET according to GSM 05.08.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>c32_qual</Name>
                <BitLen>1</BitLen>
                <Comment>C32_QUAL</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The RANDOM_ACCESS_RETRY field indicates if set to 1 that the mobile station is allowed to try to access another cell if available.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ra_retry</Name>
                <BitLen>1</BitLen>
                <Comment>RANDOM_ACCESS_RETRY</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_ra_retry</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="9" Month="9" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Change short name of parameter RANDOM_ACCESS_RETRY, add values</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>If the mobile station has performed an abnormal release with cell reselection (see subclause [2] 9.4.2) from this cell, the mobile station is not allowed to reselect this cell for T_RESEL seconds if another cell is available. The default value of T_RESEL is 5 seconds. If the field is omitted from the message, the default value shall be used by the mobile station.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>t_resel</Name>
                <BitLen>3</BitLen>
                <Comment>T_RESEL</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_t_resel</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add c-macro for default value.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The RA_RESELECT_HYSTERESIS field indicates in both STANDBY and READY state the additional hysteresis which applies when selecting a cell in a new Routing Area. If this field is not present, the default value is GPRS_CELL_RESELECT_HYSTERESIS. The value is to interpret as value*2 dB .</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ra_re_hyst</Name>
                <BitLen>3</BitLen>
                <Comment>RA_RESELECT_HYSTERESIS</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field specifies the remaining number of cells that are defined in the frequency group. For each of them the parameters 'Frequency diff' and 'Cell selection parameters' will be repeated.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>n_rest</Name>
                <BitLen>4</BitLen>
                <Comment>NR_OF_REMAINING_CELLS</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field specifies the remaining number of cells that are defined in the frequency group. For each of them the parameters 'Frequency diff' and 'Cell selection parameters' will be repeated.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>n_r_cells</Name>
                <BitLen>4</BitLen>
                <Comment>NR_OF_REMAINING_CELLS2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The FREQ_DIFF_LENGTH field specifies the number of bits to be used for the Frequency Difference field in the current Frequency Group.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>freq_diff_len</Name>
                <BitLen>3</BitLen>
                <Comment>FREQ_DIFF_LENGTH</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the minimum time the mobile station shall stay in non-DRX mode after an NC-measurement report has been sent.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>non_drx_per</Name>
                <BitLen>3</BitLen>
                <Comment>NC_NON_DRX_PERIOD</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_non_drx_per</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add values</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields indicate the time period for cell reselection measurement reporting for packet idle mode (I) and packet transfer mode (T), respectively. The reporting period is (0.48 sec) * 2 value</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rep_per_i</Name>
                <BitLen>3</BitLen>
                <Comment>NC_REPORTING_PERIOD_I</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_rep_per_i</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add values</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields indicate the time period for cell reselection measurement reporting for packet idle mode (I) and packet transfer mode (T), respectively. The reporting period is (0.48 sec) * 2 value</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rep_per_t</Name>
                <BitLen>3</BitLen>
                <Comment>NC_REPORTING_PERIOD_T</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_rep_per_i</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add values</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The EXT_REPORTING_PERIOD field indicates the time interval between extended measurement reports. The reporting period is (60 sec) * 2 value</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>xrep_per</Name>
                <BitLen>3</BitLen>
                <Comment>EXT_REPORTING_PERIOD</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_xrep_per</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="5" Year="2002"/>
                <Author>SAB</Author>
                <Comment>Add c-macro value</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This optional field indicates the frequency upon which the interference measurement shall be made. This field is an index into the EXT Frequency List. If the field is not included, no interference measurements shall be done.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>int_freq</Name>
                <BitLen>5</BitLen>
                <Comment>INT_FREQUENCY</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the type of extended measurement reporting to which the frequencies on the list are subject.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>xrep_type</Name>
                <BitLen>2</BitLen>
                <Comment>EXT_REPORTING_TYPE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_xrep_type</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add c-macro XREP_RESERVED.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is included in the structure 'PBCCH not present in cell structure' which is part of the message 'Packet System Information Type 13'</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>prio_acc_thr</Name>
                <BitLen>3</BitLen>
                <Comment>PRIORITY_ACCESS_THR</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_prio_acc_thr</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the support of the parameter SPLIT_PG_CYCLE on CCCH from the network side.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>spgc_ccch_sup</Name>
                <BitLen>1</BitLen>
                <Comment>SPGC_CCCH_SUP</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_spgc_ccch_sup</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates if the mobile station was in mode NC1 or NC2 when sending the measurement report.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>nc_mode</Name>
                <BitLen>1</BitLen>
                <Comment>NC_MODE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_nc_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add c-macro definitions and comments</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the measured RXLEV of the frequency upon which the measurement was made (see GSM 05.08). This field is encoded as the RXLEV value defined in GSM 04.08.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rxlev_scell</Name>
                <BitLen>6</BitLen>
                <Comment>RXLEV_SERVING_CELL</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the measured RXLEV of the frequency upon which the measurement was made (see GSM 05.08). This field is encoded as the RXLEV value defined in GSM 04.08.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rxlev_n</Name>
                <BitLen>6</BitLen>
                <Comment>RXLEV_N</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the measured RXLEV of the frequency upon which the measurement was made (see GSM 05.08). This field is encoded as the RXLEV value defined in GSM 04.08.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>i_scell</Name>
                <BitLen>6</BitLen>
                <Comment>INTERFERENCE_SERVING_CELL</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is included in the structure 'NC Measurement Report'.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>num_nc_meas</Name>
                <BitLen>3</BitLen>
                <Comment>NUMBER_OF_NC_MEASUREMENTS</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the frequency upon which the measurement was made. This field is an index into the Frequency List in the PSI5 or in the PACKET MEASUREMENT ORDER message used to assign the frequencies to measure. For EXT measurements the FREQUENCY_N = 0 refers to the first frequency and FREQUENCY_N = n refers to the nth frequency in the 'EXT Frequency list structure'. For NC measurements the FREQUENCY_N = 0 refers to the first frequency and FREQUENCY_N = n refers to the last frequency in the BA(GPRS) list. FREQUENCY_N = n+1 refers then to the first frequency and N = n + m to the last frequency in the 'Add Frequency list structure' defined in a PACKET MEASUREMENT ORDER message. Deletion of frequencies in a measurement order does not affect the FREQUENCY_N parameter.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>freq_n</Name>
                <BitLen>6</BitLen>
                <Comment>FREQUENZ_N</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field defines the number of measurement reports in the message are included.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>num_meas</Name>
                <BitLen>5</BitLen>
                <Comment>NUMBER_OF_MEASUREMENTS</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The RLC/MAC blocks Granted field assigns a fixed number of RLC data blocks that the mobile station shall transmit during the uplink TBF. If the RLC_DATA_BLOCKS_GRANTED field is present the mobile station shall transmit only the assigned number of RLC data blocks. Otherwise the duration of the uplink TBF is undefined. Retransmissions of negatively acknowledged RLC data blocks do not apply toward the maximum number. The number of data blocks is (value+9). The Maximum is 261 blocks.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rlc_db_granted</Name>
                <BitLen>8</BitLen>
                <Comment>RLC_DATA_BLOCKS_GRANTED</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This information field indicates the medium access mode to be used during the TBF.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>xdyn_alloc</Name>
                <BitLen>1</BitLen>
                <Comment>Extended Dynamic Allocation</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_xdyn_alloc</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This information field indicates the USF granularity to be applied by the mobile station when it is assigned a TBF using Dynamic Allocation.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>usf_grant</Name>
                <BitLen>1</BitLen>
                <Comment>USF_GRANULARITY</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_usf_grant</Name>
            </ValuesLink>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>These fields indicate the USF value assigned to the MS. These fields are encoded as a binary presentation of the USF value as defined in subclause [2] 10.4.1.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>usf</Name>
                <BitLen>3</BitLen>
                <Comment>USF</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is defined in [2] 12.14 . The PERISTENCE_LEVEL field indicates the values of the access persistence level P(i) for each Radio Priority i (i = 1..4) where Radio Priority 1 represents the highest Radio Priority of an LLC PDU to be transmitted.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>plev</Name>
                <BitLen>4</BitLen>
                <Comment>Persistence Level Radio Priority</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>consider GSM 0460d640</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 12.3</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rbb</Name>
                <BitLen>1</BitLen>
                <Comment>RECEIVE_BLOCK_BITMAP</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_rbb</Name>
            </ValuesLink>
            <History>
                <Date Day="9" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Intial</Comment>
            </History>
            <History>
                <Date Day="27" Month="8" Year="1999"/>
                <Author>CAN</Author>
                <Comment>changed form bitmap to bit</Comment>
            </History>
            <History>
                <Date Day="1" Month="9" Year="1999"/>
                <Author>CAN</Author>
                <Comment>values included</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 12.3</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>f_ack_ind</Name>
                <BitLen>1</BitLen>
                <Comment>FINAL_ACK_INDICATION</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_f_ack_ind</Name>
            </ValuesLink>
            <History>
                <Date Day="9" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 12.3</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ssn</Name>
                <BitLen>7</BitLen>
                <Comment>STARTING_SEQUENCE_NUMBER</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="9" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.23</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>nr_freq</Name>
                <BitLen>5</BitLen>
                <Comment>NR_OF_FREQUENCY</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="9" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.23</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>num_rfreq</Name>
                <BitLen>5</BitLen>
                <Comment>NR_OF_REMOVED_FREQ</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="9" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.23</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>generation</Name>
                <BitLen>2</BitLen>
                <Comment>Generation</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_generation</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="6" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="5" Month="9" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add c-macro value</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates whether the MS shall immediately move to the target cell and interrupt its on-going TBF in the serving cell, or it shall move to the target cell by applying the same procedure as for an autonomous cell reselection. Reference : [2] 11.2.4</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>im_rel</Name>
                <BitLen>1</BitLen>
                <Comment>IMMEDIATE_REL</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_im_rel</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates the downlink power control mode used by the network.</Section>
                <Section>Reference : [2] 11.2.29</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>mode</Name>
                <BitLen>1</BitLen>
                <Comment>BTS_PWR_CTRL_MODE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field indicates whether the MS shall immediately move to the target cell and interrupt its on-going TBF in the serving cell, or it shall move to the target cell by applying the same procedure as for an autonomous cell reselection. Reference : [2] 11.2.4</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>p0</Name>
                <BitLen>4</BitLen>
                <Comment>BTS_PWR_CTRL_P0</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.20</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>exc_acc</Name>
                <BitLen>1</BitLen>
                <Comment>EXC_ACC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="31" Month="5" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.9b</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ncc_permitted</Name>
                <BitLen>8</BitLen>
                <Comment>NCC_PERMITTED</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.9.c</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>tbf_cause</Name>
                <BitLen>3</BitLen>
                <Comment>TBF_CAUSE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_tbf_cause</Name>
            </ValuesLink>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.10</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ms_id_len</Name>
                <BitLen>4</BitLen>
                <Comment>Length of Mobile Identity</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="20" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.18</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>add_msg_type</Name>
                <BitLen>1</BitLen>
                <Comment>Addional Message Type</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="21" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.18</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psi_status_ind</Name>
                <BitLen>1</BitLen>
                <Comment>PSI_STATUS_IND</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_psi_status_ind</Name>
            </ValuesLink>
            <History>
                <Date Day="21" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.21</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>para_ptr</Name>
                <BitLen>2</BitLen>
                <Comment>CELL_PARAMS_POINTER</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="22" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.21</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bcc</Name>
                <BitLen>3</BitLen>
                <Comment>BTS Colour Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="22" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.21</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ncc</Name>
                <BitLen>3</BitLen>
                <Comment>Network Colour Code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="22" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 12.27</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ccch_conf</Name>
                <BitLen>3</BitLen>
                <Comment>CCCF-CONF</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="22" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 12.27.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bs_ag_blks_res</Name>
                <BitLen>3</BitLen>
                <Comment>BS_AG_BLKS_RES</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="22" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 12.27</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bs_pa_mfrms</Name>
                <BitLen>3</BitLen>
                <Comment>BS-PA-MFRMS</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="22" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 12.27</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>tx_integer</Name>
                <BitLen>4</BitLen>
                <Comment>TX_INTEGER</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="22" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.20</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>multi_band_rep</Name>
                <BitLen>2</BitLen>
                <Comment>MULTIBAND_REPORTING</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_multi_band_rep</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="9" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Add c-macro values</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 11.2.29</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pr_mode</Name>
                <BitLen>1</BitLen>
                <Comment>PR_MODE</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_pr_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The EXT_MEASUREMENT_ORDER field indicates to the mobile station how to interpret the rest of the extended measurement parameters.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>xmeas_order</Name>
                <BitLen>2</BitLen>
                <Comment>EXT_MEASUREMENT_ORDER</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">grr</DocName>
                <Name>VAL_xmeas_order</Name>
            </ValuesLink>
            <History>
                <Date Day="7" Month="1" Year="2000"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Reuse element flag_2bit which is no longer needed as xmeas_order.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] 12.27. Emergency call.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ec</Name>
                <BitLen>1</BitLen>
                <Comment>EC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="22" Month="7" Year="1999"/>
                <Author>SL</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The T1' field is coded as the binary representation of (FN div 1326)mod 32.</Section>
                <Section>Reference : [GSM_04.08] section 10.5.2.38 (Starting Time)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>t1</Name>
                <BitLen>5</BitLen>
                <Comment>T1'</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The T2 field is coded as the binary representation of FN mod 26.</Section>
                <Section>Reference : [GSM_04.08] section 10.5.2.38 (Starting Time)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>t2</Name>
                <BitLen>5</BitLen>
                <Comment>T2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The T3 field is coded as the binary representation of FN mod 51.</Section>
                <Section>Reference : [GSM_04.08] section 10.5.2.38 (Starting Time)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>t3</Name>
                <BitLen>6</BitLen>
                <Comment>T3</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="2000"/>
                <Author>ROZ</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This field is the binary representation of the PSIX count.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>psix_cnt</Name>
                <BitLen>4</BitLen>
                <Comment>PSIX_COUNT</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="18" Month="1" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The FREQ_DIFF parameter field specifies the difference in frequency to the next carrier to be defined. The Frequency Diff parameter encodes a non negative integer in binary format (W). The length of the field is defined by the Freq Diff length parameter. Note that the difference can be zero in which case the same frequency is listed twice.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>freq_diff</Name>
                <BitLen>8</BitLen>
                <Comment>FREQ_DIFF</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="21" Month="2" Year="2001"/>
                <Author>SAB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Defines the identity digits in mobile allocation.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ident_digit</Name>
                <BitLen>8</BitLen>
                <Comment>identity digit</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="11" Month="9" Year="2001"/>
                <Author>ID</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
    </MsgBasicElementsSection>
    <ValuesSection>
        <Description>
            <Section>This section contains all sets of values that are defined for the GRR AIM</Section>
        </Description>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ps</Name>
                <Comment>values for ps</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NO</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>YES</Alias>
                <Comment>present</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_msg_type</Name>
                <Comment>values for msg_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">100001</Value>
                <Alias>D_ACCESS_REJ_c</Alias>
                <Comment>Packet Access Reject</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000110</Value>
                <Alias>D_QUEUING_NOT_c</Alias>
                <Comment>Packet Queuing Notification</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000101</Value>
                <Alias>U_RESOURCE_REQ_c</Alias>
                <Comment>Packet Resource Request</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">001010</Value>
                <Alias>D_UL_ASSIGN_c</Alias>
                <Comment>Packet Uplink Assignment</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000010</Value>
                <Alias>D_DL_ASSIGN_c</Alias>
                <Comment>Packet Downlink Assignment</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">001000</Value>
                <Alias>D_TBF_RELEASE_c</Alias>
                <Comment>Packet TBF Release</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">100010</Value>
                <Alias>D_PAGING_REQ_c</Alias>
                <Comment>Packet Paging Request</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000010</Value>
                <Alias>U_DL_ACK_c</Alias>
                <Comment>Packet Downlink Ack/Nack</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">001001</Value>
                <Alias>D_UL_ACK_c</Alias>
                <Comment>Packet Uplink Ack/Nack</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">110001</Value>
                <Alias>PSI_1_c</Alias>
                <Comment>Packet System Information Type 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">110010</Value>
                <Alias>PSI_2_c</Alias>
                <Comment>Packet System Information Type 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">110011</Value>
                <Alias>PSI_3_c</Alias>
                <Comment>Packet System Information Type 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">110100</Value>
                <Alias>PSI_3_BIS_c</Alias>
                <Comment>Packet System Information Type 3 bis</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">110101</Value>
                <Alias>PSI_4_c</Alias>
                <Comment>Packet System Information Type 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">110110</Value>
                <Alias>PSI_5_c</Alias>
                <Comment>Packet System Information Type 5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">110111</Value>
                <Alias>PSI_13_c</Alias>
                <Comment>Packet System Information Type 13</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000001</Value>
                <Alias>U_CTRL_ACK_c</Alias>
                <Comment>Packet Control Acknowledgement</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000000</Value>
                <Alias>U_CELL_CHAN_FAILURE_c</Alias>
                <Comment>Packet Cell Change Failure</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000001</Value>
                <Alias>D_CELL_CHAN_ORDER_c</Alias>
                <Comment>Packet Cell Change Order</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">100101</Value>
                <Alias>D_DL_DUMMY_c</Alias>
                <Comment>Packet Downlink Dummy Control Block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000011</Value>
                <Alias>U_UL_DUMMY_c</Alias>
                <Comment>Packet Uplink Dummy Control Block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000100</Value>
                <Alias>U_MEAS_REPORT_c</Alias>
                <Comment>Packet Measurement Report</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000011</Value>
                <Alias>D_MEAS_ORDER_c</Alias>
                <Comment>Packet Measurement Order</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000110</Value>
                <Alias>U_MS_TBF_STATUS_c</Alias>
                <Comment>Packet Mobile TBF Status</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">100011</Value>
                <Alias>D_PDCH_RELEASE_c</Alias>
                <Comment>Packet PDCH Release</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000100</Value>
                <Alias>D_POLLING_REQ_c</Alias>
                <Comment>Packet Polling Request</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000101</Value>
                <Alias>D_CTRL_PWR_TA_c</Alias>
                <Comment>Packet Power Control/Timing Advance</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">100100</Value>
                <Alias>D_PRACH_PAR_c</Alias>
                <Comment>Packet PRACH Parameters</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000111</Value>
                <Alias>U_PSI_STATUS_MSG_c</Alias>
                <Comment>Packet PSI Status Message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">000111</Value>
                <Alias>D_TS_RECONFIG_c</Alias>
                <Comment>Packet Timeslot Reconfigure</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_page_mode</Name>
                <Comment>values for page_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias>NORMAL_PAGING</Alias>
                <Comment>Normal Paging</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias>EXT_PAGING</Alias>
                <Comment>Extended Paging</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10</Value>
                <Alias>REORG_PAGING</Alias>
                <Comment>Paging Reorganisation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11</Value>
                <Alias>SAME_PAGING</Alias>
                <Comment>Same as before</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_access_type</Name>
                <Comment>values for access_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias>TWO_PHASE</Alias>
                <Comment>Two Phase Access Request</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias>PAGE</Alias>
                <Comment>Page Response</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10</Value>
                <Alias>CELL_UPDATE</Alias>
                <Comment>Cell Update</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11</Value>
                <Alias>MM_PROC</Alias>
                <Comment>Mobility Management procedure</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_chan_coding_cmd</Name>
                <Comment>values for chan_coding_cmd</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias/>
                <Comment>CS-1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias/>
                <Comment>CS-2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10</Value>
                <Alias/>
                <Comment>CS-3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11</Value>
                <Alias/>
                <Comment>CS-4</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tlli_chan_coding</Name>
                <Comment>values for tlli_chan_coding</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>the MS shall use CS-1 for any RLC data block containing a TLLI in the RLC data block header</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>the MS shall use the value commanded in the CHANNEL_CODING_COMMAND for any RLC data block containing a TLLI in the RLC data block header</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_mac_mode</Name>
                <Comment>values for mac_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DYNAMIC_ALLOCATION</Alias>
                <Comment>Dynamic allocation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EXT_DYNAMIC_ALLOCATION</Alias>
                <Comment>Extended Dynamic allocation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>FIXED_ALLOCATION</Alias>
                <Comment>Fixed allocation, not half duplex mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>FA_HALF_DUPLEX</Alias>
                <Comment>Fixed allocation, half duplex mode</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_rlc_mode</Name>
                <Comment>values for rlc_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>RLC acknowledged mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>RLC unacknowledged mode</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pctrl_ack</Name>
                <Comment>values for pctrl_ack</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>reserved - this value shall not be sent. If received it shall be interpreted as bit value '1'.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>the MS received an RLC/MAC control block addressed to itself and with RBSN = 1, and did not receive an RLC/MAC control block with the same RTI value and RBSN = 0.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias/>
                <Comment>the MS received an RLC/MAC control block addressed to itself and with RBSN = 0, and did not receive an RLC/MAC control block with the same RTI value and RBSN = 1. This value is sent irrespective of the value of the FS bit.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias/>
                <Comment>the MS received two RLC/MAC blocks with the same RTI value, one with RBSN = 0 and the other with RBSN = 1.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_rel_cause</Name>
                <Comment>values for rel_cause</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NORMAL_RELEASE</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>ABNORMAL_RELEASE</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_psi_change_field</Name>
                <Comment>values for psi_change_field</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">0000</Value>
                <Alias>UPDATE_UNS_PSI</Alias>
                <Comment>Update of unspecified PSI message(s);</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0001</Value>
                <Alias>UPDATE_UNKNOWN</Alias>
                <Comment>Unknown</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0010</Value>
                <Alias>UPDATE_PSI2</Alias>
                <Comment>PSI2 updated</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0011</Value>
                <Alias>UPDATE_PSI3</Alias>
                <Comment>PSI3/PSI3bis updated</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100</Value>
                <Alias>UPDATE_PSI4</Alias>
                <Comment>PSI4 updated</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0101</Value>
                <Alias>UPDATE_PSI5</Alias>
                <Comment>PSI5 updated</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_si_change_ma</Name>
                <Comment>values for si_change_ma</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>Update of unspecified SI message or SI messages;</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>Update of SI1 message;</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias/>
                <Comment>Update of SI2, SI2 bis or SI2 ter message;</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias/>
                <Comment>Update of SI3, SI4, SI7 or SI8 message;</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias/>
                <Comment>Update of SI9 message;</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias/>
                <Comment>Update of SI15 message;</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>update of unknown SI message type</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_failure_cause</Name>
                <Comment>values for failure_cause</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>Freq_Not_Impl</Alias>
                <Comment>Frequency not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>No_Resp_On_Target_Cell</Alias>
                <Comment>No response on target cell</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>ImAssign_Rej_OR_Packet_Acc_Rej</Alias>
                <Comment>Immediate Assign Reject or Packet Access Reject on target cell</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>On_Going_Cs_Connection</Alias>
                <Comment>On going CS connection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>Annonymous_Access</Alias>
                <Comment>Anonymous Access</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>S_IN_GMM_Standby_State</Alias>
                <Comment>MS in GMM Standby State</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>Forced_To_GMM_Standby_State</Alias>
                <Comment>Forced to the Standby State</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Immediate Assign Reject or Packet Access Reject on target cell</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ctrl_order</Name>
                <Comment>values for ctrl_order</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NCMEAS_NC0</Alias>
                <Comment>NC0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NCMEAS_NC1</Alias>
                <Comment>NC1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>NCMEAS_NC2</Alias>
                <Comment>NC2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>NCMEAS_RESET</Alias>
                <Comment>RESET</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_alpha</Name>
                <Comment>values for alpha</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">0000</Value>
                <Alias/>
                <Comment>Alpha = 0.0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0001</Value>
                <Alias/>
                <Comment>Alpha = 0.1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0010</Value>
                <Alias/>
                <Comment>Alpha = 0.2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0011</Value>
                <Alias/>
                <Comment>Alpha = 0.3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100</Value>
                <Alias/>
                <Comment>Alpha = 0.4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0101</Value>
                <Alias/>
                <Comment>Alpha = 0.5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0110</Value>
                <Alias/>
                <Comment>Alpha = 0.6</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0111</Value>
                <Alias/>
                <Comment>Alpha = 0.7</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1000</Value>
                <Alias/>
                <Comment>Alpha = 0.8</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1001</Value>
                <Alias/>
                <Comment>Alpha = 0.9</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1010</Value>
                <Alias/>
                <Comment>Alpha = 1.0</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pb</Name>
                <Comment>values for pb</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">0000</Value>
                <Alias/>
                <Comment>PB = 0 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0001</Value>
                <Alias/>
                <Comment>PB = -2 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0010</Value>
                <Alias/>
                <Comment>PB = -4 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0011</Value>
                <Alias/>
                <Comment>PB = -6 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100</Value>
                <Alias/>
                <Comment>PB = -8 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0101</Value>
                <Alias/>
                <Comment>PB = -10 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0110</Value>
                <Alias/>
                <Comment>PB = -12 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0111</Value>
                <Alias/>
                <Comment>PB = -14 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1000</Value>
                <Alias/>
                <Comment>PB = -16 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1001</Value>
                <Alias/>
                <Comment>PB = -18 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1010</Value>
                <Alias/>
                <Comment>PB = -20 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1011</Value>
                <Alias/>
                <Comment>PB = -22 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100</Value>
                <Alias/>
                <Comment>PB = -24 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1101</Value>
                <Alias/>
                <Comment>PB = -26 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1110</Value>
                <Alias/>
                <Comment>PB = -28 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1111</Value>
                <Alias/>
                <Comment>PB = -30 dB</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pc_meas_chan</Name>
                <Comment>values for pc_meas_chan</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MEAS_PWR_BCCH</Alias>
                <Comment>downlink measurements for power control shall be made on BCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MEAS_PWR_PDCH</Alias>
                <Comment>downlink measurements for power control shall be made on PDCH</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_imeas_chan_list</Name>
                <Comment>values for imeas_chan_list</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PSI4_BROADCASTED</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PSI4_NOT_BROADCASTED</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_chan_need</Name>
                <Comment>values for chan_need</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias/>
                <Comment>Any channel</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias/>
                <Comment>SDCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10</Value>
                <Alias/>
                <Comment>TCH/F (Full rate)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11</Value>
                <Alias/>
                <Comment>TCH/H or TCH/F</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_nmo</Name>
                <Comment>values for nmo</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias/>
                <Comment>Network Mode 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias/>
                <Comment>Network Mode 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10</Value>
                <Alias/>
                <Comment>Network Mode 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ab_type</Name>
                <Comment>values for ab_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>AB_8_BIT</Alias>
                <Comment>8 bit access burst shall be used</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>AB_11_BIT</Alias>
                <Comment>11 bit access burst shall be used</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ctrl_ack_type</Name>
                <Comment>values for ctrl_ack_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>default format is four access bursts</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>default format is RLC/MAC control block.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tx_int</Name>
                <Comment>values for tx_int</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>2 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>3 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias/>
                <Comment>4 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias/>
                <Comment>5 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias/>
                <Comment>6 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias/>
                <Comment>7 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias/>
                <Comment>8 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias/>
                <Comment>9 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias/>
                <Comment>10 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias/>
                <Comment>12 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias/>
                <Comment>14 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias/>
                <Comment>16 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias/>
                <Comment>20 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">13</Value>
                <Alias/>
                <Comment>25 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias/>
                <Comment>32 slots used to spread transmission</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias/>
                <Comment>50 slots used to spread transmission</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_s_prach</Name>
                <Comment>values for s_prach</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>S=12</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>S=15</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias/>
                <Comment>S=20</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias/>
                <Comment>S=30</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias/>
                <Comment>S=41</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias/>
                <Comment>S=55</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias/>
                <Comment>S=76</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias/>
                <Comment>S=109</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias/>
                <Comment>S=163</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias/>
                <Comment>S=217</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_max_retrans</Name>
                <Comment>values for max_retrans</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>1 retransmission allowed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>2 retransmission allowed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias/>
                <Comment>4 retransmission allowed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias/>
                <Comment>7 retransmission allowed</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_radio_prio</Name>
                <Comment>values for radio_prio</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>Radio Priority 1 (Highest priority)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>Radio Priority 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias/>
                <Comment>Radio Priority 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias/>
                <Comment>Radio Priority 4 (Lower priority)</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_llc_pdu_type</Name>
                <Comment>values for llc_pdu_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>LLC PDU is SACK or ACK</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>LLC PDU is not SACK or ACK</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bs_pbcch_blks</Name>
                <Comment>values for bs_pbcch_blks</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias/>
                <Comment>B0 is used for PBCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias/>
                <Comment>B0, B6 is used for PBCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10</Value>
                <Alias/>
                <Comment>B0, B6, B3 is used for PBCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9 is used for PBCCH</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bs_prach_blks</Name>
                <Comment>values for bs_prach_blks</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">0000</Value>
                <Alias/>
                <Comment>No block is reserved for PRACH (default)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0001</Value>
                <Alias/>
                <Comment>B0 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0010</Value>
                <Alias/>
                <Comment>B0, B6 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0011</Value>
                <Alias/>
                <Comment>B0, B6, B3 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0101</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0110</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0111</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7, B4 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1000</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7, B4, B10 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1001</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7, B4, B10, B2 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1010</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7, B4, B10, B2, B8 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1011</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7, B4, B10, B2, B8, B5 is used for PRACH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100</Value>
                <Alias/>
                <Comment>B0, B6, B3, B9, B1, B7, B4, B10, B2, B8, B5, B11 is used for PRACH</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_cell_ba</Name>
                <Comment>values for cell_ba</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CR_ALLOWED</Alias>
                <Comment>Status for cell reselection is set to normal;</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CR_NOT_WED</Alias>
                <Comment>Status for cell reselection is set to barred.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_gprs_resel_off</Name>
                <Comment>values for gprs_resel_off</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">16</Value>
                <Alias>GPRS_RESEL_OFF_DEFAULT</Alias>
                <Comment>Default value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>GPRS_RESEL_OFF_INVALID</Alias>
                <Comment>This value is used to indicate the absence of this parameter</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_si13_loc</Name>
                <Comment>values for si13_loc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>BCCH_NORM</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>BCCH_EXT</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pbcch_loc</Name>
                <Comment>values for pbcch_loc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias>PBCCH_TN1</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias>PBCCH_TN2</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10</Value>
                <Alias>PBCCH_TN3</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11</Value>
                <Alias>PBCCH_TN4</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_gprs_prio_class</Name>
                <Comment>values for gprs_prio_class</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">FF</Value>
                <Alias>GPRS_PRIORITY_CLASS_INVALID</Alias>
                <Comment>This value is used to indicate the absence of this parameter</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_gprs_hcs_thr</Name>
                <Comment>values for gprs_hcs_thr</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">FF</Value>
                <Alias>GPRS_HCS_THR_INVALID</Alias>
                <Comment>This value is used to indicate the absence of this parameter</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_gprs_rxlev_access_min</Name>
                <Comment>values for gprs_rxlev_access_min</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">FF</Value>
                <Alias>GPRS_RXLEV_ACCESS_MIN_INVALID</Alias>
                <Comment>This value is used to indicate the absence of this parameter</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_txpwr_max_cch</Name>
                <Comment>values for txpwr_max_cch</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">FF</Value>
                <Alias>GPRS_MS_TXPWR_MAX_CCH_INVALID</Alias>
                <Comment>This value is used to indicate the absence of this parameter</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_gprs_temp_offset</Name>
                <Comment>values for gprs_temp_offset</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">000</Value>
                <Alias>GPRS_TEMPORARY_OFFSET_00_DB</Alias>
                <Comment>0 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">001</Value>
                <Alias>GPRS_TEMPORARY_OFFSET_10_DB</Alias>
                <Comment>10 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">010</Value>
                <Alias>GPRS_TEMPORARY_OFFSET_20_DB</Alias>
                <Comment>20 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">011</Value>
                <Alias>GPRS_TEMPORARY_OFFSET_30_DB</Alias>
                <Comment>30 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">100</Value>
                <Alias>GPRS_TEMPORARY_OFFSET_40_DB</Alias>
                <Comment>40 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">101</Value>
                <Alias>GPRS_TEMPORARY_OFFSET_50_DB</Alias>
                <Comment>50 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">110</Value>
                <Alias>GPRS_TEMPORARY_OFFSET_60_DB</Alias>
                <Comment>60 dB</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">111</Value>
                <Alias>GPRS_TEMPORARY_OFFSET_INFINITY</Alias>
                <Comment>infinity</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">FF</Value>
                <Alias>GPRS_TEMPORARY_OFFSET_INVALID</Alias>
                <Comment>This value is used to indicate the absence of this parameter</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_gprs_penalty_time</Name>
                <Comment>values for gprs_penalty_time</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">11111</Value>
                <Alias>GPRS_PENALTY_TIME_MAX</Alias>
                <Comment>Maximum value of GPRS_PENALTY_TIME</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">FF</Value>
                <Alias>GPRS_PENALTY_TIME_INVALID</Alias>
                <Comment>This value is used to indicate the absence of this parameter</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_waitsize</Name>
                <Comment>values for waitsize</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>WAIT_1S</Alias>
                <Comment>field is coded in units of seconds</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>WAIT_20ms</Alias>
                <Comment>field is coded in units of 20 ms</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bl_o_bl_per</Name>
                <Comment>values for bl_o_bl_per</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>BLOCKS</Alias>
                <Comment>ALLOCATION_BITMAP is to be interpreted as blocks</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>BLOCK_PERIODS</Alias>
                <Comment>ALLOCATION_BITMAP is to be interpreted as block periods</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_att</Name>
                <Comment>values for att</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CCD_ATT_NO</Alias>
                <Comment>MSs are not allowed to apply IMSI attach and detach proc.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CCD_ATT_YES</Alias>
                <Comment>MSs in the cell shall apply IMSI attach and detach procedure.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_neci</Name>
                <Comment>values for neci</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NECI_NO</Alias>
                <Comment>New establishment causes are not supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NECI_YES</Alias>
                <Comment>New establishment causes are supported</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pwcr</Name>
                <Comment>values for pwcr</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>POW_CTRL_NO</Alias>
                <Comment>PWRC is not set</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>POW_CTRL_YES</Alias>
                <Comment>PWRC is set</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_dtx</Name>
                <Comment>values for dtx</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>B_DTX_MAY_USE</Alias>
                <Comment>The MSs may use uplink DTX</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>B_DTX_SHALL_USE</Alias>
                <Comment>The MSs shall use uplink DTX</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>B_DTX_DONT_USE</Alias>
                <Comment>The MS shall not use uplink DTX</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>invalid DTX indicator</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_rfl_num</Name>
                <Comment>values for rfl_num</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">0F</Value>
                <Alias>RFL_NUMBER_4_DL_CTRL_MSG_MAX</Alias>
                <Comment>Maximum value for RFL_NUMBER when included in a downlink RLC/MAC control messsage.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ra_retry</Name>
                <Comment>values for ra_retry</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">0</Value>
                <Alias>GRR_RA_RETRY_DISABLED</Alias>
                <Comment>access to another cell is not allowed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1</Value>
                <Alias>GRR_RA_RETRY_ENABLED</Alias>
                <Comment>access to another cell is allowed</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_t_resel</Name>
                <Comment>values for t_resel</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">000</Value>
                <Alias>GRR_T_RESEL_DEFAULT</Alias>
                <Comment>5 seconds</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">001</Value>
                <Alias/>
                <Comment>10 seconds</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">010</Value>
                <Alias/>
                <Comment>15 seconds</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">011</Value>
                <Alias/>
                <Comment>20 seconds</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">100</Value>
                <Alias/>
                <Comment>30 seconds</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">101</Value>
                <Alias/>
                <Comment>60 seconds</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">110</Value>
                <Alias/>
                <Comment>120 seconds</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">111</Value>
                <Alias/>
                <Comment>300 seconds</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_non_drx_per</Name>
                <Comment>values for non_drx_per</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">010</Value>
                <Alias>NC_NON_DRX_PER_DEFAULT</Alias>
                <Comment>Non-DRX mode period default value (0.48 sec)</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_rep_per_i</Name>
                <Comment>values for rep_per_i</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">011</Value>
                <Alias>NC_REP_PER_T_DEFAULT</Alias>
                <Comment>Reporting period default value in packet transfer mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">111</Value>
                <Alias>NC_REP_PER_I_DEFAULT</Alias>
                <Comment>Reporting period default value in packet idle mode</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_xrep_per</Name>
                <Comment>values for xrep_per</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">101</Value>
                <Alias>EXT_REP_PER_DEFAULT</Alias>
                <Comment>Reporting period default value</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_xrep_type</Name>
                <Comment>values for xrep_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias>XREP_TYPE1</Alias>
                <Comment>Type 1 measurement reporting</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias>XREP_TYPE2</Alias>
                <Comment>Type 2 measurement reporting</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10</Value>
                <Alias>XREP_TYPE3</Alias>
                <Comment>Type 3 measurement reporting</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11</Value>
                <Alias>XREP_RESERVED</Alias>
                <Comment>Reserved</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_prio_acc_thr</Name>
                <Comment>values for prio_acc_thr</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">000</Value>
                <Alias>P_NOT_ALLOWED</Alias>
                <Comment>packet access is not allowed in the cell;</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">001</Value>
                <Alias/>
                <Comment>spare, shall be interpreted as '000' (packet access not allowed);</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">010</Value>
                <Alias/>
                <Comment>spare, shall be interpreted as '000' (packet access not allowed);</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">011</Value>
                <Alias>P_PRIO1</Alias>
                <Comment>packet access is allowed for priority level 1;</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">100</Value>
                <Alias>P_PRIO2</Alias>
                <Comment>packet access is allowed for priority level 1 to 2;</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">101</Value>
                <Alias>P_PRIO3</Alias>
                <Comment>packet access is allowed for priority level 1 to 3;</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">110</Value>
                <Alias>P_PRIO4</Alias>
                <Comment>packet access is allowed for priority level 1 to 4;</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">111</Value>
                <Alias/>
                <Comment>shall be interpreted as '110' (packet access allowed).</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_spgc_ccch_sup</Name>
                <Comment>values for spgc_ccch_sup</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SPLIT_PG_CYCLE_NOT_SUPPORTED</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SPLIT_PG_CYCLE_SUPPORTED</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_nc_mode</Name>
                <Comment>values for nc_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NCMODE_NC1</Alias>
                <Comment>Mobile station in mode NC1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NCMODE_NC2</Alias>
                <Comment>Mobile station in mode NC2</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_xdyn_alloc</Name>
                <Comment>values for xdyn_alloc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DYNAMIC_ALLOC</Alias>
                <Comment>Dynamic Allocation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EXT_DYNAMIC_ALLOC</Alias>
                <Comment>Extended Dynamic Allocation</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_usf_grant</Name>
                <Comment>values for usf_grant</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ONE_RLC_BLOCK</Alias>
                <Comment>the ms shall transmit one RLC/MAC block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>FOUR_C_RLC_BLOCKS</Alias>
                <Comment>the ms shall transmit four consecutive RLC/MAC blocks</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_rbb</Name>
                <Comment>values for rbb</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>INVALID</Alias>
                <Comment>Negative Ack of the RLC data block with BSN=(SSN-bit_nr)mod128</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>RECEIVED</Alias>
                <Comment>Positive Ack of the RLC data block with BSN=(SSN-bit_nr)mod128</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_f_ack_ind</Name>
                <Comment>values for f_ack_ind</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>retransmission are requested and the TBF is incomplete</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>no retransmissions are requested and this message indicates acknowledgement of all RLC data in the TBF</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_generation</Name>
                <Comment>values for generation</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias>GENERATION_DEFAULT</Alias>
                <Comment>Default value for parameter generation.</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_im_rel</Name>
                <Comment>values for im_rel</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>Same procedure as for an autonomous cell reselection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>Immediate release of the on-going TBF</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_mode</Name>
                <Comment>values for mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MODE_A</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MODE_B</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tbf_cause</Name>
                <Comment>values for tbf_cause</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias/>
                <Comment>Normal event</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias/>
                <Comment>Status, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias/>
                <Comment>Syntactically incorrect message, non-distribution part error</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias/>
                <Comment>Syntactically incorrect message, message escape</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias/>
                <Comment>Message not compatible with current protocol state</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Status, unspecified</Comment>
            </ValuesDefault>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_psi_status_ind</Name>
                <Comment>values for psi_status_ind</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NO_PSI_STATUS_SUPPORT</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PSI_STATUS_SUPPORT</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_multi_band_rep</Name>
                <Comment>values for multi_band_rep</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>GRR_MULTIBAND_REPORTING_0</Alias>
                <Comment>normal operation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>GRR_MULTIBAND_REPORTING_1</Alias>
                <Comment>one cell of the non-serving cell band</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>GRR_MULTIBAND_REPORTING_2</Alias>
                <Comment>two cells of the non-serving cell band</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>GRR_MULTIBAND_REPORTING_3</Alias>
                <Comment>three cells of the non-serving cell band</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pr_mode</Name>
                <Comment>values for pr_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PR_MODE_A</Alias>
                <Comment>for one address MS</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PR_MODE_B</Alias>
                <Comment>for all MS</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_xmeas_order</Name>
                <Comment>values for xmeas_order</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias>XMEAS_EM0</Alias>
                <Comment>EM0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias>XMEAS_EM1</Alias>
                <Comment>EM1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10</Value>
                <Alias>XMEAS_RESERVED</Alias>
                <Comment>Reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">11</Value>
                <Alias>XMEAS_RESET</Alias>
                <Comment>RESET</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
    </ValuesSection>
</AIM>
