<?xml version="1.0" encoding="UTF-8"?>
<!-- edited with SAPE SAP Editor -->
<SAP xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="sap.xsd">
    <DocInfoSection>
        <DocName DocType="SAP">mphc</DocName>
        <DocNum Number="10" Project="10"/>
        <Description>
            <Section>The Protocol Stacks are used to define the functionality of the GSM protocols for interfaces. The GSM specifications are normative when used to describe the functionality of interfaces, but the stacks and the subdivision of protocol layers does not imply or restrict any implementation.</Section>
            <Section>The base of the Protocol Stack rests on the physical layer.</Section>
            <Section>The Data Link Layer (DL) is used to handle an acknowledged connection between mobile and base station. The LAPDm protocol is used.</Section>
            <Section>Radio Resource (RR) manages the resources of the air-interface. That means configuration of physical layer, cell selection and cell reselection, data transfer, RR-Connection handling.</Section>
            <Section>Mobility Management (MM) handles registration aspects for the mobile station. It detects changes of location areas and updates a mobile station in the new location area.</Section>
            <Section>Call Control (CC) provides the call functionality. This includes call establishment, call maintenance procedures like Hold, Retrieve or Modify, and call disconnection.</Section>
            <Section>Supplementary Services (SS) handles all call independent supplementary services like call forwarding or call barring.</Section>
            <Section>Short Message Services (SMS) is used for sending and receiving point-to-point short messages. Additionally the reception of cell broadcast short messages is included.</Section>
            <Section>The man machine interface (MMI) is the interface to the user. Normally it is connected with a keypad as input device and a display as output device.</Section>
            <Section>Between the several entities data interfaces are defined. These data interfaces are called Service Access Points (SAPs), indicating that an upper layer uses the services of a lower layer.</Section>
            <Section>The GSM specification do not set out any implementation of the Protocol Stack. The following diagrams show the implementation described in all these documents for the mobile station. All entities except the Man Machine Interface and Physical Layer are implemented as part of the Protocol Stack.</Section>
            <Section>This document describes the services offered by the TI layer 1 to the upper layer.</Section>
        </Description>
        <DocHistory>
            <DocVersion Number="001" Year="10"/>
            <Date Day="6" Month="9" Year="1998"/>
            <Author>MPA</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Initial version for ALR 0.7.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="002" Year="10"/>
            <Date Day="30" Month="5" Year="1999"/>
            <Author>MPA</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Adapted Opcodes for new ALR version</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="003" Year="10"/>
            <Date Day="28" Month="8" Year="2001"/>
            <Author>MSB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Correct BCCH allocation channel list sizes.  Use new Document control.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="004" Year="10"/>
            <Date Day="14" Month="11" Year="2001"/>
            <Author>MSB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Add Multi-Band primitives</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="005" Year="10"/>
            <Date Day="18" Month="2" Year="2002"/>
            <Author>OT</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Adaptations for AMR support added</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="006" Year="10"/>
            <Date Day="15" Month="4" Year="2002"/>
            <Author>LG</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>MPHC_DEACTIVATE_REQ added</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="007" Year="10"/>
            <Date Day="30" Month="4" Year="2002"/>
            <Author>MSB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Only one type of sub_channel</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="008" Year="10"/>
            <Date Day="27" Month="6" Year="2002"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>MPHC_INIT_IDS_REQ removed, not supported any longer by L1</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="009" Year="10"/>
            <Date Day="15" Month="8" Year="2002"/>
            <Author>LG</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Adaptations for E-OTD support added</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="010" Year="10"/>
            <Date Day="4" Month="2" Year="2003"/>
            <Author>LG</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>renamed components of start_time</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="011" Year="10"/>
            <Date Day="3" Month="4" Year="2003"/>
            <Author>MSB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>- fix missalignment of MPHC_NCELL_SYNC_IND - add TST_TEST_HW_REQ/CON - add debug variables in the dedicated power measurement interface MPHC_MEAS_REPORT 0.1</Comment>
        </DocHistory>
        <DocRef>
            <RefId>[C_7010.801]</RefId>
            <RefTitle>7010.801, References and Vocabulary, Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[GSM_04.07]</RefId>
            <RefTitle>GSM 4.07, Mobile Radio Interface Signalling Layer 3 General AspectsETS 300 556, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[GSM_04.08]</RefId>
            <RefTitle>GSM 4.08, Mobile Radio Interface Layer 3 SpecificationETS 300 557, ETSI, January 1996</RefTitle>
        </DocRef>
    </DocInfoSection>
    <ConstantsSection>
        <Description>
            <Section>This section contains all constants that are defined for the MPHC SAP</Section>
        </Description>
        <Constant>
            <Alias>BA_LIST_SIZE</Alias>
            <Value ValueType="DEC">33</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_NCELL_EOTD_L1</Alias>
            <Value ValueType="DEC">12</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_NCELL</Alias>
            <Value ValueType="DEC">6</Value>
            <Comment>number of neighbour cells in measurement reports</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CARRIERS</Alias>
            <Value ValueType="DEC">548</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>BCCH_LIST_SIZE</Alias>
            <Value ValueType="DEC">32</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_MEAS_VALUES</Alias>
            <Value ValueType="DEC">8</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_L2_FRAME_SIZE</Alias>
            <Value ValueType="DEC">23</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_MA_CARRIER</Alias>
            <Value ValueType="DEC">64</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_SCHED_SIZE</Alias>
            <Value ValueType="DEC">10</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>ADC_LIST_SIZE</Alias>
            <Value ValueType="DEC">5</Value>
            <Comment/>
        </Constant>
        <History>
            <Date Day="6" Month="9" Year="1999"/>
            <Author>MPA</Author>
            <Comment>Initial</Comment>
        </History>
        <History>
            <Date Day="15" Month="11" Year="2001"/>
            <Author>MSB</Author>
            <Comment>move MAX_.._CARRIERS to MPH SAP</Comment>
        </History>
        <History>
            <Date Day="31" Month="1" Year="2002"/>
            <Author>MSB</Author>
            <Comment>decrease MAX_CARRIER (848-&gt;548)</Comment>
        </History>
        <History>
            <Date Day="14" Month="8" Year="2002"/>
            <Author>LG</Author>
            <Comment>changed MAX_NCELL to 12 and renamed</Comment>
        </History>
        <History>
            <Date Day="27" Month="8" Year="2002"/>
            <Author>LG</Author>
            <Comment>re-added MAX_NCELL again</Comment>
        </History>
        <History>
            <Date Day="3" Month="9" Year="2002"/>
            <Author>LG</Author>
            <Comment>renamed MAX_NCELL_EOTD</Comment>
        </History>
    </ConstantsSection>
    <PrimitivesSection PrimIDType="BIT16" SAPid="0">
        <Description>
            <Section>This section contains all primitives that are defined for the MPHC SAP</Section>
        </Description>
        <Primitive>
            <Description>
                <Section>The MPHC_NETWORK_SYNC_REQ requests reading the FCH and SCH of the given cell.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_NETWORK_SYNC_REQ</Name>
                <PrimID Direction="UPLINK" Number="15"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>frame offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>time_alignment</Name>
                </ItemLink>
                <Comment>time alignment</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>timing_validity</Name>
                </ItemLink>
                <Comment>timing validity</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>search_mode</Name>
                </ItemLink>
                <Comment>search mode</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_NETWORK_SYNC_IND indicates the success or failure of the synchronisation attempt with the channel.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_NETWORK_SYNC_IND</Name>
                <PrimID Direction="UPLINK" Number="16"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>sb_flag</Name>
                </ItemLink>
                <Comment>valid flag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>frame offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>time_alignment</Name>
                </ItemLink>
                <Comment>time alignment</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Comment>base station identity code</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="10" Year="1999"/>
                <Author>MPA</Author>
                <Comment>changed error cause</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>sb_flag referenced</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_NETWORK_SYNC_REQ requests the stop of the synchronisation attempts for the cell.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_NETWORK_SYNC_REQ</Name>
                <PrimID Direction="UPLINK" Number="17"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_NETWORK_SYNC_CON confirms the stop of the synchronisation attempts.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_NETWORK_SYNC_CON</Name>
                <PrimID Direction="UPLINK" Number="18"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_START_CCCH_REQ is used to configure paging.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_START_CCCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="21"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>bs_pa_mfrms</Name>
                </ItemLink>
                <Comment>Multiframe period</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>bs_ag_blks_res</Name>
                </ItemLink>
                <Comment>BS AG BLOCKS reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>bcch_combined</Name>
                </ItemLink>
                <Comment>BCCH combined</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>ccch_group</Name>
                </ItemLink>
                <Comment>CCCH group</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>page_group</Name>
                </ItemLink>
                <Comment>paging group</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>page_block_index</Name>
                </ItemLink>
                <Comment>page block index</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>page_mode</Name>
                </ItemLink>
                <Comment>page mode</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_CCCH_REQ is used to stop paging.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_CCCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="22"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_CCCH_CON is used to confirm the stop of paging.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_CCCH_CON</Name>
                <PrimID Direction="UPLINK" Number="23"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_SCELL_NBCCH_REQ is used to start or reconfigure the reading of the BCCH.</Section>
                <Section>Note: a schedule_array_size of 0 implies to stop normal BCCH reading.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_SCELL_NBCCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="24"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>schedule_array_size</Name>
                </ItemLink>
                <Comment>number of elements in schedule array</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>schedule_array</Name>
                </ItemLink>
                <Control>[MAX_SCHED_SIZE]</Control>
                <Comment>schedule array</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_SCELL_EBCCH_REQ is used to start or reconfigure the reading of the extended BCCH.</Section>
                <Section>Note: a schedule_array_size of 0 implies to stop extended BCCH reading.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_SCELL_EBCCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="25"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>schedule_array_size</Name>
                </ItemLink>
                <Comment>number of elements in schedule array</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>schedule_array</Name>
                </ItemLink>
                <Control>[MAX_SCHED_SIZE]</Control>
                <Comment>schedule array</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_SCELL_BCCH_REQ is used to stop BCCH reading.</Section>
                <Section>Note: This stops both normal and extended BCCH reading.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_SCELL_BCCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="26"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_SCELL_BCCH_CON confirms the stop for BCCH reading.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_SCELL_BCCH_CON</Name>
                <PrimID Direction="UPLINK" Number="27"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_DATA_IND forwards a message from layer 1 to layer 3 containing a data block and related information.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_DATA_IND</Name>
                <PrimID Direction="UPLINK" Number="50"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>l2_channel</Name>
                </ItemLink>
                <Comment>layer 2 channel type</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>error_flag</Name>
                </ItemLink>
                <Comment>error cause</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>l2_frame</Name>
                </ItemLink>
                <Comment>layer 2 frame</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>tc</Name>
                </ItemLink>
                <Comment>multiframe number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>ccch_lev</Name>
                </ItemLink>
                <Comment>CCCH Level</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn</Name>
                </ItemLink>
                <Comment>frame number</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>MPA</Author>
                <Comment>added ccch_lev</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_NCELL_SYNC_REQ requests reading the FCH and SCH of the given neighbour cell.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_NCELL_SYNC_REQ</Name>
                <PrimID Direction="UPLINK" Number="32"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>frame offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>time_alignment</Name>
                </ItemLink>
                <Comment>time alignment</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>timing_validity</Name>
                </ItemLink>
                <Comment>timing validity</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_NCELL_LIST_SYNC_REQ requests reading the FCH and SCH of the given list of cells.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_NCELL_LIST_SYNC_REQ</Name>
                <PrimID Direction="UPLINK" Number="122"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>eotd</Name>
                </ItemLink>
                <Comment>EOTD monitoring</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>list_size</Name>
                </ItemLink>
                <Comment>List Size</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>ncell_list</Name>
                </ItemLink>
                <Control>[MAX_NCELL_EOTD_L1]</Control>
                <Comment>Neighbour Cell List</Comment>
            </PrimItem>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="9" Year="2002"/>
                <Author>LG</Author>
                <Comment>renamed MAX_NCELL_EOTD</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_NCELL_SYNC_IND indicates the success or failure of the synchronisation attempt with the channel.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_NCELL_SYNC_IND</Name>
                <PrimID Direction="UPLINK" Number="33"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>sb_flag</Name>
                </ItemLink>
                <Comment>valid flag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>frame offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>time_alignment</Name>
                </ItemLink>
                <Comment>time alignment</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Comment>base station identity code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>neigh_id</Name>
                </ItemLink>
                <Comment>Reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>attempt</Name>
                </ItemLink>
                <Comment>Reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>pm</Name>
                </ItemLink>
                <Comment>Reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>toa</Name>
                </ItemLink>
                <Comment>Reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>angle</Name>
                </ItemLink>
                <Comment>Reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>snr</Name>
                </ItemLink>
                <Comment>Reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>eodt_data_valid</Name>
                </ItemLink>
                <Comment>EOTD Data valid</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>mode</Name>
                </ItemLink>
                <Comment>Mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>d_eotd_first</Name>
                </ItemLink>
                <Comment>Delay to first correlation</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>d_eotd_max</Name>
                </ItemLink>
                <Comment>Delay to maximum correlation</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>d_eotd_nrj</Name>
                </ItemLink>
                <Comment>Sum of Amplitudes</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>a_eotd_crosscor</Name>
                </ItemLink>
                <Control>[18]</Control>
                <Comment>Cross correlation</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>time_tag</Name>
                </ItemLink>
                <Comment>Time tag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_sb_neigh</Name>
                </ItemLink>
                <Comment>Reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_in_sb</Name>
                </ItemLink>
                <Comment>Reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>toa_correction</Name>
                </ItemLink>
                <Comment>Reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>delta_fn</Name>
                </ItemLink>
                <Comment>Reserved</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>delta_qbit</Name>
                </ItemLink>
                <Comment>Reserved</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>sb_flag referenced</Comment>
            </History>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>neigh_id until delta_qbit added</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_NCELL_SYNC_REQ requests the stop of the synchronisation attempts for the given cells.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_NCELL_SYNC_REQ</Name>
                <PrimID Direction="UPLINK" Number="34"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq_array_size</Name>
                </ItemLink>
                <Comment>number of channels</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq_array</Name>
                </ItemLink>
                <Control>[MAX_NCELL_EOTD_L1]</Control>
                <Comment>channel list</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>set length of radio_freq_array to MAX_NCELL_EOTD</Comment>
            </History>
            <History>
                <Date Day="3" Month="9" Year="2002"/>
                <Author>LG</Author>
                <Comment>renamed MAX_NCELL_EOTD</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_NCELL_SYNC_CON confirms the stop of the synchronisation attempts.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_NCELL_SYNC_CON</Name>
                <PrimID Direction="UPLINK" Number="35"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_NCELL_BCCH_REQ is used to request reading of system information from the BCCH for the acquired or confirmed neighbour cells.</Section>
                <Section>Note: This is a one-shot primitive but it can be send up to six times for different channels and layer 1 processes them independently. No "on the fly" supported.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_NCELL_BCCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="28"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>frame offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>time_alignment</Name>
                </ItemLink>
                <Comment>time alignment</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <Comment>training sequence code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>bcch_blocks_required</Name>
                </ItemLink>
                <Comment>sys info bitmap</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>gprs_prio</Name>
                </ItemLink>
                <Comment>GPRS Priority</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>MPA</Author>
                <Comment>added GPRS Priority</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_NCELL_BCCH_IND forwards a message from layer 1 to layer 3 containing a data block and related information from a non-serving cell.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_NCELL_BCCH_IND</Name>
                <PrimID Direction="UPLINK" Number="29"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>l2_channel</Name>
                </ItemLink>
                <Comment>layer 2 channel type</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>error_flag</Name>
                </ItemLink>
                <Comment>error cause</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>l2_frame</Name>
                </ItemLink>
                <Comment>layer 2 frame</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>tc</Name>
                </ItemLink>
                <Comment>multiframe number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn</Name>
                </ItemLink>
                <Comment>frame number</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_NCELL_BCCH_REQ requests the stop of the BCCH reading for the given cells.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_NCELL_BCCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="30"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq_array_size</Name>
                </ItemLink>
                <Comment>number of channels</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq_array</Name>
                </ItemLink>
                <Control>[6]</Control>
                <Comment>channel list</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_NCELL_BCCH_CON confirms the stop of the BCCH reading.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_NCELL_BCCH_CON</Name>
                <PrimID Direction="UPLINK" Number="31"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_RXLEV_PERIODIC_REQ starts periodic power measurements of the neighbour cells.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_RXLEV_PERIODIC_REQ</Name>
                <PrimID Direction="UPLINK" Number="36"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>chan_list</Name>
                </ItemLink>
                <Comment>channel list</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>num_of_chans</Name>
                </ItemLink>
                <Comment>number of channels</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>ba_id</Name>
                </ItemLink>
                <Comment>band ID</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>next_radio_freq_measured</Name>
                </ItemLink>
                <Comment>next channel</Comment>
            </PrimItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_RXLEV_PERIODIC_IND returns the power strength level of the neighbour cells.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_RXLEV_PERIODIC_IND</Name>
                <PrimID Direction="UPLINK" Number="37"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>result</Name>
                </ItemLink>
                <Control>[MAX_MEAS_VALUES]</Control>
                <Comment>measurement results</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>nbr_of_carriers</Name>
                </ItemLink>
                <Comment>number of channels</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>s_rxlev</Name>
                </ItemLink>
                <Comment>serving cell rxlev</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>ba_id</Name>
                </ItemLink>
                <Comment>band ID</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_RXLEV_PERIODIC_REQ requests the stop of measurements.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_RXLEV_PERIODIC_REQ</Name>
                <PrimID Direction="UPLINK" Number="38"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_RXLEV_PERIODIC_CON confirms the stop of the BCCH reading.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_RXLEV_PERIODIC_CON</Name>
                <PrimID Direction="UPLINK" Number="39"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_RXLEV_REQ starts power measurements. A special adaption in dl1_mem.c had to be done for ALR because the primitve MPHC_RXLEV_REQ needs more memory than is dynamically allocable. Because of that a global memory area is used. To use this memory area and conform to MPHC_RXLEV_REQ interface of TI, we had to change the SigP for this primitive to point to global memory and not to data member of T_PRIM. The value of shared_ptr is used for SigP.</Section>
                <Section>Note: The ID is hardcoded in dl1_mem.c.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_RXLEV_REQ</Name>
                <PrimID Direction="UPLINK" Number="11"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>shared_ptr</Name>
                </ItemLink>
                <Comment>pointer to measurements</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>revised for SigP interface</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_RXLEV_REQ reports the power measurement.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_RXLEV_IND</Name>
                <PrimID Direction="UPLINK" Number="12"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>shared_ptr</Name>
                </ItemLink>
                <Comment>pointer to measurements</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="10" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>revised for SigP interface</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_RXLEV_ REQ requests the stop of measurements.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_RXLEV_REQ</Name>
                <PrimID Direction="UPLINK" Number="13"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_RXLEV_CON confirms the stop of measurements.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_RXLEV_CON</Name>
                <PrimID Direction="UPLINK" Number="14"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_CONFIG_CBCH_REQ is used by layer 3 to configure the cell broadcast channel.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_CONFIG_CBCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="40"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cbch_desc</Name>
                </ItemLink>
                <Comment>CBCH channel description</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cbch_freq_list</Name>
                </ItemLink>
                <Comment>Frequency list</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_CBCH_SCHEDULE_REQ is used by layer 3 to configure CBCH scheduling</Section>
                <Section>and the type cell broadcast channel.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_CBCH_SCHEDULE_REQ</Name>
                <PrimID Direction="UPLINK" Number="41"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cbch_select</Name>
                </ItemLink>
                <Comment>extended cbch flag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>schedule_length</Name>
                </ItemLink>
                <Comment>length of schedule period</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>first_blocks_0</Name>
                </ItemLink>
                <Comment>block bitmap</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>first_blocks_1</Name>
                </ItemLink>
                <Comment>block bitmap cont.</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_CBCH_INFO_REQ requests that additional blocks should be read.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_CBCH_INFO_REQ</Name>
                <PrimID Direction="UPLINK" Number="43"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>tb_bitmap</Name>
                </ItemLink>
                <Comment>block bitmap</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_CBCH_UPDATE_REQ is used by layer 3 to update CBCH scheduling.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_CBCH_UPDATE_REQ</Name>
                <PrimID Direction="UPLINK" Number="42"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cbch_select</Name>
                </ItemLink>
                <Comment>extended cbch flag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>first_blocks_0</Name>
                </ItemLink>
                <Comment>block bitmap</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>first_blocks_1</Name>
                </ItemLink>
                <Comment>block bitmap cont.</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_CBCH_REQ is used by layer 3 to stop CBCH reading.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_CBCH_REQ</Name>
                <PrimID Direction="UPLINK" Number="44"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>normal_cbch</Name>
                </ItemLink>
                <Comment>normal cbch</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>extended_cbch</Name>
                </ItemLink>
                <Comment>extended cbch</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_CBCH_CON confirms the stop of CBCH reading.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_CBCH_CON</Name>
                <PrimID Direction="UPLINK" Number="45"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_NEW_SCELL_REQ sets the new serving cell</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_NEW_SCELL_REQ</Name>
                <PrimID Direction="UPLINK" Number="19"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>frame offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>time_alignment</Name>
                </ItemLink>
                <Comment>time alignment</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <Comment>training sequence code</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_NEW_SCELL_CON confirms the new cell selection.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_NEW_SCELL_CON</Name>
                <PrimID Direction="UPLINK" Number="20"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_RA_REQ is used to send one channel request message on RACH channel in uplink direction.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_RA_REQ</Name>
                <PrimID Direction="UPLINK" Number="46"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>txpwr</Name>
                </ItemLink>
                <Comment>Power level</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rand</Name>
                </ItemLink>
                <Comment>Delay</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_request</Name>
                </ItemLink>
                <Comment>channel request</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>powerclass_gsm</Name>
                </ItemLink>
                <Comment>GSM power class</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>powerclass_dcs</Name>
                </ItemLink>
                <Comment>DCS power class</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_RA_CON is used to confirm sending of a channel request message on RACH channel in uplink direction.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_RA_CON</Name>
                <PrimID Direction="UPLINK" Number="47"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn</Name>
                </ItemLink>
                <Comment>frame number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_request</Name>
                </ItemLink>
                <Comment>channel request</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_RA_REQ requests the stop of connection establishment.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_RA_REQ</Name>
                <PrimID Direction="UPLINK" Number="48"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_RA_CON confirms the stop of connection establishment.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_RA_CON</Name>
                <PrimID Direction="UPLINK" Number="49"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_IMMED_ASSIGN_REQ is used configure a dedicated channel after reception of an Immediate Assignment message from the network.</Section>
                <Section>Note: bcch_allocation and ba_id are not used.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_IMMED_ASSIGN_REQ</Name>
                <PrimID Direction="UPLINK" Number="51"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_desc</Name>
                </ItemLink>
                <Comment>channel description</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>timing_advance</Name>
                </ItemLink>
                <Comment>timing advance</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>frequency_list</Name>
                </ItemLink>
                <Comment>frequency list</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>starting_time</Name>
                </ItemLink>
                <Comment>starting time</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>frequency_list_bef_sti</Name>
                </ItemLink>
                <Comment>frequency list before starting time</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>maio_bef_sti</Name>
                </ItemLink>
                <Comment>Maio before starting time</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>dtx_allowed</Name>
                </ItemLink>
                <Comment>DTX allowed</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>bcch_allocation</Name>
                </ItemLink>
                <Comment>BCCH allocation</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>ba_id</Name>
                </ItemLink>
                <Comment>band indicator</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>pwrc</Name>
                </ItemLink>
                <Comment>power control indicator</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_IMMED_ASSIGN_CON confirms the connection establishment.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_IMMED_ASSIGN_CON</Name>
                <PrimID Direction="UPLINK" Number="63"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_CHANNEL_ASSIGN_REQ is used to configure an intracell handover from one dedicated channel to another dedicated channel after reception of an Assignment message from the network.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_CHANNEL_ASSIGN_REQ</Name>
                <PrimID Direction="UPLINK" Number="52"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_desc_1</Name>
                </ItemLink>
                <Comment>channel description 1</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_mode_1</Name>
                </ItemLink>
                <Comment>channel mode 1</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>txpwr</Name>
                </ItemLink>
                <Comment>TX power</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>frequency_list</Name>
                </ItemLink>
                <Comment>frequency list</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>starting_time</Name>
                </ItemLink>
                <Comment>starting time</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_desc_2</Name>
                </ItemLink>
                <Comment>channel description 2</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_mode_2</Name>
                </ItemLink>
                <Comment>channel mode 2</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>frequency_list_bef_sti</Name>
                </ItemLink>
                <Comment>frequency list before starting time</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_desc_1_bef_sti</Name>
                </ItemLink>
                <Comment>channel description 1 before starting time</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_desc_2_bef_sti</Name>
                </ItemLink>
                <Comment>channel description 2 before starting time</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cipher_mode</Name>
                </ItemLink>
                <Comment>cipher mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>a5_algorithm</Name>
                </ItemLink>
                <Comment>A5 algorithm</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cipher_key</Name>
                </ItemLink>
                <Comment>encryption key</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>dtx_allowed</Name>
                </ItemLink>
                <Comment>DTX allowed flag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>amr_configuration</Name>
                </ItemLink>
                <Comment>AMR configuration</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>AMR configuration added.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_CHANNEL_ASSIGN_CON confirms the intracell handover.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_CHANNEL_ASSIGN_CON</Name>
                <PrimID Direction="UPLINK" Number="60"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_ASYNC_HO_REQ is used to perform an asynchronous handover.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_ASYNC_HO_REQ</Name>
                <PrimID Direction="UPLINK" Number="53"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>handover_command</Name>
                </ItemLink>
                <Comment>handover parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>frame offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>time_alignmnt</Name>
                </ItemLink>
                <Comment>time alignment</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cipher_key</Name>
                </ItemLink>
                <Comment>encryption key</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>amr_configuration</Name>
                </ItemLink>
                <Comment>AMR configuration</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>AMR configuration added.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_ASYNC_HO_CON confirms the handover.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_ASYNC_HO_CON</Name>
                <PrimID Direction="UPLINK" Number="59"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_HANDOVER_FINISHED indicates success of handover.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_HANDOVER_FINISHED</Name>
                <PrimID Direction="UPLINK" Number="68"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>success indication</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_SYNC_HO_REQ is used to perform an synchronous handover.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_SYNC_HO_REQ</Name>
                <PrimID Direction="UPLINK" Number="54"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>handover_command</Name>
                </ItemLink>
                <Comment>handover parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>frame offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>time_alignmnt</Name>
                </ItemLink>
                <Comment>time alignment</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cipher_key</Name>
                </ItemLink>
                <Comment>encryption key</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>nci</Name>
                </ItemLink>
                <Comment>normal cell indication</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>amr_configuration</Name>
                </ItemLink>
                <Comment>AMR configuration</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>AMR configuration added.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_SYNC_HO_CON confirms the handover.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_SYNC_HO_CON</Name>
                <PrimID Direction="UPLINK" Number="66"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_TA_FAIL_IND indicates an error condition(if TA out of range).</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_TA_FAIL_IND</Name>
                <PrimID Direction="UPLINK" Number="67"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_PRE_SYNC_HO_REQ is used to perform an synchronous handover.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_PRE_SYNC_HO_REQ</Name>
                <PrimID Direction="UPLINK" Number="55"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>handover_command</Name>
                </ItemLink>
                <Comment>handover parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>frame offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>time_alignmnt</Name>
                </ItemLink>
                <Comment>time alignment</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cipher_key</Name>
                </ItemLink>
                <Comment>encryption key</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>nci</Name>
                </ItemLink>
                <Comment>normal cell indication</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>timing_advance_valid</Name>
                </ItemLink>
                <Comment>timing advance valid</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>timing_advance</Name>
                </ItemLink>
                <Comment>timing advance</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>amr_configuration</Name>
                </ItemLink>
                <Comment>AMR configuration</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>AMR configuration added.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_PRE_SYNC_HO_CON confirms the handover.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_PRE_SYNC_HO_CON</Name>
                <PrimID Direction="UPLINK" Number="64"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_HANDOVER_FAIL_REQ requests to abort handover and use old channel.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_HANDOVER_FAIL_REQ</Name>
                <PrimID Direction="UPLINK" Number="71"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_HANDOVER_FAIL_CON requests to abort handover and use old channel.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_HANDOVER_FAIL_CON</Name>
                <PrimID Direction="UPLINK" Number="62"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_CHANGE_FREQUENCY is used to change frequency list during an active dedicated mode (Frequency Redefinition Procedure).</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_CHANGE_FREQUENCY</Name>
                <PrimID Direction="UPLINK" Number="69"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_desc</Name>
                </ItemLink>
                <Comment>channel description</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>frequency_list</Name>
                </ItemLink>
                <Comment>frequency list</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>starting_time</Name>
                </ItemLink>
                <Comment>starting time</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_CHANGE_FREQUENCY_CON confirms frequency change.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_CHANGE_FREQUENCY_CON</Name>
                <PrimID Direction="UPLINK" Number="58"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_CHANNEL_MODE_MODIFY_REQ is used to change the channel mode during an active dedicated mode (Channel Mode Modify Procedure).</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_CHANNEL_MODE_MODIFY_REQ</Name>
                <PrimID Direction="UPLINK" Number="70"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>sub_channel</Name>
                </ItemLink>
                <Comment>change sub channel; The parameter defines the sub channel for halfrate operation</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_mode</Name>
                </ItemLink>
                <Comment>channel mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>amr_configuration</Name>
                </ItemLink>
                <Comment>AMR configuration</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change ?sub_channel' to ?modify_subchannel'.</Comment>
            </History>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>AMR configuration added.</Comment>
            </History>
            <History>
                <Date Day="15" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change ref of modify_subchannel</Comment>
            </History>
            <History>
                <Date Day="30" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>re-change ?modify_subchannel' to ?subchannel'</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_CHANNEL_MODE_MODIFY_CON confirms channel mode change.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_CHANNEL_MODE_MODIFY_CON</Name>
                <PrimID Direction="UPLINK" Number="61"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_SET_CIPHERING_REQ is used to change the ciphering parameters during an active dedicated mode (Cipher Mode Setting Procedure).</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_SET_CIPHERING_REQ</Name>
                <PrimID Direction="UPLINK" Number="72"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cipher_mode</Name>
                </ItemLink>
                <Comment>cipher mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>a5_algorithm</Name>
                </ItemLink>
                <Comment>A5 algorithm</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>new_ciph_param</Name>
                </ItemLink>
                <Comment>ciphering key</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_SET_CIPHERING_CON confirms ciphering change.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_SET_CIPHERING_CON</Name>
                <PrimID Direction="UPLINK" Number="65"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_MEAS_REPORT is used to send measurement results to RR in dedicated mode.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_MEAS_REPORT</Name>
                <PrimID Direction="UPLINK" Number="73"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>dtx_used</Name>
                </ItemLink>
                <Comment>DTX used</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>meas_valid</Name>
                </ItemLink>
                <Comment>measurements valid</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rxlev_full_acc</Name>
                </ItemLink>
                <Comment>rxlev full serving cell</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rxlev_full_nbr_meas</Name>
                </ItemLink>
                <Comment>number of full serving cell samples</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rxlev_sub_acc</Name>
                </ItemLink>
                <Comment>rxlev sub serving cell</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rxlev_sub_nbr_meas</Name>
                </ItemLink>
                <Comment>number of sub serving cell samples</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rxqual_full_acc_errors</Name>
                </ItemLink>
                <Comment>rxqual full serving cell</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rxqual_full_nbr_bits</Name>
                </ItemLink>
                <Comment>number of full serving cell samples</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rxqual_sub_acc_errors</Name>
                </ItemLink>
                <Comment>rxqual sub serving cell</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rxqual_sub_nbr_bits</Name>
                </ItemLink>
                <Comment>number of sub serving cell samples</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>no_of_ncells_meas</Name>
                </ItemLink>
                <Comment>number of neighbour cells</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>ncell_meas</Name>
                </ItemLink>
                <Comment>neighbour cell measurement values</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>ba_id</Name>
                </ItemLink>
                <Comment>band indication</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>timing_advance</Name>
                </ItemLink>
                <Comment>timing advance</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>txpwr_used</Name>
                </ItemLink>
                <Comment>txpwr used</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>facch_dl_count</Name>
                </ItemLink>
                <Comment>FACCH downlink count</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>facch_ul_count</Name>
                </ItemLink>
                <Comment>FACCH uplink count</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>Supplement of reserved facch_dl_count and facch_ul_count</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_UPDATE_BA_LIST is used if a different BCCH allocation for dedicated mode is defined.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_UPDATE_BA_LIST</Name>
                <PrimID Direction="UPLINK" Number="74"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>num_of_chans</Name>
                </ItemLink>
                <Comment>number of channels</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>chan_list</Name>
                </ItemLink>
                <Comment>channel list</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>pwrc</Name>
                </ItemLink>
                <Comment>power control indicator</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>dtx_allowed</Name>
                </ItemLink>
                <Comment>DTX allowed</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>ba_id</Name>
                </ItemLink>
                <Comment>band indication</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="8" Year="2001"/>
                <Author>MSB</Author>
                <Comment>Use the cell channel list with the correct size. Change the member name.</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_STOP_DEDICATED confirms ciphering change.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_DEDICATED_REQ</Name>
                <PrimID Direction="UPLINK" Number="57"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_NCELL_FB_SB_READ requests reading of the frequency correction burst and the synchron burst of a single channel number. This happens to one of the six strongest neighbour cells carrier.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_NCELL_FB_SB_READ</Name>
                <PrimID Direction="UPLINK" Number="75"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_NCELL_FB_SB_READ requests reading of the synchron burst of the given channel number in dedicated mode.</Section>
                <Section>Note: fn_offset,time_alignment, sb_flag and bsic are not used.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_NCELL_SB_READ</Name>
                <PrimID Direction="UPLINK" Number="76"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>sb_flag</Name>
                </ItemLink>
                <Comment>SB flag</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Comment>base station identification code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>frame offset</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>time_alignmnt</Name>
                </ItemLink>
                <Comment>time alignment</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>sb_flag referenced</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The OML1_CLOSE_TCH_LOOP_REQ is used to close a TCH loop.</Section>
            </Description>
            <PrimDef>
                <Name>OML1_CLOSE_TCH_LOOP_REQ</Name>
                <PrimID Direction="UPLINK" Number="97"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>sub_channel</Name>
                </ItemLink>
                <Comment>loop sub channel; The parameter defines the sub channel for halfrate operation</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>frame_erasure</Name>
                </ItemLink>
                <Comment>frame erasure</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>name of ?sub_channel' changed</Comment>
            </History>
            <History>
                <Date Day="30" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>re-change name</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The OML1_CLOSE_TCH_LOOP_CON is used to confirm closing of a TCH loop.</Section>
            </Description>
            <PrimDef>
                <Name>OML1_CLOSE_TCH_LOOP_CON</Name>
                <PrimID Direction="UPLINK" Number="101"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The OML1_OPEN_TCH_LOOP_REQ is used to open a TCH loop.</Section>
            </Description>
            <PrimDef>
                <Name>OML1_OPEN_TCH_LOOP_REQ</Name>
                <PrimID Direction="UPLINK" Number="98"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The OML1_OPEN_TCH_LOOP_CON is used to confirm opening of a TCH loop.</Section>
            </Description>
            <PrimDef>
                <Name>OML1_OPEN_TCH_LOOP_CON</Name>
                <PrimID Direction="UPLINK" Number="102"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The OML1_START_DAI_TEST_REQ is used to start DAI tests.</Section>
            </Description>
            <PrimDef>
                <Name>OML1_START_DAI_TEST_REQ</Name>
                <PrimID Direction="UPLINK" Number="99"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>tested_device</Name>
                </ItemLink>
                <Comment>tested device</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The OML1_START_DAI_TEST_CON is used to confirm starting of DAI tests.</Section>
            </Description>
            <PrimDef>
                <Name>OML1_START_DAI_TEST_CON</Name>
                <PrimID Direction="UPLINK" Number="103"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The OML1_STOP_DAI_TEST_REQ is used to stop DAI tests.</Section>
            </Description>
            <PrimDef>
                <Name>OML1_STOP_DAI_TEST_REQ</Name>
                <PrimID Direction="UPLINK" Number="100"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The OML1_STOP_DAI_TEST_CON is used to confirm stopping of DAI tests.</Section>
            </Description>
            <PrimDef>
                <Name>OML1_STOP_DAI_TEST_CON</Name>
                <PrimID Direction="UPLINK" Number="104"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The TST_SLEEP_REQ configures Power Management.</Section>
            </Description>
            <PrimDef>
                <Name>TST_SLEEP_REQ</Name>
                <PrimID Direction="UPLINK" Number="4"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>sleep_mode</Name>
                </ItemLink>
                <Comment>sleep mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>Clocks</Name>
                </ItemLink>
                <Comment>clocks</Comment>
            </PrimItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="10" Year="1999"/>
                <Author>MPA</Author>
                <Comment>clocks-&gt;Clocks due to compiling errors</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPHC_ADC_IND reads the 5 auxiliary analog input.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_ADC_IND</Name>
                <PrimID Direction="UPLINK" Number="105"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>adc_results</Name>
                </ItemLink>
                <Control>[9]</Control>
                <Comment>adc results</Comment>
            </PrimItem>
            <History>
                <Date Day="14" Month="3" Year="2000"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPH_INIT_L1_REQ is used for Multi-band selection E-GSM900/DCS1800/PCS1900/GSM850.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_INIT_L1_REQ</Name>
                <PrimID Direction="UPLINK" Number="114"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_band_config</Name>
                </ItemLink>
                <Comment>radio band configuration</Comment>
            </PrimItem>
            <History>
                <Date Day="14" Month="11" Year="2001"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPH_INIT_L1_CON confirms the Multi-band selection.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_INIT_L1_CON</Name>
                <PrimID Direction="UPLINK" Number="115"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="14" Month="11" Year="2001"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The MPH_DEACTIVATE_REQ is used to request the layer 1 Off mode after stopping all running processes.</Section>
                <Section>Note: Inside the TI interface description this primitive is named MPHC_NETWORK_LOST_IND.</Section>
            </Description>
            <PrimDef>
                <Name>MPHC_DEACTIVATE_REQ</Name>
                <PrimID Direction="UPLINK" Number="110"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="15" Month="4" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The TST_TEST_HW_CON checks version numbers of layer1, DSP code and patches and testmode.</Section>
            </Description>
            <PrimDef>
                <Name>TST_TEST_HW_REQ</Name>
                <PrimID Direction="UPLINK" Number="1"/>
                <PrimUsage>
                    <Sender>L3</Sender>
                    <Receiver>L1</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>The TST_TEST_HW_CON checks version numbers of layer1, DSP code and patches and testmode.</Section>
            </Description>
            <PrimDef>
                <Name>TST_TEST_HW_CON</Name>
                <PrimID Direction="UPLINK" Number="2"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>dsp_code_version</Name>
                </ItemLink>
                <Comment>Version number of the DSP code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>dsp_checksum</Name>
                </ItemLink>
                <Comment>Checksum of DSP code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>dsp_patch_version</Name>
                </ItemLink>
                <Comment>Version number of the DSP patch code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>mcu_alr_version</Name>
                </ItemLink>
                <Comment>Version  number of the MCU ALR code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>mcu_gprs_version</Name>
                </ItemLink>
                <Comment>Version  number of the MCU GPRS code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>mcu_tm_version</Name>
                </ItemLink>
                <Comment>Version  number of the Testmode</Comment>
            </PrimItem>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>SACCH Downlink Interface</Section>
            </Description>
            <PrimDef>
                <Name>PH_DATA_IND</Name>
                <PrimID Direction="UPLINK" Number="109"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>PL</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Alias>rf_chan_num</Alias>
                <Comment>Channel (radio_freq) that block was read on</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>l2_channel</Name>
                </ItemLink>
                <Alias>l2_channel_type</Alias>
                <Comment>Indicates the MF51 block type read (enum type), maps to l1s msg signal code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>error_flag</Name>
                </ItemLink>
                <Alias>error_cause</Alias>
                <Comment>Indicates if l2_frame data is invalid</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>RADIO_FRAME</Name>
                </ItemLink>
                <Alias>l2_frame</Alias>
                <Comment>Layer 2 frame</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>bsic</Name>
                </ItemLink>
                <Comment>Base station identification code</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>tc</Name>
                </ItemLink>
                <Comment>multiframe number modulo 8</Comment>
            </PrimItem>
            <History>
                <Date Day="17" Month="12" Year="2003"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section/>
            </Description>
            <PrimDef>
                <Name>MPHC_STOP_DEDICATED_CON</Name>
                <PrimID Direction="UPLINK" Number="128"/>
                <PrimUsage>
                    <Sender>L1</Sender>
                    <Receiver>L3</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>param</Name>
                </ItemLink>
                <Comment>dummy</Comment>
            </PrimItem>
            <History>
                <Date Day="28" Month="07" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
    </PrimitivesSection>
    <PrimStructElementsSection>
        <Description>
            <Section>Parameters shall be part of the primitives described below and if applied the parameters shall contain the values specified here. These values are selected to correspond element values used in the air interface protocol.</Section>
        </Description>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the positional information in the multiframe structure for BCCH reading.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>schedule_array</Name>
                <Comment>positional info</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>modulus</Name>
                </ItemLink>
                <Comment>modulo part</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>relative_position</Name>
                </ItemLink>
                <Comment>relative part</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter contains a layer 2 frame.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>l2_frame</Name>
                <Comment>layer 2 frame</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>content</Name>
                </ItemLink>
                <Control>[MAX_L2_FRAME_SIZE]</Control>
                <Comment>frame content</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>Contains the channels which should be monitored.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>chan_list</Name>
                <Comment>channel list</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Control>[BA_LIST_SIZE]</Control>
                <Comment>channel number</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="8" Year="2001"/>
                <Author>MSB</Author>
                <Comment>Titel changed for easy discrimination of size. Use Constant.</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the measurement results for neighbour cells.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>result</Name>
                <Comment>measurement results</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rxlev</Name>
                </ItemLink>
                <Comment>rx level</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter describes the CBCH channel.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>cbch_desc</Name>
                <Comment>CBCH channel description</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>channel_desc</Name>
                <Comment>channel description</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>channel_desc_1</Name>
                <Comment>channel description</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>channel_desc_2</Name>
                <Comment>channel description</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>channel_desc_1_bef_sti</Name>
                <Comment>channel description before starting time</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>channel_desc_2_bef_sti</Name>
                <Comment>channel description before starting time</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>chan_sel</Name>
                </ItemLink>
                <Comment>channel selector</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_type</Name>
                </ItemLink>
                <Comment>SDCCH channel type</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>sub_channel</Name>
                </ItemLink>
                <Comment>sub channel</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>timeslot_no</Name>
                </ItemLink>
                <Comment>timeslot number</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>tsc</Name>
                </ItemLink>
                <Comment>training sequence code</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="15" Month="4" Year="2002"/>
                <Author>LG</Author>
                <Comment>values for subchannel moved to subchannel definition</Comment>
            </History>
            <History>
                <Date Day="30" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change short name of sub_channel</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the use and the allocation of a channel. (Comment : TI uses a union which is not possible in our test environment).</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>chan_sel</Name>
                <Comment>channel selector</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>h</Name>
                </ItemLink>
                <Comment>hopping</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rf_channel</Name>
                </ItemLink>
                <Comment>channel choice</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the use and the allocation of a channel. (Comment : TI uses a union which is not possible in our test environment). In non-hopping case the arfcn is mapped into the two bytes !!</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>rf_channel</Name>
                <Comment>channel choice</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>maio</Name>
                </ItemLink>
                <Comment>mobile allocation index offset</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>hsn</Name>
                </ItemLink>
                <Comment>hopping sequence number</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines a mobile allocation</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>cbch_freq_list</Name>
                <Comment>CBCH frequency list</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>frequency_list</Name>
                <Comment>frequency list</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>frequency_list_bef_sti</Name>
                <Comment>frequency list before starting time</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rf_chan_cnt</Name>
                </ItemLink>
                <Comment>no of hopping channels</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rf_chan_no</Name>
                </ItemLink>
                <Comment>hopping channels</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines a channel list.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>rf_chan_no</Name>
                <Comment>channel list</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Control>[MAX_MA_CARRIER]</Control>
                <Comment>channel number</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines a starting time.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>start_time</Name>
                <Comment>starting time</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>t1</Name>
                </ItemLink>
                <Comment>N32; named n32 in S922.doc</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>t3</Name>
                </ItemLink>
                <Comment>N51; named n51 in S922.doc</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>t2</Name>
                </ItemLink>
                <Comment>N26; named n26 in S922.doc</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="20" Month="10" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="2" Year="2003"/>
                <Author>LG</Author>
                <Comment>renamed components to be identical with RR AIM</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines an optional starting time.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>starting_time</Name>
                <Comment>starting time</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>start_time_present</Name>
                </ItemLink>
                <Comment>start time present</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>start_time</Name>
                </ItemLink>
                <Comment>starting time</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="20" Month="10" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the cipher key.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>new_ciph_param</Name>
                <Comment>Cipher Key Kc</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>cipher_key</Name>
                <Comment>encryption key</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>A</Name>
                </ItemLink>
                <Control>[8]</Control>
                <Comment>Kc values</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comment completes</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the various handover parameter.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>handover_command</Name>
                <Comment>Handover Command</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cell_description</Name>
                </ItemLink>
                <Comment>cell description</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_desc_1</Name>
                </ItemLink>
                <Comment>channel description 1</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_mode_1</Name>
                </ItemLink>
                <Comment>channel mode 1</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>starting_time</Name>
                </ItemLink>
                <Comment>starting time</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>ho_acc</Name>
                </ItemLink>
                <Comment>handover access</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>txpwr</Name>
                </ItemLink>
                <Comment>handover power</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>report_time_diff</Name>
                </ItemLink>
                <Comment>report time difference</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>frequency_list</Name>
                </ItemLink>
                <Comment>frequency list</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_desc_2</Name>
                </ItemLink>
                <Comment>channel description 2</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_mode_2</Name>
                </ItemLink>
                <Comment>channel mode 2</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>frequency_list_bef_sti</Name>
                </ItemLink>
                <Comment>frequency list before starting time</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_desc_1_bef_sti</Name>
                </ItemLink>
                <Comment>channel description 1 before starting time</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>channel_desc_2_bef_sti</Name>
                </ItemLink>
                <Comment>channel description 2 before starting time</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>cipher_mode</Name>
                </ItemLink>
                <Comment>cipher mode</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>a5_algorithm</Name>
                </ItemLink>
                <Comment>A5 algorithm</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the cell description.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>cell_description</Name>
                <Comment>cell description</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>ncc</Name>
                </ItemLink>
                <Comment>national colour code</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>bcc</Name>
                </ItemLink>
                <Comment>base station colour code</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>bcch_carrier</Name>
                </ItemLink>
                <Comment>BCCH carrier</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the measurement results for neighbour cells.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>ncell_meas</Name>
                <Comment>neighbour cell measurement results</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>res_list</Name>
                </ItemLink>
                <Control>[BA_LIST_SIZE]</Control>
                <Comment>neighbour cell results</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the measurement results for one neighbour cell.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>res_list</Name>
                <Comment>neighbour cell measurement results</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>bcch_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rxlev_acc</Name>
                </ItemLink>
                <Comment>accumulated rx level</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rxlev_nbr_meas</Name>
                </ItemLink>
                <Comment>nbr of rxlevel samples</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter describes the BCCH allocation.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>bcch_allocation</Name>
                <Comment>BCCH allocation</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>rf_chan_cnt</Name>
                </ItemLink>
                <Comment>number of channels</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>chan_number</Name>
                </ItemLink>
                <Comment>channel list</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="11" Year="2001"/>
                <Author>HEN</Author>
                <Comment>change name of the first member suitable to the type of member</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>Contains the channels which should be monitored.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>chan_number</Name>
                <Comment>channel list</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Control>[BCCH_LIST_SIZE]</Control>
                <Comment>channel number</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="8" Year="2001"/>
                <Author>MSB</Author>
                <Comment>Titel changed for easy discrimination of size. Use Constant.</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>Encodes the adaptiv multirate configuration for the speech codec.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>amr_configuration</Name>
                <Comment>Parameters for AMR</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>noise_suppression_control_bit</Name>
                </ItemLink>
                <Comment>noise suppression control bit</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>initial_codec_mode_indicator</Name>
                </ItemLink>
                <Comment>initial code mode indicator</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>initial_codec_mode</Name>
                </ItemLink>
                <Comment>initial code mode</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>active_codec_set</Name>
                </ItemLink>
                <Comment>active codec set</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>threshold</Name>
                </ItemLink>
                <Control>[3]</Control>
                <Comment>threshold</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>hysteresis</Name>
                </ItemLink>
                <Control>[3]</Control>
                <Comment>hysteresis</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial.</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>This parameter describes a neighbour cell the MS shall synchronise to .</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>ncell_list</Name>
                <Comment>Parameters of a neighbour cell</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>radio_freq</Name>
                </ItemLink>
                <Comment>channel number</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>fn_offset</Name>
                </ItemLink>
                <Comment>frame offset</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>time_alignment</Name>
                </ItemLink>
                <Comment>time alignment</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>timing_validity</Name>
                </ItemLink>
                <Comment>timing validity</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial.</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>Contains a layer 2 frame (on SACCH the first two byte are the layer 1 header) </Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>RADIO_FRAME</Name>
                <Version>!TI_DUAL_MODE</Version>
                <Comment>Layer 2 frame</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mphc</DocName>
                    <Name>content</Name>
                </ItemLink>
                <Alias>A</Alias>
                <Control>[MAX_L2_FRAME_SIZE]</Control>
                <Comment>Primitive structure element item</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="17" Month="12" Year="2003"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
    </PrimStructElementsSection>
    <PrimBasicElementsSection>
        <Description>
            <Section>Parameters shall be part of the primitives described below and if applied the parameters shall contain the values specified here. These values are selected to correspond element values used in the air interface protocol.</Section>
        </Description>
        <PrimBasicElem>
            <Description>
                <Section>This parameter is supplied to avoid empty primitives.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>param</Name>
                <Type>U8</Type>
                <Comment>dummy parameter</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of multiframes between the paging blocks of the same paging group.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bs_pa_mfrms</Name>
                <Type>U8</Type>
                <Comment>Multiframe Period</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_bs_pa_mfrms</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the blocks reserved for access grant channels on the common control channel.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bs_ag_blks_res</Name>
                <Type>U8</Type>
                <Comment>Blocks reserved for AGCH</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines whether it is a combined BCCH or not.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bcch_combined</Name>
                <Type>U8</Type>
                <Comment>combined BCCH flag</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_bcch_combined</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the timeslot on which the CCCH can be found.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ccch_group</Name>
                <Type>U8</Type>
                <Comment>CCCH group</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_ccch_group</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the multiframe of the paging group.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>page_group</Name>
                <Type>U8</Type>
                <Comment>paging group</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines an index where page blocks should occur.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>page_block_index</Name>
                <Type>U8</Type>
                <Comment>page block index</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_page_block_index</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the type paging which should be used.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>page_mode</Name>
                <Type>U8</Type>
                <Comment>paging mode</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_page_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of valid entries in the schedule array.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>schedule_array_size</Name>
                <Type>U8</Type>
                <Comment>number of channel numbers</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the positional information in the multiframe structure for BCCH reading.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>modulus</Name>
                <Type>U16</Type>
                <Comment>modulo part</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_modulus</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the positional information in the multiframe structure for BCCH reading.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>relative_position</Name>
                <Type>U16</Type>
                <Comment>relative part</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter identifies a channel number.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>radio_freq</Name>
                <Type>U16</Type>
                <Comment>channel number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_radio_freq</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="7" Month="2" Year="2002"/>
                <Author>MSB</Author>
                <Comment>Further american frequencies added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the layer channel type.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>l2_channel</Name>
                <Type>U8</Type>
                <Comment>layer 2 channel type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_l2_channel</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the result of a data block read operation.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>error_flag</Name>
                <Type>U8</Type>
                <Comment>error cause</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_error_flag</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter contains a layer 2 frame.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>content</Name>
                <Type>U8</Type>
                <Comment>frame content</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The TC parameter defines the 51-multiframenumber modulo 8.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tc</Name>
                <Type>U8</Type>
                <Comment>multiframe number modulo 8</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_tc</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Frame number.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>fn</Name>
                <Type>U32</Type>
                <Comment>frame number</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The difference in absolute frame numbers between the serving cell and the non-serving cell.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>fn_offset</Name>
                <Type>U32</Type>
                <Comment>frame offset</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_fn_offset</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The difference in quarter bits between the first bit in a frame of the serving cell and the first bit in a frame of the non-serving cell.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>time_alignment</Name>
                <Type>U32</Type>
                <Comment>Difference in quarter bits between the first bit in a frame of the serving cell and the first bit in the next frame of the non-serving cell. Validity of time_alignment dependent upon timing_validity indication. (0 - 4999)</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_time_alignment</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The difference in quarter bits between the first bit in a frame of the serving cell and the first bit in a frame of the non-serving cell.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>time_alignmnt</Name>
                <Type>U32</Type>
                <Comment>Difference in quarter bits between serving and handover destination cell (0 to 5000)</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_time_alignment</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Describes how the timing information given to Layer 1 should used.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>timing_validity</Name>
                <Type>U8</Type>
                <Comment>timing validity</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_timing_validity</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Describes the mode used by layer 3. Determines Layer 1 frequency control algorithm.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>search_mode</Name>
                <Type>U8</Type>
                <Comment>search mode</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_search_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the base station identity code.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bsic</Name>
                <Type>U8</Type>
                <Comment>base station identification code</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_bsic</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of valid channel numbers.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>radio_freq_array_size</Name>
                <Type>U8</Type>
                <Comment>Number of entries in the radio_freq_array within a stop request. When 6 (maximum number of requests to be served in parallel) are provided the message is interpreted as a complete process stop request.</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comments completes</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of valid channel numbers.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>nbr_of_carriers</Name>
                <Type>U8</Type>
                <Comment>The number of cell carriers measured during the PCH block</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comments completes</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of valid channel numbers.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>num_of_chans</Name>
                <Type>U8</Type>
                <Comment>Number of valid carrier numbers contained in the BA list (chan_number) array (1 to 33)</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comments completes</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of valid channel numbers.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rf_chan_cnt</Name>
                <Type>U16</Type>
                <Comment>number of channels in the mobile allocation list or  number of bcch in the list</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="11" Year="2001"/>
                <Author>MSB</Author>
                <Comment>comments changed</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines a channel list</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>radio_freq_array</Name>
                <Type>U16</Type>
                <Comment>channel list</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Describes which type of training sequence code should be used.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tsc</Name>
                <Type>U8</Type>
                <Comment>training sequence code</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_tsc</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>A bitmap which indicates which blocks should be read.</Section>
                <Section>Note: the Values can be combined.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bcch_blocks_required</Name>
                <Type>U16</Type>
                <Comment>sys info bitmap</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_bcch_blocks_required</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="15" Month="2" Year="2001"/>
                <Author>MPA</Author>
                <Comment>added NCELL_BCCH*</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the measured power strength level of a cell.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev</Name>
                <Type>U8</Type>
                <Comment>The accumulated result of a power measurements. The signal strength units used are based on those described in GSM 05.08 (ETS 300 911) section 8.1.4. The measurements continue above 63 and below 0</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comments completes</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the measured power strength level of a cell.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>s_rxlev</Name>
                <Type>U8</Type>
                <Comment>The serving cell received power level (average of the 4 PCH bursts read during the particular PCH block).</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comments completes</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter is used to identify measurement results values as belonging to the band allocation list.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ba_id</Name>
                <Type>U8</Type>
                <Comment>band allocation identification</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter is used to specify an index into the channel list.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>next_radio_freq_measured</Name>
                <Type>U8</Type>
                <Comment>channel index</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter describes the CBCH channel.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>channel_type</Name>
                <Type>U8</Type>
                <Comment>SDCCH channel type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_channel_type</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="15" Month="4" Year="2002"/>
                <Author>LG</Author>
                <Comment>values for subchannel moved to subchannel definition</Comment>
            </History>
            <History>
                <Date Day="30" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change short name of sub_channel</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter describes the CBCH channel.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>timeslot_no</Name>
                <Type>U8</Type>
                <Comment>timeslot number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_timeslot_no</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="15" Month="4" Year="2002"/>
                <Author>LG</Author>
                <Comment>values for subchannel moved to subchannel definition</Comment>
            </History>
            <History>
                <Date Day="30" Month="4" Year="2002"/>
                <Author>MSB</Author>
                <Comment>change short name of sub_channel</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Defines if hopping should be used.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>h</Name>
                <Type>U8</Type>
                <Comment>hopping</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_h</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the use and the allocation of a channel. (Comment : TI uses a union which is not possible in our test environment). In non-hopping case the arfcn is mapped into the two bytes !!</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>maio</Name>
                <Type>U8</Type>
                <Comment>mobile allocation index offset</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_maio</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the use and the allocation of a channel. (Comment : TI uses a union which is not possible in our test environment). In non-hopping case the arfcn is mapped into the two bytes !!</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>hsn</Name>
                <Type>U8</Type>
                <Comment>hopping sequence number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_hsn</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines which cell broadcast should be read.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>cbch_select</Name>
                <Type>U8</Type>
                <Comment>which cbch channel to read</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_cbch_select</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Describes the length of the schedule period.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>schedule_length</Name>
                <Type>U8</Type>
                <Comment>length of schedule period</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_schedule_length</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Describes which blocks should be read during a schedule period.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>first_blocks_0</Name>
                <Type>U32</Type>
                <Comment>Bitmap defining a set of blocks to be read during the schedule period. The bits represent the blocks as follows: bit MSB=31 -&gt; block=32; bit LSB=0 -&gt; block=1.</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comment completes, discriminate blocks</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Describes which blocks should be read during a schedule period.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>first_blocks_1</Name>
                <Type>U16</Type>
                <Comment>Bitmap defining a set of blocks to be read during the schedule period. The bits represent the blocks as follows: bit MSB=15 -&gt; block=48; bit LSB=0 -&gt; block=33.</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comment completes, discriminate blocks</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Describes which additional blocks should be read after the first one.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tb_bitmap</Name>
                <Type>U8</Type>
                <Comment>blocks to read</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_tb_bitmap</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Which cell broadcast channel should stop reading.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>normal_cbch</Name>
                <Type>U8</Type>
                <Comment>normal cbch</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_normal_cbch</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Which cell broadcast channel should stop reading.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>extended_cbch</Name>
                <Type>U8</Type>
                <Comment>extended cbch</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the power level used by the physical layer according to GSM 5.08.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>txpwr</Name>
                <Type>U8</Type>
                <Comment>Indicates the power level which the mobile should use for transmission .</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_txpwr</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comments completes</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the power level used by the physical layer according to GSM 5.08.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>txpwr_used</Name>
                <Type>U8</Type>
                <Comment>TX power level currently used by L1 (For TEST MOBILE only).</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comments completes</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of TDMA frames before sending a channel request message.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rand</Name>
                <Type>U8</Type>
                <Comment>TDMA frames before sending RACH burst</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the channel request message send on RACH channel into a RACH burst.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>channel_request</Name>
                <Type>U8</Type>
                <Comment>content of channel request message</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the power class of the mobile station.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>powerclass_gsm</Name>
                <Type>U8</Type>
                <Comment>GSM power class of the MS.</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_powerclass_gsm</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the power class of the mobile station.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>powerclass_dcs</Name>
                <Type>U8</Type>
                <Comment>DCS power class of the MS.</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the timing advance of the cell to the base station.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>timing_advance</Name>
                <Type>U8</Type>
                <Comment>timing advance</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines a starting time.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>t1</Name>
                <Type>U8</Type>
                <Comment>N32; named n32 in S922.doc</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="20" Month="10" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="2" Year="2003"/>
                <Author>LG</Author>
                <Comment>renamed components to be identical with RR AIM</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines a starting time.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>t3</Name>
                <Type>U8</Type>
                <Comment>N51; named n51 in S922.doc</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="20" Month="10" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="2" Year="2003"/>
                <Author>LG</Author>
                <Comment>renamed components to be identical with RR AIM</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines a starting time.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>t2</Name>
                <Type>U8</Type>
                <Comment>N26; named n26 in S922.doc</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="20" Month="10" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="2" Year="2003"/>
                <Author>LG</Author>
                <Comment>renamed components to be identical with RR AIM</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines an optional starting time.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>start_time_present</Name>
                <Type>U8</Type>
                <Comment>start time present</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="20" Month="10" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter mobile allocation index offset is used for hopping purposes.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>maio_bef_sti</Name>
                <Type>U8</Type>
                <Comment>MAIO used before starting time</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines whether DTX is allowed or not.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dtx_allowed</Name>
                <Type>U8</Type>
                <Comment>DTX allowed</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_dtx_allowed</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the use of the power control indicator.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>pwrc</Name>
                <Type>U8</Type>
                <Comment>power control indicator</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_pwrc</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the channel mode.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>channel_mode</Name>
                <Type>U8</Type>
                <Comment>channel mode</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_channel_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>AMR added.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the channel mode.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>channel_mode_1</Name>
                <Type>U8</Type>
                <Comment>channel mode</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>AMR added.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the channel mode.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>channel_mode_2</Name>
                <Type>U8</Type>
                <Comment>channel mode</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>AMR added.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the cipher mode.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>cipher_mode</Name>
                <Type>U8</Type>
                <Comment>cipher mode</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_cipher_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines A5 algorithm.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>a5_algorithm</Name>
                <Type>U8</Type>
                <Comment>A5 algorithm</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_a5_algorithm</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the cipher key.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>A</Name>
                <Type>U8</Type>
                <Comment>Kc values</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comment completes</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the cell description.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ncc</Name>
                <Type>U8</Type>
                <Comment>national colour code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the cell description.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bcc</Name>
                <Type>U8</Type>
                <Comment>base station colour code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the cell description.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bcch_carrier</Name>
                <Type>U16</Type>
                <Comment>BCCH carrier</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the content of the handover access messages.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ho_acc</Name>
                <Type>U8</Type>
                <Comment>handover access</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines report time difference.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>report_time_diff</Name>
                <Type>U8</Type>
                <Comment>time difference</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Defines if handover was successful.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>cause</Name>
                <Type>U8</Type>
                <Comment>handover success</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_cause</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines whether timing advance out of range is accepted in the cell or not.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>nci</Name>
                <Type>U8</Type>
                <Comment>normal cell indication</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_nci</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines whether timing advance information is valid or not.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>timing_advance_valid</Name>
                <Type>U8</Type>
                <Comment>timing advance information valid flag</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_timing_advance_valid</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines whether DTX was used during the last measurement period or not.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dtx_used</Name>
                <Type>U8</Type>
                <Comment>DTX used flag</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_dtx_used</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines whether the measurement results during the last measurement period are valid or not</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>meas_valid</Name>
                <Type>U8</Type>
                <Comment>measurement valid flag</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_meas_valid</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines an accumulated value for the fieldstrength of the serving cell during dedicated mode.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev_full_acc</Name>
                <Type>U16</Type>
                <Comment>rxlevel full serving cell accumulated</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines an accumulated value for the fieldstrength of the serving cell during dedicated mode.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev_sub_acc</Name>
                <Type>U16</Type>
                <Comment>rxlevel sub serving cell accumulated</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of samples for the fieldstrength of the serving cell during dedicated mode.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev_full_nbr_meas</Name>
                <Type>U8</Type>
                <Comment>number of rxlevel full serving cell samples</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of samples for the fieldstrength of the serving cell during dedicated mode.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev_sub_nbr_meas</Name>
                <Type>U8</Type>
                <Comment>number of rxlevel sub serving cell samples</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of bit errors during the reporting period.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxqual_full_acc_errors</Name>
                <Type>U16</Type>
                <Comment>rxqual full serving cell bit errors</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of bit errors during the reporting period.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxqual_sub_acc_errors</Name>
                <Type>U16</Type>
                <Comment>rxlevel sub serving cell bit errors</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of bits examined for errors over the reporting period.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxqual_full_nbr_bits</Name>
                <Type>U16</Type>
                <Comment>number of examined bits for rxqual full serving cell</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of bits examined for errors over the reporting period.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxqual_sub_nbr_bits</Name>
                <Type>U16</Type>
                <Comment>number of examined bits for rxqual sub serving cell</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the number of neighbour cell results in dedicated mode.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>no_of_ncells_meas</Name>
                <Type>U8</Type>
                <Comment>number of neighbour cell results</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the measurement results for one neighbour cell.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bcch_freq</Name>
                <Type>U16</Type>
                <Comment>channel number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_bcch_freq</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the measurement results for one neighbour cell.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev_acc</Name>
                <Type>U16</Type>
                <Comment>accumulated rx level</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the measurement results for one neighbour cell.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rxlev_nbr_meas</Name>
                <Type>U8</Type>
                <Comment>nbr of rxlevel samples</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the sub channel for halfrate operations.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>sub_channel</Name>
                <Type>U8</Type>
                <Comment>sub channel</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_sub_channel</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>name changed</Comment>
            </History>
            <History>
                <Date Day="15" Month="4" Year="2002"/>
                <Author>LG</Author>
                <Comment>values added from Channel description</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the type of TCH loop.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>frame_erasure</Name>
                <Type>U8</Type>
                <Comment>TCH loop type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_frame_erasure</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the tested device for DAI tests.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tested_device</Name>
                <Type>U8</Type>
                <Comment>DAI test device</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_tested_device</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines sleep mode.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>sleep_mode</Name>
                <Type>U8</Type>
                <Comment>sleep mode</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_sleep_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="10" Year="2000"/>
                <Author>LE</Author>
                <Comment>Values changed</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines clocks.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>Clocks</Name>
                <Type>U16</Type>
                <Comment>clock modules</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_Clocks</Name>
            </ValuesLink>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comments completes</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the result of a data block read operation.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>sb_flag</Name>
                <Type>U8</Type>
                <Comment>Flag indicating whether synchronisation channel was read correctly or not</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_sb_flag</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="8" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="30" Month="1" Year="2002"/>
                <Author>MSB</Author>
                <Comment>comment completes</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines a pointer to the results of the power measuements.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>shared_ptr</Name>
                <Type>U32</Type>
                <Comment>Pointer</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="10" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines AD conversion result.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>adc_results</Name>
                <Type>U16</Type>
                <Comment>result</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="6" Month="9" Year="1999"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Controls the Priority of the Neighbour Cell BCCH reading.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>gprs_prio</Name>
                <Type>U8</Type>
                <Comment>Gprs priority</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_gprs_prio</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Encodes the power strength level measured on CCCH.</Section>
                <Section>It's an running average value (without forgetting factor).</Section>
                <Section>The average is made on 4 bursts.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ccch_lev</Name>
                <Type>U8</Type>
                <Comment>Power strength level</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="2" Year="2001"/>
                <Author>MPA</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines the possible frequency band configurations to set layer1 for synchronization with the network.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>radio_band_config</Name>
                <Type>U8</Type>
                <Comment>Bitmap of frequency bands</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_radio_band_config</Name>
            </ValuesLink>
            <History>
                <Date Day="14" Month="11" Year="2001"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Encodes the adaptiv multirate configuration for the speech codec.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>noise_suppression_control_bit</Name>
                <Type>U8</Type>
                <Comment>noise suppression control bit</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Encodes the adaptiv multirate configuration for the speech codec.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>initial_codec_mode_indicator</Name>
                <Type>U8</Type>
                <Comment>initial code mode indicator</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Encodes the adaptiv multirate configuration for the speech codec.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>initial_codec_mode</Name>
                <Type>U8</Type>
                <Comment>initial code mode</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_initial_codec_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Encodes the adaptiv multirate configuration for the speech codec.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>active_codec_set</Name>
                <Type>U8</Type>
                <Comment>active codec set</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Encodes the adaptiv multirate configuration for the speech codec.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>threshold</Name>
                <Type>U8</Type>
                <Comment>threshold</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Encodes the adaptiv multirate configuration for the speech codec.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>hysteresis</Name>
                <Type>U8</Type>
                <Comment>hysteresis</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="18" Month="2" Year="2002"/>
                <Author>OT</Author>
                <Comment>Initial.</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter contains real and imaginary parts for m=p-4 to p+4.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>a_eotd_crosscor</Name>
                <Type>S16</Type>
                <Comment>Cross correlation</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter describes the delay in GSM bits between the arrival of the first IQ sample and the position of the first correlation (correlation "p-4").</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>d_eotd_first</Name>
                <Type>S16</Type>
                <Comment>Delay to first correlation</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter describes the delay in GSM bits between the arrival of the first IQ sample and the position of the maximum correlation.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>d_eotd_max</Name>
                <Type>S16</Type>
                <Comment>Delay to maximum correlation</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter indicates whether EOTD data are present or not.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>eodt_data_valid</Name>
                <Type>U8</Type>
                <Comment>EOTD data present</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_eodt_data_valid</Name>
            </ValuesLink>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines the purpose the MPHC_NCELL_LIST_SYNC_REQ is used for.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>eotd</Name>
                <Type>U8</Type>
                <Comment>EOTD or neighbour cell monitoring</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_eotd</Name>
            </ValuesLink>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines the number of neighbour cells within an MPHC_NCELL_LIST_SYNC_REQ.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>list_size</Name>
                <Type>U8</Type>
                <Comment>1 up to 12 neighbour cells</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter defines the state the synchronisation is made in.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>mode</Name>
                <Type>U8</Type>
                <Comment>idle or dedicated mode</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mphc</DocName>
                <Name>VAL_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>neigh_id</Name>
                <Type>U8</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>attempt</Name>
                <Type>U8</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>pm</Name>
                <Type>U32</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>toa</Name>
                <Type>U32</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>angle</Name>
                <Type>U32</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>snr</Name>
                <Type>U32</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>fn_sb_neigh</Name>
                <Type>U32</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>fn_in_sb</Name>
                <Type>U32</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>toa_correction</Name>
                <Type>U32</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>delta_fn</Name>
                <Type>U32</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>delta_qbit</Name>
                <Type>U32</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>facch_dl_count</Name>
                <Type>U8</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameters are reserved for Layer 1 internal use or for debugging.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>facch_ul_count</Name>
                <Type>U8</Type>
                <Comment>reserved</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>supplement of toa_correction</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter contains the sum of the amplitudes of the sampled I and Q data.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>d_eotd_nrj</Name>
                <Type>U32</Type>
                <Comment>sum of amplitudes</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>This parameter contains the difference in quarter bits between first correlation of SB of serving cell and first correlation of neighbour cell.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>time_tag</Name>
                <Type>U32</Type>
                <Comment>Time tag</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="14" Month="8" Year="2002"/>
                <Author>LG</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Some version numbers.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dsp_code_version</Name>
                <Type>U16</Type>
                <Comment>Version number of the DSP code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Some version numbers.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dsp_checksum</Name>
                <Type>U16</Type>
                <Comment>Checksum of DSP code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Some version numbers.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dsp_patch_version</Name>
                <Type>U16</Type>
                <Comment>Version number of the DSP patch code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Some version numbers.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>mcu_alr_version</Name>
                <Type>U16</Type>
                <Comment>Version  number of the MCU ALR code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Some version numbers.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>mcu_gprs_version</Name>
                <Type>U16</Type>
                <Comment>Version  number of the MCU GPRS code</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Some version numbers.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>mcu_tm_version</Name>
                <Type>U16</Type>
                <Comment>Version  number of the Testmode</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="3" Month="4" Year="2003"/>
                <Author>MSB</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
    </PrimBasicElementsSection>
    <ValuesSection>
        <Description>
            <Section>This section contains all sets of values that are defined for the MPHC SAP</Section>
        </Description>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bs_pa_mfrms</Name>
                <Comment>values for bs_pa_mfrms</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias/>
                <Comment>2 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias/>
                <Comment>3 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias/>
                <Comment>4 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias/>
                <Comment>5 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias/>
                <Comment>6 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias/>
                <Comment>7 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias/>
                <Comment>8 Multiframe Periods</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias/>
                <Comment>9 Multiframe Periods</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bcch_combined</Name>
                <Comment>values for bcch_combined</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>COMB_CCCH_NOT_COMB</Alias>
                <Comment>CCCH not combined with SDCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>COMB_CCCH_COMB</Alias>
                <Comment>CCCH combined with SDCCH</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ccch_group</Name>
                <Comment>values for ccch_group</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CCCH_GROUP_TS0</Alias>
                <Comment>equal to timeslot 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CCCH_GROUP_TS2</Alias>
                <Comment>equal to timeslot 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CCCH_GROUP_TS4</Alias>
                <Comment>equal to timeslot 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CCCH_GROUP_TS6</Alias>
                <Comment>equal to timeslot 6</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_page_block_index</Name>
                <Comment>values for page_block_index</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>8</MaxValue>
                <Comment>for non-combined</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>2</MaxValue>
                <Comment>for combined</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_page_mode</Name>
                <Comment>values for page_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PGM_NORMAL</Alias>
                <Comment>Use normal paging</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PGM_EXTENDED</Alias>
                <Comment>Use extended paging</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PGM_REORG</Alias>
                <Comment>use reorganise paging</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_modulus</Name>
                <Comment>values for modulus</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>65536</MaxValue>
                <Comment>valid range for modulus</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>65535</MaxValue>
                <Comment>valid range for relative position</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_radio_freq</Name>
                <Comment>values for radio_freq</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>124</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>174</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>512</MinValue>
                <MaxValue>810</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>811</MinValue>
                <MaxValue>885</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>498</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>548</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>128</MinValue>
                <MaxValue>251</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>424</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_l2_channel</Name>
                <Version>!TI_DUAL_MODE</Version>
                <Comment>values for l2_channel</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>L2_CHANNEL_SACCH</Alias>
                <Comment>SACCH block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>L2_CHANNEL_SDCCH</Alias>
                <Comment>SDCCH block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>L2_CHANNEL_FACCH_H</Alias>
                <Comment>FACCH halfrate block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>L2_CHANNEL_FACCH_F</Alias>
                <Comment>FACCH fullrate block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>L2_CHANNEL_CCCH</Alias>
                <Comment>CCCH block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>L2_CHANNEL_NBCCH</Alias>
                <Comment>normal BCCH block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>L2_CHANNEL_PCH</Alias>
                <Comment>PCH block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>L2_CHANNEL_EPCH</Alias>
                <Comment>extended PCH block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>L2_CHANNEL_CBCH</Alias>
                <Comment>CBCH block</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>L2_CHANNEL_EBCCH</Alias>
                <Comment>extended BCCH</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_error_flag</Name>
                <Comment>values for error_flag</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>VALID_BLOCK</Alias>
                <Comment>valid block received</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>INVALID_BLOCK</Alias>
                <Comment>invalid block received</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tc</Name>
                <Comment>values for tc</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>valid range</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_fn_offset</Name>
                <Comment>values for fn_offset</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>2715647</MaxValue>
                <Comment>valid range</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_time_alignment</Name>
                <Comment>values for time_alignment</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>4999</MaxValue>
                <Comment>valid range</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_timing_validity</Name>
                <Comment>values for timing_validity</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TV_INVALID_TIMING_INFO</Alias>
                <Comment>timing info shall not be used, do full FB and SB detection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>TV_APPROX_TIMING_INFO</Alias>
                <Comment>timing info may be used, do full FB and SB detection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>TV_VALID_TIMING_INFO</Alias>
                <Comment>read SB based based on timing info (only for ncell)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_search_mode</Name>
                <Comment>values for search_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SM_WIDE_MODE</Alias>
                <Comment>wideband capture and open-loop afc algorithm</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SM_NARROW_MODE</Alias>
                <Comment>narrowband capture and open-loop afc algorithm</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bsic</Name>
                <Comment>values for bsic</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>base station identification code</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tsc</Name>
                <Comment>values for tsc</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>type of sequence code</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bcch_blocks_required</Name>
                <Comment>values for bcch_blocks_required</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SI_NBLOCK_0</Alias>
                <Comment>TC 0 normal</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SI_NBLOCK_1</Alias>
                <Comment>TC 1 normal</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SI_NBLOCK_2</Alias>
                <Comment>TC 2 normal</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>SI_NBLOCK_3</Alias>
                <Comment>TC 3 normal</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">16</Value>
                <Alias>SI_NBLOCK_4</Alias>
                <Comment>TC 4 normal</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">32</Value>
                <Alias>SI_NBLOCK_5</Alias>
                <Comment>TC 5 normal</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">64</Value>
                <Alias>SI_NBLOCK_6</Alias>
                <Comment>TC 6 normal</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">128</Value>
                <Alias>SI_NBLOCK_7</Alias>
                <Comment>TC 7 normal</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">256</Value>
                <Alias>SI_EBLOCK_0</Alias>
                <Comment>TC 0 extended</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">512</Value>
                <Alias>SI_EBLOCK_1</Alias>
                <Comment>TC 1 extended</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1024</Value>
                <Alias>SI_EBLOCK_2</Alias>
                <Comment>TC 2 extended</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2048</Value>
                <Alias>SI_EBLOCK_3</Alias>
                <Comment>TC 3 extended</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4096</Value>
                <Alias>SI_EBLOCK_4</Alias>
                <Comment>TC 4 extended</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8192</Value>
                <Alias>SI_EBLOCK_5</Alias>
                <Comment>TC 5 extended</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">16384</Value>
                <Alias>SI_EBLOCK_6</Alias>
                <Comment>TC 6 extended</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">32768</Value>
                <Alias>SI_EBLOCK_7</Alias>
                <Comment>TC 7 extended</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0002</Value>
                <Alias>NCELL_BCCH_SI_2</Alias>
                <Comment>PLMN Search</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">00CC</Value>
                <Alias>NCELL_BCCH_SI_3_4</Alias>
                <Comment>Ncell BCCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">00CE</Value>
                <Alias>NCELL_BCCH_SI_2_3_4</Alias>
                <Comment>PLMN Search</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">8844</Value>
                <Alias>NCELL_BCCH_SI_3_7_8</Alias>
                <Comment>Ncell BCCH</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_channel_type</Name>
                <Comment>values for channel_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CH_TCH_F</Alias>
                <Comment>TCH/F</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CH_TCH_H</Alias>
                <Comment>TCH/H</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CH_SDCCH_4</Alias>
                <Comment>SDCCH/4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CH_SDCCH_8</Alias>
                <Comment>SDCCH/8</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_timeslot_no</Name>
                <Comment>values for timeslot_no</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>timeslot number 0-7</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_h</Name>
                <Comment>values for h</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NO_HOPPING</Alias>
                <Comment>no hopping</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>HOPPING</Alias>
                <Comment>hopping</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_hsn</Name>
                <Comment>values for hsn</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>hopping sequence number</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_maio</Name>
                <Comment>values for maio</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>mobile allocation index offset</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_cbch_select</Name>
                <Comment>values for cbch_select</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CBCH_READ_EXT</Alias>
                <Comment>read extended CBCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CBCH_READ_NORM</Alias>
                <Comment>read normal CBCH</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_schedule_length</Name>
                <Comment>values for schedule_length</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CBCH_NO_SCHED</Alias>
                <Comment>no scheduling provided</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>49</MaxValue>
                <Comment>length of the schedule period in blocks</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tb_bitmap</Name>
                <Comment>values for tb_bitmap</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CBCH_NORM_BLOCK2</Alias>
                <Comment>norm block 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CBCH_NORM_BLOCK3</Alias>
                <Comment>norm block 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CBCH_NORM_BLOCK4</Alias>
                <Comment>norm block 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>CBCH_EXT_BLOCK2</Alias>
                <Comment>ext block 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">16</Value>
                <Alias>CBCH_EXT_BLOCK3</Alias>
                <Comment>ext block 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">32</Value>
                <Alias>CBCH_EXT_BLOCK4</Alias>
                <Comment>ext block 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>CBCH_NORM_BLOCK234</Alias>
                <Comment>request all blocks</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">56</Value>
                <Alias>CBCH_EXT_BLOCK234</Alias>
                <Comment>all ext blocks</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_normal_cbch</Name>
                <Comment>values for normal_cbch</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CBCH_DONT_STOP</Alias>
                <Comment>dont stop cbch</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CBCH_STOP</Alias>
                <Comment>stop cbch</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_txpwr</Name>
                <Comment>values for txpwr</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>31</MaxValue>
                <Comment>Coded as the binary representation of the power control level as defined in GSM 05.05 section 4.1 and is in the range 0 - 31.</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_powerclass_gsm</Name>
                <Comment>values for powerclass_gsm</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>POW_CLASS_1</Alias>
                <Comment>Class 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>POW_CLASS_2</Alias>
                <Comment>Class 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>POW_CLASS_3</Alias>
                <Comment>Class 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>POW_CLASS_4</Alias>
                <Comment>Class 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>POW_CLASS_5</Alias>
                <Comment>Class 5</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_dtx_allowed</Name>
                <Comment>values for dtx_allowed</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DTX_NOTALLOWED</Alias>
                <Comment>DTX is not allowed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DTX_ALLOWED</Alias>
                <Comment>DTX is allowed</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pwrc</Name>
                <Comment>values for pwrc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PWRC_NOT_SET</Alias>
                <Comment>PWRC is not set</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PWRC_SET</Alias>
                <Comment>PWRC is set</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_channel_mode</Name>
                <Comment>values for channel_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CM_SIGNALLING_ONLY</Alias>
                <Comment>signalling only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CM_TCH_FS</Alias>
                <Comment>TCH full rate speech</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CM_TCH_HS</Alias>
                <Comment>TCH half rate speech</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CM_TCH_96</Alias>
                <Comment>TCH data 9600</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CM_TCH_F_48</Alias>
                <Comment>TCH data full rate 4800</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>CM_TCH_H_48</Alias>
                <Comment>TCH data half rate 4800</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>CM_TCH_F_24</Alias>
                <Comment>TCH data full rate 2400</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>CM_TCH_H_24</Alias>
                <Comment>TCH data half rate 2400</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>CM_TCH_EFR</Alias>
                <Comment>TCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>CM_TCH_144</Alias>
                <Comment>TCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>CM_TCH_AHS</Alias>
                <Comment>TCH AMR half rate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>CM_TCH_AFS</Alias>
                <Comment>TCH AMR full rate</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_cipher_mode</Name>
                <Comment>values for cipher_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CI_NO_CIPHERING</Alias>
                <Comment>ciphering off</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CI_CIPHERING</Alias>
                <Comment>ciphering on</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_a5_algorithm</Name>
                <Comment>values for a5_algorithm</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>A5_1</Alias>
                <Comment>A5/1 algorithm</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>A5_2</Alias>
                <Comment>A5/2 algorithm</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>A5_3</Alias>
                <Comment>A5/3 algorithm</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>A5_4</Alias>
                <Comment>A5/4 algorithm</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>A5_5</Alias>
                <Comment>A5/5 algorithm</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>A5_6</Alias>
                <Comment>A5/6 algorithm</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>A5_7</Alias>
                <Comment>A5/7 algorithm</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_cause</Name>
                <Comment>values for cause</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>HO_COMPLETE</Alias>
                <Comment>success</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>HO_TIMEOUT</Alias>
                <Comment>timeout</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_nci</Name>
                <Comment>values for nci</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>HO_TA_OUT_IGNORED</Alias>
                <Comment>timing advance out of range is ignored</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>HO_TA_OUT_NOT_IGNORED</Alias>
                <Comment>timing advance out of range is not ignored</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_timing_advance_valid</Name>
                <Comment>values for timing_advance_valid</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>HO_TA_NOT_VALID</Alias>
                <Comment>timing advance information is not valid</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>HO_TA_VALID</Alias>
                <Comment>timing advance information is valid</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_dtx_used</Name>
                <Comment>values for dtx_used</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DTX_NOT_USED</Alias>
                <Comment>DTX was not used</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DTX_USED</Alias>
                <Comment>DTX was used</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_meas_valid</Name>
                <Comment>values for meas_valid</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MEAS_ARE_NOT_VALID</Alias>
                <Comment>measurement values are not valid</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MEAS_ARE_VALID</Alias>
                <Comment>measurement values are valid</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bcch_freq</Name>
                <Comment>values for bcch_freq</Comment>
            </ValuesDef>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>124</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>174</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>512</MinValue>
                <MaxValue>810</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>512</MinValue>
                <MaxValue>885</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>498</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>1</MinValue>
                <MaxValue>548</MaxValue>
                <Comment>Layer 1 Encoded Frequency</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_sub_channel</Name>
                <Comment>values for sub_channel</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SUB_CH_0</Alias>
                <Comment>sub channel 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SUB_CH_1</Alias>
                <Comment>sub channel 1</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>3</MaxValue>
                <Comment>SDCCH/4</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>7</MaxValue>
                <Comment>SDCCH/8</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>1</MaxValue>
                <Comment>TCH/H</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_frame_erasure</Name>
                <Comment>values for frame_erasure</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TCH_LOOP_A</Alias>
                <Comment>TCH loop A</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>TCH_LOOP_B</Alias>
                <Comment>TCH loop B</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>TCH_LOOP_C</Alias>
                <Comment>TCH loop C</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>TCH_LOOP_D</Alias>
                <Comment>TCH loop D</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>TCH_LOOP_E</Alias>
                <Comment>TCH loop E</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>TCH_LOOP_F</Alias>
                <Comment>TCH loop F</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>TCH_LOOP_I</Alias>
                <Comment>TCH loop I</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tested_device</Name>
                <Comment>values for tested_device</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DAI_NO_TEST</Alias>
                <Comment>no test</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DAI_S_DEC</Alias>
                <Comment>speech decoder</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>DAI_S_COD</Alias>
                <Comment>speech coder</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>DAI_ACOUSTIC</Alias>
                <Comment>acoustic tests</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_sleep_mode</Name>
                <Comment>values for sleep_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NO_SLEEP</Alias>
                <Comment>no sleep mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SMALL_SLEEP</Alias>
                <Comment>small sleep mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>BIG_SLEEP</Alias>
                <Comment>big sleep mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>DEEP_SLEEP</Alias>
                <Comment>deep sleep mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>ALL_SLEEP</Alias>
                <Comment>all sleep modes</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_Clocks</Name>
                <Comment>values for Clocks</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CL_ARMIO</Alias>
                <Comment>ARMIO_CLK</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CL_RIFR</Alias>
                <Comment>RIF_CLKR</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CL_RIFX</Alias>
                <Comment>RIF_CLKX</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">16</Value>
                <Alias>CL_RIF13</Alias>
                <Comment>RIF_CLK13</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">32</Value>
                <Alias>CL_NCLK</Alias>
                <Comment>UWIRE_CLK</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">64</Value>
                <Alias>CL_SIM</Alias>
                <Comment>SIM_CLK</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">128</Value>
                <Alias>CL_TSP</Alias>
                <Comment>TSP_CLK</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">256</Value>
                <Alias>CL_TIMER</Alias>
                <Comment>TIMER_CLK</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">512</Value>
                <Alias>CL_TPU</Alias>
                <Comment>TPU_CLK</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1024</Value>
                <Alias>CL_UART</Alias>
                <Comment>UART_CLK</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2048</Value>
                <Alias>CL_SW_CLOCK</Alias>
                <Comment>SWITCH_IRQ_CLK</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_sb_flag</Name>
                <Comment>values for sb_flag</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NO_SB_FOUND</Alias>
                <Comment>synchron burst not found (fn_offset, time_alignment and bsic are not valid)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SB_FOUND</Alias>
                <Comment>synchron burst found (fn_offset, time_alignment and bsic are valid</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_gprs_prio</Name>
                <Comment>values for gprs_prio</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>GPRS_PRIO_TOP</Alias>
                <Comment>Higher than serving cell</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>GPRS_PRIO_HIGH</Alias>
                <Comment>Higher than normal ncell bcch reading</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>GPRS_PRIO_NORM</Alias>
                <Comment>Normal</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_radio_band_config</Name>
                <Comment>values for radio_band_config</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>STD_900</Alias>
                <Comment>GSM 900</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>STD_EGSM</Alias>
                <Comment>extended GSM</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>STD_1900</Alias>
                <Comment>PCS 1900</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>STD_1800</Alias>
                <Comment>DCS 1800</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>STD_DUAL</Alias>
                <Comment>GSM 900 / DCS 1800</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>STD_DUAL_EGSM</Alias>
                <Comment>extended GSM / DCS 1800</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>STD_850</Alias>
                <Comment>GSM 850</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>STD_DUAL_US</Alias>
                <Comment>GSM 850 / PCS 1900</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_initial_codec_mode</Name>
                <Comment>values for initial_codec_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CODEC_MODE_1</Alias>
                <Comment>lowest codec mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CODEC_MODE_2</Alias>
                <Comment>second lowest mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CODEC_MODE_3</Alias>
                <Comment>third lowest mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CODEC_MODE_4</Alias>
                <Comment>highest mode</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_eodt_data_valid</Name>
                <Comment>values for eodt_data_valid</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>EOTD_NOT_PRES</Alias>
                <Comment>EOTD data not present</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EOTD_PRES</Alias>
                <Comment>EOTD data present</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_eotd</Name>
                <Comment>values for eotd</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NC_MON</Alias>
                <Comment>neighbour cell monitoring</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>EOTD_MON</Alias>
                <Comment>EOTD monitoring</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_mode</Name>
                <Comment>values for mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MODE_IDLE</Alias>
                <Comment>idle</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MODE_DEDIC</Alias>
                <Comment>dedicated or packet transfer</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
    </ValuesSection>
</SAP>
