<?xml version="1.0" encoding="UTF-8"?>
<!-- edited with SAPE SAP Editor -->
<AIM xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="aim.xsd">
    <DocInfoSection>
        <DocName DocType="AIM">cc</DocName>
        <DocNum Number="600" Project="6147"/>
        <Description>
            <Section>The Protocol Stacks are used to define the functionality of the GSM protocols for interfaces. The GSM specifications are normative when used to describe the functionality of interfaces, but the stacks and the subdivision of protocol layers does not imply or restrict any implementation.</Section>
            <Section>The base of the Protocol Stack rests on the physical layer.</Section>
            <Section>The Data Link Layer (DL) is used to handle an acknowledged connection between mobile and base station. The LAPDm protocol is used.</Section>
            <Section>Radio Resource (RR) manages the resources of the air-interface. That means configuration of physical layer, cell selection and cell reselection, data transfer, RR-Connection handling.</Section>
            <Section>Mobility Management (MM) handles registration aspects for the mobile station. It detects changes of location areas and updates a mobile station in the new location area.</Section>
            <Section>Call Control (CC) provides the call functionality. This includes call establishment, call maintenance procedures like Hold, Retrieve or Modify, and call disconnection.</Section>
            <Section>Supplementary Services (SS) handles all call independent supplementary services like call forwarding or call barring.</Section>
            <Section>Short Message Services (SMS) is used for sending and receiving point-to-point short messages.</Section>
            <Section>The man machine interface (MMI) is the interface to the user. Normally it is connected with a keypad as input device and a display as output device.</Section>
            <Section>Between the several entities data interfaces are defined. These data interfaces are called Service Access Points (SAPs), indicating that an upper layer uses the services of a lower layer.</Section>
            <Section>The GSM specification do not set out any implementation of the Protocol Stack. The following diagrams show the implementation described in all these documents for the mobile station. All entities except the Man Machine Interface and Physical Layer are implemented as part of the Protocol Stack.</Section>
            <Section>Figure 1: Mobile-station protocol architecture</Section>
            <Section>This document describes the messages processed by the Call Control entity.</Section>
        </Description>
        <DocHistory>
            <DocVersion Number="100" Year="97"/>
            <Date Day="25" Month="6" Year="1997"/>
            <Author>LE</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Initial version.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="101" Year="97"/>
            <Date Day="1" Month="8" Year="2001"/>
            <Author>FK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Changed ITC_AUX_SPEECH to correct value</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="102" Year="97"/>
            <Date Day="7" Month="2" Year="2002"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Added cause 25, per-emption for R99/Cause Concept</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="103" Year="97"/>
            <Date Day="7" Month="2" Year="2002"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Switched to new template</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="104" Year="97"/>
            <Date Day="8" Month="3" Year="2002"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Long number dialling</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="105" Year="97"/>
            <Date Day="9" Month="4" Year="2002"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Call Deflection, redirected party into MT SETUP</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="106" Year="97"/>
            <Date Day="18" Month="4" Year="2002"/>
            <Author>OT</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Speech version indication modified</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="107" Year="97"/>
            <Date Day="27" Month="9" Year="2002"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Conquest Issues 4967, 6614 / rebase from g23m / merge from 133</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="108" Year="97"/>
            <Date Day="4" Month="2" Year="2003"/>
            <Author>LG</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Cause concept, TTY support, Conquest issue 8938</Comment>
        </DocHistory>
        <DocRef>
            <RefId>[1]</RefId>
            <RefTitle>Digital celluar telecommunications system (Phase 2+);            Mobile radio interface layer 3 specification            (GSM 4.08, December 1995, version 5.0.0)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[1a]</RefId>
            <RefTitle>GSM 2.81, Line Identification Supplementary Services - Stage 1 ETS 300 514, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[2]</RefId>
            <RefTitle>GSM 2.82, Call Forwarding Supplementary Services - Stage 1 ETS 300 515, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[3]</RefId>
            <RefTitle>GSM 2.83, Call Waiting and Call Hold Supplementary Services - Stage 1 ETS 300 516, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[4]</RefId>
            <RefTitle>GSM 2.84, Multi Party Supplementary Services - Stage 1 ETS 300 517, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[5]</RefId>
            <RefTitle>GSM 2.85, Closed User Group Supplementary Services - Stage 1 ETS 300 518, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[6]</RefId>
            <RefTitle>GSM 2.86, Advice of Charge Supplementary Services - Stage 1 ETS 300 519, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[7]</RefId>
            <RefTitle>GSM 2.88, Call Barring Supplementary Services - Stage 1 ETS 300 520, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[8]</RefId>
            <RefTitle>GSM 3.14, Support of Dual Tone Multi Frequency Signalling via the GSM System ETS 300 532, ETSI, April 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[9]</RefId>
            <RefTitle>GSM 3.40, Technical Realization of the Short Message Service Point-to-Point ETS 300 536, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[10]</RefId>
            <RefTitle>GSM 3.41, Technical Realization of Short Message Service Cell Broadcast ETS 300 537, ETSI, June 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[11]</RefId>
            <RefTitle>GSM 3.81, Line Identification Supplementary Services - Stage 2 ETS 300 542, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[12]</RefId>
            <RefTitle>GSM 3.82, Call Forwarding Supplementary Services - Stage 2 ETS 300 543, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[13]</RefId>
            <RefTitle>GSM 3.83, Call Waiting and Call Hold Supplementary Services - Stage 2 ETS 300 544, ETSI, November 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[14]</RefId>
            <RefTitle>GSM 3.84, Multi Party Supplementary Services - Stage 2 ETS 300 545, ETSI, November 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[15]</RefId>
            <RefTitle>GSM 3.85, Closed User Group Supplementary Services - Stage 2 ETS 300 546, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[16]</RefId>
            <RefTitle>GSM 3.86, Advice of Charge Supplementary Services - Stage 2 ETS 300 547, ETSI, March 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[17]</RefId>
            <RefTitle>GSM 3.88, Call Barring Supplementary Services - Stage 2 ETS 300 548, ETSI, November 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[18]</RefId>
            <RefTitle>GSM 4.01, MS-BSS Interface General Aspects and Principles ETS 300 550, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[18a]</RefId>
            <RefTitle>GSM 4.03, MS-BSS Interface Channel Structures and Access Capabilities ETS 300 552, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[19]</RefId>
            <RefTitle>GSM 4.05, Data Link Layer General Aspects ETS 300 554, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[20]</RefId>
            <RefTitle>GSM 4.06, MS-BSS Interface Data Link Layer Specification ETS 300 555, ETSI, September 1994</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[21]</RefId>
            <RefTitle>GSM 4.07, Mobile Radio Interface Signalling Layer 3 General Aspects ETS 300 556, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[22]</RefId>
            <RefTitle>GSM 4.08, Mobile Radio Interface Layer 3 Specification ETS 300 557, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[23]</RefId>
            <RefTitle>GSM 4.10, Mobile Radio Interface Layer 3 Supplementary Services Specification  General Aspects ETS 300 558, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[24]</RefId>
            <RefTitle>GSM 4.11, Point-to-Point Short Message Service Support on Mobile Radio Interface ETS 300 559, ETSI, October 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[25]</RefId>
            <RefTitle>GSM 4.12, Short Message Service Cell Broadcast Support on Mobile Radio Interface ETS 300 560, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[26]</RefId>
            <RefTitle>GSM 4.80, Mobile Radio Interface Supplementary Services Specification Formats and Coding ETS 300 564, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[27]</RefId>
            <RefTitle>GSM 4.81, Line Identification Supplementary Services - Stage 3 ETS 300 565, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[28]</RefId>
            <RefTitle>GSM 4.82, Call Forwarding Supplementary Services - Stage 3 ETS 300 566, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[29]</RefId>
            <RefTitle>GSM 4.83, Call Waiting and Call Hold Supplementary Services - Stage 3 ETS 300 567, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[30]</RefId>
            <RefTitle>GSM 4.84, Multi Party Supplementary Services - Stage 3 ETS 300 568, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[31]</RefId>
            <RefTitle>GSM 4.85, Closed User Group Supplementary Services - Stage 3 ETS 300 569, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[32]</RefId>
            <RefTitle>GSM 4.86, Advice of Charge Supplementary Services - Stage 3 ETS 300 570, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[33]</RefId>
            <RefTitle>GSM 4.88, Call Barring Supplementary Services - Stage 3 ETS 300 571, ETSI, February 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[34]</RefId>
            <RefTitle>GSM 5.01, Physical Layer on the Radio Path General Description ETS 300 573, ETSI, October 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[35]</RefId>
            <RefTitle>GSM 5.02, Multiplexing and Multiple Access on the Radio Path ETS 300 574, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[36]</RefId>
            <RefTitle>GSM 5.08, Radio Sub-system Link Control ETS 300 578, ETSI, January 1996</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[37]</RefId>
            <RefTitle>GSM 5.10, Radio Sub-system Synchronisation ETS 300 579, ETSI, October 1995</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[38]</RefId>
            <RefTitle>Service Access Point MMREG 6147.100.96.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[39]</RefId>
            <RefTitle>Service Access Point MNCC 6147.101.96.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[40]</RefId>
            <RefTitle>Service Access Point MNSS 6147.102.96.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[41]</RefId>
            <RefTitle>Service Access Point MNSMS 6147.103.96.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[42]</RefId>
            <RefTitle>Service Access Point MMCC 6147.104.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[43]</RefId>
            <RefTitle>Service Access Point MMSS 6147.105.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[44]</RefId>
            <RefTitle>Service Access Point MMSMS 6147.106.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[45]</RefId>
            <RefTitle>Service Access Point RR 6147.107.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[46]</RefId>
            <RefTitle>Service Access Point SIM 6147.108.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[47]</RefId>
            <RefTitle>Service Access Point MPH 6147.109.96.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[48]</RefId>
            <RefTitle>Service Access Point DL 6147.110.96.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[49]</RefId>
            <RefTitle>Service Access Point MDL 6147.111.96.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[50]</RefId>
            <RefTitle>Service Access Point PH 6147.112.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[51]</RefId>
            <RefTitle>Service Access Point MMI 6147.113.96.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[52]</RefId>
            <RefTitle>Message Sequence Charts CC 6147.200.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[53]</RefId>
            <RefTitle>Message Sequence Charts SS 6147.201.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[54]</RefId>
            <RefTitle>Message Sequence Charts SMS 6147.202.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[55]</RefId>
            <RefTitle>Message Sequence Charts MM 6147.203.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[56]</RefId>
            <RefTitle>Message Sequence Charts RR 6147.204.96.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[57]</RefId>
            <RefTitle>Message Sequence Charts DL 6147.205.96.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[58]</RefId>
            <RefTitle>Users Guide 6147.300.96.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[59]</RefId>
            <RefTitle>Test Specification CC 6147.400.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[60]</RefId>
            <RefTitle>Test Specification SS 6147.401.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[61]</RefId>
            <RefTitle>Test Specification SMS 6147.402.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[62]</RefId>
            <RefTitle>Test Specification MM 6147.403.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[63]</RefId>
            <RefTitle>Test Specification RR 6147.404.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[64]</RefId>
            <RefTitle>Test Specification DL 6147.405.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[65]</RefId>
            <RefTitle>Test Specification CCD 6147.406.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[66]</RefId>
            <RefTitle>SDL Specification CC 6147.500.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[67]</RefId>
            <RefTitle>SDL Specification SS 6147.501.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[68]</RefId>
            <RefTitle>SDL Specification SMS 6147.502.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[69]</RefId>
            <RefTitle>SDL Specification MM 6147.503.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[70]</RefId>
            <RefTitle>SDL Specification RR 6147.504.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[71]</RefId>
            <RefTitle>SDL Specification DL 6147.505.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[72]</RefId>
            <RefTitle>Message Specification CC 6147.600.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[73]</RefId>
            <RefTitle>Message Specification SS 6147.601.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[74]</RefId>
            <RefTitle>Message Specification SMS 6147.602.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[75]</RefId>
            <RefTitle>Message Specification MM 6147.603.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[76]</RefId>
            <RefTitle>Message Specification RR 6147.604.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[77]</RefId>
            <RefTitle>Message Specification DL 6147.605.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[78]</RefId>
            <RefTitle>Technical Documentation CC 6147.700.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[79]</RefId>
            <RefTitle>Technical Documentation SS 6147.701.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[80]</RefId>
            <RefTitle>Technical Documentation SMS 6147.702.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[81]</RefId>
            <RefTitle>Technical Documentation MM 6147.703.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[82]</RefId>
            <RefTitle>Technical Documentation RR 6147.704.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[83]</RefId>
            <RefTitle>Technical Documentation DL 6147.705.97.100; Condat AG</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[84]</RefId>
            <RefTitle>Technical Documentation CCD 6147.706.97.100; Condat AG</RefTitle>
        </DocRef>
    </DocInfoSection>
    <ConstantsSection>
        <Description>
            <Section>2 Constants</Section>
        </Description>
        <Constant>
            <Alias>L3MAX</Alias>
            <Value ValueType="DEC">251</Value>
            <Comment>maximum size of a L3 buffer</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_SS_VERSION</Alias>
            <Value ValueType="DEC">1</Value>
            <Comment>maximum length in SS version</Comment>
        </Constant>
        <History>
            <Date Day="1" Month="1" Year="2000"/>
            <Author>VK</Author>
            <Comment>Initial</Comment>
        </History>
        <History>
            <Date Day="4" Month="2" Year="2003"/>
            <Author>LG</Author>
            <Comment>added MAX_SS_VERSION</Comment>
        </History>
    </ConstantsSection>
    <MessagesSection>
        <Description>
            <Section>This section contains all messages that are defined for the CC AIM</Section>
        </Description>
        <Message>
            <Description>
                <Section>This message is sent by the network to the calling mobile station to indicate that the called user alerting has been initiated.</Section>
                <Section>Reference : [1] section 9.3.1.1</Section>
            </Description>
            <MsgDef>
                <Name>d_alert</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000001</MsgID>
                <Comment>Alerting</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>progress</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>10.5.4.21</SpecRef>
                <Comment>Progress indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the called mobile station to the network, to indicate that the called user alerting has been initiated.</Section>
                <Section>Reference : [1] section 9.3.1.2</Section>
            </Description>
            <MsgDef>
                <Name>u_alert</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00000001</MsgID>
                <Comment>Alerting</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ss_version</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7F</ItemTag>
                <SpecRef>10.5.4.24</SpecRef>
                <Comment>SS version</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the called mobile station to confirm an incoming call request.</Section>
                <Section>Reference : [1] section 9.3.2</Section>
            </Description>
            <MsgDef>
                <Name>u_call_conf</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00001000</MsgID>
                <Comment>Call confirmed</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>repeat</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>10.5.4.22</SpecRef>
                <Comment>Repeat Indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability 1</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap_2</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability 2</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>call_ctrl_cap</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">15</ItemTag>
                <SpecRef>10.5.4.5a</SpecRef>
                <Comment>CC Capabilities</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to the calling mobile station to indicate that the requested call establishment information has been received, and no more call establishment information will be accepted.</Section>
                <Section>Reference : [1] section 9.3.3</Section>
            </Description>
            <MsgDef>
                <Name>d_call_proceed</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000010</MsgID>
                <Comment>Call proceeding</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>repeat</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>10.5.4.22</SpecRef>
                <Comment>Repeat Indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability 1</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap_2</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability 2</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>progress</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>10.5.4.21</SpecRef>
                <Comment>Progress indicator</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile station or the network to indicate the establishment or termination of flow control on the transmission of USER INFORMATION messages.</Section>
                <Section>Reference : [1] section 9.3.4</Section>
            </Description>
            <MsgDef>
                <Name>b_congest_ctrl</Name>
                <MsgID Direction="BOTH" IDType="BIN">00111001</MsgID>
                <Comment>Congestion control</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>congest_lev</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.4.12</SpecRef>
                <Comment>Congestion level</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <SpecRef>10.5.1.8</SpecRef>
                <Comment>Spare half octet</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to the calling mobile station to indicate call acceptance by the called user.</Section>
                <Section>Reference : [1] section 9.3.5.1</Section>
            </Description>
            <MsgDef>
                <Name>d_connect</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000111</MsgID>
                <Comment>Connect</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>progress</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>10.5.4.21</SpecRef>
                <Comment>Progress indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>connect_num</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">4C</ItemTag>
                <SpecRef>10.5.4.13</SpecRef>
                <Comment>Connected number</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>connect_subaddr</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">4D</ItemTag>
                <SpecRef>10.5.4.14</SpecRef>
                <Comment>Connected subaddress</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the called mobile station to the network to indicate call acceptance by the called user.</Section>
                <Section>Reference : [1] section 9.3.5.2</Section>
            </Description>
            <MsgDef>
                <Name>u_connect</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00000111</MsgID>
                <Comment>Connect</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>connect_subaddr</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">4D</ItemTag>
                <SpecRef>10.5.4.14</SpecRef>
                <Comment>Connected subaddress</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ss_version</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7F</ItemTag>
                <SpecRef>10.5.4.24</SpecRef>
                <Comment>SS version</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to the called mobile station to indicate that the mobile station has been awarded the call. It shall also be sent by the calling mobile station to the network to acknowledge the offered connection.</Section>
                <Section>Reference : [1] section 9.3.6</Section>
            </Description>
            <MsgDef>
                <Name>b_connect_ack</Name>
                <MsgID Direction="BOTH" IDType="BIN">00001111</MsgID>
                <Comment>Connect acknowledge</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to indicate that the end-to-end connection is cleared.</Section>
                <Section>Reference : [1] section 9.3.7.1</Section>
            </Description>
            <MsgDef>
                <Name>d_disconnect</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00100101</MsgID>
                <Comment>Disconnect</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>progress</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>10.5.4.21</SpecRef>
                <Comment>Progress indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>allowed_actions</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7B</ItemTag>
                <SpecRef>10.5.4.27</SpecRef>
                <Comment>Allowed Actions</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>allowed actions added</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile station to request the network to clear an end-to-end connection.</Section>
                <Section>Reference : [1] section 9.3.7.2</Section>
            </Description>
            <MsgDef>
                <Name>u_disconnect</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00100101</MsgID>
                <Comment>Disconnect</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ss_version</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7F</ItemTag>
                <SpecRef>10.5.4.24</SpecRef>
                <Comment>SS version</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent from the mobile station to initiate emergency call establishment.</Section>
                <Section>Reference : [1] section 9.3.8</Section>
            </Description>
            <MsgDef>
                <Name>u_emerge_setup</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00001110</MsgID>
                <Comment>Emergency setup</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to the mobile station to request or acknowledge a supplementary service. The supplementary service to be invoked and its associated parameters are specified in the facility information element.</Section>
                <Section>Reference : [1] section 9.3.9.1</Section>
            </Description>
            <MsgDef>
                <Name>d_facility</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00111010</MsgID>
                <Comment>Facility</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile station to the network to request or acknowledge a supplementary service. The supplementary service to be invoked and its associated parameters are specified in the facility information element.</Section>
                <Section>Reference : [1] section 9.3.9.2</Section>
            </Description>
            <MsgDef>
                <Name>u_facility</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00111010</MsgID>
                <Comment>Facility</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ss_version</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7F</ItemTag>
                <SpecRef>10.5.4.24</SpecRef>
                <Comment>SS version</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile user to request the hold function for an existing call.</Section>
                <Section>Reference : [1] section 9.3.10</Section>
            </Description>
            <MsgDef>
                <Name>u_hold</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00011000</MsgID>
                <Comment>Hold</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to indicate that the hold function has been successfully performed.</Section>
                <Section>Reference : [1] section 9.3.11</Section>
            </Description>
            <MsgDef>
                <Name>d_hold_ack</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00011001</MsgID>
                <Comment>Hold Acknowledge</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to indicate the denial of a request to hold a call.</Section>
                <Section>Reference : [1] section 9.3.12</Section>
            </Description>
            <MsgDef>
                <Name>d_hold_rej</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00011010</MsgID>
                <Comment>Hold Reject</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile station to the network or by the network to the mobile station to request a change in bearer capability for a call.</Section>
                <Section>Reference : [1] section 9.3.13</Section>
            </Description>
            <MsgDef>
                <Name>b_modify</Name>
                <MsgID Direction="BOTH" IDType="BIN">00010111</MsgID>
                <Comment>Modify</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>low_layer_comp</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.4.18</SpecRef>
                <Comment>Low layer comp.</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>high_layer_comp</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7D</ItemTag>
                <SpecRef>10.5.4.16</SpecRef>
                <Comment>High layer comp.</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>reverse_call</Name>
                </ItemLink>
                <Type>GSM2_T</Type>
                <ItemTag TagType="HEX">A3</ItemTag>
                <SpecRef>10.5.4.22a</SpecRef>
                <Comment>Reverse call setup direction direction</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile station to the network or by the network to the mobile station to indicate completion of a request to change bearer capability for a call.</Section>
                <Section>Reference : [1] section 9.3.14</Section>
            </Description>
            <MsgDef>
                <Name>b_modify_comp</Name>
                <MsgID Direction="BOTH" IDType="BIN">00011111</MsgID>
                <Comment>Modify complete</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>low_layer_comp</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.4.18</SpecRef>
                <Comment>Low layer comp.</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>high_layer_comp</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7D</ItemTag>
                <SpecRef>10.5.4.16</SpecRef>
                <Comment>High layer comp.</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>reverse_call</Name>
                </ItemLink>
                <Type>GSM2_T</Type>
                <ItemTag TagType="HEX">A3</ItemTag>
                <SpecRef>10.5.4.22a</SpecRef>
                <Comment>Reverse call setup direction direction</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile station to the network or by the network to the mobile station to indicate failure of a request to change the bearer capability for a call.</Section>
                <Section>Reference : [1] section 9.3.15</Section>
            </Description>
            <MsgDef>
                <Name>b_modify_rej</Name>
                <MsgID Direction="BOTH" IDType="BIN">00010011</MsgID>
                <Comment>Modify reject</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>low_layer_comp</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>Low layer comp.</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>high_layer_comp</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7D</ItemTag>
                <SpecRef>10.5.4.16</SpecRef>
                <Comment>High layer comp.</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent either from the mobile station or from the network to indicate information pertaining to a call, such as user suspended.</Section>
                <Section>Reference : [1] section 9.3.16</Section>
            </Description>
            <MsgDef>
                <Name>b_notify</Name>
                <MsgID Direction="BOTH" IDType="BIN">00111110</MsgID>
                <Comment>Notify</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>notific</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.4.20</SpecRef>
                <Comment>Notification indicator</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent from the network to the mobile station to indicate the progress of a call in the event of interworking or in connection with the provision of in-band information/patterns.</Section>
                <Section>Reference : [1] section 9.3.17</Section>
            </Description>
            <MsgDef>
                <Name>d_progress</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000011</MsgID>
                <Comment>Progress</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>progress</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.21</SpecRef>
                <Comment>Progress indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent, from the network to the mobile station to indicate that the network intends to release the transaction identifier, and that the receiving equipment shall release the transaction identifier after sending RELEASE COMPLETE.</Section>
                <Section>Reference : [1] section 9.3.18.1</Section>
            </Description>
            <MsgDef>
                <Name>d_release</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00101101</MsgID>
                <Comment>Release</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause_2</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>Second cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent from the mobile station to the network to indicate that the mobile station intends to release the transaction identifier, and that the receiving equipment shall release the transaction identifier after sending RELEASE COMPLETE.</Section>
                <Section>Reference : [1] section 9.3.18.2</Section>
            </Description>
            <MsgDef>
                <Name>u_release</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00101101</MsgID>
                <Comment>Release</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause_2</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>Second cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ss_version</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7F</ItemTag>
                <SpecRef>10.5.4.24</SpecRef>
                <Comment>SS version</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent from the network to the mobile station to indicate that the network has released the transaction identifier and that the mobile station shall release the transaction identifier.</Section>
                <Section>Reference : [1] section 9.3.19.1</Section>
            </Description>
            <MsgDef>
                <Name>d_release_comp</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00101010</MsgID>
                <Comment>Release complete</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent from the mobile station to the network to indicate that the mobile station has released the transaction identifier and that the network shall release the transaction identifier.</Section>
                <Section>Reference : [1] section 9.3.19.2</Section>
            </Description>
            <MsgDef>
                <Name>u_release_comp</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00101010</MsgID>
                <Comment>Release complete</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ss_version</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7F</ItemTag>
                <SpecRef>10.5.4.24</SpecRef>
                <Comment>SS version</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile user to request the retrieval of a held call.</Section>
                <Section>Reference : [1] section 9.3.20</Section>
            </Description>
            <MsgDef>
                <Name>u_retrieve</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00011100</MsgID>
                <Comment>Retrieve</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to indicate that the retrieve function has been successfully performed.</Section>
                <Section>Reference : [1] section 9.3.21</Section>
            </Description>
            <MsgDef>
                <Name>d_retrieve_ack</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00011101</MsgID>
                <Comment>Retrieve Acknowledge</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to indicate the inability to perform the requested retrieve function.</Section>
                <Section>Reference : [1] section 9.3.22</Section>
            </Description>
            <MsgDef>
                <Name>d_retrieve_rej</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00011110</MsgID>
                <Comment>Retrieve Reject</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to the mobile station to initiate a mobile terminated call establishment.</Section>
                <Section>Reference : [1] section 9.3.23.1</Section>
            </Description>
            <MsgDef>
                <Name>d_setup</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000101</MsgID>
                <Comment>Setup</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>repeat</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>10.5.4.22</SpecRef>
                <Comment>BC repeat indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability 1</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap_2</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability 2</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>progress</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>10.5.4.21</SpecRef>
                <Comment>Progress indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>signal</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">34</ItemTag>
                <SpecRef>10.5.4.23</SpecRef>
                <Comment>Signal</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>calling_num</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">5C</ItemTag>
                <SpecRef>10.5.4.9</SpecRef>
                <Comment>Calling party number BCD</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>calling_subaddr</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">5D</ItemTag>
                <SpecRef>10.5.4.10</SpecRef>
                <Comment>Calling party sub-address</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>dl_called_num</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">5E</ItemTag>
                <SpecRef>10.5.4.7</SpecRef>
                <Comment>Called party BCD number</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>called_subaddr</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">6D</ItemTag>
                <SpecRef>10.5.4.8</SpecRef>
                <Comment>Called party sub-address</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>redirecting_num</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">74</ItemTag>
                <SpecRef>10.5.4.21b</SpecRef>
                <Comment>Redirecting party BCD number</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>redirecting_subaddr</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">75</ItemTag>
                <SpecRef>10.5.4.21c</SpecRef>
                <Comment>Redirecting party sub-address</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>repeat_2</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>10.5.4.22</SpecRef>
                <Comment>LLC repeat indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>low_layer_comp</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.4.18</SpecRef>
                <Comment>Low layer compatibility I</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>low_layer_comp_2</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.4.18</SpecRef>
                <Comment>Low layer compatibility II</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>repeat_3</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>10.5.4.22</SpecRef>
                <Comment>HLC repeat indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>high_layer_comp</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7D</ItemTag>
                <SpecRef>10.5.4.16</SpecRef>
                <Comment>High layer compatibility i</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>high_layer_comp_2</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7D</ItemTag>
                <SpecRef>10.5.4.16</SpecRef>
                <Comment>High layer compatibility ii</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="1" Year="2002"/>
                <Author>OT</Author>
                <Comment>Length of bearer capapility 1-2 adjusted.</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>HM</Author>
                <Comment>called_num => dl_called_num (long number dialling)</Comment>
            </History>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>redirecting party number and subaddress inserted</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent from the mobile station to the network to initiate a mobile originating call establishment.</Section>
                <Section>Reference : [1] section 9.3.23.2</Section>
            </Description>
            <MsgDef>
                <Name>u_setup</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00000101</MsgID>
                <Comment>Setup</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>repeat</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>10.5.4.22</SpecRef>
                <Comment>BC repeat indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability 1</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap_2</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability 2</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1C</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility (simple recall alignment)</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>calling_subaddr</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">5D</ItemTag>
                <SpecRef>10.5.4.10</SpecRef>
                <Comment>Calling party sub-address</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ul_called_num</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">5E</ItemTag>
                <SpecRef>10.5.4.7</SpecRef>
                <Comment>Called party BCD number</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>called_subaddr</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">6D</ItemTag>
                <SpecRef>10.5.4.8</SpecRef>
                <Comment>Called party sub-address</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>repeat_2</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>10.5.4.22</SpecRef>
                <Comment>LLC repeat indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>low_layer_comp</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.4.18</SpecRef>
                <Comment>Low layer compatibility I</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>low_layer_comp_2</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7C</ItemTag>
                <SpecRef>10.5.4.18</SpecRef>
                <Comment>Low layer compatibility II</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>repeat_3</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>10.5.4.22</SpecRef>
                <Comment>HLC repeat indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>high_layer_comp</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7D</ItemTag>
                <SpecRef>10.5.4.16</SpecRef>
                <Comment>High layer compatibility i</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>high_layer_comp_2</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7D</ItemTag>
                <SpecRef>10.5.4.16</SpecRef>
                <Comment>High layer compatibility ii</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7E</ItemTag>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ss_version</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">7F</ItemTag>
                <SpecRef>10.5.4.24</SpecRef>
                <Comment>SS version</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>clir_suppr</Name>
                </ItemLink>
                <Type>GSM2_T</Type>
                <ItemTag TagType="HEX">A1</ItemTag>
                <SpecRef>10.5.4.11a</SpecRef>
                <Comment>CLIR suppression</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>clir_invoc</Name>
                </ItemLink>
                <Type>GSM2_T</Type>
                <ItemTag TagType="HEX">A2</ItemTag>
                <SpecRef>10.5.4.11b</SpecRef>
                <Comment>CLIR invocation</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>call_ctrl_cap</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">15</ItemTag>
                <SpecRef>10.5.4.5a</SpecRef>
                <Comment>CC capabilities</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>fac_adv</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">1D</ItemTag>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility (advanced recall alignment)</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="31" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Added fac_adv for CCBS</Comment>
            </History>
            <History>
                <Date Day="21" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>Max length for bearer caps increased</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>HM</Author>
                <Comment>called_num => ul_called_num (long number dialling)</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="2002"/>
                <Author>SBK</Author>
                <Comment>issue 6614</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile station to the network and contains the digit the network should reconvert back into a DTMF tone which is then applied towards the remote user.</Section>
                <Section>Reference : [1] section 9.3.24</Section>
            </Description>
            <MsgDef>
                <Name>u_start_dtmf</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00110101</MsgID>
                <Comment>Start DTMF</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>key_facility</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">2C</ItemTag>
                <SpecRef>10.5.4.17</SpecRef>
                <Comment>Keypad facility</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to the mobile station to indicate the successful initiation of the action requested by the START DTMF message (conversion of the digit contained in this message into a DTMF tone).</Section>
                <Section>Reference : [1] section 9.3.25</Section>
            </Description>
            <MsgDef>
                <Name>d_start_dtmf_ack</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00110110</MsgID>
                <Comment>Start DTMF Acknowledge</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>key_facility</Name>
                </ItemLink>
                <Type>GSM3_TV</Type>
                <ItemTag TagType="HEX">2C</ItemTag>
                <SpecRef>10.5.4.17</SpecRef>
                <Comment>Keypad facility</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to the mobile station, if the network can not accept the START DTMF message.</Section>
                <Section>Reference : [1] section 9.3.26</Section>
            </Description>
            <MsgDef>
                <Name>d_start_dtmf_rej</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00110111</MsgID>
                <Comment>Start DTMF reject</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile station or the network at any time during a call to report certain error conditions listed in section 8. It shall also be sent in response to a STATUS ENQUIRY message.</Section>
                <Section>Reference : [1] section 9.3.27</Section>
            </Description>
            <MsgDef>
                <Name>b_status</Name>
                <MsgID Direction="BOTH" IDType="BIN">00111101</MsgID>
                <Comment>Status</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>call_state</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.4.6</SpecRef>
                <Comment>Call state</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>aux_states</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">24</ItemTag>
                <SpecRef>10.5.4.4</SpecRef>
                <Comment>Auxiliary states</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile station or the network at any time to solicit a STATUS message from the peer layer 3 entity. Sending of STATUS message in response to a STATUS ENQUIRY message is mandatory.</Section>
                <Section>Reference : [1] section 9.3.28</Section>
            </Description>
            <MsgDef>
                <Name>b_status_enq</Name>
                <MsgID Direction="BOTH" IDType="BIN">00110100</MsgID>
                <Comment>Status enquiry</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by a mobile station to the network and is used to stop the DTMF tone sent towards the remote user.</Section>
                <Section>Reference : [1] section 9.3.29</Section>
            </Description>
            <MsgDef>
                <Name>u_stop_dtmf</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00110001</MsgID>
                <Comment>Stop DTMF</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to the mobile station to indicate that the sending of the DTMF tone has been stopped.</Section>
                <Section>Reference : [1] section 9.3.30</Section>
            </Description>
            <MsgDef>
                <Name>d_stop_dtmf_ack</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00110010</MsgID>
                <Comment>Stop DTMF acknowledge</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile station to the network to transfer information to the remote user. This message is also sent by the network to the mobile station to deliver information transferred from the remote user. This message is used if the user-to-user transfer is part of an allowed information transfer as defined in TS GSM 04.10.</Section>
                <Section>Reference : [1] section 9.3.31</Section>
            </Description>
            <MsgDef>
                <Name>b_user_info</Name>
                <MsgID Direction="BOTH" IDType="BIN">00010000</MsgID>
                <Comment>User information</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_user</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.25</SpecRef>
                <Comment>User-user</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>more_data</Name>
                </ItemLink>
                <Type>GSM2_T</Type>
                <ItemTag TagType="HEX">A0</ItemTag>
                <SpecRef>10.5.4.19</SpecRef>
                <Comment>More data</Comment>
            </MsgItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the mobile station to the network to open a Call Control Transaction which the network has requested the mobile station to open.</Section>
                <Section>Reference : [1] section 9.3.23a</Section>
            </Description>
            <MsgDef>
                <Name>u_start_cc</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00001001</MsgID>
                <Comment>Start_CC</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>call_ctrl_cap</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">15</ItemTag>
                <SpecRef>10.5.4.5a</SpecRef>
                <Comment>CC Capabilities</Comment>
            </MsgItem>
            <History>
                <Date Day="18" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent from the network to the mobile station to initiate the sending of a SETUP message. In addition it provides information for user notification. The purpose of the recall type information is to describe the reason for the call.</Section>
                <Section>Reference : [1] section 9.3.18a</Section>
            </Description>
            <MsgDef>
                <Name>d_recall</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00001011</MsgID>
                <Comment>Recall</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>recall_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.4.21a</SpecRef>
                <Comment>Recall Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>facility</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.15</SpecRef>
                <Comment>Facility</Comment>
            </MsgItem>
            <History>
                <Date Day="18" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the called mobile station to the network to indicate the requested channel characteristics for the call which may be initiated by the mobile station.</Section>
                <Section>Reference : [1] section 9.3.17b</Section>
            </Description>
            <MsgDef>
                <Name>u_cc_est_conf</Name>
                <MsgID Direction="UPLINK" IDType="BIN">00000110</MsgID>
                <Comment>CC-Establishment confirmed</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="CONDITIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>repeat</Name>
                </ItemLink>
                <Type>GSM1_TV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>10.5.4.22</SpecRef>
                <Comment>Repeat Indicator</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability 1</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>bearer_cap_2</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>10.5.4.5</SpecRef>
                <Comment>Bearer capability 2</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cc_cause</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>10.5.4.11</SpecRef>
                <Comment>CC Cause</Comment>
            </MsgItem>
            <History>
                <Date Day="18" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent from the network to the mobile station to provide information on the call that the mobile station should attempt to establish. From the 4th IE onwards the message is coded in the same way as the SETUP message in MS to network direction from the 4th IE onwards.</Section>
                <Section>Reference : [1] section 9.3.17a</Section>
            </Description>
            <MsgDef>
                <Name>d_cc_establishment</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">00000100</MsgID>
                <Comment>CC-Establishment</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4.</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>setup_cont</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.4.22a</SpecRef>
                <Comment>Setup Container</Comment>
            </MsgItem>
            <History>
                <Date Day="18" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
    </MessagesSection>
    <MsgStructElementsSection>
        <Description>
            <Section>This section contains all structured elements that are defined for the CC AIM</Section>
        </Description>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the auxiliary states information element is to describe the current status of the auxiliary states of a call in the call control states &quot;active&quot; and &quot;mobile originating modify&quot;.</Section>
                <Section>Reference : [1] section 10.5.4.4</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>aux_states</Name>
                <Comment>Auxiliary states</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>hold</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Hold auxiliary state</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>mpty</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>MPTY auxiliary state</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the bearer capability information element is to describe a bearer service.</Section>
                <Section>Reference : [1] section 10.5.4.5</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>bearer_cap</Name>
                <Comment>Bearer capability</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>bearer_cap_2</Name>
                <Comment>Bearer capability</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>rad_chan_req</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Radio channel requirement</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>code</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Coding standard</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>trans_mode</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Transfer mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>trans_cap</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Information transfer capability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>coding_bc3x1</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Meaning of octet 3a</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ctm</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Support of CTM text telephony</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>speech_vers1</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Speech version indication no. 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>coding_bc3x2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Meaning of octet 3b</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>speech_vers2</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Speech version indication no. 2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>coding_bc3x3</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Meaning of octet 3c</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>speech_vers3</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Speech version indication no. 3</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>coding_bc3x4</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Meaning of octet 3d</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>speech_vers4</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Speech version indication no. 4</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>coding_bc3x5</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Meaning of octet 3e</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>speech_vers5</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Speech version indication no. 5</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>compress</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Compression</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>structure</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Structure</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>duplex</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Duplex mode</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>config</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Configuration</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>nirr</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Negotiation of intermed. rate req.</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>establish</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Establishment</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>access_ident</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Access identity</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>rate_adapt</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Rate adaption</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>sig_access_prot</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Signalling access protocol</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>l1_ident</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Layer 1 identity</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_inf_l1_prot</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>User information layer 1 protocol</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>sync_async</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Synchronous / Asyncronous</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>num_stop</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Number of stop bits</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>negotiate</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Negotiation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>num_data</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Number of data bits</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_rate</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>User rate</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>intermed_rate</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Intermediate rate</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>nic_tx</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Network independent clock on Tx</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>nic_rx</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Network independent clock on Rx</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>parity</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Parity</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>conn_elem</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Connection element</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>modem_type</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Modem type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>modem_type_2</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Other Modem type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>fnur</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Fixed network user rate</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>acc</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Acceptable Channel Codings</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>mTch</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Maximum Traffic Channels</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>uimi</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>User initiated Modification Ind</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>waiur</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Wanted Air Interface User Rate</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>l2_ident</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Layer 2 identity</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>user_inf_l2_prot</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>User information layer 2 protocol</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Octet Groups revised</Comment>
            </History>
            <History>
                <Date Day="3" Month="11" Year="1997"/>
                <Author>PZ</Author>
                <Comment>Octet Groups revised too.</Comment>
            </History>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Octet 6d,6e,6f added</Comment>
            </History>
            <History>
                <Date Day="21" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>speech_vers4/5 added (AMR)</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the Call Control Capabilities information element is to identify the call control capabilities of the mobile station.</Section>
                <Section>Reference : [1] section 10.5.4.5a</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>call_ctrl_cap</Name>
                <Comment>Call Control Capabilities</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000000</Pattern>
                    <BitLen>6</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>pcp</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PCP</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>dtmf</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>DTMF</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>pcp added</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the call state information element is to describe the current status of a call.</Section>
                <Section>Reference : [1] section 10.5.4.6</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>call_state</Name>
                <Comment>Call state</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cs</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Coding standard II</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>state</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Call state value</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the called party BCD number information element is to identify the called party.</Section>
                <Section>Reference : [1] section 10.5.4.7</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>dl_called_num</Name>
                <Comment>Called party BCD number</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ton</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Type of number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>npi</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Numbering plan identification</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>num</Name>
                </ItemLink>
                <Type>BCDEVEN</Type>
                <Control>
                    <TypeModifier>[0..32]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Number digit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>HM</Author>
                <Comment>Changed max. length of num from 20 to 32</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the called party BCD number information element is to identify the called party.</Section>
                <Section>Reference : [1] section 10.5.4.7</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ul_called_num</Name>
                <Comment>Called party BCD number</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ton</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Type of number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>npi</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Numbering plan identification</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>num</Name>
                </ItemLink>
                <Type>BCDEVEN</Type>
                <Control>
                    <TypeModifier>[0..80]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Number digit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>HM</Author>
                <Comment>Changed max. length of num from 20 to 80</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the Called party subaddress is to identify the subaddress of the called party of a call. For the definition of a subaddress see Rec. CCITT I.330.</Section>
                <Section>Reference : [1] section 10.5.4.8</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>called_subaddr</Name>
                <Comment>Called party subaddress</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>tos</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Type of subaddress</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>odd_even</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Odd / even indication</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>subaddr</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..20]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Subaddress information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the calling party BCD number information element is to identify the origin of a call.</Section>
                <Section>Reference : [1] section 10.5.4.9</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>calling_num</Name>
                <Comment>Calling party BCD number</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ton</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Type of number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>npi</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Numbering plan identification</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>present</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Presentation indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>screen</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Screening indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>num</Name>
                </ItemLink>
                <Type>BCDEVEN</Type>
                <Control>
                    <TypeModifier>[0..22]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Number digit (0..20)</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Octett Groups revised</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>HM</Author>
                <Comment>Changed max. length of num from 20 to 22</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the Calling party subaddress is to identify a subaddress associated with the origin of a call. For the definition of a subaddress see Rec. CCITT I.330.</Section>
                <Section>Reference : [1] section 10.5.4.10</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>calling_subaddr</Name>
                <Comment>Calling party subaddress</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>tos</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Type of subaddress</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>odd_even</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Odd / even Indication</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>subaddr</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..20]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Subaddress information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Octett Groups revised</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the cause information element is to describe the reason for generating certain messages, to provide diagnostic information in the event of procedural errors and to indicate the location of the cause originator.</Section>
                <Section>Reference : [1] section 10.5.4.11</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cc_cause</Name>
                <Comment>Cause</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>cc_cause_2</Name>
                <Comment>Cause</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cs</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Coding standard II</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>loc</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Location</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>rec</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Recommendation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Cause value</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>diag</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..27]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Diagnostics</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Octett Groups revised</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The CLIR suppression information element may be sent by the mobile station to the network in the SETUP message. The use is defined in TS GSM 04.81.</Section>
                <Section>Reference : [1] section 10.5.4.11a</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>clir_suppr</Name>
                <Comment>CLIR suppression</Comment>
            </MsgStructElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The CLIR invocation information element may be sent by the mobile station to the network in the SETUP message. The use is defined in TS GSM 04.81.</Section>
                <Section>Reference : [1] section 10.5.4.11a</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>clir_invoc</Name>
                <Comment>CLIR invocation</Comment>
            </MsgStructElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the connected number information element is to identify the connected party of a call.</Section>
                <Section>Reference : [1] section 10.5.4.13</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>connect_num</Name>
                <Comment>Connected number</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ton</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Type of number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>npi</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Number plan identification</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>present</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Presentation indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>screen</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Screening indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>num</Name>
                </ItemLink>
                <Type>BCDEVEN</Type>
                <Control>
                    <TypeModifier>[0..22]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Number digit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Octett Groups revised</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>HM</Author>
                <Comment>Changed max. length of num from 20 to 22</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the connected subaddress information element is to identify a subaddress associated with the connected party of a call.</Section>
                <Section>Reference : [1] section 10.5.4.14</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>connect_subaddr</Name>
                <Comment>Connected subaddress</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>tos</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Type of subaddress</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>odd_even</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Odd / even indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>subaddr</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..20]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Subaddress information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the facility information element is to transport supplementary service related information. Within the scope of TS GSM 04.08 the content of the Facility information field is an array of octets. The usage of this transportation mechanism is defined in TS GSM 04.80.</Section>
                <Section>Reference : [1] section 10.5.4.15</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>facility</Name>
                <Comment>Facility</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>fac_adv</Name>
                <Comment>Facility</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>fac</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..L3MAX]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Facility information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="31" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Added fac_adv for CCBS</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the high layer compatibility information element is to provide a means which should be used by the remote user for compatibility checking. See Annex B.</Section>
                <Section>Reference : [1] section 10.5.4.16</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>high_layer_comp</Name>
                <Comment>High layer compatibility</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>high_layer_comp_2</Name>
                <Comment>High layer compatibility</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cs</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Coding standard II</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>interpret</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Interpretation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>prot_prof</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Presentation method of protocol profile</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>hlci</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>High layer characteristics identification</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ext_hlci</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Extended high layer characteristics identification</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Octett Groups revised (Octett Group 4 problem outstanding)</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the keypad facility information element is to convey IA5 characters, e.g. entered by means of a terminal keypad.</Section>
                <Section>Reference : [1] section 10.5.4.17</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>key_facility</Name>
                <Comment>Keypad facility</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>key</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Keypad information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the low layer compatibility information element is to provide a means which should be used for compatibility checking by an addressed entity (e.g., a remote user or an interworking unit or a high layer function network node addressed by the calling user). The low layer compatibility information element is transferred transparently by a PLMN between the call originating entity (e.g. the calling user) and the addressed entity.</Section>
                <Section>The coding of the Low Layer Information is described in ETS 300 102-1.</Section>
                <Section>Reference : [1] section 10.5.4.18</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>low_layer_comp</Name>
                <Comment>Low layer compatibility</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>low_layer_comp_2</Name>
                <Comment>Low layer compatibility</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>llc</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..13]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Low layer information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The more data information element is sent by the mobile station to the network or to the network to the mobile station in a USER INFORMATION message. The presence of the more data information element indicates to the destination remote user/mobile station that another USER INFORMATION message will follow containing information belonging to the same block.</Section>
                <Section>Reference : [1] section 10.5.4.19</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>more_data</Name>
                <Comment>More data</Comment>
            </MsgStructElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the notification indicator information element is to indicate information pertaining to a call.</Section>
                <Section>Reference : [1] section 10.5.4.20</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>notific</Name>
                <Comment>Notification indicator</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>nd</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Notification description</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the progress indicator information element is to describe an event which has occurred during the life of a call.</Section>
                <Section>Reference : [1] section 10.5.4.21</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>progress</Name>
                <Comment>Progress indicator</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>cs</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Coding standard II</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>loc</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Location</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>progress_desc</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Progress description</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>This information element may be included in a MODIFY and MODIFY COMPLETE message to indicate that the direction of the data call to which the MODIFY message relates is opposite to the call setup direction.</Section>
                <Section>Reference : [1] section 10.5.4.22a</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>reverse_call</Name>
                <Comment>Reverse call setup direction</Comment>
            </MsgStructElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the SS version indicator information element is to aid the decoding of the Facility information element as described in TS GSM 04.10. Within the scope of TS GSM 04.08 the contents of the SS Version information field is an array of one or more octets. The usage of the SS version information field is defined in TS GSM 04.80.</Section>
                <Section>Reference : [1] section 10.5.4.24</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ss_version</Name>
                <Comment>SS Version Indicator</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ver</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0.. MAX_SS_VERSION]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>SS version information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="2" Year="2003"/>
                <Author>LG</Author>
                <Comment>length by symbol</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the user-user information element is to convey information between the mobile station and the remote ISDN user.</Section>
                <Section>Reference : [1] section 10.5.4.25</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>user_user</Name>
                <Comment>User-user</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>pd</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>User-user protocol discriminator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>info</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..131]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>User-user information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the Allowed actions information element is to indicate whether CCBS is possible or not.</Section>
                <Section>Reference : [1] section 10.5.4.27</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>allowed_actions</Name>
                <Comment>Allowed Actions</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ccbs_act</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>ccbs_activation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000000</Pattern>
                    <BitLen>7</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the Recall Type information element is to describe the reason for the recall.</Section>
                <Section>Reference : [1] section 10.5.4.21a</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>recall_type</Name>
                <Comment>Recall Type</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00000</Pattern>
                    <BitLen>5</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>rcl_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>recall_type</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the Setup Container information element is to deliver the MO setup message to the mobile while performing a CCBS recall.</Section>
                <Section>Reference : [1] section 10.5.4.22b</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>setup_cont</Name>
                <Comment>Setup Container</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>setup_msg</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..L3MAX]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Setup message</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="3" Month="2" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the redirecting party BCD number information element is to identify the redirecting party of a call.</Section>
                <Section>Reference : [1] section 10.5.4.21b</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>redirecting_num</Name>
                <Comment>Redirecting party BCD number</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>ton</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Type of number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>npi</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>-</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Numbering plan identification</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>present</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Presentation indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>screen</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Screening indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>num</Name>
                </ItemLink>
                <Type>BCDEVEN</Type>
                <Control>
                    <TypeModifier>[0..32]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Number digits</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the Redirecting party subaddress is to identify a subaddress associated with the redirecting party of a call. For the definition of a subaddress see Rec. CCITT I.330.</Section>
                <Section>Reference : [1] section 10.5.4.21c</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>redirecting_subaddr</Name>
                <Comment>Redirection party subaddress</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>tos</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Type of subaddress</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>odd_even</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Odd / even Indication</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">cc</DocName>
                    <Name>subaddr</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..20]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Subaddress information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
    </MsgStructElementsSection>
    <MsgBasicElementsSection>
        <Description>
            <Section>This section contains all basic elements that are defined for the CC AIM</Section>
        </Description>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>access_ident</Name>
                <BitLen>2</BitLen>
                <Comment>Access identity</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_access_ident</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.6 (Call State)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>state</Name>
                <BitLen>6</BitLen>
                <Comment>Call state value</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_state</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="27" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Added states for CCBS</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.11 (Cause)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cause</Name>
                <BitLen>7</BitLen>
                <Comment>Cause value</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_cause</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="1" Month="2" Year="2002"/>
                <Author>SBK</Author>
                <Comment>Add Pre-emption cause (of R99)</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>code</Name>
                <BitLen>1</BitLen>
                <Comment>Coding standard</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_code</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.6 (Call state)</Section>
                <Section>[1] section 10.5.4.11 (Cause)</Section>
                <Section>[1] section 10.5.4.16 (High layer compatibility)</Section>
                <Section>[1] section 10.5.4.21 (Progress indicator)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cs</Name>
                <BitLen>2</BitLen>
                <Comment>Coding standard</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_cs</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>compress</Name>
                <BitLen>1</BitLen>
                <Comment>Compression</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_compress</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>config</Name>
                <BitLen>1</BitLen>
                <Comment>Configuration</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_config</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The purpose of the congestion level information element is to describe the congestion status of the call.</Section>
                <Section>Reference : [1] section 10.5.4.12</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>congest_lev</Name>
                <BitLen>4</BitLen>
                <Comment>Congestion level</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_congest_lev</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>conn_elem</Name>
                <BitLen>2</BitLen>
                <Comment>Connection element</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_conn_elem</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.11 (Cause)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>diag</Name>
                <BitLen>8</BitLen>
                <Comment>Diagnostics</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5a (Call Control Capabilities)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dtmf</Name>
                <BitLen>1</BitLen>
                <Comment>DTMF</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_dtmf</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>duplex</Name>
                <BitLen>1</BitLen>
                <Comment>Duplex mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_duplex</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>establish</Name>
                <BitLen>1</BitLen>
                <Comment>Establishment</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_establish</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ext_hlci</Name>
                <BitLen>7</BitLen>
                <Comment>Extended high layer characteristics identification</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.15 (Facility)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>fac</Name>
                <BitLen>8</BitLen>
                <Comment>Facility information</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.16 (High layer compatibility)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>hlci</Name>
                <BitLen>7</BitLen>
                <Comment>High layer characteristics identification</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.4 (Auxiliary states)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>hold</Name>
                <BitLen>2</BitLen>
                <Comment>Hold auxiliary state</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_hold</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>trans_cap</Name>
                <BitLen>3</BitLen>
                <Comment>Information transfer capability</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_trans_cap</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="9" Year="2000"/>
                <Author>LE</Author>
                <Comment>Auxiliary Speech added</Comment>
            </History>
            <History>
                <Date Day="10" Month="7" Year="2001"/>
                <Author>FK</Author>
                <Comment>Value of Auxiliary Speech corrected (4 -> 6)</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>intermed_rate</Name>
                <BitLen>2</BitLen>
                <Comment>Intermediate rate</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_intermed_rate</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="1" Year="1999"/>
                <Author>lE</Author>
                <Comment>constant value modified</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.16 (High layer compatibility)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>interpret</Name>
                <BitLen>3</BitLen>
                <Comment>Interpretation</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.17 (Keypad facility)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>key</Name>
                <BitLen>7</BitLen>
                <Comment>Keypad information</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>l1_ident</Name>
                <BitLen>2</BitLen>
                <Comment>Layer 1 identity</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_l1_ident</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>l2_ident</Name>
                <BitLen>2</BitLen>
                <Comment>Layer 2 identity</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_l2_ident</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.11 (Cause)</Section>
                <Section>[1] section 10.5.4.21 (Progress indicator)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>loc</Name>
                <BitLen>4</BitLen>
                <Comment>Location</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_loc</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The coding of the Low Layer Compatibility information is described in ETS 300 102-1.</Section>
                <Section>Reference: [1] section 10.5.4.18 (Low layer compatibility)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>llc</Name>
                <BitLen>8</BitLen>
                <Comment>Low layer information</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 10.4</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>msg_type</Name>
                <BitLen>8</BitLen>
                <Comment>Message Type</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>modem_type</Name>
                <BitLen>5</BitLen>
                <Comment>Modem type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_modem_type</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.4 (Auxiliary states)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>mpty</Name>
                <BitLen>2</BitLen>
                <Comment>Multi party auxiliary state</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_mpty</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>negotiate</Name>
                <BitLen>1</BitLen>
                <Comment>Negotiation</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_negotiate</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>nirr</Name>
                <BitLen>1</BitLen>
                <Comment>Negotiation of intermediate rate request</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_nirr</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>nic_rx</Name>
                <BitLen>1</BitLen>
                <Comment>Network independent clock on Rx</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_nic_rx</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>nic_tx</Name>
                <BitLen>1</BitLen>
                <Comment>Network independent clock on Tx</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_nic_tx</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.20 (Notification indicator)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>nd</Name>
                <BitLen>7</BitLen>
                <Comment>Notification description</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_nd</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.7 (Called party BCD number)</Section>
                <Section>[1] section 10.5.4.9 (Calling party BCD number)</Section>
                <Section>[1] section 10.5.4.13 (Connected number)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>num</Name>
                <BitLen>4</BitLen>
                <Comment>Number digit</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.7 (Called party BCD number)</Section>
                <Section>[1] section 10.5.4.9 (Calling party BCD number)</Section>
                <Section>[1] section 10.5.4.13 (Connected number)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>npi</Name>
                <BitLen>4</BitLen>
                <Comment>Numbering plan identification</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_npi</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>num_data</Name>
                <BitLen>1</BitLen>
                <Comment>Number of data bits</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_num_data</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>num_stop</Name>
                <BitLen>1</BitLen>
                <Comment>Number of stop bits</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_num_stop</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.8 (Call party subaddress)</Section>
                <Section>[1] section 10.5.4.10 (Calling party subaddress)</Section>
                <Section>[1] section 10.5.4.14 (Connected subaddress)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>odd_even</Name>
                <BitLen>1</BitLen>
                <Comment>Odd / even indication</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_odd_even</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>parity</Name>
                <BitLen>3</BitLen>
                <Comment>Parity</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_parity</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.9 (Calling party BCD number)</Section>
                <Section>[1] section 10.5.4.13 (Connected number)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>present</Name>
                <BitLen>2</BitLen>
                <Comment>Presentation indicator</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_present</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.16 (High layer compatibility)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>prot_prof</Name>
                <BitLen>2</BitLen>
                <Comment>Presentation method of protocol profile</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.21 (Progress indicator)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>progress_desc</Name>
                <BitLen>7</BitLen>
                <Comment>Progress description</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_progress_desc</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="2002"/>
                <Author>SBK</Author>
                <Comment>Issue 4967</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rad_chan_req</Name>
                <BitLen>2</BitLen>
                <Comment>Radio channel requirement</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_rad_chan_req</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rate_adapt</Name>
                <BitLen>2</BitLen>
                <Comment>Rate adaption</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_rate_adapt</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.11 (Cause)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rec</Name>
                <BitLen>7</BitLen>
                <Comment>Recommendation</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The purpose of the repeat indicator information element is to indicate how the associated repeated information elements shall be interpreted, when included in a message. The repeat indicator information element is included immediately before the first occurrence of the associated information element which will be repeated in a message. &quot;Mode 1&quot; refers to the first occurrence of that information element, &quot;mode 2&quot; refers to the second occurrence of that information element in the same message.</Section>
                <Section>Reference : [1] section 10.5.4.22</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>repeat</Name>
                <BitLen>4</BitLen>
                <Comment>Repeat indicator</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_repeat</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The purpose of the repeat indicator information element is to indicate how the associated repeated information elements shall be interpreted, when included in a message. The repeat indicator information element is included immediately before the first occurrence of the associated information element which will be repeated in a message. &quot;Mode 1&quot; refers to the first occurrence of that information element, &quot;mode 2&quot; refers to the second occurrence of that information element in the same message.</Section>
                <Section>Reference : [1] section 10.5.4.22</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>repeat_2</Name>
                <BitLen>4</BitLen>
                <Comment>Repeat indicator</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_repeat</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The purpose of the repeat indicator information element is to indicate how the associated repeated information elements shall be interpreted, when included in a message. The repeat indicator information element is included immediately before the first occurrence of the associated information element which will be repeated in a message. &quot;Mode 1&quot; refers to the first occurrence of that information element, &quot;mode 2&quot; refers to the second occurrence of that information element in the same message.</Section>
                <Section>Reference : [1] section 10.5.4.22</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>repeat_3</Name>
                <BitLen>4</BitLen>
                <Comment>Repeat indicator</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_repeat</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.9 (Calling party BCD number)</Section>
                <Section>[1] section 10.5.4.13 (Connected number)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>screen</Name>
                <BitLen>2</BitLen>
                <Comment>Screening indicator</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_screen</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The purpose of the signal information element is to allow the network to convey information to a user regarding tones and alerting signals</Section>
                <Section>Reference : [1] section 10.5.4.23</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>signal</Name>
                <BitLen>8</BitLen>
                <Comment>Signal</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_signal</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>sig_access_prot</Name>
                <BitLen>3</BitLen>
                <Comment>Signalling access protocol</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_sig_access_prot</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.24 (SS Version Indicator)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ver</Name>
                <BitLen>8</BitLen>
                <Comment>SS version information</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>structure</Name>
                <BitLen>2</BitLen>
                <Comment>Structure</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_structure</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>STRC_UNSTRUCTURED was assigned 1, now it is 3</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.8 (Called party subaddress)</Section>
                <Section>[1] section 10.5.4.10 (Calling party subaddress)</Section>
                <Section>[1] section 10.5.4.14 (Connected subaddress)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>subaddr</Name>
                <BitLen>8</BitLen>
                <Comment>Subaddress information</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>sync_async</Name>
                <BitLen>1</BitLen>
                <Comment>Synchronous / Asyncronous</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_sync_async</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>trans_mode</Name>
                <BitLen>1</BitLen>
                <Comment>Transfer mode</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_trans_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.7 (Called party BCD number)</Section>
                <Section>[1] section 10.5.4.9 (Calling party BCD number)</Section>
                <Section>[1] section 10.5.4.13 (Connected number)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ton</Name>
                <BitLen>3</BitLen>
                <Comment>Type of number</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_ton</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.8 (Called party subaddress)</Section>
                <Section>[1] section 10.5.4.10 (Calling party subaddress)</Section>
                <Section>[1] section 10.5.4.14 (Connected subaddress)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>tos</Name>
                <BitLen>3</BitLen>
                <Comment>Type of subaddress</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_tos</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>user_inf_l1_prot</Name>
                <BitLen>4</BitLen>
                <Comment>User information layer 1 protocol</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_user_inf_l1_prot</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>user_inf_l2_prot</Name>
                <BitLen>5</BitLen>
                <Comment>User information layer 2 protocol</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_user_inf_l2_prot</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5 (Bearer capability)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>user_rate</Name>
                <BitLen>4</BitLen>
                <Comment>User rate</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_user_rate</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.25 (User-user)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>info</Name>
                <BitLen>8</BitLen>
                <Comment>User-user information</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.25 (User-user)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pd</Name>
                <BitLen>8</BitLen>
                <Comment>User-user protocol discriminator</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_pd</Name>
            </ValuesLink>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: GSM 11.10 section 11.8.2.9.2 (Version 5.3.0)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>speech_vers1</Name>
                <BitLen>4</BitLen>
                <Comment>Speech Version Indication No. 1</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_speech_vers1</Name>
            </ValuesLink>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>Speech version 3 half/full (AMR) added.</Comment>
            </History>
            <History>
                <Date Day="18" Month="4" Year="2002"/>
                <Author>OT</Author>
                <Comment>Value for AHS from 3 to 5 changed.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: GSM 11.10 section 11.8.2.9.2 (Version 5.3.0)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>speech_vers2</Name>
                <BitLen>4</BitLen>
                <Comment>Speech Version Indication No. 2</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_speech_vers1</Name>
            </ValuesLink>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>Speech version 3 half/full (AMR) added.</Comment>
            </History>
            <History>
                <Date Day="18" Month="4" Year="2002"/>
                <Author>OT</Author>
                <Comment>Value for AHS from 3 to 5 changed.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: GSM 11.10 section 11.8.2.9.2 (Version 5.3.0)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>speech_vers3</Name>
                <BitLen>4</BitLen>
                <Comment>Speech Version Indication No. 3</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_speech_vers1</Name>
            </ValuesLink>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>Speech version 3 half/full (AMR) added.</Comment>
            </History>
            <History>
                <Date Day="18" Month="4" Year="2002"/>
                <Author>OT</Author>
                <Comment>Value for AHS from 3 to 5 changed.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: GSM 11.10 section 11.8.2.9.2 (Version 5.3.0)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>speech_vers4</Name>
                <BitLen>4</BitLen>
                <Comment>Speech Version Indication No. 4</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_speech_vers1</Name>
            </ValuesLink>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>Speech version 3 half/full (AMR) added.</Comment>
            </History>
            <History>
                <Date Day="18" Month="4" Year="2002"/>
                <Author>OT</Author>
                <Comment>Value for AHS from 3 to 5 changed.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: GSM 11.10 section 11.8.2.9.2 (Version 5.3.0)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>speech_vers5</Name>
                <BitLen>4</BitLen>
                <Comment>Speech Version Indication No. 5</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_speech_vers1</Name>
            </ValuesLink>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="11" Year="2001"/>
                <Author>OT</Author>
                <Comment>Speech version 3 half/full (AMR) added.</Comment>
            </History>
            <History>
                <Date Day="18" Month="4" Year="2002"/>
                <Author>OT</Author>
                <Comment>Value for AHS from 3 to 5 changed.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: GSM 4.08 section 10.5.4.5 (Version 6.3.0)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>modem_type_2</Name>
                <BitLen>2</BitLen>
                <Comment>Other Modem Type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_modem_type_2</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: GSM 4.08 section 10.5.4.5 (Version 6.3.0)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>fnur</Name>
                <BitLen>5</BitLen>
                <Comment>Fixed Network User Rate</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_fnur</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: GSM 4.08 section 10.5.4.5 (Version 6.3.0)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>acc</Name>
                <BitLen>4</BitLen>
                <Comment>Acceptable Channel Codings</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_acc</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: GSM 4.08 section 10.5.4.5 (Version 6.3.0)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>mTch</Name>
                <BitLen>3</BitLen>
                <Comment>Maximum Traffic Channels</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_mTch</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: GSM 4.08 section 10.5.4.5 (Version 6.3.0)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>uimi</Name>
                <BitLen>3</BitLen>
                <Comment>User Initiated Modification Ind</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_uimi</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: GSM 4.08 section 10.5.4.5 (Version 6.3.0)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>waiur</Name>
                <BitLen>4</BitLen>
                <Comment>Wanted Air Interface User Rate</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_waiur</Name>
            </ValuesLink>
            <History>
                <Date Day="13" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.27 (Allowed Actions)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ccbs_act</Name>
                <BitLen>1</BitLen>
                <Comment>ccbs_activation</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_ccbs_act</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.5a (CC Capabilities)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pcp</Name>
                <BitLen>1</BitLen>
                <Comment>PCP</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_pcp</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.21a (Recall Type)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>rcl_type</Name>
                <BitLen>3</BitLen>
                <Comment>Recall Type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_rcl_type</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference: [1] section 10.5.4.22b (Setup Container)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>setup_msg</Name>
                <BitLen>8</BitLen>
                <Comment>Setup message</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="18" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This element indicates whether octet 3a, 3b, ... is used for giving the speech codecs supported by the MS.</Section>
                <Section>Reference: [1] section 10.5.4.5 (Bearer Capabilities)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>coding_bc3x1</Name>
                <BitLen>1</BitLen>
                <Comment>Meaning of BC octet 3a</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_coding_bc3x1</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="11" Year="2002"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This element indicates whether octet 3a, 3b, ... is used for giving the speech codecs supported by the MS.</Section>
                <Section>Reference: [1] section 10.5.4.5 (Bearer Capabilities)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>coding_bc3x2</Name>
                <BitLen>1</BitLen>
                <Comment>Meaning of BC octet 3b</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_coding_bc3x1</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="11" Year="2002"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This element indicates whether octet 3a, 3b, ... is used for giving the speech codecs supported by the MS.</Section>
                <Section>Reference: [1] section 10.5.4.5 (Bearer Capabilities)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>coding_bc3x3</Name>
                <BitLen>1</BitLen>
                <Comment>Meaning of BC octet 3c</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_coding_bc3x1</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="11" Year="2002"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This element indicates whether octet 3a, 3b, ... is used for giving the speech codecs supported by the MS.</Section>
                <Section>Reference: [1] section 10.5.4.5 (Bearer Capabilities)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>coding_bc3x4</Name>
                <BitLen>1</BitLen>
                <Comment>Meaning of BC octet 3d</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_coding_bc3x1</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="11" Year="2002"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This element indicates whether octet 3a, 3b, ... is used for giving the speech codecs supported by the MS.</Section>
                <Section>Reference: [1] section 10.5.4.5 (Bearer Capabilities)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>coding_bc3x5</Name>
                <BitLen>1</BitLen>
                <Comment>Meaning of BC octet 3e</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_coding_bc3x1</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="11" Year="2002"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This element indicates whether the mobile supports CTM text telephony.</Section>
                <Section>Reference: [1] section 10.5.4.5 (Bearer Capabilities)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ctm</Name>
                <BitLen>1</BitLen>
                <Comment>Support of CTM text telephony</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">cc</DocName>
                <Name>VAL_ctm</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="11" Year="2002"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
    </MsgBasicElementsSection>
    <ValuesSection>
        <Description>
            <Section>This section contains all sets of values that are defined for the CC AIM</Section>
        </Description>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_access_ident</Name>
                <Comment>values for access_ident</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>AI_OCT_ID</Alias>
                <Comment>octet identifier</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_state</Name>
                <Comment>values for state</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CS_0</Alias>
                <Comment>null</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CS_01</Alias>
                <Comment>MM connection pending</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">35</Value>
                <Alias>CS_03</Alias>
                <Comment>Wait for network information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">37</Value>
                <Alias>CS_05</Alias>
                <Comment>CC-Establishment confirmed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">38</Value>
                <Alias>CS_06</Alias>
                <Comment>Recall present</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CS_1</Alias>
                <Comment>call initiated</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CS_3</Alias>
                <Comment>mobile originating call proceeding</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CS_4</Alias>
                <Comment>call delivered</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>CS_6</Alias>
                <Comment>call present</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>CS_7</Alias>
                <Comment>call received</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>CS_8</Alias>
                <Comment>connect request</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>CS_9</Alias>
                <Comment>mobile terminating call confirmed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>CS_10</Alias>
                <Comment>active</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>CS_11</Alias>
                <Comment>disconnect request</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>CS_12</Alias>
                <Comment>disconnect indication</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">19</Value>
                <Alias>CS_19</Alias>
                <Comment>release request</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">26</Value>
                <Alias>CS_26</Alias>
                <Comment>mobile originating modify</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">27</Value>
                <Alias>CS_27</Alias>
                <Comment>mobile terminating modify</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">28</Value>
                <Alias>CS_28</Alias>
                <Comment>connect indication</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_cause</Name>
                <Comment>values for cause</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CAUSE_UNASSIGN</Alias>
                <Comment>Unassigned (unallocated) Note 9 number</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CAUSE_NO_ROUTE</Alias>
                <Comment>No route to destination</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>CAUSE_CHAN_UNACCEPT</Alias>
                <Comment>Channel unacceptable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>CAUSE_BARRED</Alias>
                <Comment>Operator determined barring</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">16</Value>
                <Alias>CAUSE_CALL_CLEAR</Alias>
                <Comment>Normal call clearing</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">17</Value>
                <Alias>CAUSE_USER_BUSY</Alias>
                <Comment>User busy</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">18</Value>
                <Alias>CAUSE_NO_RESPONSE</Alias>
                <Comment>No user responding</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">19</Value>
                <Alias>CAUSE_ALERT_NO_ANSWER</Alias>
                <Comment>User alerting, no answer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">21</Value>
                <Alias>CAUSE_CALL_REJECT</Alias>
                <Comment>Call rejected</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">22</Value>
                <Alias>CAUSE_NUM_CHANGED</Alias>
                <Comment>Number changed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">25</Value>
                <Alias>CAUSE_PREEMPTION</Alias>
                <Comment>Pre-emption</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">26</Value>
                <Alias>CAUSE_USER_CLEAR</Alias>
                <Comment>Non selected user clearing</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">27</Value>
                <Alias>CAUSE_DEST_ORDER</Alias>
                <Comment>Destination out of order</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">28</Value>
                <Alias>CAUSE_NUM_FORMAT</Alias>
                <Comment>Invalid number format (incomplete number)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">29</Value>
                <Alias>CAUSE_FACILITY_REJECT</Alias>
                <Comment>Facility rejected</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">30</Value>
                <Alias>CAUSE_STATUS_ENQUIRY</Alias>
                <Comment>Response to STATUS ENQUIRY</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">31</Value>
                <Alias>CAUSE_UNSPECIFIED</Alias>
                <Comment>Normal, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">34</Value>
                <Alias>CAUSE_NO_CHAN_AVAIL</Alias>
                <Comment>No circuit/channel available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">38</Value>
                <Alias>CAUSE_NETWORK_ORDER</Alias>
                <Comment>Network out of order</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">41</Value>
                <Alias>CAUSE_TEMP_FAIL</Alias>
                <Comment>Temporary failure</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">42</Value>
                <Alias>CAUSE_SWITCH_CONGEST</Alias>
                <Comment>Switching equipment congestion</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">43</Value>
                <Alias>CAUSE_INFO_DISCARD</Alias>
                <Comment>Access information discarded</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">44</Value>
                <Alias>CAUSE_REQ_CHAN_UNAVAIL</Alias>
                <Comment>requested circuit/channel not available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">47</Value>
                <Alias>CAUSE_RESOURCE_UNAVAIL</Alias>
                <Comment>Resources unavailable, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">49</Value>
                <Alias>CAUSE_QOS_UNAVAIL</Alias>
                <Comment>Quality of service unavailable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">50</Value>
                <Alias>CAUSE_FACILITY_UNSUBSCRIB</Alias>
                <Comment>Requested facility not subscribed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">55</Value>
                <Alias>CAUSE_BARRED_IN_CUG</Alias>
                <Comment>Incoming calls barred within the CUG</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">57</Value>
                <Alias>CAUSE_BEARER_CAP_AUTHORIZ</Alias>
                <Comment>Bearer capability not authorized</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">58</Value>
                <Alias>CAUSE_BEARER_CAP_UNAVAIL</Alias>
                <Comment>Bearer capability not presently available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">63</Value>
                <Alias>CAUSE_SERVICE_UNAVAIL</Alias>
                <Comment>Service or option not available, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">65</Value>
                <Alias>CAUSE_BEARER_NOT_IMPLEM</Alias>
                <Comment>Bearer service not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">68</Value>
                <Alias>CAUSE_ACM_MAX</Alias>
                <Comment>ACM equal to or greater than ACMmax</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">69</Value>
                <Alias>CAUSE_FACILITY_NOT_IMPLEM</Alias>
                <Comment>Requested facility not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">70</Value>
                <Alias>CAUSE_RESTICT_BEARER_CAP</Alias>
                <Comment>Only restricted digital information bearer capability is available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">79</Value>
                <Alias>CAUSE_SERVICE_NOT_IMPLEM</Alias>
                <Comment>Service or option not implemented, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">81</Value>
                <Alias>CAUSE_INVALID_TI</Alias>
                <Comment>Invalid transaction identifier value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">87</Value>
                <Alias>CAUSE_USER_NOT_IN_CUG</Alias>
                <Comment>User not member of CUG</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">88</Value>
                <Alias>CAUSE_INCOMPAT_DEST</Alias>
                <Comment>Incompatible destination</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">91</Value>
                <Alias>CAUSE_INVALID_TRANS_NET</Alias>
                <Comment>Invalid transit network selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">95</Value>
                <Alias>CAUSE_INCORRECT_MESSAGE</Alias>
                <Comment>Semantically incorrect message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">96</Value>
                <Alias>CAUSE_INVALID_MAND_INFO</Alias>
                <Comment>Invalid mandatory information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">97</Value>
                <Alias>CAUSE_MESSAGE_TYPE_NOT_IMPLEM</Alias>
                <Comment>Message type non-existent or not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">98</Value>
                <Alias>CAUSE_MESSAGE_TYPE_INCOMPAT</Alias>
                <Comment>Message type not compatible with protocol state</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">99</Value>
                <Alias>CAUSE_INFO_ELEM_NOT_IMPLEM</Alias>
                <Comment>Information element nonistent or not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">100</Value>
                <Alias>CAUSE_COND_INFO_ELEM</Alias>
                <Comment>Conditional IE error</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">101</Value>
                <Alias>CAUSE_MESSAGE_INCOMPAT</Alias>
                <Comment>Message not compatible with protocol state</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">102</Value>
                <Alias>CAUSE_TIMER</Alias>
                <Comment>Recovery on timer expiry</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">111</Value>
                <Alias>CAUSE_PROTOCOL</Alias>
                <Comment>Protocol error, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">127</Value>
                <Alias>CAUSE_INTERWORKING</Alias>
                <Comment>Interworking, unspecified</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>31</MaxValue>
                <Comment>Normal, unspecified</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>32</MinValue>
                <MaxValue>47</MaxValue>
                <Comment>Resources unavailable, unspecified</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>48</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>Service or option not available, unspecified</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>64</MinValue>
                <MaxValue>79</MaxValue>
                <Comment>Service or option not implemented, unspecified</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>80</MinValue>
                <MaxValue>95</MaxValue>
                <Comment>Semantically incorrect message</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>96</MinValue>
                <MaxValue>111</MaxValue>
                <Comment>Protocol error, unspecified</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>112</MinValue>
                <MaxValue>127</MaxValue>
                <Comment>Interworking, unspecified</Comment>
            </ValuesRange>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_code</Name>
                <Comment>values for code</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CSTD_GSM</Alias>
                <Comment>GSM standardized coding</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_cs</Name>
                <Comment>values for cs</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CS_Q931</Alias>
                <Comment>standardized coding as described in CCITT Rec. Q.931</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CS_INTERNATIONAL</Alias>
                <Comment>reserved for other international standards</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CS_NATIONAL</Alias>
                <Comment>national standard</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CS_GSM_PLMN</Alias>
                <Comment>standard defined for the GSM PLMNS as described in 10.86/GSM 04.08</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_compress</Name>
                <Comment>values for compress</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>COMP_NO</Alias>
                <Comment>data compression not possible</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>COMP_YES</Alias>
                <Comment>data compression possible</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_config</Name>
                <Comment>values for config</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CONF_POINT_TO_POINT</Alias>
                <Comment>point-to-point</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_congest_lev</Name>
                <Comment>values for congest_lev</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CL_RECEIVER_READY</Alias>
                <Comment>receiver ready</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>CL_RECEIVER_NOT_READY</Alias>
                <Comment>receiver not ready</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_conn_elem</Name>
                <Comment>values for conn_elem</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CE_TRANSPA</Alias>
                <Comment>transparent</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CE_RLP</Alias>
                <Comment>non transparent (RLP)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CE_TRANSPA_PREF</Alias>
                <Comment>both, transparent preferred</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CE_RLP_PREF</Alias>
                <Comment>both, non transparent preferred</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_dtmf</Name>
                <Comment>values for dtmf</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DTMF_EARLY</Alias>
                <Comment>Reserved for earlier versions of the protocol.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DTMF_CURRENT</Alias>
                <Comment>The mobile station supports DTMF as specified in section 5.5.7 of GSM 4.08.</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_duplex</Name>
                <Comment>values for duplex</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DUPLEX_HALF</Alias>
                <Comment>half duplex</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DUPLEX_FULL</Alias>
                <Comment>full duplex</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_establish</Name>
                <Comment>values for establish</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ESTAB_DEMAND</Alias>
                <Comment>demand</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_hold</Name>
                <Comment>values for hold</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>HLD_IDLE</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>HLD_HOLD_REQ</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>HLD_CALL_HELD</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>HLD_RETRIEVE_REQ</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_trans_cap</Name>
                <Comment>values for trans_cap</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ITC_SPEECH</Alias>
                <Comment>speech</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ITC_DIGITAL_UNRESTRICTED</Alias>
                <Comment>unrestricted digital information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>ITC_AUDIO</Alias>
                <Comment>audio 3.1 kHz, ex PLMN</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>ITC_FAX_GROUP_3</Alias>
                <Comment>fascimile group 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>ITC_AUXILIARY_SPEECH</Alias>
                <Comment>Auxiliary speech</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>ITC_NETWORK_RESERVED</Alias>
                <Comment>reserved, to be used in the network.</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_intermed_rate</Name>
                <Comment>values for intermed_rate</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>IR_8_KBIT</Alias>
                <Comment>8 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>IR_16_KBIT</Alias>
                <Comment>16 kbit/s</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_l1_ident</Name>
                <Comment>values for l1_ident</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>L1_OCT_ID</Alias>
                <Comment>octet identifier</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_l2_ident</Name>
                <Comment>values for l2_ident</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>L2_OCT_ID</Alias>
                <Comment>octet identifier</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_loc</Name>
                <Comment>values for loc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>LOC_USER</Alias>
                <Comment>user</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>LOC_PRIV_NET_LOCAL_USER</Alias>
                <Comment>private network serving the local user</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>LOC_PUB_NET_LOCAL_USER</Alias>
                <Comment>public network serving the local user</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>LOC_TRANSIT_NET</Alias>
                <Comment>transit network</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>LOC_PUB_NET_REMOTE_USER</Alias>
                <Comment>public network serving the remote user</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>LOC_PRIV_NET_REMOTE_USER</Alias>
                <Comment>private network serving the remote user</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>LOC_INTERNATIONAL_NET</Alias>
                <Comment>international network</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>LOC_BEYOND_POINT</Alias>
                <Comment>network beyond interworking point</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_modem_type</Name>
                <Comment>values for modem_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MT_NONE</Alias>
                <Comment>none</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MT_V21</Alias>
                <Comment>V.21</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MT_V22</Alias>
                <Comment>V.22</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MT_V22BIS</Alias>
                <Comment>V.22 bis</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>MT_V23</Alias>
                <Comment>V.23</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>MT_V26TER</Alias>
                <Comment>V.26 ter</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>MT_V32</Alias>
                <Comment>V.32</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>MT_UNDEF</Alias>
                <Comment>modem for undefined interface</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>MT_AUTO</Alias>
                <Comment>autobauding type 1</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_mpty</Name>
                <Comment>values for mpty</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MPTY_IDLE</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MPTY_REQ</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MPTY_CALL</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MPTY_SPLIT</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_negotiate</Name>
                <Comment>values for negotiate</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NEGOTIATE_NO</Alias>
                <Comment>in-band negotiation not possible</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_nirr</Name>
                <Comment>values for nirr</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NIRR_NO_MEANING</Alias>
                <Comment>No meaning is associated with this value.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NIRR_DATA</Alias>
                <Comment>Data up to and including 4.8 kb/s, full rate, non-transparent, 6 kb/s radio interface rate is requested.</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_nic_rx</Name>
                <Comment>values for nic_rx</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NIC_RX_NO</Alias>
                <Comment>cannot accept data with network independent clock (i.e. sender does not support this optional procedure)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NIC_RX_YES</Alias>
                <Comment>can accept data with network independent clock (i.e. sender does support this optional procedure)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_nic_tx</Name>
                <Comment>values for nic_tx</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NIC_TX_NO</Alias>
                <Comment>does not require to send data with network independent clock</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NIC_TX_YES</Alias>
                <Comment>requires to send data with network independent clock</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_nd</Name>
                <Comment>values for nd</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ND_USER_SUSPEND</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ND_USED_RESUME</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>ND_BEARER_CHANGE</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_npi</Name>
                <Comment>values for npi</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NPI_UNKNOWN</Alias>
                <Comment>unknown</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NPI_ISDN</Alias>
                <Comment>ISDN/telephony numbering plan (Rec. E.164/E.163)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>NPI_X121</Alias>
                <Comment>data numbering plan (Recommendation X.121)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>NPI_F69</Alias>
                <Comment>telex numbering plan (Recommendation F.69)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>NPI_NATIONAL</Alias>
                <Comment>national numbering plan</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>NPI_PRIVATE</Alias>
                <Comment>private numbering plan</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>NPI_EXTENSTION</Alias>
                <Comment>reserved for extension</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_num_data</Name>
                <Comment>values for num_data</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NDATA_7</Alias>
                <Comment>7 bits</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NDATA_8</Alias>
                <Comment>8 bits (this value is also used in the case of bit oriented protocols)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_num_stop</Name>
                <Comment>values for num_stop</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NSTOP_1</Alias>
                <Comment>1 bit (This value is also used in the case of synchronous mode)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NSTOP_2</Alias>
                <Comment>2 bits</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_odd_even</Name>
                <Comment>values for odd_even</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>OE_EVEN</Alias>
                <Comment>even number of address signals</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>OE_ODD</Alias>
                <Comment>odd number of address signals</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_parity</Name>
                <Comment>values for parity</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PARITY_ODD</Alias>
                <Comment>odd</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PARITY_EVEN</Alias>
                <Comment>even</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>PARITY_NONE</Alias>
                <Comment>none</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>PARITY_0</Alias>
                <Comment>forced to 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>PARITY_1</Alias>
                <Comment>forced to 1</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_present</Name>
                <Comment>values for present</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PRES_ALLOWED</Alias>
                <Comment>Presentation allowed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PRES_RESTRICTED</Alias>
                <Comment>Presentation restricted</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PRES_NOT_AVAIL</Alias>
                <Comment>Number not available due to interworking</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_progress_desc</Name>
                <Comment>values for progress_desc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PROG_NO_END_TO_END_PLMN</Alias>
                <Comment>Call is not end-to-end PLMN/ISDN, further call progress information may be available in-band</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PROG_DEST_NON_PLMN</Alias>
                <Comment>Destination address in non-PLMN/ISDN</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>PROG_ORIGIN_NON_PLMN</Alias>
                <Comment>Origination address in non-PLMN/ISDN</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>PROG_RETURN_TO_PLMN</Alias>
                <Comment>Call has returned to the PLMN/ISDN</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>PROG_INBAND_AVAIL</Alias>
                <Comment>In-band information or appropriate pattern now available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">32</Value>
                <Alias>PROG_END_TO_END_PLMN</Alias>
                <Comment>Call is end-to-end PLMN/ISDN</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">64</Value>
                <Alias>PROG_QUEUEING</Alias>
                <Comment>Queueing</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Unspecific</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_rad_chan_req</Name>
                <Comment>values for rad_chan_req</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>RCR_FULL_ONLY</Alias>
                <Comment>full rate support only mobile station</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>RCR_HALF_PREF</Alias>
                <Comment>dual rate support mobile station/half rate preferred</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>RCR_FULL_PREF</Alias>
                <Comment>dual rate support mobile station/full rate preferred</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_rate_adapt</Name>
                <Comment>values for rate_adapt</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>RA_NONE</Alias>
                <Comment>no rate adaption</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>RA_V110</Alias>
                <Comment>V.110/X.30 rate adaption</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>RA_X31</Alias>
                <Comment>CCITT X.31 flag stuffing</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_repeat</Name>
                <Comment>values for repeat</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>REPEAT_CIRCULAR</Alias>
                <Comment>Circular for successive selection 'mode 1 alternate mode 2'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>REPEAT_SEQUENTIAL</Alias>
                <Comment>Sequential for successive selection 'mode 1 and then mode 2'</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_screen</Name>
                <Comment>values for screen</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SCR_USER_UNSCREENED</Alias>
                <Comment>User-provided, not screened</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SCR_USER_PASSED</Alias>
                <Comment>User-provided, verified and passed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SCR_USER_FAILED</Alias>
                <Comment>User-provided, verified and failed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SCR_NETWORD</Alias>
                <Comment>Network provided</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_signal</Name>
                <Comment>values for signal</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SIGNAL_DIAL_ON</Alias>
                <Comment>dial tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SIGNAL_BACK_ON</Alias>
                <Comment>ring back tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SIGNAL_INTERCEPT_ON</Alias>
                <Comment>intercept tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SIGNAL_CONGEST_ON</Alias>
                <Comment>network congestion tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SIGNAL_BUSY_ON</Alias>
                <Comment>busy tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SIGNAL_CONFIRM_ON</Alias>
                <Comment>confirm tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>SIGNAL_ANSWER_ON</Alias>
                <Comment>answer tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>SIGNAL_WAITING_ON</Alias>
                <Comment>call waiting tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>SIGNAL_HOOK_OFF_ON</Alias>
                <Comment>off-hook warning tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">63</Value>
                <Alias>SIGNAL_TONES_OFF</Alias>
                <Comment>tones off</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">79</Value>
                <Alias>SIGNAL_ALERT_OFF</Alias>
                <Comment>alerting off</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_sig_access_prot</Name>
                <Comment>values for sig_access_prot</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SIAP_I440</Alias>
                <Comment>I.440/450</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SIAP_X21</Alias>
                <Comment>X.21</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SIAP_X28_INDIV_NUI</Alias>
                <Comment>X.28 - dedicated PAD, individual NUI</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SIAP_X28_UNIV_NUI</Alias>
                <Comment>X.28 - dedicated PAD, universal NUI</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SIAP_X28_NON_DEDIC</Alias>
                <Comment>X.28 - non dedicated PAD</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>SIAP_X32</Alias>
                <Comment>X.32</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_structure</Name>
                <Comment>values for structure</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>STRC_SERV_DATA_INTEG</Alias>
                <Comment>service data unit integrity</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>STRC_UNSTRUCTURED</Alias>
                <Comment>unstructured</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_sync_async</Name>
                <Comment>values for sync_async</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SYNCHRONOUS</Alias>
                <Comment>synchronous</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ASYNCHRONOUS</Alias>
                <Comment>asynchronous</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_trans_mode</Name>
                <Comment>values for trans_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TM_CIRCUIT</Alias>
                <Comment>circuit mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>TM_PACKET</Alias>
                <Comment>packet mode</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ton</Name>
                <Comment>values for ton</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TON_UNKNOWN</Alias>
                <Comment>unknown</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>TON_INTERNATIONAL</Alias>
                <Comment>international number</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>TON_NATIONAL</Alias>
                <Comment>national number</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>TON_NETWORK</Alias>
                <Comment>network specific number</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>TON_DEDICATED</Alias>
                <Comment>dedicated access, short code</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>TON_EXTENSION</Alias>
                <Comment>reserved for extention</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tos</Name>
                <Comment>values for tos</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TOS_NSAP</Alias>
                <Comment>NSAP (X.213/ISO 8348 AD2)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>TOS_USER</Alias>
                <Comment>User specified</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_user_inf_l1_prot</Name>
                <Comment>values for user_inf_l1_prot</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>L1_DEFAULT</Alias>
                <Comment>default layer 1 protocol</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_user_inf_l2_prot</Name>
                <Comment>values for user_inf_l2_prot</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>L2_X25</Alias>
                <Comment>recommendation X.25, link level</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>L2_ISO6429</Alias>
                <Comment>ISO 6429, codeset 0 (DC1/DC3)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>L2_X75</Alias>
                <Comment>X.75 layer 2 modified (teletex)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>L2_VIDEOTEX</Alias>
                <Comment>videotex profile 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>L2_COPFC</Alias>
                <Comment>COPnoFlCt (Character oriented Protocol with no Flow Control mechanism)</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_user_rate</Name>
                <Comment>values for user_rate</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>UR_0_3_KBIT</Alias>
                <Comment>rate : 0.3 kbit/s Recommendation X.1 and V.110</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>UR_1_2_KBIT</Alias>
                <Comment>rate : 1.2 kbit/s Recommendation X.1 and V.110</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>UR_2_4_KBIT</Alias>
                <Comment>rate : 2.4 kbit/s Recommendation X.1 and V.110</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>UR_4_8_KBIT</Alias>
                <Comment>rate : 4.8 kbit/s Recommendation X.1 and V.110</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>UR_9_6_KBIT</Alias>
                <Comment>rate : 9.6 kbit/s Recommendation X.1 and V.110</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>UR_12_0_KBIT_TRANS</Alias>
                <Comment>rate : 12.0 kbit/s transparent</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>UR_1_2_KBIT_V23</Alias>
                <Comment>rate : 1.2 kbit/s/75 bit/s Recommendation V.23, X.1,V.110.</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pd</Name>
                <Comment>values for pd</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PD_USER</Alias>
                <Comment>User specific protocol</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PD_HIGH_LAYER</Alias>
                <Comment>OSI high layer protocols</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PD_X244</Alias>
                <Comment>X.244</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>PD_SYS_MANAGE</Alias>
                <Comment>Reserved for system management convergence function</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>PD_IA5</Alias>
                <Comment>IA5 characters</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>PD_V120</Alias>
                <Comment>Rec.V.120 rate adaption</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>PD_Q931</Alias>
                <Comment>Q.931 (I.451) user-network call control messages</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>16</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>Reserved for other network layer or through layer 3 protocols including Rec.X.25</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>64</MinValue>
                <MaxValue>79</MaxValue>
                <Comment>National use</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>80</MinValue>
                <MaxValue>254</MaxValue>
                <Comment>Reserved for other network through layer or layer 3 protocols including Rec.X.25</Comment>
            </ValuesRange>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_speech_vers1</Name>
                <Comment>values for speech_vers1</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SPEECH_VERS_FR</Alias>
                <Comment>full rate speech version 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SPEECH_VERS_HR</Alias>
                <Comment>half rate speech version 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SPEECH_VERS_EFR</Alias>
                <Comment>full rate speech version 2 (enhanced full rate)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SPEECH_VERS_AMR_HR</Alias>
                <Comment>half rate speech version 3 (AHS)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SPEECH_VERS_AMR_FR</Alias>
                <Comment>full rate speech version 3 (AFS)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">F</Value>
                <Alias>SPEECH_VERS_NONE</Alias>
                <Comment>no speech version given</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_modem_type_2</Name>
                <Comment>values for modem_type_2</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>OTHER_MODEM_TYPE_NONE</Alias>
                <Comment>No other modem type specified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>OTHER_MODEM_TYPE_V32BIS</Alias>
                <Comment>V.32bis</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>OTHER_MODEM_TYPE_V34</Alias>
                <Comment>V.34</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_fnur</Name>
                <Comment>values for fnur</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>FNUR_NOT_APPLICABLE</Alias>
                <Comment>Fixed network user rate not applicable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>FNUR_9600</Alias>
                <Comment>FNUR 9.6 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>FNUR_14400</Alias>
                <Comment>FNUR 14.4 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>FNUR_19200</Alias>
                <Comment>FNUR 19.2 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>FNUR_28800</Alias>
                <Comment>FNUR 28.8 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>FNUR_38400</Alias>
                <Comment>FNUR 38.4 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>FNUR_48000</Alias>
                <Comment>FNUR 48.0 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>FNUR_56000</Alias>
                <Comment>FNUR 56.0 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>FNUR_64000</Alias>
                <Comment>FNUR 64.0 kbit/s</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_acc</Name>
                <Comment>values for acc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ACC_EMPTY</Alias>
                <Comment>No channel codings acceptable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ACC_48</Alias>
                <Comment>TCH 4.8 acceptable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>ACC_96</Alias>
                <Comment>TCH 9.6 acceptable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>ACC_48_96</Alias>
                <Comment>TCH 4.8/9.6 acceptable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>ACC_144</Alias>
                <Comment>TCH 14.4 acceptable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>ACC_48_144</Alias>
                <Comment>TCH 4.8/14.4 acceptable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>ACC_96_144</Alias>
                <Comment>TCH 9.6/14.4 acceptable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>ACC_ALL</Alias>
                <Comment>All channel codings acceptable</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_mTch</Name>
                <Comment>values for mTch</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MAX_TCH_1</Alias>
                <Comment>Maximum of 1 TCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MAX_TCH_2</Alias>
                <Comment>Maximum of 2 TCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MAX_TCH_3</Alias>
                <Comment>Maximum of 3 TCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MAX_TCH_4</Alias>
                <Comment>Maximum of 4 TCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>MAX_TCH_5</Alias>
                <Comment>Maximum of 5 TCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>MAX_TCH_6</Alias>
                <Comment>Maximum of 6 TCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>MAX_TCH_7</Alias>
                <Comment>Maximum of 7 TCH</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>MAX_TCH_8</Alias>
                <Comment>Maximum of 8 TCH</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_uimi</Name>
                <Comment>values for uimi</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>UIMI_NOT_ALLOWED</Alias>
                <Comment>User initiated modification not allowed/required</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>UIMI_MAX_1_TCH</Alias>
                <Comment>User initiated modification up to 1 TCH/F</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>UIMI_MAX_2_TCH</Alias>
                <Comment>User initiated modification up to 2 TCH/F</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>UIMI_MAX_3_TCH</Alias>
                <Comment>User initiated modification up to 3 TCH/F</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>UIMI_MAX_4_TCH</Alias>
                <Comment>User initiated modification up to 4 TCH/F</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_waiur</Name>
                <Comment>values for waiur</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>WAIUR_NOT_APPLICABLE</Alias>
                <Comment>Wanted Air Interface user rate not applicable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>WAIUR_9600</Alias>
                <Comment>WAIUR 9.6 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>WAIUR_14400</Alias>
                <Comment>WAIUR 14.4 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>WAIUR_19200</Alias>
                <Comment>WAIUR 19.2 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>WAIUR_28800</Alias>
                <Comment>WAIUR 28.8 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>WAIUR_38400</Alias>
                <Comment>WAIUR 38.4 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>WAIUR_43200</Alias>
                <Comment>WAIUR 43.2 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>WAIUR_57600</Alias>
                <Comment>WAIUR 57.6 kbit/s</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ccbs_act</Name>
                <Comment>values for ccbs_act</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CCBS_NO</Alias>
                <Comment>CCBS is not possible</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CCBS_YES</Alias>
                <Comment>CCBS is possible</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pcp</Name>
                <Comment>values for pcp</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PCP_NO</Alias>
                <Comment>Mobile does not support prolonged clearing procedure</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PCP_YES</Alias>
                <Comment>Mobile supports prolonged clearing procedure</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_rcl_type</Name>
                <Comment>values for rcl_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CCBS</Alias>
                <Comment>CCBS</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CCBS_1</Alias>
                <Comment>Shall be treated as CCBS (intended for other similar types of Recall)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CCBS_2</Alias>
                <Comment>Shall be treated as CCBS (intended for other similar types of Recall)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CCBS_3</Alias>
                <Comment>Shall be treated as CCBS (intended for other similar types of Recall)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>CCBS_4</Alias>
                <Comment>Shall be treated as CCBS (intended for other similar types of Recall)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>CCBS_5</Alias>
                <Comment>Shall be treated as CCBS (intended for other similar types of Recall)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>CCBS_6</Alias>
                <Comment>Shall be treated as CCBS (intended for other similar types of Recall)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_coding_bc3x1</Name>
                <Comment>values for coding_bc3x1</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CODING_BC3X_SPEECH</Alias>
                <Comment>Octet 3x of IE Bearer Capabilities indicates speech codec version</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CODING_BC3X_OTHER</Alias>
                <Comment>Octet 3x of IE Bearer Capabilities used for other extension of octet 3</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ctm</Name>
                <Comment>values for ctm</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CTM_NO</Alias>
                <Comment>Mobile does not support prolonged clearing procedure</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CTM_YES</Alias>
                <Comment>Mobile supports prolonged clearing procedure</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
    </ValuesSection>
</AIM>
