<?xml version="1.0" encoding="UTF-8"?>
<!-- edited with SAPE SAP Editor -->
<AIM xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="aim.xsd">
    <DocInfoSection>
        <DocName DocType="AIM">sm</DocName>
        <DocNum Number="605" Project="8441"/>
        <Description>
            <Section>The Protocol Stacks are used to define the functionality of the GSM protocols for interfaces. The GSM specifications are normative when used to describe the functionality of interfaces, but the stacks and the subdivision of protocol layers does not imply or restrict any implementation.</Section>
            <Section>The protocol stack for fax and data transmission consists of several entities. Each entity has one ore more service access points, over which the entity provides a service for the upper entity. The entity, which is described in this document, is coloured grey in the following figure :</Section>
            <Section>Figure 1-1: Architecture of the GSM/GPRS protocol stack</Section>
            <Section>The information units passed via the SAPs are called primitives and consists of an operation code and several parameters. See the Users Guide for details.</Section>
            <Section>The entities of the GPRS protocol stack are:</Section>
            <Section>1.1 GRR (RLC/MAC) - Radio Link Control/Medium Access Control</Section>
            <Section>This layer contains two functions: The Radio Link Control function provides a radio-solution-dependent reliable link. The Medium Access Control function controls the access signalling (request and grant) procedures for the radio channel, and the mapping of LLC frames onto the GSM physical channel.</Section>
            <Section>1.2 LLC - Logical Link Control</Section>
            <Section>The LLC entity provides multiple highly reliable logical links for asynchronous data transfer between the MS and the network. It supports variable-length information frames, acknowledged and unacknowledged data transfer, flow and sequence control, error detection and recovery, notification of unrecoverable errors, user identity confidentiality, and ciphering of user and signaling data.</Section>
            <Section>1.3 GMM - GPRS Mobility Management</Section>
            <Section>The GMM entity provides procedures for the mobility of the MS, such as informing the network of its present location, and user identity confidentiality. It manages the GMM context (attach, detach, routing area updating), supports security functions such as authentication of user and MS, controls ciphering of data, and initiates the response to paging messages.</Section>
            <Section>1.4 SM - Session Management</Section>
            <Section>The main function of the session management (SM) is to support PDP context handling of the user terminal. Session Management activates, modifies and deletes the contexts for packet data protocols (PDP). Session Management services are provided at the SMREG-SAP and the SNSM-SAP for anonymous and non-anonymous access. The non-anonymous and anonymous access procedures for PDP context activation and PDP context deactivation are available at the SMREG-SAP. In addition there exists a PDP context modification for non-anonymous PDP contexts.</Section>
            <Section>1.5 SNDCP - Subnetwork Dependant Convergence Protocol</Section>
            <Section>SNDCP carries out all functions related to transfer of Network layer Protocol Data Units (N-PDUs) over GPRS in a transparent way. SNDCP helps to improve channel efficiency by means of compression techniques. The set of protocol entities above SNDCP consists of commonly used network protocols. They all use the same SNDCP entity, which then performs multiplexing of data coming from different sources to be sent using the service provided by the LLC layer.</Section>
            <Section>1.6 GACI - GPRS Application Control Interface</Section>
            <Section>The GACI is the GPRS extension of the ACI. It is specified in GSM 07.07 and 07.60. It is responsible for processing of the GPRS related AT Commands to setup, activate and deactivate the PDP context parameter. It also provides functionality for the interworking between GMM/SM/SNDCP and a packet oriented protocol like PPP.</Section>
            <Section>1.7 USART - Universal Synchronous Asynchronous Receiver Transmitter Driver</Section>
            <Section>The USART is a hardware component that facilitates a connection between the mobile station and terminal equipment (e.g. a PC). This interface uses some of the circuits described in V.24.</Section>
            <Section>The data exchange provided by this unit is serial and asynchronous (synchronous communication is not in the scope of this document). A driver that uses interrupts to manage a circular buffer for the sending and receiving direction is necessary in order to use this component in the GPRS. The driver has to be able to perform flow control.</Section>
            <Section>1.8 TOM - Tunnelling of Messages</Section>
            <Section>The TOM entity is present if and only if HS136 is supported (the feature flag FF_HS136 is enabled).</Section>
            <Section>The main function of TOM is to tunnel non-GSM signalling messages between the MS and the SGSN. The only non-GSM signalling which is currently supported by TOM is for the EGPRS-136 system (according to TIA/EIA-136-376). Data transfer in both uplink and downlink direction is possible. Two different priorities (high, low) of signalling data transfer are supported. TOM uses the unacknowledged mode of LLC and the acknowledged mode of GRR (RLC/MAC).</Section>
        </Description>
        <DocHistory>
            <DocVersion Number="001" Year="99"/>
            <Date Day="31" Month="3" Year="1999"/>
            <Author>Harald</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Krug Initial</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="002" Year="99"/>
            <Date Day="2" Month="6" Year="2000"/>
            <Author>Harald</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Krug S3, Added parameter 'apn' to REQ_PDP_ACT</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="003" Year="99"/>
            <Date Day="9" Month="8" Year="2000"/>
            <Author>Harald</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Krug Modified 'pco' IE.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="004" Year="99"/>
            <Date Day="5" Month="10" Year="2000"/>
            <Author>Harald</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Krug Modified 'apn' IE.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="005" Year="99"/>
            <Date Day="13" Month="10" Year="2000"/>
            <Author>Harald</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Krug Modified 'cause' values acc. to GSM 4.08.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="006" Year="99"/>
            <Date Day="31" Month="10" Year="2000"/>
            <Author>Harald</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Krug Skip unused elements.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="007" Year="99"/>
            <Date Day="29" Month="4" Year="2002"/>
            <Author>Harald</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Krug Skip anonymous access.</Comment>
        </DocHistory>
        <DocRef>
            <RefId>[1]</RefId>
            <RefTitle>GSM 05.02 version 8.0.0 Release 1999Digital cellular telecommunications system (Phase 2+);Multiplexing and multiple access on the radio path</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[2]</RefId>
            <RefTitle>GSM 04.60 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);General Packet Radio Service (GPRS);Mobile Station (MS) - Base Station System (BSS) interface;Radio Link Control/ Medium Access Control (RLC/MAC) protocol</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[3]</RefId>
            <RefTitle>GSM 04.08 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);Mobile radio interface layer 3 specification</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[4]</RefId>
            <RefTitle>GSM 03.64 version 6.1.0 Release 1997Digital cellular telecommunications system (Phase 2+);General Packet Radio Service (GPRS);Overall description of the GPRS radio interface; Stage 2</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[5]</RefId>
            <RefTitle>GSM 03.60 version 6.3.1 Release 1997Digital cellular telecommunications system (Phase 2+);General Packet Radio Service (GPRS);Service description; Stage 2</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[6]</RefId>
            <RefTitle>GSM 04.07 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);Mobile radio interface signalling layer 3; General aspects</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[7]</RefId>
            <RefTitle>GSM 04.64 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);General Packet Radio Service (GPRS);Mobile Station - Serving GPRS Support Node (MS-SGSN)Logical Link Control (LLC) layer specification</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[8]</RefId>
            <RefTitle>GSM 05.08 version 6.4.0 Release 1997Digital cellular telecommunications system (Phase 2+);Radio subsystem link control</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[9]</RefId>
            <RefTitle>GSM 05.10 version 6.3.0 Release 1997Digital cellular telecommunications system (Phase 2+);Radio subsystem synchronization</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[10]</RefId>
            <RefTitle>GSM 03.20 TS 100 929: July 1998 (GSM 03.20 version 6.0.1)Security related network functions, ETSI</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[11]</RefId>
            <RefTitle>Draft GSM 03.22: August 1998 (GSM 03.22 version 6.1.0)Functions related to Mobile Station (MS) in idle mode and group receive mode, ETSI</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[12]</RefId>
            <RefTitle>GSM 04.65 V6.3.0: Subnetwork Dependant Convergence Protocol ETSI, March 1999</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[13]</RefId>
            <RefTitle>ITU-T V42bis ITU-T, Recommendation V.42 bis 1990</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[14]</RefId>
            <RefTitle>GSM 09.60 GPRS Tunneling Protocol (GTP) across the Gn and Gp Interface</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[15]</RefId>
            <RefTitle>RFC 1661 IETF STD 51 July 1994The Point-to-Point Protocol (PPP)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[16]</RefId>
            <RefTitle>RFC 1662 IETF STD 51 July 1994PPP in HDLC-like Framing</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[17]</RefId>
            <RefTitle>RFC 1570 January 1994PPP LCP Extensions</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[18]</RefId>
            <RefTitle>RFC 1989 August 1996PPP Link Quality Monitoring</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[19]</RefId>
            <RefTitle>RFC 1332 May 1992The PPP Internet Protocol Control Protocol (IPCP)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[20]</RefId>
            <RefTitle>RFC 1877 December 1995PPP IPCP Extensions for Name Server Addresses</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[21]</RefId>
            <RefTitle>RFC 2153 May 1997PPP Vendor Extensions</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[22]</RefId>
            <RefTitle>RFC 1334 October 1992PPP Authentication Protocols (for Password Authentication Protocol only)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[23]</RefId>
            <RefTitle>RFC 1994 August 1996PPP Challenge Handshake Authentication Protocol (CHAP)</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[24]</RefId>
            <RefTitle>TIA/EIA-136-370Packet-Data Services - Enhanced General Packet Radio for TIA/EIA-136 (EGPRS-136) - Overview, Telecommunications Industry Association</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[25]</RefId>
            <RefTitle>TIA/EIA-136-376Packet-Data Services - EGPRS-136 Mobility Management, Telecommunications Industry Association</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[26]</RefId>
            <RefTitle>TIA/EIA-136-972Packet-Data Services - Stage 2 Description, Telecommunications Industry Association</RefTitle>
        </DocRef>
    </DocInfoSection>
    <ConstantsSection>
        <Description>
            <Section>This section contains all constants that are defined for the SM AIM</Section>
        </Description>
        <Constant>
            <Alias>L3MAX</Alias>
            <Value ValueType="DEC">251</Value>
            <Comment>maximum size of a L3 buffer</Comment>
        </Constant>
        <History>
            <Date Day="1" Month="1" Year="2000"/>
            <Author>VK</Author>
            <Comment>Initial</Comment>
        </History>
    </ConstantsSection>
    <MessagesSection>
        <Description>
            <Section>This section contains all messages that are defined for the SM AIM</Section>
        </Description>
        <Message>
            <Description>
                <Section>This message is sent by the MS to the network to request activation of a PDP context.</Section>
                <Section>Access point name is included when the MS selects a specific external network to be connected to.</Section>
                <Section>Protocol configuration options are included when the MS provides protocol configuration options for the external PDN.</Section>
                <Section>Reference : [GSM 04.08, 9.5.1]</Section>
            </Description>
            <MsgDef>
                <Name>activate_pdp_req</Name>
                <MsgID Direction="UPLINK" IDType="DEC">65</MsgID>
                <Comment>activate PDP context request</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4</SpecRef>
                <Comment>Message type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>nsapi</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.6.2</SpecRef>
                <Comment>requested NSAPI</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>llc_sapi</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.6.9</SpecRef>
                <Comment>Requested LLC sapi</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>qos</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.6.5</SpecRef>
                <Comment>Requested QoS</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>address</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.6.4</SpecRef>
                <Comment>Requested PDP address</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>apn</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">28</ItemTag>
                <SpecRef>10.5.6.1</SpecRef>
                <Comment>Access point name</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>pco</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">27</ItemTag>
                <SpecRef>10.5.6.3</SpecRef>
                <Comment>Protocol configuration options</Comment>
            </MsgItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to the MS to acknowledge activation of a PDP context.</Section>
                <Section>If the MS did not request a static address in the corresponding ACTIVATE PDP CONTEXT REQUEST message, the network shall include the PDP address IE in this message, otherwise not.</Section>
                <Section>Protocol configuration options are included in the message when the network wishes to transmit protocol configuration options for the external PDN.</Section>
                <Section>Reference : [GSM 04.08, 9.5.2]</Section>
            </Description>
            <MsgDef>
                <Name>activate_pdp_acc</Name>
                <MsgID Direction="DOWNLINK" IDType="DEC">66</MsgID>
                <Comment>activate PDP context accept</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4</SpecRef>
                <Comment>Message type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>llc_sapi</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.6.9</SpecRef>
                <Comment>Negotiated LLC SAPI</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>qos</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.6.5</SpecRef>
                <Comment>Negotiated QoS</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>radio_prio</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.7.2</SpecRef>
                <Comment>Radio Priority</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <SpecRef>10.5.1.8</SpecRef>
                <Comment>Spare half octet</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>address</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">2B</ItemTag>
                <SpecRef>10.5.6.4</SpecRef>
                <Comment>Packet data protocol address</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>pco</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">27</ItemTag>
                <SpecRef>10.5.6.3</SpecRef>
                <Comment>Protocol configuration options</Comment>
            </MsgItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to the MS to reject activation of a PDP context.</Section>
                <Section>The protocol configuration options IE may only be inserted by the network (see GSM 09.60) if the SM cause indicates &quot;activation rejected by GGSN&quot;.</Section>
                <Section>Reference : [GSM 04.08, 9.5.3]</Section>
            </Description>
            <MsgDef>
                <Name>activate_pdp_rej</Name>
                <MsgID Direction="DOWNLINK" IDType="DEC">67</MsgID>
                <Comment>activate PDP context reject</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4</SpecRef>
                <Comment>Message type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>sm_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.6.6</SpecRef>
                <Comment>SM cause</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>pco</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">27</ItemTag>
                <SpecRef>10.5.6.3</SpecRef>
                <Comment>Protocol configuration options</Comment>
            </MsgItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to the MS to initiate activation of a PDP context.</Section>
                <Section>Reference : [GSM 04.08, 9.5.4]</Section>
            </Description>
            <MsgDef>
                <Name>req_pdp_act</Name>
                <MsgID Direction="DOWNLINK" IDType="DEC">68</MsgID>
                <Comment>request PDP context activation</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4</SpecRef>
                <Comment>Message type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>address</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.6.4</SpecRef>
                <Comment>Offered PDP address</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>apn</Name>
                </ItemLink>
                <Type>GSM4_TLV</Type>
                <ItemTag TagType="HEX">28</ItemTag>
                <SpecRef>10.5.6.1</SpecRef>
                <Comment>Access point name</Comment>
            </MsgItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the MS to the network to reject initiation of a PDP context activation.</Section>
                <Section>Reference : [GSM 04.08, 9.5.5]</Section>
            </Description>
            <MsgDef>
                <Name>req_pdp_act_rej</Name>
                <MsgID Direction="UPLINK" IDType="DEC">69</MsgID>
                <Comment>request PDP context activation reject</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4</SpecRef>
                <Comment>Message type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>sm_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.6.6</SpecRef>
                <Comment>SM cause</Comment>
            </MsgItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="7" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Remove APN</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network to the MS to request the modification of an active PDP context.</Section>
                <Section>Reference : [GSM 04.08, 9.5.6]</Section>
            </Description>
            <MsgDef>
                <Name>mod_pdp_req</Name>
                <MsgID Direction="DOWNLINK" IDType="DEC">72</MsgID>
                <Comment>Modify PDP context request</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4</SpecRef>
                <Comment>Message type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>radio_prio</Name>
                </ItemLink>
                <Type>GSM1_V</Type>
                <SpecRef>10.5.7.2</SpecRef>
                <Comment>Radio Priority</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <SpecRef>10.5.1.8</SpecRef>
                <Comment>Spare half octet</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>llc_sapi</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.6.9</SpecRef>
                <Comment>Requested LLC sapi</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>qos</Name>
                </ItemLink>
                <Type>GSM4_LV</Type>
                <SpecRef>10.5.6.5</SpecRef>
                <Comment>New QoS</Comment>
            </MsgItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the MS to the network to acknowledge the modification of an active PDP context.</Section>
                <Section>Reference : [GSM 04.08, 9.5.7]</Section>
            </Description>
            <MsgDef>
                <Name>mod_pdp_acc</Name>
                <MsgID Direction="UPLINK" IDType="DEC">73</MsgID>
                <Comment>Modify PDP context accept</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4</SpecRef>
                <Comment>Message type</Comment>
            </MsgItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent  to request deactivation of an active PDP context.</Section>
                <Section>Reference : [GSM 04.08, 9.5.8]</Section>
            </Description>
            <MsgDef>
                <Name>deact_pdp_req</Name>
                <MsgID Direction="BOTH" IDType="DEC">70</MsgID>
                <Comment>Deactivate PDP context request</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4</SpecRef>
                <Comment>Message type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>sm_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.6.6</SpecRef>
                <Comment>SM cause</Comment>
            </MsgItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent  to acknowledge deactivation of the PDP context requested in the corresponding Deactivate PDP context request message.</Section>
                <Section>Reference : [GSM 04.08, 9.5.9]</Section>
            </Description>
            <MsgDef>
                <Name>deact_pdp_acc</Name>
                <MsgID Direction="BOTH" IDType="DEC">71</MsgID>
                <Comment>deactivate PDP context accept</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4</SpecRef>
                <Comment>Message type</Comment>
            </MsgItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This message is sent by the network or the MS to pass information on the status of the indicated context and report certain error conditions.</Section>
                <Section>Reference : [GSM 04.08, 9.5.15]</Section>
            </Description>
            <MsgDef>
                <Name>sm_status</Name>
                <MsgID Direction="BOTH" IDType="DEC">85</MsgID>
                <Comment>SM Status</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.4</SpecRef>
                <Comment>Message type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>sm_cause</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>10.5.6.6</SpecRef>
                <Comment>SM cause</Comment>
            </MsgItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="20" Month="6" Year="2000"/>
                <Author>HK</Author>
                <Comment>Changed direction to 'both'</Comment>
            </History>
        </Message>
    </MessagesSection>
    <MsgStructElementsSection>
        <Description>
            <Section>This section contains all structured elements that are defined for the SM AIM</Section>
        </Description>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the NSAPI is to identify the service access point that is used for the data transfer at layer 3.</Section>
                <Section>Reference : [1] section 10.5.6.2</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nsapi</Name>
                <Comment>network service access point identifier</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>nsapi_val</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>NSAPI value</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the LLC service access point identifier information element is to identify the service access point that is used for the GPRS data transfer at LLC layer.</Section>
                <Section>Reference : [1] section 10.5.6.9</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>llc_sapi</Name>
                <Comment>LLC service access point identifier</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>sapi</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>LLC SAPI value</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the quality of service information element is to specify the QoS parameters for a PDP context.</Section>
                <Section>Reference : [1] section 10.5.6.5</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>qos</Name>
                <Comment>Quality of service</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>00</Pattern>
                    <BitLen>2</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>delay</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Delay class</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>reliability</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Reliability class</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>peak</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Peak throughput</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>precedence</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>precedence class</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>mean</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>mean throughput</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the packet data protocol address information element is to identify an address associated with a PDP. Reference : [1] section 10.5.6.4</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>address</Name>
                <Comment>Packet data protocol address</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>pdp_type_org</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PDP type organisation</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>pdp_type_no</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>PDP type number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>add_info</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..20]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>address information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the access point name information element is to identify the packet data network to which the GPRS user wishes to connect.</Section>
                <Section>The Access Point Name is a label or a full qualified domain name according to DNS naming conventions (see GSM 03.03 [10]).</Section>
                <Section>Reference : [1] section 10.5.6.1</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>apn</Name>
                <Comment>Access point name</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>apn_value</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[3..102]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>access point name value</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="12" Month="6" Year="2000"/>
                <Author>HK</Author>
                <Comment>Changed bit len from 824</Comment>
            </History>
            <History>
                <Date Day="4" Month="10" Year="2000"/>
                <Author>HK</Author>
                <Comment>Made len variable.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the protocol configuration options information element is to transfer external network protocol options associated with a PDP context activation.</Section>
                <Section>Reference : [1] section 10.5.6.3</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pco</Name>
                <Comment>Protocol information options</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>pco_value</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[2..253]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>options</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="5" Year="2000"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="9" Month="8" Year="2000"/>
                <Author>HK</Author>
                <Comment>Replaced all elements by the one 'pco_val'.</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the radio priority information element is to specify the priority level that the MS shall use at the lower</Section>
                <Section>layers for transmission of data related to a PDP context or for mobile originated SMS transmission.</Section>
                <Section>Reference : [1] section 10.5.7.2</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>radio_prio</Name>
                <Comment>Radio priority</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0</Pattern>
                    <BitLen>1</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>radio_prio_val</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Radio priority value</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>The purpose of the SM cause information element is to indicate the reason why a session management request is</Section>
                <Section>rejected.</Section>
                <Section>Reference : [1] section 10.5.7.2</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>sm_cause</Name>
                <Comment>SM cause</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sm</DocName>
                    <Name>sm_cause_val</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>SM cause value</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="26" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
    </MsgStructElementsSection>
    <MsgBasicElementsSection>
        <Description>
            <Section>This section contains all basic elements that are defined for the SM AIM</Section>
        </Description>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 10.5.6.2 (NSAPI)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>nsapi_val</Name>
                <BitLen>4</BitLen>
                <Comment>NSAPI value</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sm</DocName>
                <Name>VAL_nsapi_val</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 10.5.6.5 (Quality of service)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>delay</Name>
                <BitLen>3</BitLen>
                <Comment>Delay class</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sm</DocName>
                <Name>VAL_delay</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 10.5.6.5 (Quality of service)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>reliability</Name>
                <BitLen>3</BitLen>
                <Comment>Reliability class</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sm</DocName>
                <Name>VAL_reliability</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 10.4</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>msg_type</Name>
                <BitLen>8</BitLen>
                <Comment>Message Type</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="1" Month="1" Year="2000"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 10.5.5.11</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>sapi</Name>
                <BitLen>4</BitLen>
                <Comment>SAPI</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sm</DocName>
                <Name>VAL_sapi</Name>
            </ValuesLink>
            <History>
                <Date Day="5" Month="5" Year="1999"/>
                <Author>ANS</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 10.5.6.5 (Quality of service)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>peak</Name>
                <BitLen>4</BitLen>
                <Comment>Peak throughput</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sm</DocName>
                <Name>VAL_peak</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 10.5.6.5 (Quality of service)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>precedence</Name>
                <BitLen>3</BitLen>
                <Comment>Precedence class</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sm</DocName>
                <Name>VAL_precedence</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 10.5.6.5 (Quality of service)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>mean</Name>
                <BitLen>5</BitLen>
                <Comment>Mean throughput</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sm</DocName>
                <Name>VAL_mean</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The bit len field is in reality 24-824.</Section>
                <Section>Reference : [1] section 10.5.6.1</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>apn_value</Name>
                <BitLen>8</BitLen>
                <Comment>Access point name value</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="5" Year="2000"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="10" Year="2000"/>
                <Author>HK</Author>
                <Comment>Changed to variable length</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The organisation by which the address was allocated.</Section>
                <Section>Reference : [1] section 10.5.6.4 (Protocol configuration options)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pdp_type_org</Name>
                <BitLen>4</BitLen>
                <Comment>PDP type organisation</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sm</DocName>
                <Name>VAL_pdp_type_org</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The type of the PDP address.</Section>
                <Section>X.121 address type will only be present if the pdp_type_org was ETSI_ORG. Ipv4 and Ipv6 address type will only be given if the pdp_type_org was IEFT_ORG.</Section>
                <Section>digit 2  digit 1</Section>
                <Section>digit 4  digit 3</Section>
                <Section>digit m + 1  digit m</Section>
                <Section>Reference : [1] section 10.5.6.4 (Protocol configuration options)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pdp_type_no</Name>
                <BitLen>8</BitLen>
                <Comment>PDP type number</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sm</DocName>
                <Name>VAL_pdp_type_no</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Value of the radio priority.</Section>
                <Section>Reference : [1] section 10.5.7.2 (Radio priority)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>radio_prio_val</Name>
                <BitLen>3</BitLen>
                <Comment>Radio priority value</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sm</DocName>
                <Name>VAL_radio_prio_val</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The purpose of the SM cause information element is to indicate the reason why a session management request is rejected.</Section>
                <Section>Reference : [1] section 10.5.6.6 (SM cause)</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>sm_cause_val</Name>
                <BitLen>8</BitLen>
                <Comment>SM cause value</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sm</DocName>
                <Name>VAL_sm_cause_val</Name>
            </ValuesLink>
            <History>
                <Date Day="25" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="9" Year="2002"/>
                <Author>HK</Author>
                <Comment>Add &quot;Semantically incorrect message&quot;.</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>If  the address is an X.121 address then digit 1 contains the first BCD coded digit of the X.121 address. If the X.121 has an odd number of digits then digit m + 1 shall be padded with HEX(F).</Section>
                <Section>If PDP type number indicates IPv4, the Address information in octet 5 to octet 8 contains the IPv4 address. Bit 8 of octet 5 represents the most significant bit of the IP address and bit 1 of octet 8 the least significant bit.</Section>
                <Section>If PDP type number indivates IPv6, the Address information in octet 5 to octet 20 contains the IPv6 address. Bit 8 of octet 5 represents the most sgnificant bit of the IP address and bit 1 of octet 20 the least significant bit.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>add_info</Name>
                <BitLen>8</BitLen>
                <Comment>Adress information</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="25" Month="5" Year="1999"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>The bit len field is in reality 2-253.</Section>
                <Section>Reference : [1] section 10.5.6.1</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>pco_value</Name>
                <BitLen>8</BitLen>
                <Comment>Protocol config value</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="9" Month="8" Year="2000"/>
                <Author>HK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
    </MsgBasicElementsSection>
    <ValuesSection>
        <Description>
            <Section>This section contains all sets of values that are defined for the SM AIM</Section>
        </Description>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_nsapi_val</Name>
                <Comment>values for nsapi_val</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>NSAPI_5</Alias>
                <Comment>NSAPI 5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>NSAPI_6</Alias>
                <Comment>NSAPI 6</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>NSAPI_7</Alias>
                <Comment>NSAPI 7</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>NSAPI_8</Alias>
                <Comment>NSAPI 8</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>NSAPI_9</Alias>
                <Comment>NSAPI 9</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>NSAPI_10</Alias>
                <Comment>NSAPI 10</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>NSAPI_11</Alias>
                <Comment>NSAPI 11</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>NSAPI_12</Alias>
                <Comment>NSAPI 12</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">13</Value>
                <Alias>NSAPI_13</Alias>
                <Comment>NSAPI 13</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias>NSAPI_14</Alias>
                <Comment>NSAPI 14</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>NSAPI_15</Alias>
                <Comment>NSAPI 15</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_delay</Name>
                <Comment>values for delay</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DELAY_SUB</Alias>
                <Comment>Subscribed delay class (uplink only)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DELAY_RES_DL</Alias>
                <Comment>Reserved (downlink only)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DELAY_1</Alias>
                <Comment>Delay class 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>DELAY_2</Alias>
                <Comment>Delay class 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>DELAY_3</Alias>
                <Comment>Delay class 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>DELAY_4</Alias>
                <Comment>Delay class 4 (best effort)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>DELAY_RES</Alias>
                <Comment>Reserved</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Delay class 4 (best effort)</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_reliability</Name>
                <Comment>values for reliability</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>RELY_SUB</Alias>
                <Comment>Subscribed reliability class (uplink only)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>RELY_RES_DL</Alias>
                <Comment>Reserved (dowwnlink only)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>RELY_1</Alias>
                <Comment>Acknowledged GTP, LLC, and RLC; Protected data</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>RELY_2</Alias>
                <Comment>Unacknowledged GTP; Acknowledged LLC and RLC, Protected data</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>RELY_3</Alias>
                <Comment>Unacknowledged GTP and LLC; Acknowledged RLC, Protected data</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>RELY_4</Alias>
                <Comment>Unacknowledged GTP, LLC, and RLC, Protected data</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>RELY_5</Alias>
                <Comment>Unacknowledged GTP, LLC, and RLC, Unprotected data</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>RELY_RES</Alias>
                <Comment>Reserved</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Unacknowledged GTP and LLC; Acknowledged RLC, Protected data</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_sapi</Name>
                <Comment>values for sapi</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SAPI_3</Alias>
                <Comment>SAPI 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SAPI_5</Alias>
                <Comment>SAPI 5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>SAPI_9</Alias>
                <Comment>SAPI 9</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>SAPI_11</Alias>
                <Comment>SAPI 11</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_peak</Name>
                <Comment>values for peak</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PEAK_SUB</Alias>
                <Comment>Subscribed peak throughput (uplink only)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PEAK_RES_DL</Alias>
                <Comment>reserved (downlink only)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PEAK_1000</Alias>
                <Comment>Up to 1000 octet/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PEAK_2000</Alias>
                <Comment>Up to 2000 octet/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>PEAK_4000</Alias>
                <Comment>Up to 4000 octet/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>PEAK_8000</Alias>
                <Comment>Up to 8000 octet/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>PEAK_16000</Alias>
                <Comment>Up to 16000 octet/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>PEAK_32000</Alias>
                <Comment>Up to 32000 octet/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>PEAK_64000</Alias>
                <Comment>Up to 64000 octet/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>PEAK_128000</Alias>
                <Comment>Up to 128000 octet/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>PEAK_256000</Alias>
                <Comment>Up to 256000 octet/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>PEAK_RES</Alias>
                <Comment>Reserved</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Up to 1000 octet/s</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_precedence</Name>
                <Comment>values for precedence</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PRECED_SUB</Alias>
                <Comment>Subscribed precedence (uplink only)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PRECED_RES_DL</Alias>
                <Comment>Reserved (downlink only)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PRECED_HIGH</Alias>
                <Comment>High priority</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PRECED_NORM</Alias>
                <Comment>Normal Priority</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>PRECED_LOW</Alias>
                <Comment>Low priority</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>PRECED_RES</Alias>
                <Comment>Reserved</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Normal Priority</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_mean</Name>
                <Comment>values for mean</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MEAN_SUB</Alias>
                <Comment>Subscribed mean throughput (uplink only)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MEAN_RES_DL</Alias>
                <Comment>reserved (downlink only)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MEAN_100</Alias>
                <Comment>100 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MEAN_200</Alias>
                <Comment>200 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MEAN_500</Alias>
                <Comment>500 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>MEAN_1000</Alias>
                <Comment>1000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>MEAN_2000</Alias>
                <Comment>2000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>MEAN_5000</Alias>
                <Comment>5000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>MEAN_10000</Alias>
                <Comment>10000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>MEAN_20000</Alias>
                <Comment>20000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>MEAN_50000</Alias>
                <Comment>50000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>MEAN_100000</Alias>
                <Comment>100000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>MEAN_200000</Alias>
                <Comment>200000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>MEAN_500000</Alias>
                <Comment>500000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">13</Value>
                <Alias>MEAN_1000000</Alias>
                <Comment>1000000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">14</Value>
                <Alias>MEAN_2000000</Alias>
                <Comment>2000000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>MEAN_5000000</Alias>
                <Comment>5000000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">16</Value>
                <Alias>MEAN_10000000</Alias>
                <Comment>10000000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">17</Value>
                <Alias>MEAN_20000000</Alias>
                <Comment>20000000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">18</Value>
                <Alias>MEAN_50000000</Alias>
                <Comment>50000000 octet/h</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">30</Value>
                <Alias>MEAN_RES</Alias>
                <Comment>Reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">31</Value>
                <Alias>MEAN_BEST</Alias>
                <Comment>Best effort</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Best effort</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pdp_type_org</Name>
                <Comment>values for pdp_type_org</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ETSI_ORG</Alias>
                <Comment>ETSI allocated address (e.g. X.121)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>IETF_ORG</Alias>
                <Comment>IETF allocated address</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>PDP_MT</Alias>
                <Comment>Dynamic PDP addressing is applied, (uplink only)</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>ETSI allocated address (e.g. X.121)</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pdp_type_no</Name>
                <Comment>values for pdp_type_no</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>X121_TYPE</Alias>
                <Comment>X.121 address</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100001</Value>
                <Alias>IP4_TYPE</Alias>
                <Comment>IPv4 address</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01010111</Value>
                <Alias>IP6_TYPE</Alias>
                <Comment>IPv6 address</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>IPv4 address</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_radio_prio_val</Name>
                <Comment>values for radio_prio_val</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>RADIO_PRIO_1</Alias>
                <Comment>priority level 1 (highest)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>RADIO_PRIO_2</Alias>
                <Comment>priority level 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>RADIO_PRIO_3</Alias>
                <Comment>priority level 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>RADIO_PRIO_4</Alias>
                <Comment>priority level 4 (lowest)</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>priority level 4 (lowest)</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_sm_cause_val</Name>
                <Comment>values for sm_cause_val</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00011001</Value>
                <Alias>LLC_OR_SNDCP</Alias>
                <Comment>LLC or SNDCP failure</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00011010</Value>
                <Alias>INSUF_RES</Alias>
                <Comment>Insufficient resources</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00011011</Value>
                <Alias>APN_MISS</Alias>
                <Comment>Missing or unknown APN</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00011100</Value>
                <Alias>UNK_PDP</Alias>
                <Comment>Unknown PDP address or PDP type</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00011101</Value>
                <Alias>AUTH_FAIL</Alias>
                <Comment>User Aauthentication failed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00011110</Value>
                <Alias>GGSN_ACT_REJ</Alias>
                <Comment>Activation rejected by GGSN</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00011111</Value>
                <Alias>UNSPEC_ACT_REJ</Alias>
                <Comment>Activation rejected, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100000</Value>
                <Alias>SERV_OPT_NO_SP</Alias>
                <Comment>Service option not supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100001</Value>
                <Alias>SERV_OPT_NO_SC</Alias>
                <Comment>Requested service option not subscribed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100010</Value>
                <Alias>SERV_OPT_TMP</Alias>
                <Comment>Service option temporarily out of order</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100011</Value>
                <Alias>NSAPI_USED</Alias>
                <Comment>NSAPI already used</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100100</Value>
                <Alias>REGULAR</Alias>
                <Comment>Regular deactivation</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100101</Value>
                <Alias>QOS_NOT_ACC</Alias>
                <Comment>QoS not accepted</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100110</Value>
                <Alias>NET_FAIL</Alias>
                <Comment>Network failure</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00100111</Value>
                <Alias>REACT_REQ</Alias>
                <Comment>Reactivation required</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01011111</Value>
                <Alias>SEM_INCORRECT</Alias>
                <Comment>Semantically incorrect message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01010001</Value>
                <Alias>TI_INVAL</Alias>
                <Comment>Invalid transaction identifier value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01100000</Value>
                <Alias>MAND_INF_INVAL</Alias>
                <Comment>Invalid mandatory information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01100001</Value>
                <Alias>MSG_T_NON_X</Alias>
                <Comment>Message type non-existent or not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01100010</Value>
                <Alias>MSG_T_NOT_COMP</Alias>
                <Comment>Message type not compatible with the protocol state</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01100011</Value>
                <Alias>IE_NON_X</Alias>
                <Comment>Information element non-existent or not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01100100</Value>
                <Alias>COND_IE</Alias>
                <Comment>Conditional IE error</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01100101</Value>
                <Alias>NO_STATE_COMP</Alias>
                <Comment>Message not compatible with the protocol state</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01101111</Value>
                <Alias>UNSPEC</Alias>
                <Comment>Protocol error, unspecified</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Service option temporarily out of order ( received by MS)</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
    </ValuesSection>
</AIM>
