<?xml version="1.0"?>
<!-- Translated from Tutorial_1.cmd, used by the Tutorial_1 recipe. Created on November 30, 2000. -->


<strategy
   version="6"
   host="windows"
   name="Tutorial_1"
   full_path="C:\\ti\\bin\\utilities\\vislink\\Templates\\c55x\\Examples\\Tutorial_1\\Tutorial_1.str"
   comment="Translated from Tutorial_1.cmd, used by the Tutorial_1 recipe. Created on November 30, 2000."
>

   <!-- CHANGE  vectors  OF  rts553.lib\vectors.obj\vectors  TO  TRUE -->
   <instr
      op="48"
      s0="All Input Files\\Tutorial_1\\rts553.lib\\vectors.obj\\vectors"
      u1="1"
   />

   <!-- CHANGE  entry  OF  rts553.lib\boot.obj\.text\_c_int00  TO  TRUE -->
   <instr
      op="1d"
      s0="All Input Files\\Tutorial_1\\rts553.lib\\boot.obj\\.text\\_c_int00"
      u1="1"
   />

   <!-- NEW  child output file  OF  Output Files  WITH  full_path=.\tutorial_1.out  HOLDING  map C55x -->
   <instr
      op="27"
      s0="Output Files"
      s1=".\\tutorial_1.out"
      s2="Memory Maps\\C55x"
      u3="12f17c"
   />

   <!-- NEW  child output section  OF  run_view\memory_space\VECTORS  WITH  name=vectors, data_kind=hole -->
   <instr
      op="22"
      s0="Memory Maps\\C55x\\run_view\\memory_space\\VECTORS"
      s1="vectors"
      u3="8"
   />

   <!-- ALIGN  run address of run_view\memory_space\VECTORS\vectors  TO  absolute address ==  0ffff00h -->
   <instr
      op="2f"
      s0="Memory Maps\\C55x\\run_view\\memory_space\\VECTORS\\vectors"
      u1="ffff00"
      u2="ffffffff"
   />

   <!-- ADD  rts553.lib\vectors.obj\vectors  TO  run_view\memory_space\VECTORS\vectors -->
   <instr
      op="2"
      s0="All Input Files\\Tutorial_1\\rts553.lib\\vectors.obj\\vectors"
      s1="Memory Maps\\C55x\\run_view\\memory_space\\VECTORS\\vectors"
   />

   <!-- END  Tutorial_1 -->
   <instr
      op="0"
   />
</strategy>
