<?xml version="1.0" encoding="UTF-8"?>
<!-- edited with SAPE SAP Editor -->
<AIM xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="aim.xsd">
    <DocInfoSection>
        <DocName DocType="AIM">sat</DocName>
        <DocNum Number="609" Project="6147"/>
        <Description>
            <Section>The Protocol Stacks are used to define the functionality of the GSM protocols for interfaces. The GSM specifications are normative when used to describe the functionality of interfaces, but the stacks and the subdivision of protocol layers does not imply or restrict any implementation.</Section>
            <Section>The base of the Protocol Stack rests on the physical layer.</Section>
            <Section>The Data Link Layer (DL) is used to handle an acknowledged connection between mobile and base station. The LAPDm protocol is used.</Section>
            <Section>Radio Resource (RR) manages the resources of the air-interface. That means configuration of physical layer, cell selection and cell reselection, data transfer, RR-Connection handling.</Section>
            <Section>Mobility Management (MM) handles registration aspects for the mobile station. It detects changes of location areas and updates a mobile station in the new location area.</Section>
            <Section>Call Control (CC) provides the call functionality. This includes call establishment, call maintenance procedures like Hold, Retrieve or Modify, and call disconnection.</Section>
            <Section>Supplementary Services (SS) handles all call independent supplementary services like call forwarding or call barring.</Section>
            <Section>Short Message Services (SMS) is used for sending and receiving point-to-point short messages.</Section>
            <Section>The man machine interface (MMI) is the interface to the user. Normally it is connected with a keypad as input device and a display as output device.</Section>
            <Section>Between the several entities data interfaces are defined. These data interfaces are called Service Access Points (SAPs), indicating that an upper layer uses the services of a lower layer.</Section>
            <Section>The GSM specification do not set out any implementation of the Protocol Stack. The following diagrams show the implementation described in all these documents for the mobile station. All entities except the Man Machine Interface and Physical Layer are implemented as part of the Protocol Stack.</Section>
            <Section>Figure 1: Mobile-station protocol architecture</Section>
            <Section>This document describes the facility IE coding for the supplementary service processing in MMI(ACI).</Section>
        </Description>
        <DocHistory>
            <DocVersion Number="001" Year="99"/>
            <Date Day="1" Month="7" Year="1999"/>
            <Author>AK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Initial version.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="002" Year="99"/>
            <Date Day="4" Month="2" Year="2000"/>
            <Author>UB</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Condat AG change</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="003" Year="99"/>
            <Date Day="11" Month="1" Year="2002"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>No comment.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="004" Year="99"/>
            <Date Day="21" Month="3" Year="2002"/>
            <Author>RM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>corrected document number; applied new template</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="005" Year="99"/>
            <Date Day="4" Month="4" Year="2002"/>
            <Author>STW</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>dynamic Channel Data element</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="006" Year="99"/>
            <Date Day="8" Month="4" Year="2002"/>
            <Author>AK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>bearer description element corrected</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="007" Year="99"/>
            <Date Day="9" Month="4" Year="2002"/>
            <Author>AK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>bearer description element modified, other address, channel status in term. response and net.acc.name corrected</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="008" Year="99"/>
            <Date Day="12" Month="4" Year="2002"/>
            <Author>STW</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Location Information element renamed because of double use in the protocol stack</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="009" Year="99"/>
            <Date Day="12" Month="6" Year="2002"/>
            <Author>STW</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>update upper border of TLV Channel Data</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="010" Year="99"/>
            <Date Day="5" Month="9" Year="2002"/>
            <Author>RM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>rebase data</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="011" Year="99"/>
            <Date Day="25" Month="2" Year="2003"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>issue 9228</Comment>
        </DocHistory>
        <DocRef>
            <RefId>[1]</RefId>
            <RefTitle>GSM 11.14 version 7.3.1 Release 1998, Specification of the SIM application toolkit for the Subscriber Identity Module -  Mobile Equipment (SIM-ME) TS 101 267, ETSI, July 1999</RefTitle>
        </DocRef>
        <DocRef>
            <RefId>[2]</RefId>
            <RefTitle>GSM 4.08, Mobile radio interface layer 3 specification EN 300 940, ETSI, April 1999</RefTitle>
        </DocRef>
    </DocInfoSection>
    <ConstantsSection>
        <Description>
            <Section>2 Constants</Section>
        </Description>
        <Constant>
            <Alias>MAX_PARTY_NUM_SAT</Alias>
            <Value ValueType="DEC">480</Value>
            <Comment>Maximum number length of a cld/clg party</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_SUBADDR_NUM</Alias>
            <Value ValueType="DEC">20</Value>
            <Comment>Maximum number length of a cld/clg party subaddress</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CH_DATA_LEN</Alias>
            <Value ValueType="DEC">241</Value>
            <Comment>Maximum length of channel data string</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CMD_AT_LEN</Alias>
            <Value ValueType="DEC">241</Value>
            <Comment>Maximum length of an AT command string</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_ALPHA_ID_LEN</Alias>
            <Value ValueType="DEC">241</Value>
            <Comment>Maximum bytelength of alpha identifier</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_SS_STRING_LEN</Alias>
            <Value ValueType="DEC">60</Value>
            <Comment>Maximum length of SS string</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_SAT_USSD_LEN</Alias>
            <Value ValueType="DEC">160</Value>
            <Comment>Maximum length of USSD string</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_SMS_DIGIT_LEN</Alias>
            <Value ValueType="DEC">20</Value>
            <Comment>Maximum number of digits in SMS addresses</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_SMS_TPDU_LEN</Alias>
            <Value ValueType="DEC">184</Value>
            <Comment>Maximum length of SMS SUBMIT or COMMAND</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CAP_CNF_LEN</Alias>
            <Value ValueType="DEC">112</Value>
            <Comment>Maximum bitlength of capability configuration</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_TEXT_LEN</Alias>
            <Value ValueType="DEC">160</Value>
            <Comment>Maximum length of text (response to Send USSD)</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_EVENT_LIST_LEN</Alias>
            <Value ValueType="DEC">10</Value>
            <Comment>Maximum number of supported events</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_TI_LEN</Alias>
            <Value ValueType="DEC">16</Value>
            <Comment>Maximum number of different transaction identifier</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_DTMF_LEN</Alias>
            <Value ValueType="DEC">80</Value>
            <Comment>Maximum number of DTMF digits</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_PROV_F_PATH_LEN</Alias>
            <Value ValueType="DEC">16</Value>
            <Comment>Maximum number of supported paths</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_BEARER_LIST_LEN</Alias>
            <Value ValueType="DEC">253</Value>
            <Comment>Maximum list length of supported bearer</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CAUSE_LEN</Alias>
            <Value ValueType="DEC">30</Value>
            <Comment>Maximum length of cause information element</Comment>
        </Constant>
        <Constant>
            <Alias>CCR_ALLW_NO_MDFY</Alias>
            <Value ValueType="HEX">00</Value>
            <Comment>Allowed, no modification</Comment>
        </Constant>
        <Constant>
            <Alias>CCR_NOT_ALLW</Alias>
            <Value ValueType="HEX">01</Value>
            <Comment>Not allowed</Comment>
        </Constant>
        <Constant>
            <Alias>CCR_ALLW_WITH_MDFY</Alias>
            <Value ValueType="HEX">02</Value>
            <Comment>Allowed, with modification</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_SAT_APN_LEN</Alias>
            <Value ValueType="DEC">102</Value>
            <Comment>Maximum byte length of APN string</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_URL_LEN</Alias>
            <Value ValueType="DEC">253</Value>
            <Comment>Maximum length for URL</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_PFP_ELEM</Alias>
            <Value ValueType="DEC">10</Value>
            <Comment>Maximum provisioning file path elements</Comment>
        </Constant>
        <History>
            <Date Day="12" Month="7" Year="1999"/>
            <Author>AK</Author>
            <Comment>Initial</Comment>
        </History>
        <History>
            <Date Day="13" Month="9" Year="2000"/>
            <Author>FK</Author>
            <Comment>Constant value and name for number of digits changed</Comment>
        </History>
        <History>
            <Date Day="5" Month="10" Year="2000"/>
            <Author>FK</Author>
            <Comment>Length definitions for SMS and USSD added</Comment>
        </History>
        <History>
            <Date Day="17" Month="10" Year="2000"/>
            <Author>FK</Author>
            <Comment>Length definitions for Event List added</Comment>
        </History>
        <History>
            <Date Day="18" Month="3" Year="2002"/>
            <Author>RM</Author>
            <Comment>Length definition for Event List changed Length definition for Bearer List added Number of paths added</Comment>
        </History>
        <History>
            <Date Day="26" Month="3" Year="2002"/>
            <Author>JK</Author>
            <Comment>Length definition for channel data</Comment>
        </History>
        <History>
            <Date Day="9" Month="4" Year="2002"/>
            <Author>AK</Author>
            <Comment>APN length added</Comment>
        </History>
        <History>
            <Date Day="25" Month="4" Year="2002"/>
            <Author>RIE</Author>
            <Comment>URL length and prov. file path elem. length added</Comment>
        </History>
        <History>
            <Date Day="12" Month="6" Year="2002"/>
            <Author>STW</Author>
            <Comment>MAX_CH_DATA_LEN changed to 241</Comment>
        </History>
    </ConstantsSection>
    <MessagesSection>
        <Description>
            <Section>This section contains all messages that are defined for the SAT AIM</Section>
        </Description>
        <Message>
            <Description>
                <Section>The SAT command coding is used to distinguish the different commands (send SS, set up call) in the first decoding stage of the SAT .</Section>
            </Description>
            <MsgDef>
                <Name>stk_cmd</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">11100000</MsgID>
                <Comment>SAT Command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef/>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>pas_cmd</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">D0</ItemTag>
                <SpecRef>13.2</SpecRef>
                <Comment>Proactive SIM Command</Comment>
            </MsgItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2002"/>
                <Author>AK</Author>
                <Comment>msg ID changed due to conflict with class e command ID's</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>Command parameters which are used to send a supplementary service control string.</Section>
            </Description>
            <MsgDef>
                <Name>send_ss</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_SEND_SS</MsgID>
                <Comment>Send SS string</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.10</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>alpha identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ss_string</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">89</ItemTag>
                <SpecRef>12.14</SpecRef>
                <Comment>ss_string</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2000"/>
                <Author>FK</Author>
                <Comment>Optional elements defined without CR flag</Comment>
            </History>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Icon Identifier added</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>Command parameters which are used to set up a call.</Section>
            </Description>
            <MsgDef>
                <Name>setup_call</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_SETUP_CALL</MsgID>
                <Comment>Set up call</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.12</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>alpha identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>addr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">86</ItemTag>
                <SpecRef>12.1</SpecRef>
                <Comment>address</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cap_cnf_parms</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">07</ItemTag>
                <SpecRef>12.4</SpecRef>
                <Comment>capability conf. parameter</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>subaddr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>12.3</SpecRef>
                <Comment>subaddress</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dur</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>12.8</SpecRef>
                <Comment>duration</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id_2</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>alpha identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon_2</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2000"/>
                <Author>FK</Author>
                <Comment>Optional elements defined without CR flag</Comment>
            </History>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Second Alpha Identifier and 2 Icon Identifier added</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>Command parameters which are used to send a short message.</Section>
            </Description>
            <MsgDef>
                <Name>send_sm</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_SEND_SMS</MsgID>
                <Comment>Send Short Message</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.9</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>alpha identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>addr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">06</ItemTag>
                <SpecRef>12.1</SpecRef>
                <Comment>address</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>smpdu</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">8B</ItemTag>
                <SpecRef>12.13</SpecRef>
                <Comment>SMS TPDU</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgItem>
            <History>
                <Date Day="28" Month="9" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Icon Identifier added</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>Command parameters which are used to send Unstructured Supplementary Service Data.</Section>
            </Description>
            <MsgDef>
                <Name>send_ussd</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_SEND_USSD</MsgID>
                <Comment>Send USSD string</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.11</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>alpha identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ussd_string</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">8A</ItemTag>
                <SpecRef>12.17</SpecRef>
                <Comment>USSD string</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgItem>
            <History>
                <Date Day="28" Month="9" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Icon Identifier added</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>Command parameters which are used to send Unstructured Supplementary Service Data.</Section>
            </Description>
            <MsgDef>
                <Name>send_dtmf</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_SEND_DTMF</MsgID>
                <Comment>Send DTMF string</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.11</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>alpha identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dtmf_string</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">AC</ItemTag>
                <SpecRef>12.17</SpecRef>
                <Comment>DTMF string</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgItem>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>Command parameters which includes a list of events about which the SIM requests a notification.</Section>
            </Description>
            <MsgDef>
                <Name>setup_event</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_EVENT_LIST</MsgID>
                <Comment>Setup Event List</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.11</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ev_list</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">99</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Event list</Comment>
            </MsgItem>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This is the parameter coding for a terminal response to a previous proactive SIM command.</Section>
            </Description>
            <MsgDef>
                <Name>term_resp</Name>
                <MsgID Direction="UPLINK" IDType="BIN">11100000</MsgID>
                <Comment>Terminal response</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.8</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cmd_details</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">81</ItemTag>
                <SpecRef>12.6</SpecRef>
                <Comment>Command details</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dev_ids</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">82</ItemTag>
                <SpecRef>12.7</SpecRef>
                <Comment>Device identities</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>res</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">83</ItemTag>
                <SpecRef>12.12</SpecRef>
                <Comment>Result</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dur</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">84</ItemTag>
                <SpecRef>12.8</SpecRef>
                <Comment>Duration</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>text</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">8D</ItemTag>
                <SpecRef>12.15</SpecRef>
                <Comment>Text string</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>item_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">90</ItemTag>
                <SpecRef>12.10</SpecRef>
                <Comment>Item identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cc_smc_loc_info</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">93</ItemTag>
                <SpecRef>12.19</SpecRef>
                <Comment>CC and SMC Location Information</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>imei</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">94</ItemTag>
                <SpecRef>12.20</SpecRef>
                <Comment>IMEI</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ntw_msr_res</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">96</ItemTag>
                <SpecRef>12.22</SpecRef>
                <Comment>Network measurement results</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>bcch_list</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">9D</ItemTag>
                <SpecRef>12.29</SpecRef>
                <Comment>BCCH channel list</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dtt</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">A6</ItemTag>
                <SpecRef>12.39</SpecRef>
                <Comment>Date-Time and Time zone</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cc_req_act</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">A7</ItemTag>
                <SpecRef>12.30</SpecRef>
                <Comment>CC requested action</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>res_2</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">83</ItemTag>
                <SpecRef>12.12</SpecRef>
                <Comment>Result 2</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>at_resp</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">A9</ItemTag>
                <SpecRef>12.41</SpecRef>
                <Comment>AT Response</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>chan_data</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">B6</ItemTag>
                <SpecRef>12.53</SpecRef>
                <Comment>Channel data</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>chan_stat</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">B8</ItemTag>
                <Control>
                    <TypeModifier>[1..7]</TypeModifier>
                </Control>
                <SpecRef>12.56</SpecRef>
                <Comment>Channel status</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>chan_dat_lth</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">B7</ItemTag>
                <SpecRef>12.54</SpecRef>
                <Comment>Channel data length</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>bear_desc</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">B5</ItemTag>
                <SpecRef>12.52</SpecRef>
                <Comment>Bearer Description</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>buffer_size</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">B9</ItemTag>
                <SpecRef>12.55</SpecRef>
                <Comment>Buffer size</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>lang</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">AD</ItemTag>
                <SpecRef>12.45</SpecRef>
                <Comment>Language Preferance</Comment>
            </MsgItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>add channel status, bearer description, buffer size</Comment>
            </History>
            <History>
                <Date Day="22" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>add channel data, add channel data length</Comment>
            </History>
            <History>
                <Date Day="28" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>added timer identifier, timer value</Comment>
            </History>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>channel status could exist more than once</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2002"/>
                <Author>AK</Author>
                <Comment>msg ID changed due to conflict with class e command ID's</Comment>
            </History>
            <History>
                <Date Day="12" Month="6" Year="2002"/>
                <Author>STW</Author>
                <Comment>changed Channel Data upper border to 241</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This is the parameter coding for a SIM envelope command.</Section>
            </Description>
            <MsgDef>
                <Name>env_cmd</Name>
                <MsgID Direction="UPLINK" IDType="BIN">11100001</MsgID>
                <Comment>Envelope command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.8</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cbd_cmd</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">D2</ItemTag>
                <SpecRef>7.2</SpecRef>
                <Comment>CB download command</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cc_cmd</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">D4</ItemTag>
                <SpecRef>9.1</SpecRef>
                <Comment>Call control command</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>smc_cmd</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">D5</ItemTag>
                <SpecRef>9.2</SpecRef>
                <Comment>MO-SM control command</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>evd_cmd</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">D6</ItemTag>
                <SpecRef>11</SpecRef>
                <Comment>Event download command</Comment>
            </MsgItem>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>MO-SM control and Event download added</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2002"/>
                <Author>AK</Author>
                <Comment>msg ID changed due to conflict with class e command ID's</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This is the parameter coding for a SIM Call Control result.</Section>
            </Description>
            <MsgDef>
                <Name>env_res</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">11100001</MsgID>
                <Comment>Envelope command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.8</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ccr_allw</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">00</ItemTag>
                <SpecRef>9.6</SpecRef>
                <Comment>Call control result, allowed</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ccr_not_allw</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">01</ItemTag>
                <SpecRef>9.6</SpecRef>
                <Comment>Call control result, not allowed</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ccr_allw_mdfy</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">02</ItemTag>
                <SpecRef>9.6</SpecRef>
                <Comment>Call control result, allowed with modification</Comment>
            </MsgItem>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2002"/>
                <Author>AK</Author>
                <Comment>msg ID changed due to conflict with class e command ID's</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This is the parameter coding for a SIM MO Short Message Control result.</Section>
            </Description>
            <MsgDef>
                <Name>env_res_smc</Name>
                <MsgID Direction="DOWNLINK" IDType="BIN">11100010</MsgID>
                <Comment>Envelope command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.8</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>smcr_allw</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">00</ItemTag>
                <SpecRef>9.6</SpecRef>
                <Comment>Call control result, allowed</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>smcr_not_allw</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">01</ItemTag>
                <SpecRef>9.6</SpecRef>
                <Comment>Call control result, not allowed</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>smcr_allw_mdfy</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">02</ItemTag>
                <SpecRef>9.6</SpecRef>
                <Comment>Call control result, allowed with modification</Comment>
            </MsgItem>
            <History>
                <Date Day="19" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="3" Month="5" Year="2002"/>
                <Author>AK</Author>
                <Comment>msg ID changed due to conflict with class e command ID's</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>parameter coding for SAT sending at commands to TE.</Section>
            </Description>
            <MsgDef>
                <Name>run_at</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_RUN_AT</MsgID>
                <Comment>Run AT command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.11</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>alpha identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>at_string</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">A8</ItemTag>
                <Control>
                    <TypeModifier>[MAX_CMD_AT_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.40</SpecRef>
                <Comment>AT string</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgItem>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>CLB</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This is the parameter coding for a proactive SIM open channel command, only class e.</Section>
            </Description>
            <MsgDef>
                <Name>open_channel</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_OPEN_CHANNEL</MsgID>
                <Comment>Open Channel command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.28</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>alpha identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>addr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">06</ItemTag>
                <SpecRef>12.1</SpecRef>
                <Comment>address</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>subaddr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>12.3</SpecRef>
                <Comment>subaddress</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dur</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>12.8</SpecRef>
                <Comment>duration</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dur2</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">04</ItemTag>
                <SpecRef>12.8</SpecRef>
                <Comment>duration2</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>bear_desc</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">B5</ItemTag>
                <SpecRef>12.52</SpecRef>
                <Comment>bearer description</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>buffer_size</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">B9</ItemTag>
                <SpecRef>12.55</SpecRef>
                <Comment>Buffer size</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>nan_buf</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">47</ItemTag>
                <SpecRef>12.61</SpecRef>
                <Comment>Network Acc Name</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>other_addr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">3E</ItemTag>
                <SpecRef>12.58</SpecRef>
                <Comment>other address</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>text</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>12.15</SpecRef>
                <Comment>Text string</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>text2</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>12.15</SpecRef>
                <Comment>Text string2</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>if_transp_lev</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">3C</ItemTag>
                <SpecRef>12.59</SpecRef>
                <Comment>IF transport level</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>data_dest_addr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">3E</ItemTag>
                <SpecRef>12.58</SpecRef>
                <Comment>Data dest address</Comment>
            </MsgItem>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="24" Month="5" Year="2002"/>
                <Author>AK</Author>
                <Comment>change n_acc_name to nan_buf</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This is the parameter coding for a proactive SIM close channel command, only class e.</Section>
            </Description>
            <MsgDef>
                <Name>close_channel</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_CLOSE_CHANNEL</MsgID>
                <Comment>Close Channel command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.28</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>alpha identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgItem>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This is the parameter coding for a proactive SIM Receive Data command, class e only.</Section>
                <Section>Reference : [1] section 6.6.29</Section>
            </Description>
            <MsgDef>
                <Name>receive_data</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_RECEIVE_DATA</MsgID>
                <Comment>Receive Data command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.29</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>alpha identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>chan_dat_lth</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">B7</ItemTag>
                <SpecRef>12.54</SpecRef>
                <Comment>Channel data length</Comment>
            </MsgItem>
            <History>
                <Date Day="26" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This is the parameter coding for a proactive SIM Send Data command, class e only.</Section>
                <Section>Reference : [1] section 6.6.30</Section>
            </Description>
            <MsgDef>
                <Name>send_data</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_SEND_DATA</MsgID>
                <Comment>Send Data command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.29</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>alpha identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>chan_data</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">B6</ItemTag>
                <SpecRef>12.53</SpecRef>
                <Comment>Channel data</Comment>
            </MsgItem>
            <History>
                <Date Day="26" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="4" Year="2002"/>
                <Author>STW</Author>
                <Comment>dynamic length of Channel Data element</Comment>
            </History>
            <History>
                <Date Day="12" Month="6" Year="2002"/>
                <Author>STW</Author>
                <Comment>changed Channel Data upper border to 241</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This is the parameter coding for a proactive SIM get channel status command, only class e.</Section>
            </Description>
            <MsgDef>
                <Name>get_cha_stat</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_GET_CHANNEL_STATUS</MsgID>
                <Comment>Get Channel Status command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.28</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </Message>
        <Message>
            <Description>
                <Section>This is the parameter coding for a proactive SIM launch browser command, only class c.</Section>
            </Description>
            <MsgDef>
                <Name>launch_browser</Name>
                <MsgID Direction="DOWNLINK" IDType="ALPHA">SAT_CMD_LAUNCH_BROWSER</MsgID>
                <Comment>Launch Browser command</Comment>
            </MsgDef>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>msg_type</Name>
                </ItemLink>
                <Type>GSM3_V</Type>
                <SpecRef>6.6.28</SpecRef>
                <Comment>Message Type</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>browser_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">30</ItemTag>
                <SpecRef>12.47</SpecRef>
                <Comment>Browser Identity</Comment>
            </MsgItem>
            <MsgItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>url</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">B1</ItemTag>
                <SpecRef>12.48</SpecRef>
                <Comment>Universal Res Loc</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>bearer</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">32</ItemTag>
                <Control>
                    <TypeModifier>[0..MAX_BEARER_LIST_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.49</SpecRef>
                <Comment>Bearer</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>prov_file_ref</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">33</ItemTag>
                <Control>
                    <TypeModifier>[0..MAX_PFP_ELEM]</TypeModifier>
                </Control>
                <SpecRef>12.50</SpecRef>
                <Comment>Prov File Reference</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>text</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">0D</ItemTag>
                <SpecRef>12.15</SpecRef>
                <Comment>Text string</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[0..MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>alpha identifier</Comment>
            </MsgItem>
            <MsgItem Presentation="OPTIONAL">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1E</ItemTag>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgItem>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="4" Year="2002"/>
                <Author>RIE</Author>
                <Comment>url, prov_file_ref changed</Comment>
            </History>
            <History>
                <Date Day="5" Month="9" Year="2002"/>
                <Author>RM</Author>
                <Comment>Rebase</Comment>
            </History>
        </Message>
    </MessagesSection>
    <MsgStructElementsSection>
        <Description>
            <Section>This section contains all structured elements that are defined for the SAT AIM</Section>
        </Description>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 6.6</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>pas_cmd</Name>
                <Comment>Proactive SIM Command</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cmd_details</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">81</ItemTag>
                <SpecRef>12.6</SpecRef>
                <Comment>Command details</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dev_ids</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">82</ItemTag>
                <SpecRef>12.7</SpecRef>
                <Comment>Device identities</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cmd_prms</Name>
                </ItemLink>
                <Type>GSM5_V</Type>
                <SpecRef>12</SpecRef>
                <Comment>Command parameters</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.6</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cmd_details</Name>
                <Comment>Command details</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cmd_nr</Name>
                </ItemLink>
                <SpecRef>12.6</SpecRef>
                <Comment>Command number</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cmd_typ</Name>
                </ItemLink>
                <SpecRef>12.6</SpecRef>
                <Comment>Command type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cmd_qlf</Name>
                </ItemLink>
                <SpecRef>12.6</SpecRef>
                <Comment>Command qualifier</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.7</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>dev_ids</Name>
                <Comment>Device identities</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>src_dev</Name>
                </ItemLink>
                <SpecRef>12.7</SpecRef>
                <Comment>Source device</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dest_dev</Name>
                </ItemLink>
                <SpecRef>12.7</SpecRef>
                <Comment>Destination device</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] 12.14</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ss_string</Name>
                <Comment>SS string</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>noa</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Nature of address</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>npi</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Numbering plan identification</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ss_ctrl_string</Name>
                </ItemLink>
                <Type>BCDEVEN</Type>
                <Control>
                    <TypeModifier>[0..MAX_SS_STRING_LEN]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>SS control string</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] 12.1</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>addr</Name>
                <Comment>Address</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>noa</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Nature of address</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>npi</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Numbering plan identification</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>bcdDigit</Name>
                </ItemLink>
                <Type>BCDEVEN</Type>
                <Control>
                    <TypeModifier>[0..MAX_PARTY_NUM_SAT]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>BCD digit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="9" Year="2000"/>
                <Author>FK</Author>
                <Comment>Name for number of digits changed</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] Annex 12.3</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>subaddr</Name>
                <Comment>Subaddress</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>tos</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Type of subaddress</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>oei</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Odd/even indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>000</Pattern>
                    <BitLen>3</BitLen>
                </Spare>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>bcdDigit</Name>
                </ItemLink>
                <Type>BCDEVEN</Type>
                <Control>
                    <TypeModifier>[0..MAX_SUBADDR_NUM]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>BCD digit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.12</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>res</Name>
                <Comment>Result</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>res_2</Name>
                <Comment>Result 2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>gen</Name>
                </ItemLink>
                <SpecRef>12.12</SpecRef>
                <Comment>General result</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>add</Name>
                </ItemLink>
                <Type>GSM5_V</Type>
                <SpecRef>12.12</SpecRef>
                <Comment>Additional information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.12</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>text</Name>
                <Comment>Text string</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>text2</Name>
                <Comment>Text string2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dcs</Name>
                </ItemLink>
                <SpecRef>12.15</SpecRef>
                <Comment>Data coding scheme</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>text_str</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..MAX_TEXT_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.15</SpecRef>
                <Comment>text string</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.10</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>item_id</Name>
                <Comment>Item identifier</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>item</Name>
                </ItemLink>
                <SpecRef>12.10</SpecRef>
                <Comment>Choosen item</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.19</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cc_smc_loc_info</Name>
                <Comment>CC and SMC Location Information</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>mnc_mcc</Name>
                </ItemLink>
                <SpecRef>12.19</SpecRef>
                <Comment>MNC and MCC</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>lac</Name>
                </ItemLink>
                <SpecRef>12.19</SpecRef>
                <Comment>Location Area Code</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cid</Name>
                </ItemLink>
                <SpecRef>12.19</SpecRef>
                <Comment>Cell Identity Value</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 7.2</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cbd_cmd</Name>
                <Comment>CB download</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dev_ids</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">82</ItemTag>
                <SpecRef>12.7</SpecRef>
                <Comment>Device identities</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cb_page</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">8C</ItemTag>
                <SpecRef>12.5</SpecRef>
                <Comment>Cell broadcast page</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 9.1.6</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cc_cmd</Name>
                <Comment>Call control</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dev_ids</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">82</ItemTag>
                <SpecRef>12.7</SpecRef>
                <Comment>Device identities</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>addr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">86</ItemTag>
                <SpecRef>12.1</SpecRef>
                <Comment>Address</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ss_string</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">89</ItemTag>
                <SpecRef>12.14</SpecRef>
                <Comment>SS string</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ussd_string</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">8A</ItemTag>
                <SpecRef>12.17</SpecRef>
                <Comment>USSD string</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cap_cnf_parms</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">07</ItemTag>
                <SpecRef>12.4</SpecRef>
                <Comment>Capabilitiy configuration parameter 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>subaddr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>12.3</SpecRef>
                <Comment>Subaddress</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cc_smc_loc_info</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">13</ItemTag>
                <SpecRef>12.19</SpecRef>
                <Comment>CC and SMC Location Information</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cap_cnf_parms_2</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">07</ItemTag>
                <SpecRef>12.4</SpecRef>
                <Comment>Capabilitiy configuration parameter 2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="19" Month="4" Year="1999"/>
                <Author>AK</Author>
                <Comment>Location information added</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2000"/>
                <Author>FK</Author>
                <Comment>USSD String added</Comment>
            </History>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Capability Configuration Parameter 2 added</Comment>
            </History>
            <History>
                <Date Day="16" Month="3" Year="2001"/>
                <Author>FK</Author>
                <Comment>CR flag of tag 'Location Information' unset (Clause 9.1.6)</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] section 9.1.6</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ccr_allw</Name>
                <Comment>Call control result, allowed</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>ccr_not_allw</Name>
                <Comment>Call control result, not allowed</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>ccr_allw_mdfy</Name>
                <Comment>Call Control result, allowed with modifications</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>addr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">06</ItemTag>
                <SpecRef>12.1</SpecRef>
                <Comment>Address</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ss_string</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">09</ItemTag>
                <SpecRef>12.14</SpecRef>
                <Comment>SS string</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ussd_string</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">0A</ItemTag>
                <SpecRef>12.17</SpecRef>
                <Comment>USSD string</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cap_cnf_parms</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">07</ItemTag>
                <SpecRef>12.4</SpecRef>
                <Comment>Capabilitiy conf. parameter 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>subaddr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>12.3</SpecRef>
                <Comment>Subaddress</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>Alpha identifier</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>bc_rpi</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">2A</ItemTag>
                <SpecRef>12.42</SpecRef>
                <Comment>BC Repeat Indicator</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cap_cnf_parms_2</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">07</ItemTag>
                <SpecRef>12.4</SpecRef>
                <Comment>Capabilitiy conf. parameter 2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="9" Year="2000"/>
                <Author>FK</Author>
                <Comment>Alpha Identifier without CR flag</Comment>
            </History>
            <History>
                <Date Day="28" Month="9" Year="2000"/>
                <Author>FK</Author>
                <Comment>USSD String added</Comment>
            </History>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>BC Repeat Indicator and CCP 2 added</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.8</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>dur</Name>
                <Comment>Duration</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>dur2</Name>
                <Comment>Duration2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>time_unit</Name>
                </ItemLink>
                <SpecRef>12.8</SpecRef>
                <Comment>Time unit</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>time_ivl</Name>
                </ItemLink>
                <SpecRef>12.8</SpecRef>
                <Comment>Time interval</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.17</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ussd_string</Name>
                <Comment>USSD string</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dcs</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Data coding scheme</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ussd_str</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..MAX_SAT_USSD_LEN]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>USSD string</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.13</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>smpdu</Name>
                <Comment>SMS TPDU</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>tpdu_data</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[7..MAX_SMS_TPDU_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.13</SpecRef>
                <Comment>Short Message Data</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.31</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>icon</Name>
                <Comment>Icon Identifier</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>icon_2</Name>
                <Comment>Icon Identifier</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon_qu</Name>
                </ItemLink>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Qualifier</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>icon_id</Name>
                </ItemLink>
                <SpecRef>12.31</SpecRef>
                <Comment>Icon Identifier</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="17" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.25</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ev_list</Name>
                <Comment>Event list</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>event</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[1..MAX_EVENT_LIST_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.25</SpecRef>
                <Comment>List of events</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="17" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.44</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>dtmf_string</Name>
                <Comment>DTMF string</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>bcdDigit</Name>
                </ItemLink>
                <Type>BCDEVEN</Type>
                <Control>
                    <TypeModifier>[0..MAX_DTMF_LEN]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>BCD digit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.28</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ti_oct</Name>
                <Comment>Transaction Identifier octet</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>Transaction Identifier</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <Spare>
                    <Pattern>0000</Pattern>
                    <BitLen>4</BitLen>
                </Spare>
                <SpecRef>-</SpecRef>
                <Comment>Spare</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.28</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>ti_list</Name>
                <Comment>Transaction identifier list</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ti_oct</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[1..MAX_TI_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.28</SpecRef>
                <Comment>Single Transaction Identifier</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.25</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>cause</Name>
                <Comment>Cause information element</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cs</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..MAX_CAUSE_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.26</SpecRef>
                <Comment>Cause</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] 12.1</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>sm_addr</Name>
                <Comment>Address 1</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>sm_addr_2</Name>
                <Comment>Address 2</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>noa</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>+</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Nature of address</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>npi</Name>
                </ItemLink>
                <Control>
                    <BitGroupDef>*</BitGroupDef>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Numbering plan identification</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>bcdDigit</Name>
                </ItemLink>
                <Type>BCDEVEN</Type>
                <Control>
                    <TypeModifier>[0..MAX_SMS_DIGIT_LEN]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>BCD digit</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 9.2.2</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>smc_cmd</Name>
                <Comment>Call control</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dev_ids</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">82</ItemTag>
                <SpecRef>12.7</SpecRef>
                <Comment>Device identities</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>sm_addr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">86</ItemTag>
                <SpecRef>12.1</SpecRef>
                <Comment>Short Message Address 1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>sm_addr_2</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">86</ItemTag>
                <SpecRef>12.1</SpecRef>
                <Comment>Short Message Address 2</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cc_smc_loc_info</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">93</ItemTag>
                <SpecRef>12.19</SpecRef>
                <Comment>CC and SMC Location Information</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="19" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 9.2.2</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>smcr_allw</Name>
                <Comment>Call control result, allowed</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>smcr_not_allw</Name>
                <Comment>Call control result, not allowed</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>smcr_allw_mdfy</Name>
                <Comment>Call Control result, allowed with modifications</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>sm_addr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">06</ItemTag>
                <SpecRef>12.1</SpecRef>
                <Comment>Service Center Address</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>sm_addr_2</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">06</ItemTag>
                <SpecRef>12.1</SpecRef>
                <Comment>Destination Address</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>alpha_id</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">05</ItemTag>
                <Control>
                    <TypeModifier>[MAX_ALPHA_ID_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.2</SpecRef>
                <Comment>Alpha identifier</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="19" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 11</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>evd_cmd</Name>
                <Comment>Call control</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ev_list</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">99</ItemTag>
                <SpecRef>12.25</SpecRef>
                <Comment>Event list</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>dev_ids</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">82</ItemTag>
                <SpecRef>12.7</SpecRef>
                <Comment>Device identities</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ti_list</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">9C</ItemTag>
                <SpecRef>12.28</SpecRef>
                <Comment>Transaction identifier list</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>addr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">06</ItemTag>
                <SpecRef>12.1</SpecRef>
                <Comment>Address</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>subaddr</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">08</ItemTag>
                <SpecRef>12.3</SpecRef>
                <Comment>Subaddress</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">1A</ItemTag>
                <SpecRef>12.26</SpecRef>
                <Comment>Cause information element</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>loc_state</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">9B</ItemTag>
                <SpecRef>12.27</SpecRef>
                <Comment>Location status</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>cc_smc_loc_info</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">13</ItemTag>
                <SpecRef>12.19</SpecRef>
                <Comment>CC and SMC Location Information</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>brows_term_cause</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">35</ItemTag>
                <SpecRef>12.51</SpecRef>
                <Comment>Browser Termination cause</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>chan_stat</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">B8</ItemTag>
                <SpecRef>12.56</SpecRef>
                <Comment>Channel status</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>chan_dat_lth</Name>
                </ItemLink>
                <Type>GSM5_TLV</Type>
                <ItemTag TagType="HEX">B7</ItemTag>
                <SpecRef>12.54</SpecRef>
                <Comment>Channel data length</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="19" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Browser Termination Cause, Channel status added</Comment>
            </History>
            <History>
                <Date Day="25" Month="3" Year="2001"/>
                <Author>JK</Author>
                <Comment>Channel data length added</Comment>
            </History>
            <History>
                <Date Day="7" Month="6" Year="2002"/>
                <Author>JK</Author>
                <Comment>Channel status ID corrected from 38 to B8 (Mandatory)</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.41</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>at_resp</Name>
                <Comment>AT response</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>text_str</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..MAX_CMD_AT_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.41</SpecRef>
                <Comment>text string</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="7" Month="11" Year="2001"/>
                <Author>CLB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.52</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>bear_desc</Name>
                <Comment>Bearer description</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>bear_type</Name>
                </ItemLink>
                <SpecRef>12.52</SpecRef>
                <Comment>Bearer type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>csd_bear_prm</Name>
                </ItemLink>
                <Control>
                    <Condition>bear_type = 1</Condition>
                </Control>
                <SpecRef>12.52.1</SpecRef>
                <Comment>CSD bearer parameter</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>gprs_bear_prm</Name>
                </ItemLink>
                <Control>
                    <Condition>bear_type = 2</Condition>
                </Control>
                <SpecRef>12.52.2</SpecRef>
                <Comment>GPRS bearer parameter</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>use control column for separation of bearer parameter</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.53</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_data</Name>
                <Comment>Channel data</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ch_dat_str</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..241]</TypeModifier>
                </Control>
                <SpecRef>12.53</SpecRef>
                <Comment>Channel data string</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="25" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="4" Year="2002"/>
                <Author>STW</Author>
                <Comment>dynamic Channel Data element</Comment>
            </History>
            <History>
                <Date Day="12" Month="6" Year="2002"/>
                <Author>STW</Author>
                <Comment>changed Channel Data upper border to 241</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.58</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>other_addr</Name>
                <Comment>Other Address</Comment>
            </MsgStructElemDef>
            <MsgStructElemDef Type="STRUCT">
                <Name>data_dest_addr</Name>
                <Comment>Data Destination Address</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>oth_addr_type</Name>
                </ItemLink>
                <SpecRef>12.58</SpecRef>
                <Comment>Other Address  type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ipv4_addr</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[4]</TypeModifier>
                    <Condition>oth_addr_type = 0x21</Condition>
                </Control>
                <SpecRef>12.58</SpecRef>
                <Comment>IPv4 parameter</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>ipv6_addr</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[16]</TypeModifier>
                    <Condition>oth_addr_type = 0x57</Condition>
                </Control>
                <SpecRef>12.58</SpecRef>
                <Comment>IPv6 parameter</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>use control column for separation of ip addresses</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.59</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>if_transp_lev</Name>
                <Comment>Interface transport level</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>trans_prot_type</Name>
                </ItemLink>
                <SpecRef>12.59</SpecRef>
                <Comment>Transport protocol type</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>port_number</Name>
                </ItemLink>
                <SpecRef>12.59</SpecRef>
                <Comment>Port number</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.47</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>browser_id</Name>
                <Comment>Browser Identity</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>browser</Name>
                </ItemLink>
                <SpecRef>12.47</SpecRef>
                <Comment>Browser Identity</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.48</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>url</Name>
                <Comment>URL</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>url_value</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..MAX_URL_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.48</SpecRef>
                <Comment>URL Value</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="4" Year="2002"/>
                <Author>RIE</Author>
                <Comment>change url_value to a array</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.50</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>prov_file_ref</Name>
                <Comment>Provisioning File Reference</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>prov_file_id</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..MAX_PROV_F_PATH_LEN]</TypeModifier>
                </Control>
                <SpecRef>12.50</SpecRef>
                <Comment>Provisioning File Path Id</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="25" Month="4" Year="2002"/>
                <Author>RIE</Author>
                <Comment>prov_file_id changed</Comment>
            </History>
            <History>
                <Date Day="1" Month="11" Year="2002"/>
                <Author>RM</Author>
                <Comment>prov_file_id changed: no ID, no type are allowed</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.51</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>brows_term_cause</Name>
                <Comment>Browser Termination Cause</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>brows_term_s</Name>
                </ItemLink>
                <SpecRef>12.51</SpecRef>
                <Comment>Browser Termination Source</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] section 12.56</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>chan_stat</Name>
                <Comment>Channel Status Parameter</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>chan_stat_link</Name>
                </ItemLink>
                <SpecRef>12.56</SpecRef>
                <Comment>Channel Status Link</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>chan_stat_inf1</Name>
                </ItemLink>
                <SpecRef>12.56</SpecRef>
                <Comment>Channel Status Information1</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>chan_id</Name>
                </ItemLink>
                <SpecRef>12.56</SpecRef>
                <Comment>Channel Identifier</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>chan_stat_inf2</Name>
                </ItemLink>
                <SpecRef>12.56</SpecRef>
                <Comment>Channel Status Information2</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Parameter specific to the CSD bearer.</Section>
                <Section>Reference : [1] section 12.61</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>csd_bear_prm</Name>
                <Comment>CSD bearer parameter</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>csd_speed</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CSD speed</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>csd_name</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CSD name</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>csd_ce</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>CSD connection elem</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Parameter specific to the GPRS bearer.</Section>
                <Section>Reference : [1] section 12.61</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>gprs_bear_prm</Name>
                <Comment>GPRS bearer parameter</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>gprs_prec</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS precedence</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>gprs_delay</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS delay</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>gprs_rely</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS reliability</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>gprs_peak</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS peak throughput</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>gprs_mean</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS mean throughput</Comment>
            </MsgStructElemItem>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>gprs_pdp_type</Name>
                </ItemLink>
                <SpecRef>-</SpecRef>
                <Comment>GPRS PDP type</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Buffer for Network access name (APN).</Section>
                <Section>Reference : [1] section 12.61</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>nan_buf</Name>
                <Comment>Network access name buffer</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>n_acc_name</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..MAX_SAT_APN_LEN]</TypeModifier>
                </Control>
                <SpecRef>-</SpecRef>
                <Comment>Network access name</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="24" Month="5" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section>Reference : [1] sections 12.39</Section>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>dtt</Name>
                <Comment>Date-Time and Time zone</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>text_str</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..7]</TypeModifier>
                </Control>
                <SpecRef>12.39</SpecRef>
                <Comment>text string</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="23" Month="5" Year="2002"/>
                <Author>TLU</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
        <MsgStructElem>
            <Description>
                <Section/>
            </Description>
            <MsgStructElemDef Type="STRUCT">
                <Name>lang</Name>
                <Comment>language Preferance</Comment>
            </MsgStructElemDef>
            <MsgStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="AIM">sat</DocName>
                    <Name>lang_buf</Name>
                </ItemLink>
                <Control>
                    <TypeModifier>[0..2]</TypeModifier>
                </Control>
                <SpecRef>12.45</SpecRef>
                <Comment>text string</Comment>
            </MsgStructElemItem>
            <History>
                <Date Day="29" Month="09" Year="2005"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgStructElem>
    </MsgStructElementsSection>
    <MsgBasicElementsSection>
        <Description>
            <Section>This section contains all basic elements that are defined for the SAT AIM</Section>
        </Description>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cmd_prms</Name>
                <BitLen>1952</BitLen>
                <Comment>Parameters</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Maximum possible bytes is 244</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.6</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cmd_nr</Name>
                <BitLen>8</BitLen>
                <Comment>Command number</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.6 and 13.4</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cmd_typ</Name>
                <BitLen>8</BitLen>
                <Comment>Command type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_cmd_typ</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="9" Year="2000"/>
                <Author>FK</Author>
                <Comment>Class 3 commands added</Comment>
            </History>
            <History>
                <Date Day="4" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>Class c and e commands added</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.6</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cmd_qlf</Name>
                <BitLen>8</BitLen>
                <Comment>Command qualifier</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_cmd_qlf</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>Additionsfor class c and e</Comment>
            </History>
            <History>
                <Date Day="23" Month="5" Year="2002"/>
                <Author>TLU</Author>
                <Comment>QLF_PLOI_DTT added</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.7</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>src_dev</Name>
                <BitLen>8</BitLen>
                <Comment>Source device</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_src_dev</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>Additions for class c and e</Comment>
            </History>
            <History>
                <Date Day="17" Month="02" Year="2004"/>
                <Author>KJF</Author>
                <Comment>added card reader</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.7</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dest_dev</Name>
                <BitLen>8</BitLen>
                <Comment>Destination device</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_dest_dev</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="5" Month="4" Year="2002"/>
                <Author>STW</Author>
                <Comment>Additions for class c and e</Comment>
            </History>
            <History>
                <Date Day="17" Month="02" Year="2004"/>
                <Author>KJF</Author>
                <Comment>added card reader</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.2</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>alpha_id</Name>
                <BitLen>8</BitLen>
                <Comment>Alpha identifier</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.2</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>alpha_id_2</Name>
                <BitLen>8</BitLen>
                <Comment>Alpha identifier</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.14</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ss_ctrl_string</Name>
                <BitLen>4</BitLen>
                <Comment>SS control string</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.4</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cap_cnf_parms</Name>
                <BitLen>MAX_CAP_CNF_LEN</BitLen>
                <Comment>Capability configuration parameter 1</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.4</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cap_cnf_parms_2</Name>
                <BitLen>MAX_CAP_CNF_LEN</BitLen>
                <Comment>Capability configuration parameter 2</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.7</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>time_unit</Name>
                <BitLen>8</BitLen>
                <Comment>Time unit</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_time_unit</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.8</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>time_ivl</Name>
                <BitLen>8</BitLen>
                <Comment>Time interval</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>This element is only defined for orthogonality of the CCD messages. This element is not really present in the facility element.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>msg_type</Name>
                <BitLen>8</BitLen>
                <Comment>Message type</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 14.7.8</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>noa</Name>
                <BitLen>3</BitLen>
                <Comment>Nature of address</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_noa</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] section 14.7.8</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>npi</Name>
                <BitLen>4</BitLen>
                <Comment>Numbering plan indication</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_npi</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Defines a BCD digit for the packed representation.</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bcdDigit</Name>
                <BitLen>4</BitLen>
                <Comment>BCD digit</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.7</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gen</Name>
                <BitLen>8</BitLen>
                <Comment>General result</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_gen</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="7" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>Addisions for class e</Comment>
            </History>
            <History>
                <Date Day="23" Month="5" Year="2002"/>
                <Author>TLU</Author>
                <Comment>RSLT_PERF_LIM_SRV added</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.7</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>add</Name>
                <BitLen>1952</BitLen>
                <Comment>Additional information</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_add</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="19" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Length aligned</Comment>
            </History>
            <History>
                <Date Day="7" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>Addisions for class c and e</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.15, 12.17</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>dcs</Name>
                <BitLen>8</BitLen>
                <Comment>Data coding scheme</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.15</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>text_str</Name>
                <BitLen>8</BitLen>
                <Comment>Text string</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.10</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>item</Name>
                <BitLen>8</BitLen>
                <Comment>Choosen item</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="12" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.19</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>mnc_mcc</Name>
                <BitLen>24</BitLen>
                <Comment>MNC and MCC</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.19</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>lac</Name>
                <BitLen>16</BitLen>
                <Comment>Location area code</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.19</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cid</Name>
                <BitLen>16</BitLen>
                <Comment>Cell identity value</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.20</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>imei</Name>
                <BitLen>64</BitLen>
                <Comment>IMEI</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.22</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ntw_msr_res</Name>
                <BitLen>128</BitLen>
                <Comment>Network measurement results</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.29</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bcch_list</Name>
                <BitLen>384</BitLen>
                <Comment>BCCH channel list</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.5</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cb_page</Name>
                <BitLen>704</BitLen>
                <Comment>Cell broadcast page</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.30</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cc_req_act</Name>
                <BitLen>1936</BitLen>
                <Comment>CC requested action</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="14" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="19" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Length aligned</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] section 10.5.4.8</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>tos</Name>
                <BitLen>3</BitLen>
                <Comment>Type of subaddress</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_tos</Name>
            </ValuesLink>
            <History>
                <Date Day="19" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [2] section 10.5.4.8</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>oei</Name>
                <BitLen>1</BitLen>
                <Comment>Odd/even indicator</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_oei</Name>
            </ValuesLink>
            <History>
                <Date Day="19" Month="7" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.13</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>tpdu_data</Name>
                <BitLen>8</BitLen>
                <Comment>Short Message Data</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="7" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.17</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ussd_str</Name>
                <BitLen>8</BitLen>
                <Comment>USSD string</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="28" Month="9" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.31</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>icon_qu</Name>
                <BitLen>8</BitLen>
                <Comment>Icon Qualifier</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="17" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.31</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>icon_id</Name>
                <BitLen>8</BitLen>
                <Comment>Icon Identifier</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="17" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.25</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>event</Name>
                <BitLen>8</BitLen>
                <Comment>List of events</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_event</Name>
            </ValuesLink>
            <History>
                <Date Day="17" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="4" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>Event values for class c and e</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.28</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ti</Name>
                <BitLen>4</BitLen>
                <Comment>Transaction Identifier</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.26</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>cs</Name>
                <BitLen>8</BitLen>
                <Comment>Cause</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.42</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bc_rpi</Name>
                <BitLen>8</BitLen>
                <Comment>BC Repeat Indicator</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_bc_rpi</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.27</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>loc_state</Name>
                <BitLen>8</BitLen>
                <Comment>Location status</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_loc_state</Name>
            </ValuesLink>
            <History>
                <Date Day="19" Month="10" Year="2000"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.40</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>at_string</Name>
                <BitLen>8</BitLen>
                <Comment>AT string</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="28" Month="10" Year="2001"/>
                <Author>CLB</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.52.1, 12.52.2</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>csd_speed</Name>
                <BitLen>8</BitLen>
                <Comment>CSD speed</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="8" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.52.1, 12.52.2</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>csd_name</Name>
                <BitLen>8</BitLen>
                <Comment>CSD name</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="8" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.52.1, 12.52.2</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>csd_ce</Name>
                <BitLen>8</BitLen>
                <Comment>CSD connection elem</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="8" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.52.1, 12.52.2</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_prec</Name>
                <BitLen>8</BitLen>
                <Comment>GPRS precedence</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="8" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.52.1, 12.52.2</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_delay</Name>
                <BitLen>8</BitLen>
                <Comment>GPRS delay</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="8" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.52.1, 12.52.2</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_rely</Name>
                <BitLen>8</BitLen>
                <Comment>GPRS reliability</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="8" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.52.1, 12.52.2</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_peak</Name>
                <BitLen>8</BitLen>
                <Comment>GPRS peak throughput</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="8" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.52.1, 12.52.2</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_mean</Name>
                <BitLen>8</BitLen>
                <Comment>GPRS mean throughput</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="8" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.52.2</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>gprs_pdp_type</Name>
                <BitLen>8</BitLen>
                <Comment>GPRS PDP type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_gprs_pdp_type</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.53</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ch_dat_str</Name>
                <BitLen>8</BitLen>
                <Comment>Channel data string</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="26" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.54</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_dat_lth</Name>
                <BitLen>8</BitLen>
                <Comment>Channel data length</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="26" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Requested or offered No of bytes. Reference : [1] section 12.55</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>buffer_size</Name>
                <BitLen>16</BitLen>
                <Comment>Buffer size</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="26" Month="3" Year="2002"/>
                <Author>JK</Author>
                <Comment>bit len corrected</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.58</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>oth_addr_type</Name>
                <BitLen>8</BitLen>
                <Comment>Type of local Address</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_oth_addr_type</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.58</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ipv4_addr</Name>
                <BitLen>8</BitLen>
                <Comment>IPv4 address</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>changed to ipv4/ipv6 address</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.58</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>ipv6_addr</Name>
                <BitLen>8</BitLen>
                <Comment>IPv6 address</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>changed to ipv4/ipv6 address</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.59</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>trans_prot_type</Name>
                <BitLen>8</BitLen>
                <Comment>Transport protocol type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_trans_prot_type</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.59</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>port_number</Name>
                <BitLen>16</BitLen>
                <Comment>Port number</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.47</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>browser</Name>
                <BitLen>8</BitLen>
                <Comment>Browser</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_browser</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.48</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>url_value</Name>
                <BitLen>8</BitLen>
                <Comment>URL value</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.49</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bearer</Name>
                <BitLen>8</BitLen>
                <Comment>Bearer List</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_bearer</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.50</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>prov_file_id</Name>
                <BitLen>8</BitLen>
                <Comment>Provisioning File Path Id</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.51</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>brows_term_s</Name>
                <BitLen>8</BitLen>
                <Comment>Browser Termination Source</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_brows_term_s</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.56</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_id</Name>
                <BitLen>3</BitLen>
                <Comment>Channel Status Identifier</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_chan_id</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.56</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_stat_inf1</Name>
                <BitLen>4</BitLen>
                <Comment>Channel Status Information1</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_chan_stat_inf1</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.56</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_stat_link</Name>
                <BitLen>1</BitLen>
                <Comment>Channel Status Link</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_chan_stat_link</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.56</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>chan_stat_inf2</Name>
                <BitLen>8</BitLen>
                <Comment>Channel Status Information2</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_chan_stat_inf2</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.61</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>n_acc_name</Name>
                <BitLen>8</BitLen>
                <Comment>Network Access name</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="18" Month="3" Year="2002"/>
                <Author>RM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>Changed to network access name</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section>Reference : [1] section 12.52</Section>
            </Description>
            <MsgBasicElemDef>
                <Name>bear_type</Name>
                <BitLen>8</BitLen>
                <Comment>Bearer type</Comment>
            </MsgBasicElemDef>
            <ValuesLink>
                <DocName DocType="AIM">sat</DocName>
                <Name>VAL_bear_type</Name>
            </ValuesLink>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
        <MsgBasicElem>
            <Description>
                <Section/>
            </Description>
            <MsgBasicElemDef>
                <Name>lang_buf</Name>
                <BitLen>8</BitLen>
                <Comment>Provide Local Info/Language Setting</Comment>
            </MsgBasicElemDef>
            <History>
                <Date Day="29" Month="09" Year="2005"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </MsgBasicElem>
    </MsgBasicElementsSection>
    <ValuesSection>
        <Description>
            <Section>This section contains all sets of values that are defined for the SAT AIM</Section>
        </Description>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_cmd_typ</Name>
                <Comment>values for cmd_typ</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>SAT_CMD_REFRESH</Alias>
                <Comment>Refresh command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>SAT_CMD_MORE_TIME</Alias>
                <Comment>More time command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>SAT_CMD_POLL_INTERVAL</Alias>
                <Comment>Poll interval command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>SAT_CMD_POLL_OFF</Alias>
                <Comment>Polling off command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">05</Value>
                <Alias>SAT_CMD_EVENT_LIST</Alias>
                <Comment>Setup event list command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">10</Value>
                <Alias>SAT_CMD_SETUP_CALL</Alias>
                <Comment>Set up call command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">11</Value>
                <Alias>SAT_CMD_SEND_SS</Alias>
                <Comment>Send SS command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">12</Value>
                <Alias>SAT_CMD_SEND_USSD</Alias>
                <Comment>Send USSD Command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">13</Value>
                <Alias>SAT_CMD_SEND_SMS</Alias>
                <Comment>Send Short Message command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">14</Value>
                <Alias>SAT_CMD_SEND_DTMF</Alias>
                <Comment>Send DTMF command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">15</Value>
                <Alias>SAT_CMD_LAUNCH_BROWSER</Alias>
                <Comment>Launch WWW Browser class c</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">20</Value>
                <Alias>SAT_CMD_PLAY_TONE</Alias>
                <Comment>Play tone command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">21</Value>
                <Alias>SAT_CMD_DISPLAY_TEXT</Alias>
                <Comment>Display text command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">22</Value>
                <Alias>SAT_CMD_GET_INKEY</Alias>
                <Comment>Get inkey command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">23</Value>
                <Alias>SAT_CMD_GET_INPUT</Alias>
                <Comment>Get input command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">24</Value>
                <Alias>SAT_CMD_SEL_ITEM</Alias>
                <Comment>Select item command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">25</Value>
                <Alias>SAT_CMD_SETUP_MENU</Alias>
                <Comment>Set up menu command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">26</Value>
                <Alias>SAT_CMD_PROV_LOC_INFO</Alias>
                <Comment>Provide loacal information command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">27</Value>
                <Alias>SAT_CMD_TIMER_MNG</Alias>
                <Comment>Timer Managemant command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">28</Value>
                <Alias>SAT_CMD_IDLE_TEXT</Alias>
                <Comment>Set up idle mode text command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">34</Value>
                <Alias>SAT_CMD_RUN_AT</Alias>
                <Comment>Run AT command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">40</Value>
                <Alias>SAT_CMD_OPEN_CHANNEL</Alias>
                <Comment>Open data channel for CS or GPRS              class e</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">41</Value>
                <Alias>SAT_CMD_CLOSE_CHANNEL</Alias>
                <Comment>Close data channel                                  class e</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">42</Value>
                <Alias>SAT_CMD_RECEIVE_DATA</Alias>
                <Comment>Receive data from ME from the channel     class e</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">43</Value>
                <Alias>SAT_CMD_SEND_DATA</Alias>
                <Comment>Send the data to the channel via ME         class e</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">44</Value>
                <Alias>SAT_CMD_GET_CHANNEL_STATUS</Alias>
                <Comment>Get the status of the data channel opened class e</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">81</Value>
                <Alias>SAT_CMD_END_SESSION</Alias>
                <Comment>End of proactive session command</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_cmd_qlf</Name>
                <Comment>values for cmd_qlf</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>QLF_RFSH_INIT</Alias>
                <Comment>Refresh: SIM initialization</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>QLF_RFSH_INIT_FULL_CHNG_NTFY</Alias>
                <Comment>Refresh: SIM initialization and full file change notification</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>QLF_RFSH_FILE_CHNG_NTFY</Alias>
                <Comment>Refresh: File change notification</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>QLF_RFSH_INIT_FILE_CHNG_NTFY</Alias>
                <Comment>Refresh: SIM initialization and file change notification</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>QLF_RFSH_RESET</Alias>
                <Comment>Refresh: SIM reset</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>QLF_CALL_IDLE</Alias>
                <Comment>Set up call: idle</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>QLF_CALL_IDLE_RDL</Alias>
                <Comment>Set up call: idle with redial</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>QLF_CALL_HOLD</Alias>
                <Comment>Set up call: hold</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>QLF_CALL_HOLD_RDL</Alias>
                <Comment>Set up call: hold with redial</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>QLF_CALL_DISC</Alias>
                <Comment>Set up call: disconnect</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">05</Value>
                <Alias>QLF_CALL_DISC_RDL</Alias>
                <Comment>Set up call: disconnect with redial</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_SMS_NO_PACK</Alias>
                <Comment>Send SMS: packing not required</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias>QLF_SMS_PACK</Alias>
                <Comment>Send SMS: packing required</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_DISP_PRIO_NORM</Alias>
                <Comment>Display text: normal priority</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias>QLF_DISP_PRIO_HIGH</Alias>
                <Comment>Display text: high priority</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_DISP_CLR_DELAY</Alias>
                <Comment>Display text: clear message after delay</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10000000</Value>
                <Alias>QLF_DISP_CLR_USER</Alias>
                <Comment>Display text: wait for user to clear message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_INKY_DIGITS</Alias>
                <Comment>Get inkey: digits (0-9, *,# and +) only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias>QLF_INKY_ALPHA</Alias>
                <Comment>Get inkey: alphabet set</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_INKY_SMS_DEF</Alias>
                <Comment>Get inkey; SMS default alphabet</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000010</Value>
                <Alias>QLF_INKY_UCS2</Alias>
                <Comment>Get inkey: UCS2 alphabet</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_INKY_NO_HELP</Alias>
                <Comment>Get inkey: no help information available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10000000</Value>
                <Alias>QLF_INKY_HELP</Alias>
                <Comment>Get inkey: help information available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_INPT_DIGITS</Alias>
                <Comment>Get input: digits (0-9, *,# and +) only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias>QLF_INPT_ALPHA</Alias>
                <Comment>Get input: alphabet set</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_INPT_SMS_DEF</Alias>
                <Comment>Get input; SMS default alphabet</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000010</Value>
                <Alias>QLF_INPT_UCS2</Alias>
                <Comment>Get input: UCS2 alphabet</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_INPT_ECHO</Alias>
                <Comment>Get input: ME may echo input</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000100</Value>
                <Alias>QLF_INPT_NO_ECHO</Alias>
                <Comment>Get input: input shall not revealed in any way</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_INPT_NO_PACK</Alias>
                <Comment>Get input: unpacket input format</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00001000</Value>
                <Alias>QLF_INPT_PACK</Alias>
                <Comment>Get input: SMS packed input format</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_INPT_NO_HELP</Alias>
                <Comment>Get input: no help information available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10000000</Value>
                <Alias>QLF_INPT_HELP</Alias>
                <Comment>Get input: help information available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_SITM_NOPRES</Alias>
                <Comment>Select item: presentation type is not specified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias>QLF_SITM_PRES</Alias>
                <Comment>Select item: presentation type is specified in bit 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_SITM_CHVAL</Alias>
                <Comment>Select item: presentation as a choice of data values if bit 1 = '1'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000010</Value>
                <Alias>QLF_SITM_CHNAV</Alias>
                <Comment>Select item: presentation as a choice of navigation options if bit 1 is '1'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_SITM_SEL_NOPREF</Alias>
                <Comment>Select item: no selection preference</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000100</Value>
                <Alias>QLF_SITM_SEL_PREF_SOFTKEY</Alias>
                <Comment>Select item: selection using soft key preferred</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_SITM_NO_HELP</Alias>
                <Comment>Select item: no help information available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10000000</Value>
                <Alias>QLF_SITM_HELP</Alias>
                <Comment>Select item: help information available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_SMNU_SEL_NOPREF</Alias>
                <Comment>Set up menu: no selection preference</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias>QLF_SMNU_SEL_PREF_SOFTKEY</Alias>
                <Comment>Set up menu: selection using soft key preferred</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_SMNU_NO_HELP</Alias>
                <Comment>Set up menu: no help information available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">10000000</Value>
                <Alias>QLF_SMNU_HELP</Alias>
                <Comment>Set up menu: help information available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>QLF_PLOI_LOC_INFO</Alias>
                <Comment>Provide local information: Local information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>QLF_PLOI_IMEI</Alias>
                <Comment>Provide local information: IMEI of ME</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>QLF_PLOI_NTW_MSR</Alias>
                <Comment>Provide local information: Network measurement results</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>QLF_PLOI_DTT</Alias>
                <Comment>Provide local information: Date, Time and Timezone</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>QLF_PLOI_LANG_SET</Alias>
                <Comment>Provide local information: Language Setting</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">05</Value>
                <Alias>QLF_PLOI_TIM_ADV</Alias>
                <Comment>Provide local information: Timing Advance</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>QLF_LABR_IF_NOT_LCHD</Alias>
                <Comment>Launch Browser: launch browser, if not already launched</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>QLF_LABR_NOT_USED1</Alias>
                <Comment>Launch Browser: not used</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>QLF_LABR_USE_EXISTING</Alias>
                <Comment>Launch Browser: use the existing browser</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>QLF_LABR_CLOSE_AND_NEW</Alias>
                <Comment>Launch Browser: close the existing browser session and launch new browser session</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>QLF_LABR_NOT_USED2</Alias>
                <Comment>Launch Browser: not used</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_OPCH_ON_DEMD_LINK_EST</Alias>
                <Comment>Open Channel: on demand link establishment (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias>QLF_OPCH_IMMDT_LINK_EST</Alias>
                <Comment>Open Channel: immediate link establishment (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_OPCH_NO_AUTO_RECONNECT</Alias>
                <Comment>Open Channel: no automatic reconnection (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000010</Value>
                <Alias>QLF_OPCH_AUTO_RECONNECT</Alias>
                <Comment>Open Channel: automatic reconnection (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>QLF_SNDDAT_TX</Alias>
                <Comment>Send Data: store data in Tx buffer (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias>QLF_SNDDAT_IM</Alias>
                <Comment>Send Data: Send data immediately (class e)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_src_dev</Name>
                <Comment>values for src_dev</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>DEV_SRC_KBD</Alias>
                <Comment>Device keypad</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>DEV_SRC_DSP</Alias>
                <Comment>Device display</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>DEV_SRC_EAR</Alias>
                <Comment>Device earpiece</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">10</Value>
                <Alias>DEV_SRC_CDR0</Alias>
                <Comment>Device Additional Card Reader 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">11</Value>
                <Alias>DEV_SRC_CDR1</Alias>
                <Comment>Device Additional Card Reader 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">12</Value>
                <Alias>DEV_SRC_CDR2</Alias>
                <Comment>Device Additional Card Reader 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">13</Value>
                <Alias>DEV_SRC_CDR3</Alias>
                <Comment>Device Additional Card Reader 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">14</Value>
                <Alias>DEV_SRC_CDR4</Alias>
                <Comment>Device Additional Card Reader 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">15</Value>
                <Alias>DEV_SRC_CDR5</Alias>
                <Comment>Device Additional Card Reader 5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">16</Value>
                <Alias>DEV_SRC_CDR6</Alias>
                <Comment>Device Additional Card Reader 6</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">17</Value>
                <Alias>DEV_SRC_CDR7</Alias>
                <Comment>Device Additional Card Reader 7</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">21</Value>
                <Alias>DEV_SRC_CH1</Alias>
                <Comment>Device Channel 1 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">22</Value>
                <Alias>DEV_SRC_CH2</Alias>
                <Comment>Device Channel 2 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">23</Value>
                <Alias>DEV_SRC_CH3</Alias>
                <Comment>Device Channel 3 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">24</Value>
                <Alias>DEV_SRC_CH4</Alias>
                <Comment>Device Channel 4 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">25</Value>
                <Alias>DEV_SRC_CH5</Alias>
                <Comment>Device Channel 5 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">26</Value>
                <Alias>DEV_SRC_CH6</Alias>
                <Comment>Device Channel 6 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">27</Value>
                <Alias>DEV_SRC_CH7</Alias>
                <Comment>Device Channel 7 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">81</Value>
                <Alias>DEV_SRC_SIM</Alias>
                <Comment>Device SIM</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">82</Value>
                <Alias>DEV_SRC_ME</Alias>
                <Comment>Device mobile equipment</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">83</Value>
                <Alias>DEV_SRC_NTW</Alias>
                <Comment>Device network</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="02" Year="2004"/>
                <Author>KJF</Author>
                <Comment>additional device values</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_dest_dev</Name>
                <Comment>values for dest_dev</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>DEV_DST_KBD</Alias>
                <Comment>Device keypad</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>DEV_DST_DSP</Alias>
                <Comment>Device display</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>DEV_DST_EAR</Alias>
                <Comment>Device earpiece</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">10</Value>
                <Alias>DEV_DST_CDR0</Alias>
                <Comment>Device Additional Card Reader 0</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">11</Value>
                <Alias>DEV_DST_CDR1</Alias>
                <Comment>Device Additional Card Reader 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">12</Value>
                <Alias>DEV_DST_CDR2</Alias>
                <Comment>Device Additional Card Reader 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">13</Value>
                <Alias>DEV_DST_CDR3</Alias>
                <Comment>Device Additional Card Reader 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">14</Value>
                <Alias>DEV_DST_CDR4</Alias>
                <Comment>Device Additional Card Reader 4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">15</Value>
                <Alias>DEV_DST_CDR5</Alias>
                <Comment>Device Additional Card Reader 5</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">16</Value>
                <Alias>DEV_DST_CDR6</Alias>
                <Comment>Device Additional Card Reader 6</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">17</Value>
                <Alias>DEV_DST_CDR7</Alias>
                <Comment>Device Additional Card Reader 7</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">21</Value>
                <Alias>DEV_DST_CH1</Alias>
                <Comment>Device Channel 1 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">22</Value>
                <Alias>DEV_DST_CH2</Alias>
                <Comment>Device Channel 2 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">23</Value>
                <Alias>DEV_DST_CH3</Alias>
                <Comment>Device Channel 3 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">24</Value>
                <Alias>DEV_DST_CH4</Alias>
                <Comment>Device Channel 4 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">25</Value>
                <Alias>DEV_DST_CH5</Alias>
                <Comment>Device Channel 5 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">26</Value>
                <Alias>DEV_DST_CH6</Alias>
                <Comment>Device Channel 6 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">27</Value>
                <Alias>DEV_DST_CH7</Alias>
                <Comment>Device Channel 7 (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">81</Value>
                <Alias>DEV_DST_SIM</Alias>
                <Comment>Device SIM</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">82</Value>
                <Alias>DEV_DST_ME</Alias>
                <Comment>Device mobile equipment</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">83</Value>
                <Alias>DEV_DST_NTW</Alias>
                <Comment>Device network</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="17" Month="02" Year="2004"/>
                <Author>kjf</Author>
                <Comment>additional device values</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_time_unit</Name>
                <Comment>values for time_unit</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>TU_MIN</Alias>
                <Comment>Minutes</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>TU_SEC</Alias>
                <Comment>Seconds</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>TU_100_MSEC</Alias>
                <Comment>Tenth of seconds</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_noa</Name>
                <Comment>values for noa</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">000</Value>
                <Alias>NOA_UNKNOWN</Alias>
                <Comment>unknown</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">001</Value>
                <Alias>NOA_INTER_NUM</Alias>
                <Comment>international number</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">010</Value>
                <Alias>NOA_NATIO_NUM</Alias>
                <Comment>national significant number</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">011</Value>
                <Alias>NOA_NETW_NUM</Alias>
                <Comment>network specific number</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">100</Value>
                <Alias>NOA_SUBSC_NUM</Alias>
                <Comment>subscriber number</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">110</Value>
                <Alias>NOA_ABBRV_NUM</Alias>
                <Comment>abbreviated number</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_npi</Name>
                <Comment>values for npi</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">0000</Value>
                <Alias>NPI_UNKNOWN</Alias>
                <Comment>unknown</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0001</Value>
                <Alias>NPI_ISDN</Alias>
                <Comment>ISDN/Telephony Numbering Plan (Rec CCITT E.164)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0011</Value>
                <Alias>NPI_X121</Alias>
                <Comment>data numbering plan (CCITT Rec X.121)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100</Value>
                <Alias>NPI_F69</Alias>
                <Comment>telex numbering plan (CCITT Rec F.69)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0110</Value>
                <Alias>NPI_LAND_MOBILE</Alias>
                <Comment>land mobile numbering plan (CCITT Rec E.212)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1000</Value>
                <Alias>NPI_NATIONAL</Alias>
                <Comment>land mobile numbering plan (CCITT Rec E.212)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1001</Value>
                <Alias>NPI_PRIVATE</Alias>
                <Comment>Private numbering plan</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_gen</Name>
                <Comment>values for gen</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>RSLT_PERF_SUCCESS</Alias>
                <Comment>Command performed successfully</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>RSLT_PERF_PART_CMPR</Alias>
                <Comment>Command performed with partial comprehension</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>RSLT_PERF_MISS_INFO</Alias>
                <Comment>Command performed with missing information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>RSLT_RFSH_ADD_EF</Alias>
                <Comment>Refresh performed with additional EF read</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">05</Value>
                <Alias>RSLT_PERF_MDFY_SIM</Alias>
                <Comment>Command performed but modified by SIM</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">06</Value>
                <Alias>RSLT_PERF_LIM_SRV</Alias>
                <Comment>Command performed successfully, limited service</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">07</Value>
                <Alias>RSLT_PERF_MDFIED</Alias>
                <Comment>Command performed with modification  (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">10</Value>
                <Alias>RSLT_SESS_USR_TERM</Alias>
                <Comment>Proactive SIM session terminated by user</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">11</Value>
                <Alias>RSLT_SESS_USR_BACK</Alias>
                <Comment>Backward move in proactive SIM session</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">12</Value>
                <Alias>RSLT_NO_RESP</Alias>
                <Comment>No response from user</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">13</Value>
                <Alias>RSLT_HELP_USR_REQ</Alias>
                <Comment>Help information required by user</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">14</Value>
                <Alias>RSLT_USER_TERM_SS</Alias>
                <Comment>SS or USSD transaction terminated by user</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">20</Value>
                <Alias>RSLT_ME_UNAB_PROC</Alias>
                <Comment>ME is unable to process command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">21</Value>
                <Alias>RSLT_NTW_UNAB_PROC</Alias>
                <Comment>Network is unable to process command</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">22</Value>
                <Alias>RSLT_USR_REJ</Alias>
                <Comment>User did not accept set up request</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">23</Value>
                <Alias>RSLT_USR_CLR_DWN</Alias>
                <Comment>User cleared down call before connection or network release</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">25</Value>
                <Alias>RSLT_CC_SIM_TMP</Alias>
                <Comment>Interaction with call control by SIM temporary problem</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">26</Value>
                <Alias>RSLT_LABRWS_GENERIC</Alias>
                <Comment>Launch browser generic error code  (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">30</Value>
                <Alias>RSLT_ME_CAP</Alias>
                <Comment>Command beyond ME capabilities</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">31</Value>
                <Alias>RSLT_UNKN_TYPE</Alias>
                <Comment>Command type not understood</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">32</Value>
                <Alias>RSLT_UNKN_DATA</Alias>
                <Comment>Command data not understood</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">33</Value>
                <Alias>RSLT_UNKN_NR</Alias>
                <Comment>Command number not understood</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">34</Value>
                <Alias>RSLT_SS_ERR</Alias>
                <Comment>SS return error</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">35</Value>
                <Alias>RSLT_SMS_ERR</Alias>
                <Comment>SMS RP-ERROR</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">36</Value>
                <Alias>RSLT_ERR_REQ_VAL</Alias>
                <Comment>Error, required values are missing</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">37</Value>
                <Alias>RSLT_USSD_ERR</Alias>
                <Comment>USSD return error</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">39</Value>
                <Alias>RSLT_CC_SIM_PRM</Alias>
                <Comment>interaction with call control by SIM or SMS control by SIM permanent problem</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">3A</Value>
                <Alias>RSLT_BEARIND_PERR</Alias>
                <Comment>Bearer Independent Protocol error  (class e)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_add</Name>
                <Comment>values for add</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>ADD_NO_CAUSE</Alias>
                <Comment>No specific cause can be given</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>ADD_ME_SCR_BUSY</Alias>
                <Comment>ME: Screen is busy</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>ADD_ME_CALL_BUSY</Alias>
                <Comment>ME: currently busy on call</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>ADD_ME_SS_BUSY</Alias>
                <Comment>ME: currently busy on SS transaction</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>ADD_ME_NO_SERV</Alias>
                <Comment>ME: no service</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">05</Value>
                <Alias>ADD_ME_ACC_BAR</Alias>
                <Comment>ME: Access control class bar</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">06</Value>
                <Alias>ADD_ME_RR_DENIED</Alias>
                <Comment>ME: Radio resource not granted</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">07</Value>
                <Alias>ADD_ME_NO_SPCH_CALL</Alias>
                <Comment>ME: Not in speech call</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">08</Value>
                <Alias>ADD_ME_USSD_BUSY</Alias>
                <Comment>ME: currently busy on USSD transaction</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>ADD_CC_NOT_ALLWD</Alias>
                <Comment>Call Control: Action not allowed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>ADD_CC_REQ_CHNG</Alias>
                <Comment>Call Control: Type of request has changed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>ADD_LBP_BEARR_NAVAIL</Alias>
                <Comment>Launch browser: Bearer unavailable (class c)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>ADD_LBP_BRWSR_NAVAIL</Alias>
                <Comment>Launch browser: Browser unavailable (class c)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>ADD_LBP_ME_UNABL_RDPD</Alias>
                <Comment>Launch browser: ME unable to read provisioning data (class c)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>ADD_BIP_NO_CHAN_AVAIL</Alias>
                <Comment>No channel available (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>ADD_BIP_CHAN_CLOSD</Alias>
                <Comment>Channel closed (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>ADD_BIP_CHANID_NT_VLD</Alias>
                <Comment>Channel identifier not valid (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>ADD_BIP_BUF_SIZ_NAVAIL</Alias>
                <Comment>Requested buffer size not available (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">05</Value>
                <Alias>ADD_BIP_SECUR_ERR</Alias>
                <Comment>Security error (unsuccessful authentication) (class e)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">06</Value>
                <Alias>ADD_BIP_SIME_ITL_NAVAIL</Alias>
                <Comment>Requested SIM/ME interface transport level not available (class e)</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tos</Name>
                <Comment>values for tos</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">000</Value>
                <Alias>TOS_X213</Alias>
                <Comment>NSAP (X.213/ISO 8348 AD2)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">010</Value>
                <Alias>TOS_USER</Alias>
                <Comment>User Specified</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_oei</Name>
                <Comment>values for oei</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">0</Value>
                <Alias>OEI_EVEN</Alias>
                <Comment>even number of address signals</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1</Value>
                <Alias>OEI_ODD</Alias>
                <Comment>odd number of address signals</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_event</Name>
                <Comment>values for event</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>EVENT_MT_CALL</Alias>
                <Comment>Incoming Call</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>EVENT_CALL_CONN</Alias>
                <Comment>Call is connected</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>EVENT_CALL_DISC</Alias>
                <Comment>Call is disconnected</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>EVENT_LOC_STATUS</Alias>
                <Comment>Service status change</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">04</Value>
                <Alias>EVENT_USER_ACTIVE</Alias>
                <Comment>User activity</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">05</Value>
                <Alias>EVENT_IDLE_SCREEN</Alias>
                <Comment>Idle screen is available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">08</Value>
                <Alias>EVENT_BROWS_TERMIN</Alias>
                <Comment>Browser Termination (if class c supported)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">09</Value>
                <Alias>EVENT_DATA_AVAIL</Alias>
                <Comment>Data available (if class e supported)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">0A</Value>
                <Alias>EVENT_CHAN_STAT</Alias>
                <Comment>Channel Status (if class e supported)</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bc_rpi</Name>
                <Comment>values for bc_rpi</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>BC_RPI_ALT</Alias>
                <Comment>Alternate mode</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>BC_RPI_SEQ</Alias>
                <Comment>Sequential mode</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_loc_state</Name>
                <Comment>values for loc_state</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>LOC_ST_NORMAL</Alias>
                <Comment>Normal service</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>LOC_ST_LIMITED</Alias>
                <Comment>Limited service</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>LOC_ST_NOSERV</Alias>
                <Comment>No service</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>Reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_gprs_pdp_type</Name>
                <Comment>values for gprs_pdp_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>PDP_TYPE_IP</Alias>
                <Comment>Internet Protocol, IETF STD 5</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_oth_addr_type</Name>
                <Comment>values for oth_addr_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">21</Value>
                <Alias>IPv4</Alias>
                <Comment>Internet Protocal vers.4</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">57</Value>
                <Alias>IPv6</Alias>
                <Comment>Internet Protocal vers.6</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_trans_prot_type</Name>
                <Comment>values for trans_prot_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">1</Value>
                <Alias>UDP</Alias>
                <Comment>User Datagramm Protocol</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">2</Value>
                <Alias>TCP</Alias>
                <Comment>Transmission Control Protocol</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_browser</Name>
                <Comment>values for browser</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>DEFAULT_BROWSER</Alias>
                <Comment>Default browser usage</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bearer</Name>
                <Comment>values for bearer</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>B_SMS</Alias>
                <Comment>short message service</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>B_CSD</Alias>
                <Comment>circle switched data</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>B_USSD</Alias>
                <Comment>unstructured supplementary service data</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>B_GPRS</Alias>
                <Comment>generel packet radio systeme</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_brows_term_s</Name>
                <Comment>values for brows_term_s</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">00</Value>
                <Alias>USER_TERMINATION</Alias>
                <Comment>terminated by user action</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>ERROR_TERMINATION</Alias>
                <Comment>terminated by error</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_chan_id</Name>
                <Comment>values for chan_id</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">000</Value>
                <Alias>NO_CHAN_AVAIL</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">001</Value>
                <Alias>CHANNEL_ID_1</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">010</Value>
                <Alias>CHANNEL_ID_2</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">011</Value>
                <Alias>CHANNEL_ID_3</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">100</Value>
                <Alias>CHANNEL_ID_4</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">101</Value>
                <Alias>CHANNEL_ID_5</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">110</Value>
                <Alias>CHANNEL_ID_6</Alias>
                <Comment/>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">111</Value>
                <Alias>CHANNEL_ID_7</Alias>
                <Comment/>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_chan_stat_inf1</Name>
                <Comment>values for chan_stat_inf1</Comment>
            </ValuesDef>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_chan_stat_link</Name>
                <Comment>values for chan_stat_link</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00</Value>
                <Alias>LINK_NO_ESTABL</Alias>
                <Comment>link not established or PDP context not activated</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">01</Value>
                <Alias>LINK_ESTABL</Alias>
                <Comment>link established or PDP context activated</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_chan_stat_inf2</Name>
                <Comment>values for chan_stat_inf2</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">00000000</Value>
                <Alias>NO_FURTH_INFO</Alias>
                <Comment>no further info can be given</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000001</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000010</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000011</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000100</Value>
                <Alias/>
                <Comment>reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">00000101</Value>
                <Alias>LINK_DROPPED</Alias>
                <Comment>link dropped</Comment>
            </ValuesItem>
            <ValuesDefault>
                <Comment>reserved</Comment>
            </ValuesDefault>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bear_type</Name>
                <Comment>values for bear_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">01</Value>
                <Alias>BT_CSD</Alias>
                <Comment>bearer type CSD</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">02</Value>
                <Alias>BT_GPRS</Alias>
                <Comment>bearer type GPRS</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">03</Value>
                <Alias>BT_DEFAULT</Alias>
                <Comment>default bearer parameters</Comment>
            </ValuesItem>
            <History>
                <Date Day="4" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
    </ValuesSection>
</AIM>
