<?xml version="1.0" encoding="UTF-8"?>
<!-- edited with SAPE SAP Editor -->
<SAP xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xsi:noNamespaceSchemaLocation="sap.xsd">
    <DocInfoSection>
        <DocName DocType="SAP">mncc</DocName>
        <DocNum Number="101" Project="6147"/>
        <Description>
            <Section>The Protocol Stacks are used to define the functionality of the GSM protocols for interfaces. The GSM specifications are normative when used to describe the functionality of interfaces, but the stacks and the subdivision of protocol layers does not imply or restrict any implementation.</Section>
            <Section>The base of the Protocol Stack rests on the physical layer.</Section>
            <Section>The Data Link Layer (DL) is used to handle an acknowledged connection between mobile and base station. The LAPDm protocol is used.</Section>
            <Section>Radio Resource (RR) manages the resources of the air-interface. That means configuration of physical layer, cell selection and cell reselection, data transfer, RR-Connection handling.</Section>
            <Section>Mobility Management (MM) handles registration aspects for the mobile station. It detects changes of location areas and updates a mobile station in the new location area.</Section>
            <Section>Call Control (CC) provides the call functionality. This includes call establishment, call maintenance procedures like Hold, Retrieve or Modify, and call disconnection.</Section>
            <Section>Supplementary Services (SS) handles all call independent supplementary services like call forwarding or call barring.</Section>
            <Section>Short Message Services (SMS) is used for sending and receiving point-to-point short messages.</Section>
            <Section>The man machine interface (MMI) is the interface to the user. Normally it is connected with a keypad as input device and a display as output device.</Section>
            <Section>Between the several entities data interfaces are defined. These data interfaces are called Service Access Points (SAPs), indicating that an upper layer uses the services of a lower layer.</Section>
            <Section>The GSM specification does not set out any implementation of the Protocol Stack. The following diagrams show the implementation described in all these documents for the mobile station. All entities except the Man Machine Interface and Physical Layer are implemented as part of the Protocol Stack.</Section>
            <Section>Figure 1: Mobile-station protocol architecture</Section>
            <Section>This document describes the services offered by the call control to the man machine interface.</Section>
        </Description>
        <DocHistory>
            <DocVersion Number="001" Year="96"/>
            <Date Day="12" Month="2" Year="2002"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Initial version.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="101" Year="96"/>
            <Date Day="20" Month="11" Year="2001"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Introduce MNCC_SYNC_REQ</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="102" Year="96"/>
            <Date Day="18" Month="12" Year="2002"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Repaired somewhat broken document</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="103" Year="96"/>
            <Date Day="12" Month="2" Year="2002"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Switched to new template.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="104" Year="96"/>
            <Date Day="12" Month="2" Year="2002"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Cause Concept realization.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="105" Year="96"/>
            <Date Day="30" Month="7" Year="2002"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Cause Concept: switch remaining primitives containing a "res" (result) to containing a cause to avoid conflicts in ACI (e.g. for +CERR). Removed chapter 4.7 and 4.8, result and reject cause respectively.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="106" Year="96"/>
            <Date Day="1" Month="8" Year="2002"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Long number dialling</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="107" Year="96"/>
            <Date Day="1" Month="8" Year="2002"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Removed PRIO_CCBS_CALL, not needed anymore</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="108" Year="96"/>
            <Date Day="1" Month="8" Year="2002"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>added TON_NOT_PRES, NPI_NOT_PRES, fixed typo.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="109" Year="96"/>
            <Date Day="1" Month="8" Year="2002"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Changed SAP for CD implementation.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="110" Year="96"/>
            <Date Day="1" Month="8" Year="2002"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Considered 04.06 clause 5.8.5 (max. L3 msg length = 251) as an upper limit for facilities and set FACILITY_LEN to 251.</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="111" Year="96"/>
            <Date Day="30" Month="9" Year="2002"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>issue 4967</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="112" Year="96"/>
            <Date Day="30" Month="9" Year="2002"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>issue 7743: add PROG_UNSPECIFIC</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="113" Year="96"/>
            <Date Day="28" Month="11" Year="2002"/>
            <Author>FK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Support of CTM implemented</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="114" Year="96"/>
            <Date Day="12" Month="12" Year="2002"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>MNCC_STATUS_IND, MNCC_STATUS_RES to pass 31.4.x</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="115" Year="96"/>
            <Date Day="28" Month="1" Year="2003"/>
            <Author>SBK</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>Corrected twice allocated value for cause (0b1100010100000110)</Comment>
        </DocHistory>
        <DocHistory>
            <DocVersion Number="116" Year="96"/>
            <Date Day="3" Month="7" Year="2003"/>
            <Author>HM</Author>
            <DocStatus State="BEING_PROCESSED"/>
            <Comment>MNCC_CAUSE_DTMF_STOP_SUCCESS added</Comment>
        </DocHistory>
        <DocRef>
            <RefId>[C_7010.801]</RefId>
            <RefTitle>7010.801, References and Vocabulary, Condat AG infrastructure).</RefTitle>
        </DocRef>
    </DocInfoSection>
    <ConstantsSection>
        <Description>
            <Section>This section contains all constants that are defined for the MNCC SAP</Section>
        </Description>
        <Constant>
            <Alias>FACILITY_LEN</Alias>
            <Value ValueType="DEC">251</Value>
            <Comment>Max. length of facility considering L2 constraints</Comment>
        </Constant>
        <Constant>
            <Alias>USER_LEN</Alias>
            <Value ValueType="DEC">131</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_CC_CALLING_NUMBER</Alias>
            <Value ValueType="DEC">22</Value>
            <Comment>max. length of calling party BCD number (MT SETUP)</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CC_REDIR_NUMBER</Alias>
            <Value ValueType="DEC">32</Value>
            <Comment>max. length of redirecting number (MT SETUP)</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CC_CALLED_NUMBER</Alias>
            <Value ValueType="DEC">80</Value>
            <Comment>max. length of called party BCD number (MO SETUP)</Comment>
        </Constant>
        <Constant>
            <Alias>SUB_LENGTH</Alias>
            <Value ValueType="DEC">20</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>MAX_BC_LEN</Alias>
            <Value ValueType="DEC">10</Value>
            <Comment/>
        </Constant>
        <Constant>
            <Alias>CC_ORIGINATING_ENTITY</Alias>
            <ItemLink>
                <DocName DocType="SAP">gsmcom</DocName>
                <Name>CC_ORIGINATING_ENTITY</Name>
            </ItemLink>
            <Comment>mask for indicating the originating entity of a cause is CC</Comment>
        </Constant>
        <Constant>
            <Alias>ACI_ORIGINATING_ENTITY</Alias>
            <ItemLink>
                <DocName DocType="SAP">gsmcom</DocName>
                <Name>ACI_ORIGINATING_ENTITY</Name>
            </ItemLink>
            <Comment>mask for indicating the originating entity of a cause is ACI</Comment>
        </Constant>
        <Constant>
            <Alias>MAX_CC_CAUSE_LENGTH</Alias>
            <Value ValueType="DEC">30</Value>
            <Comment>Max. length of the raw cause variable</Comment>
        </Constant>
        <History>
            <Date Day="9" Month="5" Year="1997"/>
            <Author>MS</Author>
            <Comment>Initial</Comment>
        </History>
        <History>
            <Date Day="22" Month="5" Year="1997"/>
            <Author>VK</Author>
            <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
        </History>
        <History>
            <Date Day="28" Month="5" Year="1999"/>
            <Author>AK</Author>
            <Comment>Facility changed from 251 to 600</Comment>
        </History>
        <History>
            <Date Day="3" Month="11" Year="1999"/>
            <Author>FK</Author>
            <Comment>changed identifier MAX_BCD_DIGITS (new name) to avoid double definition warning</Comment>
        </History>
        <History>
            <Date Day="8" Month="11" Year="1999"/>
            <Author>AK</Author>
            <Comment>MAX_BC_LEN added</Comment>
        </History>
        <History>
            <Date Day="12" Month="2" Year="2002"/>
            <Author>SBK</Author>
            <Comment>Added constant for identification of CC+ACI due to Cause Concept</Comment>
        </History>
        <History>
            <Date Day="8" Month="3" Year="2002"/>
            <Author>HM</Author>
            <Comment>Long number dialling, MAX_BCD_DIGITS eliminated</Comment>
        </History>
        <History>
            <Date Day="11" Month="4" Year="2002"/>
            <Author>HM</Author>
            <Comment>MAX_CC_REDIR_NUMBER added</Comment>
        </History>
        <History>
            <Date Day="11" Month="7" Year="2002"/>
            <Author>HM</Author>
            <Comment>Considered 04.06 5.8.5 to determine FACILITY_LEN</Comment>
        </History>
    </ConstantsSection>
    <PrimitivesSection PrimIDType="BIT32" SAPid="11">
        <Description>
            <Section>This section contains all primitives that are defined for the MNCC SAP</Section>
        </Description>
        <Primitive>
            <Description>
                <Section>MNCC_ALERT_IND shall be used to indicate that an ALERT message has received in call control. That means that the called party is alarmed.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_ALERT_IND</Name>
                <PrimID Direction="DOWNLINK" Number="0"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>progress_desc</Name>
                </ItemLink>
                <Comment>progress indicator</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="27" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>facility and user user removed</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_ALERT_IND shall be used to indicate that an ALERT message has received in call control. That means that the called party is alarmed.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_CALL_PROCEED_IND</Name>
                <PrimID Direction="DOWNLINK" Number="1"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>progress_desc</Name>
                </ItemLink>
                <Comment>progress indicator</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ri</Name>
                </ItemLink>
                <Comment>repeat indicator</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara</Name>
                </ItemLink>
                <Comment>bearer cap parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara2</Name>
                </ItemLink>
                <Comment>bearer cap parameter</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>repeat indicator and BC parameter added, serv code removed</Comment>
            </History>
            <History>
                <Date Day="27" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>facility removed</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_DISCONNECT_IND shall be used to indicate that the call is disconnected.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_DISCONNECT_IND</Name>
                <PrimID Direction="DOWNLINK" Number="2"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>cause; The following causes can occur within this primitive:  all those  of 4.6 defined by the GSM standard and originated by the network, i.e. those starting with 0b00...  and MNCC_CAUSE_MS_COND_INFO_ELEM, MNCC_CAUSE_MS_INVALID_MAND_INFO and all those previously indicated via MNCC_DISCONNECT_REQ.</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>diagnostic</Name>
                </ItemLink>
                <Comment>Additional cause info</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ss_diag</Name>
                </ItemLink>
                <Comment>Additional supplementary service diagnostic info</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>progress_desc</Name>
                </ItemLink>
                <Comment>progress description</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>c_raw_cause</Name>
                </ItemLink>
                <Comment>Number of cause bytes</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>raw_cause</Name>
                </ItemLink>
                <Control>[MAX_CC_CAUSE_LENGTH]</Control>
                <Comment>cause as received from NW</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="27" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>facility and user user removed</Comment>
            </History>
            <History>
                <Date Day="29" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>diagnostic info added for CCBS</Comment>
            </History>
            <History>
                <Date Day="18" Month="08" Year="2004"/>
                <Author>MDF</Author>
                <Comment>ss_diag added for general supplementary service diagnostic  needed by %DIAG command</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_HOLD_CNF is send by call control if a connection is into the hold state. Previously MMI requests this with a MNCC_HOLD_REQ primitive.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_HOLD_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="3"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>Cause; The following causes can occur within this primitive:  all those  of 4.6 defined by the GSM standard and originated by the network, i.e. those starting with 0b00...  and  MNCC_CAUSE_HOLD_SUCCESS. It is possible for the network to not add a Cause IE. In this case, cause is MNCC_CAUSE_NO_NET_CAUSE</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="13" Month="2" Year="2002"/>
                <Author>SBK</Author>
                <Comment>Changed res to cause (to reflect air interface)</Comment>
            </History>
            <History>
                <Date Day="4" Month="12" Year="2002"/>
                <Author>ZMM</Author>
                <Comment>Added extra cause value when network has sent no cause</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_MODIFY_CNF is send by call control if a mobile originated in-call modification has finished.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_MODIFY_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="4"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>cause; The following causes can occur within this primitive:  all those  of 4.6 defined by the GSM standard and originated by the network, i.e. those starting with 0b00...  and  MNCC_CAUSE_MODIFY_SUCCESS, MNCC_CAUSE_MS_TIMER.</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="13" Month="2" Year="2002"/>
                <Author>SBK</Author>
                <Comment>Changed res to cause (to reflect air interface)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_MODIFY_IND is send by call control if a mobile terminated in-call modification has finished.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_MODIFY_IND</Name>
                <PrimID Direction="DOWNLINK" Number="5"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>serv</Name>
                </ItemLink>
                <Comment>service code</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_NOTIFY_IND is send by call control if a notification for a connection has received.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_NOTIFY_IND</Name>
                <PrimID Direction="DOWNLINK" Number="6"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>nd</Name>
                </ItemLink>
                <Comment>notification</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_PROGRESS_IND is sent to MMI if call control has received a progress message.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_PROGRESS_IND</Name>
                <PrimID Direction="DOWNLINK" Number="7"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>progress_desc</Name>
                </ItemLink>
                <Comment>progress indicator</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="27" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>user user removed</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_REJECT_IND is sent to MMI if call control rejects the call attempt or if lower layers indicate a failure.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_REJECT_IND</Name>
                <PrimID Direction="DOWNLINK" Number="8"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>reject cause; The following causes can occur within this primitive: MNCC_CAUSE_MS_INCOMPAT_DEST, MNCC_CAUSE_MS_TIMER of 4.6 and all possible within the MMCC_RELEASE_IND and MMCC_ERROR_IND primitives of the MMCC SAP.</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="13" Month="2" Year="2002"/>
                <Author>SBK</Author>
                <Comment>Changed rej to cause (to fully implement cause concept)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_RELEASE_CNF is sent to MMI if a mobile originated call release has completed.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_RELEASE_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="9"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>cause; The following causes can occur within this primitive: all those  of 4.6 defined by the GSM standard and originated by the network, i.e. those starting with 0b00...  and MNCC_CAUSE_NO_NET_CAUSE and MNCC_CAUSE_MS_MESSAGE_INCOMPAT, MNCC_CAUSE_MS_TIMER.</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>c_raw_cause</Name>
                </ItemLink>
                <Comment>Number of cause bytes</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>raw_cause</Name>
                </ItemLink>
                <Control>[MAX_CC_CAUSE_LENGTH]</Control>
                <Comment>cause as received from NW</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="20" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>facility info added for CCBS</Comment>
            </History>
            <History>
                <Date Day="21" Month="3" Year="2000"/>
                <Author>HM</Author>
                <Comment>reverted to version of 22-May-97 (facility info removed)</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_RELEASE_IND is sent to MMI if a mobile terminated call release has occurred. It is also sent in case lower layers indicate a failure.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_RELEASE_IND</Name>
                <PrimID Direction="DOWNLINK" Number="10"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>cause; The following causes can occur within this primitive:  all those  of 4.6 defined by the GSM standard and originated by the network, i.e. those starting with 0b00...  and MNCC_CAUSE_NO_NET_CAUSE and MNCC_CAUSE_MS_MESSAGE_INCOMPAT, MNCC_CAUSE_MS_INVALID_TI, MNCC_CAUSE_MS_BEARER_NOT_IMPLEM, MNCC_CAUSE_MS_COND_INFO_ELEM, MNCC_CAUSE_MS_INVALID_MAND_INFO, MNCC_CAUSE_MAX_NO_CALLS_REACHED, MNCC_CAUSE_MAX_NO_RECALLS_REACHED, MNCC_CAUSE_MS_INCOMPAT_DEST, MNCC_CAUSE_MS_FACILITY_REJECT, MNCC_CAUSE_MS_TIMER of 4.6 and all possible within the MMCC_RELEASE_IND (CCBS) and all causes sent by higher layers within MNCC_DISCONNECT_REQ (CCBS and when no network connection) and the MMCC_ERROR_IND primitive of the MMCC SAP.</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>c_raw_cause</Name>
                </ItemLink>
                <Comment>Number of cause bytes</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>raw_cause</Name>
                </ItemLink>
                <Control>[MAX_CC_CAUSE_LENGTH]</Control>
                <Comment>cause as received from NW</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="27" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>facility and user user removed</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_RETRIEVE_CNF is sent to MMI if call control has executed the retrieve procedure. That means a connection has changed from state hold to state active.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_RETRIEVE_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="11"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>cause; The following causes can occur within this primitive:  all those  of 4.6 defined by the GSM standard and originated by the network, i.e. those starting with 0b00...  and  MNCC_CAUSE_RETRIEVE_SUCCESS. It is possible for the network to not add a Cause IE. In this case, cause is MNCC_CAUSE_NO_NET_CAUSE</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="13" Month="2" Year="2002"/>
                <Author>SBK</Author>
                <Comment>Changed res to cause (to reflect air interface)</Comment>
            </History>
            <History>
                <Date Day="4" Month="12" Year="2002"/>
                <Author>ZMM</Author>
                <Comment>Added extra cause value when network has sent no cause</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_SETUP_CNF is sent to MMI if a mobile originated call attempt is accepted or rejected by the called party.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_SETUP_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="12"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>(resulting) cause; The following causes can occur within this primitive:  MNCC_CAUSE_SUCCESS, MNCC_CAUSE_MS_TIMER.</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>progress_desc</Name>
                </ItemLink>
                <Comment>progress description</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>connected_number</Name>
                </ItemLink>
                <Comment>connected number</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>connected_number_sub</Name>
                </ItemLink>
                <Comment>connected sub address</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="28" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>rename prog_desc into progress_desc</Comment>
            </History>
            <History>
                <Date Day="27" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>facility and user user removed</Comment>
            </History>
            <History>
                <Date Day="30" Month="7" Year="2002"/>
                <Author>SBK</Author>
                <Comment>Changed res to cause</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_SETUP_COMPL_IND is sent to MMI if call control has acknowledged an incoming call.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_SETUP_COMPL_IND</Name>
                <PrimID Direction="DOWNLINK" Number="13"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>(resulting) cause; The following causes can occur within this primitive:  MNCC_CAUSE_SUCCESS, MNCC_CAUSE_MS_TIMER.</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="30" Month="7" Year="2002"/>
                <Author>SBK</Author>
                <Comment>Changed res to cause</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_SETUP_IND is sent to MMI if call control has received an incoming call.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_SETUP_IND</Name>
                <PrimID Direction="DOWNLINK" Number="14"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ri</Name>
                </ItemLink>
                <Comment>repeat indicator</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara</Name>
                </ItemLink>
                <Comment>bearer cap parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara2</Name>
                </ItemLink>
                <Comment>bearer cap parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>progress_desc</Name>
                </ItemLink>
                <Comment>progress indicator</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>sig</Name>
                </ItemLink>
                <Comment>signal</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>calling_party</Name>
                </ItemLink>
                <Comment>calling party</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>calling_party_sub</Name>
                </ItemLink>
                <Comment>calling party sub</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>called_party</Name>
                </ItemLink>
                <Comment>called party</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>called_party_sub</Name>
                </ItemLink>
                <Comment>called party sub</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>redirecting_party</Name>
                </ItemLink>
                <Comment>redirecting party</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>redirecting_party_sub</Name>
                </ItemLink>
                <Comment>redirecting party sub</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>repeat indicator and BC parameter added, serv code removed</Comment>
            </History>
            <History>
                <Date Day="27" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>facility and user user removed</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>redirecting party added for CD</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_START_DTMF_CNF is sent to MMI if the network has accepted the DTMF signalling. It is also sent in other scenarios as response to the MNCC_START_DTMF_REQ.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_START_DTMF_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="15"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>key</Name>
                </ItemLink>
                <Comment>keypad digit</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>cause; The following causes can occur within this primitive:  all those  of 4.6 defined by the GSM standard and originated by the network, i.e. those starting with 0b00...  and MNCC_CAUSE_DTMF_NOT_ALLOWED, MNCC_CAUSE_DTMF_BUFFER_FULL, MNCC_CAUSE_DTMF_ABORTED, MNCC_CAUSE_DTMF_START_SUCCESS, MNCC_CAUSE_MS_TIMER.</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>dtmf_mod</Name>
                </ItemLink>
                <Comment>dtmf mode</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="24" Month="9" Year="1999"/>
                <Author>AK</Author>
                <Comment>DTMF mode added</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_BEARER_CAP_CNF is sent to MMI after a MNCC_BEARER_CAP_REQ. It contains at least a valid pair of coded and decoded bearer capability parameters and a result whether the bearer capabilities are supported by CC. If bcconf2.bc_len equals to zero, bcconf2 is considered as not present. If bcpara2.bearer_serv equals to BEARER_SERV_NOT_PRES, bcpara2 is considered as not present.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_BEARER_CAP_CNF</Name>
                <PrimID Direction="DOWNLINK" Number="19"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>req_id</Name>
                </ItemLink>
                <Comment>request id</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bc_mod</Name>
                </ItemLink>
                <Comment>conversion mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcconf</Name>
                </ItemLink>
                <Comment>coded bearer cap</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara</Name>
                </ItemLink>
                <Comment>decoded bearer cap</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcconf2</Name>
                </ItemLink>
                <Comment>coded bearer cap2</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara2</Name>
                </ItemLink>
                <Comment>decoded bearer cap2</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>translation cause; The following causes can occur within this primitive:  MNCC_CAUSE_SUCCESS, MNCC_CAUSE_MS_INCOMPAT_DEST.</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="11" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="3" Year="2000"/>
                <Author>HM</Author>
                <Comment>Added fields for second bearer cap</Comment>
            </History>
            <History>
                <Date Day="30" Month="7" Year="2002"/>
                <Author>SBK</Author>
                <Comment>Changed res to cause</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_SYNC_IND is sent to MMI if the channel mode has changed.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_SYNC_IND</Name>
                <PrimID Direction="DOWNLINK" Number="16"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>cause; The following causes can occur within this primitive: MNCC_CAUSE_CHANNEL_SYNC, MNCC_CAUSE_REEST_STARTED, MNCC_CAUSE_REEST_FINISHED.</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>chm</Name>
                </ItemLink>
                <Comment>channel mode</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_USER_IND is sent to MMI to indicate that user-to-user data has been received.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_USER_IND</Name>
                <PrimID Direction="DOWNLINK" Number="17"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>congest_lev</Name>
                </ItemLink>
                <Comment>congestion level</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>more_data</Name>
                </ItemLink>
                <Comment>more data</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>user</Name>
                </ItemLink>
                <Comment>user to user</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_FACILITY_IND shall be used to indicate that a FACILITY message has received in call control.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_FACILITY_IND</Name>
                <PrimID Direction="DOWNLINK" Number="18"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>fac_context</Name>
                </ItemLink>
                <Comment>facility context</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>fac_inf</Name>
                </ItemLink>
                <Comment>facility information</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="29" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Facility changed to T_sdu, context splitted</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_PROMPT_IND is given by CC to inform of the completion of the MM connection to the MMI. for a mobile station which supports "Network Initiated MO CM Connection Request". The primitive has no parameters.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_PROMPT_IND</Name>
                <PrimID Direction="DOWNLINK" Number="20"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="20" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_RECALL_IND is given by CC to send the relevant informations received by the CC ESTABLISHMENT and RECALL message to the MMI. This primitive is used by a mobile station which supports "Network Initiated MO CM Connection Request".</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_RECALL_IND</Name>
                <PrimID Direction="DOWNLINK" Number="21"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ri</Name>
                </ItemLink>
                <Comment>repeat indicator</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara</Name>
                </ItemLink>
                <Comment>bearer cap parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara2</Name>
                </ItemLink>
                <Comment>bearer cap parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>called_party</Name>
                </ItemLink>
                <Comment>called party address</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>called_party_sub</Name>
                </ItemLink>
                <Comment>called party sub</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>rcl_type</Name>
                </ItemLink>
                <Comment>recall type</Comment>
            </PrimItem>
            <History>
                <Date Day="4" Month="2" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="3" Year="2000"/>
                <Author>HM</Author>
                <Comment>Facility info removed</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_STATUS_IND is used by CC to indicate to ACI that a STATUS ENQUIRY message was received in U10. CC does not send the STATUS possibly containing auxiliary states to the ACI but waits until the MNCC_STATUS_RES has been received by ACI. This is a synchronization mechanism to pass 31.4.x safely.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_STATUS_IND</Name>
                <PrimID Direction="DOWNLINK" Number="22"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>ACI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <History>
                <Date Day="28" Month="11" Year="2002"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_SETUP_REQ is used to start a mobile originated call.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_SETUP_REQ</Name>
                <PrimID Direction="UPLINK" Number="0"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>prio</Name>
                </ItemLink>
                <Comment>priority</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ri</Name>
                </ItemLink>
                <Comment>repeat indicator</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara</Name>
                </ItemLink>
                <Comment>bearer cap parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara2</Name>
                </ItemLink>
                <Comment>bearer cap parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>called_party</Name>
                </ItemLink>
                <Comment>called party address</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>called_party_sub</Name>
                </ItemLink>
                <Comment>called party sub</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>clir_sup</Name>
                </ItemLink>
                <Comment>clir suppression</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>fac_inf</Name>
                </ItemLink>
                <Comment>facility information</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>repeat indicator and BC parameter added, serv code removed</Comment>
            </History>
            <History>
                <Date Day="29" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>facility info added for CUG</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_SETUP_RES is used to indicate that a mobile terminated call is accepted by the MMI.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_SETUP_RES</Name>
                <PrimID Direction="UPLINK" Number="1"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_ALERT_REQ is used to indicate that the user is informed about the incoming call (e.g. by alerting)</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_ALERT_REQ</Name>
                <PrimID Direction="UPLINK" Number="2"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_DISCONNECT_REQ is used to indicate that the user disconnects an active call or a call in set-up phase.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_DISCONNECT_REQ</Name>
                <PrimID Direction="UPLINK" Number="3"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>cause; Only standard-defined, MS originated values shall be used which are in addition compliant to the CC peer to peer protocol.</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>fac_inf</Name>
                </ItemLink>
                <Comment>facility information</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ss_version</Name>
                </ItemLink>
                <Comment>ss version</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>fac_inf and ss_version added for CD</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_RELEASE_REQ is used if the other side has disconnected a call (by MNCC_DISCONNECT_IND) and the user has hooked on.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_RELEASE_REQ</Name>
                <PrimID Direction="UPLINK" Number="4"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>cause; Only standard-defined, MS originated values shall be used which are in addition compliant to the CC peer to peer protocol. In addition MNCC_CAUSE_NO_MS_CAUSE could be used if compliant to the CC peer to peer protocol in the current situation.</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>fac_inf</Name>
                </ItemLink>
                <Comment>facility information</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ss_version</Name>
                </ItemLink>
                <Comment>ss version</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="28" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>correct type for 'cause'</Comment>
            </History>
            <History>
                <Date Day="20" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>fac_inf and ss_version added for CCBS</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_MODIFY_REQ is used to start a mobile originated in-call modification.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_MODIFY_REQ</Name>
                <PrimID Direction="UPLINK" Number="5"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>serv</Name>
                </ItemLink>
                <Comment>service code</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_CONFIGURE_REQ is used to configure CC. It defines the own subaddress.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_CONFIGURE_REQ</Name>
                <PrimID Direction="UPLINK" Number="6"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>called_party_sub</Name>
                </ItemLink>
                <Comment>called party subaddress</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara</Name>
                </ItemLink>
                <Comment>bearer cap parameter</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>sns_mode</Name>
                </ItemLink>
                <Comment>single numbering mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ctm_ena</Name>
                </ItemLink>
                <Comment>CTM support enabled</Comment>
            </PrimItem>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>repeat indicator and BC parameter removed</Comment>
            </History>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>AK</Author>
                <Comment>bearer capabilities and SNS mode added</Comment>
            </History>
            <History>
                <Date Day="28" Month="11" Year="2003"/>
                <Author>FK</Author>
                <Comment>element 'ctm_ena' added</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_NOTIFY_REQ is used to request CC to send a notification to the network.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_NOTIFY_REQ</Name>
                <PrimID Direction="UPLINK" Number="7"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>nd</Name>
                </ItemLink>
                <Comment>notification description</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_START_DTMF_REQ is used to start sending of a DTMF tone.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_START_DTMF_REQ</Name>
                <PrimID Direction="UPLINK" Number="8"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>key</Name>
                </ItemLink>
                <Comment>keypad digit</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>dtmf_mod</Name>
                </ItemLink>
                <Comment>DTMF mode</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="24" Month="9" Year="1999"/>
                <Author>AK</Author>
                <Comment>DTMF mode added</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_HOLD_REQ is used to change the call state from active to hold.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_HOLD_REQ</Name>
                <PrimID Direction="UPLINK" Number="9"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_RETRIEVE_REQ is used to change the call state from hold to active.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_RETRIEVE_REQ</Name>
                <PrimID Direction="UPLINK" Number="10"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_FACILITY_REQ is used to send a facility information element for a call dependent supplementary service (e.q. multi party service).</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_FACILITY_REQ</Name>
                <PrimID Direction="UPLINK" Number="11"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>fac_inf</Name>
                </ItemLink>
                <Comment>facility information</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ss_version</Name>
                </ItemLink>
                <Comment>ss version</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_USER_REQ is used to send a user-to-user data.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_USER_REQ</Name>
                <PrimID Direction="UPLINK" Number="12"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>congest_lev</Name>
                </ItemLink>
                <Comment>congestion level</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>more_data</Name>
                </ItemLink>
                <Comment>more data</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>user</Name>
                </ItemLink>
                <Comment>user to user</Comment>
            </PrimItem>
            <History>
                <Date Day="9" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_BEARER_CAP_REQ is used to convert bearer capability settings from coded to decoded representation and vice versa. The mode parameter defines the way of conversion. CC responds with a MNCC_BEARER_CAP_CNF providing the result of the conversion. If bcconf2.bc_len equals to zero, bcconf2 is considered as not present. If bcpara2.bearer_serv equals to BEARER_SERV_NOT_PRES, bcpara2 is considered as not present.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_BEARER_CAP_REQ</Name>
                <PrimID Direction="UPLINK" Number="13"/>
                <PrimUsage>
                    <Sender>CC</Sender>
                    <Receiver>MMI</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>req_id</Name>
                </ItemLink>
                <Comment>request id</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bc_mod</Name>
                </ItemLink>
                <Comment>conversion mode</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcconf</Name>
                </ItemLink>
                <Comment>coded bearer cap</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara</Name>
                </ItemLink>
                <Comment>decoded bearer cap</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcconf2</Name>
                </ItemLink>
                <Comment>coded bearer cap2</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bcpara2</Name>
                </ItemLink>
                <Comment>decoded bearer cap2</Comment>
            </PrimItem>
            <History>
                <Date Day="8" Month="11" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="3" Year="2000"/>
                <Author>HM</Author>
                <Comment>Added fields for second bearer cap</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_PROMPT_RSP assigns a newly allocated transaction identifier to CC. This is used for network originated MO call.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_PROMPT_RSP</Name>
                <PrimID Direction="UPLINK" Number="14"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <History>
                <Date Day="20" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_PROMPT_REJ is used if the MMI is out of transaction identifiers and cannot assigns a newly allocated transaction identifier to CC. This is used for network originated MO call. The primitive has no parameters.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_PROMPT_REJ</Name>
                <PrimID Direction="UPLINK" Number="15"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <History>
                <Date Day="20" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_REJECT_REQ is used by the MMI to cause CC to clear a call by a RELEASE COMPLETE message. It is only expected in the context of CCBS.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_REJECT_REQ</Name>
                <PrimID Direction="UPLINK" Number="16"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>cause</Name>
                </ItemLink>
                <Comment>cause; Only standard-defined, MS originated values shall be used which are in addition compliant to the CC peer to peer protocol. In addition MNCC_CAUSE_NO_MS_CAUSE could be used if compliant to the CC peer to peer protocol in the current situation.</Comment>
            </PrimItem>
            <History>
                <Date Day="20" Month="1" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_SYNC_REQ is used by the MMI to inform CC about some events occured which may affect the hold and/or multi party auxiliary states in CC This is needed to fulfill the needs of the status enquiry procedure and to pass the GSM 11.11 31.4.x test cases.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_SYNC_REQ</Name>
                <PrimID Direction="UPLINK" Number="17"/>
                <PrimUsage>
                    <Sender>MMI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>synccs</Name>
                </ItemLink>
                <Comment>synchronization cause</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>mpty_event</Name>
                </ItemLink>
                <Comment>multi party event</Comment>
            </PrimItem>
            <History>
                <Date Day="26" Month="11" Year="2001"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
        <Primitive>
            <Description>
                <Section>MNCC_STATUS_RES is used by the ACI to response to MNCC_STATUS_IND. This causes CC to send the STATUS message containing the correct auxiliary states to the network. This is a synchronization mechanism to pass 31.4.x safely.</Section>
            </Description>
            <PrimDef>
                <Name>MNCC_STATUS_RES</Name>
                <PrimID Direction="UPLINK" Number="18"/>
                <PrimUsage>
                    <Sender>ACI</Sender>
                    <Receiver>CC</Receiver>
                </PrimUsage>
            </PrimDef>
            <PrimItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ti</Name>
                </ItemLink>
                <Comment>transaction identifier</Comment>
            </PrimItem>
            <History>
                <Date Day="28" Month="11" Year="2002"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </Primitive>
    </PrimitivesSection>
    <PrimStructElementsSection>
        <Description>
            <Section>Parameters shall be part of the primitives described below and if applied the parameters shall contain the values specified here. These values are selected to correspond element values used in the air interface protocol.</Section>
        </Description>
        <PrimStructElem>
            <Description>
                <Section>The parameter contains a user to user information element.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>user</Name>
                <Comment>user to user data</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>info_context</Name>
                </ItemLink>
                <Comment>user to user message context</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>pd</Name>
                </ItemLink>
                <Comment>user to user protocol discriminator</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>c_info</Name>
                </ItemLink>
                <Comment>length of user to user data</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>info</Name>
                </ItemLink>
                <Control>[USER_LEN]</Control>
                <Comment>user to user information</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="30" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>c_info changed from USHORT to UBYTE</Comment>
            </History>
            <History>
                <Date Day="27" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>user info context added</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter indicates the address of the calling or connected party.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>calling_party</Name>
                <Comment>calling party</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>connected_number</Name>
                <Comment>connected number</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ton</Name>
                </ItemLink>
                <Comment>type of number</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>npi</Name>
                </ItemLink>
                <Comment>numbering plan identification</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>present</Name>
                </ItemLink>
                <Comment>presentation indicator</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>screen</Name>
                </ItemLink>
                <Comment>screening indicator</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>c_num</Name>
                </ItemLink>
                <Comment>number of BCD digits</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>num</Name>
                </ItemLink>
                <Control>[MAX_CC_CALLING_NUMBER]</Control>
                <Comment>bcd</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>HM</Author>
                <Comment>MAX_BCD_DIGITS =&gt; MAX_CC_CALLING_NUMBER</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>added TON_NOT_PRES, NPI_NOT_PRES, fixed typo</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Made references to chapter "Elements"</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter indicates the address of the called party.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>called_party</Name>
                <Comment>called party address</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ton</Name>
                </ItemLink>
                <Comment>numbering type</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>npi</Name>
                </ItemLink>
                <Comment>numbering plan</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>c_called_num</Name>
                </ItemLink>
                <Comment>number of BCD digits</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>called_num</Name>
                </ItemLink>
                <Control>[MAX_CC_CALLED_NUMBER]</Control>
                <Comment>bcd</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>HM</Author>
                <Comment>MAX_BCD_DIGITS =&gt; MAX_CC_CALLED_NUMBER</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>added TON_NOT_PRES, NPI_NOT_PRES, fixed typo</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Made references to chapter "Elements"</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter indicates a called, calling or connected sub address.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>calling_party_sub</Name>
                <Comment>calling party subaddress</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>called_party_sub</Name>
                <Comment>called party subaddress</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>connected_number_sub</Name>
                <Comment>connected number subaddress</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>redirecting_party_sub</Name>
                <Comment>redirecting party subaddress</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>tos</Name>
                </ItemLink>
                <Comment>type of subaddress</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>odd_even</Name>
                </ItemLink>
                <Comment>odd / even indicator</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>c_subaddr</Name>
                </ItemLink>
                <Comment>length of subaddress information</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>subaddr</Name>
                </ItemLink>
                <Control>[SUB_LENGTH]</Control>
                <Comment>subaddress information</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Added redirecting party subaddress</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter defines the used channel mode.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>chm</Name>
                <Comment>Channel using mode</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ch_type</Name>
                </ItemLink>
                <Comment>Channel Type</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ch_mode</Name>
                </ItemLink>
                <Comment>Channel Mode</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="29" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>changed to struct with channel type and mode</Comment>
            </History>
            <History>
                <Date Day="19" Month="10" Year="2000"/>
                <Author>HM</Author>
                <Comment>+CHM_SPEECH_V2, +CHM_SPEECH_V3, -CHM_EFR_SPEECH</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter indicates the relevant parameter to build a bearer capability</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>bcpara</Name>
                <Comment>bearer capability parameter</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>bcpara2</Name>
                <Comment>bearer capability parameter</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>rate</Name>
                </ItemLink>
                <Comment>user rate</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bearer_serv</Name>
                </ItemLink>
                <Comment>bearer service</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>conn_elem</Name>
                </ItemLink>
                <Comment>connection element</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>stop_bits</Name>
                </ItemLink>
                <Comment>stop bits</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>data_bits</Name>
                </ItemLink>
                <Comment>data bits</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>parity</Name>
                </ItemLink>
                <Comment>parity</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>flow_control</Name>
                </ItemLink>
                <Comment>flow control</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>modem_type</Name>
                </ItemLink>
                <Comment>modem type</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="26" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Values part changed</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>CE_ELEM_NOT_PRES renamed to CONN_ELEM_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>RATE_NOT_PRES renamed to UR_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>data and stop bits added</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>parity and flow control added</Comment>
            </History>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>AK</Author>
                <Comment>conn_elem extended and modem_type added</Comment>
            </History>
            <History>
                <Date Day="16" Month="9" Year="1999"/>
                <Author>AK</Author>
                <Comment>new modem type added</Comment>
            </History>
            <History>
                <Date Day="4" Month="9" Year="2000"/>
                <Author>LE</Author>
                <Comment>Auxiliary speech added</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter contains a facility information element.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>fac_inf</Name>
                <Comment>facility information</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>l_fac</Name>
                </ItemLink>
                <Comment>facility length</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>o_fac</Name>
                </ItemLink>
                <Comment>facility offset</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>fac</Name>
                </ItemLink>
                <Control>[FACILITY_LEN]</Control>
                <Comment>facility content</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="29" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter indicates the coded bearer capability configuration</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>bcconf</Name>
                <Comment>bearer capability configuration</Comment>
            </PrimStructElemDef>
            <PrimStructElemDef Type="STRUCT">
                <Name>bcconf2</Name>
                <Comment>second bearer capability configuration</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bc_len</Name>
                </ItemLink>
                <Comment>coded bearer cap length</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>bc</Name>
                </ItemLink>
                <Control>[MAX_BC_LEN]</Control>
                <Comment>coded bearer cap</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="8" Month="11" Year="1999"/>
                <Author>AK</Author>
                <Comment>initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="3" Year="2000"/>
                <Author>HM</Author>
                <Comment>Added bcconf2</Comment>
            </History>
        </PrimStructElem>
        <PrimStructElem>
            <Description>
                <Section>The parameter indicates the address of the redirecting party. For values of ton, npi, present and screen, see the definition of the calling party address.</Section>
            </Description>
            <PrimStructElemDef Type="STRUCT">
                <Name>redirecting_party</Name>
                <Comment>redirecting party address</Comment>
            </PrimStructElemDef>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>ton</Name>
                </ItemLink>
                <Comment>numbering type</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>npi</Name>
                </ItemLink>
                <Comment>numbering plan</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>present</Name>
                </ItemLink>
                <Comment>presentation indicator</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>screen</Name>
                </ItemLink>
                <Comment>screening indicator</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>c_redir_num</Name>
                </ItemLink>
                <Comment>number of BCD digits</Comment>
            </PrimStructElemItem>
            <PrimStructElemItem Presentation="MANDATORY">
                <ItemLink>
                    <DocName DocType="SAP">mncc</DocName>
                    <Name>redir_num</Name>
                </ItemLink>
                <Control>[MAX_CC_REDIR_NUMBER]</Control>
                <Comment>bcd</Comment>
            </PrimStructElemItem>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimStructElem>
    </PrimStructElementsSection>
    <PrimBasicElementsSection>
        <Description>
            <Section>Parameters shall be part of the primitives described below and if applied the parameters shall contain the values specified here. These values are selected to correspond element values used in the air interface protocol.</Section>
        </Description>
        <PrimBasicElem>
            <Description>
                <Section>The parameter identifies a transaction.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ti</Name>
                <Type>U8</Type>
                <Comment>transaction identifier</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_ti</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter contains the progress description</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>progress_desc</Name>
                <Type>U8</Type>
                <Comment>progress description</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_progress_desc</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="2002"/>
                <Author>SBK</Author>
                <Comment>Issue 4967</Comment>
            </History>
            <History>
                <Date Day="30" Month="9" Year="2002"/>
                <Author>SBK</Author>
                <Comment>Issue 7743, add PROG_UNSPECIFIC</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter contains the context of a facility information element, that means the message which has carried the facility information element.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>fac_context</Name>
                <Type>U8</Type>
                <Comment>facility information element context</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_fac_context</Name>
            </ValuesLink>
            <History>
                <Date Day="29" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="21" Month="3" Year="2000"/>
                <Author>HM</Author>
                <Comment>Added FAC_IN_RELEASE_COMP, FAC_IN_RECALL</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter contains a user to user information element.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>info_context</Name>
                <Type>U8</Type>
                <Comment>user to user message context</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_info_context</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="30" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>c_info changed from USHORT to UBYTE</Comment>
            </History>
            <History>
                <Date Day="27" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>user info context added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter contains a user to user information element.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>pd</Name>
                <Type>U8</Type>
                <Comment>user to user protocol discriminator</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_pd</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="30" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>c_info changed from USHORT to UBYTE</Comment>
            </History>
            <History>
                <Date Day="27" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>user info context added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter contains a user to user information element.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c_info</Name>
                <Type>U8</Type>
                <Comment>length of user to user data</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="30" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>c_info changed from USHORT to UBYTE</Comment>
            </History>
            <History>
                <Date Day="27" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>user info context added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter contains a user to user information element.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>info</Name>
                <Type>U8</Type>
                <Comment>user to user information</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="30" Month="10" Year="1997"/>
                <Author>LE</Author>
                <Comment>c_info changed from USHORT to UBYTE</Comment>
            </History>
            <History>
                <Date Day="27" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>user info context added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the kind of service which shall be used.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>serv</Name>
                <Type>U8</Type>
                <Comment>service code</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_serv</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines a cause for call related events/actions.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>cause</Name>
                <Type>U16</Type>
                <Comment>cause</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_cause</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="12" Month="2" Year="2002"/>
                <Author>SBK</Author>
                <Comment>Cause Concept</Comment>
            </History>
            <History>
                <Date Day="28" Month="1" Year="2003"/>
                <Author>SBK</Author>
                <Comment>Corrected twice allocated value for cause (0b1100010100000110)</Comment>
            </History>
            <History>
                <Date Day="3" Month="7" Year="2003"/>
                <Author>HM</Author>
                <Comment>MNCC_CAUSE_DTMF_STOP_SUCCESS added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the content of the notification information element.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>nd</Name>
                <Type>U8</Type>
                <Comment>notification description</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_nd</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the address of the calling or connected party.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c_num</Name>
                <Type>U8</Type>
                <Comment>number of BCD digits</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>HM</Author>
                <Comment>MAX_BCD_DIGITS =&amp;gt; MAX_CC_CALLING_NUMBER</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>added TON_NOT_PRES, NPI_NOT_PRES, fixed typo</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Made references to chapter "Elements"</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the address of the calling or connected party.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>num</Name>
                <Type>U8</Type>
                <Comment>bcd</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>HM</Author>
                <Comment>MAX_BCD_DIGITS =&amp;gt; MAX_CC_CALLING_NUMBER</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>added TON_NOT_PRES, NPI_NOT_PRES, fixed typo</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Made references to chapter "Elements"</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the address of the called party.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c_called_num</Name>
                <Type>U8</Type>
                <Comment>number of BCD digits</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>HM</Author>
                <Comment>MAX_BCD_DIGITS =&amp;gt; MAX_CC_CALLED_NUMBER</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>added TON_NOT_PRES, NPI_NOT_PRES, fixed typo</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Made references to chapter "Elements"</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the address of the called party.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>called_num</Name>
                <Type>U8</Type>
                <Comment>bcd</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="8" Month="3" Year="2002"/>
                <Author>HM</Author>
                <Comment>MAX_BCD_DIGITS =&amp;gt; MAX_CC_CALLED_NUMBER</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>added TON_NOT_PRES, NPI_NOT_PRES, fixed typo</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Made references to chapter "Elements"</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates a called, calling or connected sub address.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>tos</Name>
                <Type>U8</Type>
                <Comment>type of subaddress</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_tos</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Added redirecting party subaddress</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates a called, calling or connected sub address.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>odd_even</Name>
                <Type>U8</Type>
                <Comment>odd / even indicator</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_odd_even</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Added redirecting party subaddress</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates a called, calling or connected sub address.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c_subaddr</Name>
                <Type>U8</Type>
                <Comment>length of subaddress information</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Added redirecting party subaddress</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates a called, calling or connected sub address.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>subaddr</Name>
                <Type>U8</Type>
                <Comment>subaddress information</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Added redirecting party subaddress</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter contains one DTMF digit.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>key</Name>
                <Type>U8</Type>
                <Comment>DTMF digit</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_key</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="7" Month="1" Year="1998"/>
                <Author>PZ</Author>
                <Comment>DIG_XXX values changes to IE5</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the used channel mode.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ch_type</Name>
                <Type>U8</Type>
                <Comment>Channel Type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_ch_type</Name>
            </ValuesLink>
            <History>
                <Date Day="29" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>changed to struct with channel type and mode</Comment>
            </History>
            <History>
                <Date Day="19" Month="10" Year="2000"/>
                <Author>HM</Author>
                <Comment>+CHM_SPEECH_V2, +CHM_SPEECH_V3, -CHM_EFR_SPEECH</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the used channel mode.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ch_mode</Name>
                <Type>U8</Type>
                <Comment>Channel Mode</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_ch_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="29" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>changed to struct with channel type and mode</Comment>
            </History>
            <History>
                <Date Day="19" Month="10" Year="2000"/>
                <Author>HM</Author>
                <Comment>+CHM_SPEECH_V2, +CHM_SPEECH_V3, -CHM_EFR_SPEECH</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines whether more user information is coming with the next user information block.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>more_data</Name>
                <Type>U8</Type>
                <Comment>more data</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_more_data</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the kind of call, normal call, emergency call or CCBS call.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>prio</Name>
                <Type>U8</Type>
                <Comment>priority</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_prio</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="7" Month="2" Year="2000"/>
                <Author>HM</Author>
                <Comment>added PRIO_CCBS_CALL to mark a call as CCBS</Comment>
            </History>
            <History>
                <Date Day="3" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>removed PRIO_CCBS_CALL, not needed anymore</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the CLIR suppression.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>clir_sup</Name>
                <Type>U8</Type>
                <Comment>CLIR suppression</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_clir_sup</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="13" Month="8" Year="2002"/>
                <Author>HM</Author>
                <Comment>CLR_NOT_PRES added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the signal information element.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>sig</Name>
                <Type>U8</Type>
                <Comment>signal</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_sig</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the congestion status of the call.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>congest_lev</Name>
                <Type>U8</Type>
                <Comment>Congestion Level</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_congest_lev</Name>
            </ValuesLink>
            <History>
                <Date Day="12" Month="5" Year="1997"/>
                <Author>MS</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="1" Month="8" Year="1997"/>
                <Author>VK</Author>
                <Comment>rename constants, adapt to message constants</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter defines the supplementary service version</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ss_version</Name>
                <Type>U8</Type>
                <Comment>SS Version number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_ss_version</Name>
            </ValuesLink>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="28" Month="2" Year="2000"/>
                <Author>HM</Author>
                <Comment>Added SS_VERSION_2 and SS_VERSION_3</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates a new repeat indicator value.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ri</Name>
                <Type>U8</Type>
                <Comment>repeat indicator</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_ri</Name>
            </ValuesLink>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the relevant parameter to build a bearer capability</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rate</Name>
                <Type>U8</Type>
                <Comment>user rate</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_rate</Name>
            </ValuesLink>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="26" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Values part changed</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>CE_ELEM_NOT_PRES renamed to CONN_ELEM_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>RATE_NOT_PRES renamed to UR_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>data and stop bits added</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>parity and flow control added</Comment>
            </History>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>AK</Author>
                <Comment>conn_elem extended and modem_type added</Comment>
            </History>
            <History>
                <Date Day="16" Month="9" Year="1999"/>
                <Author>AK</Author>
                <Comment>new modem type added</Comment>
            </History>
            <History>
                <Date Day="4" Month="9" Year="2000"/>
                <Author>LE</Author>
                <Comment>Auxiliary speech added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the relevant parameter to build a bearer capability</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bearer_serv</Name>
                <Type>U8</Type>
                <Comment>bearer service</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_bearer_serv</Name>
            </ValuesLink>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="26" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Values part changed</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>CE_ELEM_NOT_PRES renamed to CONN_ELEM_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>RATE_NOT_PRES renamed to UR_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>data and stop bits added</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>parity and flow control added</Comment>
            </History>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>AK</Author>
                <Comment>conn_elem extended and modem_type added</Comment>
            </History>
            <History>
                <Date Day="16" Month="9" Year="1999"/>
                <Author>AK</Author>
                <Comment>new modem type added</Comment>
            </History>
            <History>
                <Date Day="4" Month="9" Year="2000"/>
                <Author>LE</Author>
                <Comment>Auxiliary speech added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the relevant parameter to build a bearer capability</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>conn_elem</Name>
                <Type>U8</Type>
                <Comment>connection element</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_conn_elem</Name>
            </ValuesLink>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="26" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Values part changed</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>CE_ELEM_NOT_PRES renamed to CONN_ELEM_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>RATE_NOT_PRES renamed to UR_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>data and stop bits added</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>parity and flow control added</Comment>
            </History>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>AK</Author>
                <Comment>conn_elem extended and modem_type added</Comment>
            </History>
            <History>
                <Date Day="16" Month="9" Year="1999"/>
                <Author>AK</Author>
                <Comment>new modem type added</Comment>
            </History>
            <History>
                <Date Day="4" Month="9" Year="2000"/>
                <Author>LE</Author>
                <Comment>Auxiliary speech added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the relevant parameter to build a bearer capability</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>stop_bits</Name>
                <Type>U8</Type>
                <Comment>stop bits</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_stop_bits</Name>
            </ValuesLink>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="26" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Values part changed</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>CE_ELEM_NOT_PRES renamed to CONN_ELEM_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>RATE_NOT_PRES renamed to UR_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>data and stop bits added</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>parity and flow control added</Comment>
            </History>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>AK</Author>
                <Comment>conn_elem extended and modem_type added</Comment>
            </History>
            <History>
                <Date Day="16" Month="9" Year="1999"/>
                <Author>AK</Author>
                <Comment>new modem type added</Comment>
            </History>
            <History>
                <Date Day="4" Month="9" Year="2000"/>
                <Author>LE</Author>
                <Comment>Auxiliary speech added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the relevant parameter to build a bearer capability</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>data_bits</Name>
                <Type>U8</Type>
                <Comment>data bits</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_data_bits</Name>
            </ValuesLink>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="26" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Values part changed</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>CE_ELEM_NOT_PRES renamed to CONN_ELEM_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>RATE_NOT_PRES renamed to UR_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>data and stop bits added</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>parity and flow control added</Comment>
            </History>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>AK</Author>
                <Comment>conn_elem extended and modem_type added</Comment>
            </History>
            <History>
                <Date Day="16" Month="9" Year="1999"/>
                <Author>AK</Author>
                <Comment>new modem type added</Comment>
            </History>
            <History>
                <Date Day="4" Month="9" Year="2000"/>
                <Author>LE</Author>
                <Comment>Auxiliary speech added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the relevant parameter to build a bearer capability</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>parity</Name>
                <Type>U8</Type>
                <Comment>parity</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_parity</Name>
            </ValuesLink>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="26" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Values part changed</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>CE_ELEM_NOT_PRES renamed to CONN_ELEM_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>RATE_NOT_PRES renamed to UR_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>data and stop bits added</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>parity and flow control added</Comment>
            </History>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>AK</Author>
                <Comment>conn_elem extended and modem_type added</Comment>
            </History>
            <History>
                <Date Day="16" Month="9" Year="1999"/>
                <Author>AK</Author>
                <Comment>new modem type added</Comment>
            </History>
            <History>
                <Date Day="4" Month="9" Year="2000"/>
                <Author>LE</Author>
                <Comment>Auxiliary speech added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the relevant parameter to build a bearer capability</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>flow_control</Name>
                <Type>U8</Type>
                <Comment>flow control</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_flow_control</Name>
            </ValuesLink>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="26" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Values part changed</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>CE_ELEM_NOT_PRES renamed to CONN_ELEM_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>RATE_NOT_PRES renamed to UR_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>data and stop bits added</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>parity and flow control added</Comment>
            </History>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>AK</Author>
                <Comment>conn_elem extended and modem_type added</Comment>
            </History>
            <History>
                <Date Day="16" Month="9" Year="1999"/>
                <Author>AK</Author>
                <Comment>new modem type added</Comment>
            </History>
            <History>
                <Date Day="4" Month="9" Year="2000"/>
                <Author>LE</Author>
                <Comment>Auxiliary speech added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the relevant parameter to build a bearer capability</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>modem_type</Name>
                <Type>U8</Type>
                <Comment>modem type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_modem_type</Name>
            </ValuesLink>
            <History>
                <Date Day="22" Month="5" Year="1997"/>
                <Author>VK</Author>
                <Comment>adapt to MNCC.DOC version 6 (VSS), 22-May-97, 11:01</Comment>
            </History>
            <History>
                <Date Day="26" Month="6" Year="1997"/>
                <Author>VK</Author>
                <Comment>Values part changed</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>CE_ELEM_NOT_PRES renamed to CONN_ELEM_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="14" Month="7" Year="1997"/>
                <Author>VK</Author>
                <Comment>RATE_NOT_PRES renamed to UR_NOT_PRES</Comment>
            </History>
            <History>
                <Date Day="23" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>data and stop bits added</Comment>
            </History>
            <History>
                <Date Day="24" Month="7" Year="1998"/>
                <Author>LE</Author>
                <Comment>parity and flow control added</Comment>
            </History>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>AK</Author>
                <Comment>conn_elem extended and modem_type added</Comment>
            </History>
            <History>
                <Date Day="16" Month="9" Year="1999"/>
                <Author>AK</Author>
                <Comment>new modem type added</Comment>
            </History>
            <History>
                <Date Day="4" Month="9" Year="2000"/>
                <Author>LE</Author>
                <Comment>Auxiliary speech added</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter contains a facility information element.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>l_fac</Name>
                <Type>U16</Type>
                <Comment>facility length</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="29" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter contains a facility information element.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>o_fac</Name>
                <Type>U16</Type>
                <Comment>facility offset</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="29" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter contains a facility information element.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>fac</Name>
                <Type>U8</Type>
                <Comment>facility content</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="29" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates additional cause information coming from the diagnostic field of CC messages.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>diagnostic</Name>
                <Type>U8</Type>
                <Comment>Diagnostic Information</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_diagnostic</Name>
            </ValuesLink>
            <History>
                <Date Day="29" Month="4" Year="1999"/>
                <Author>LE</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the mode for single numbering scheme.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>sns_mode</Name>
                <Type>U8</Type>
                <Comment>Single numbering scheme mode</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_sns_mode</Name>
            </ValuesLink>
            <History>
                <Date Day="11" Month="6" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the mode for sending a DTMF digit.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>dtmf_mod</Name>
                <Type>U8</Type>
                <Comment>Mode for sending DTMF digit</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_dtmf_mod</Name>
            </ValuesLink>
            <History>
                <Date Day="24" Month="9" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the mode of conversion for bearer capability parameter.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bc_mod</Name>
                <Type>U8</Type>
                <Comment>Mode for conversion of bearer capabilities</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_bc_mod</Name>
            </ValuesLink>
            <History>
                <Date Day="8" Month="11" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the coded bearer capability configuration</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bc_len</Name>
                <Type>U8</Type>
                <Comment>coded bearer cap length</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="11" Year="1999"/>
                <Author>AK</Author>
                <Comment>initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="3" Year="2000"/>
                <Author>HM</Author>
                <Comment>Added bcconf2</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the coded bearer capability configuration</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>bc</Name>
                <Type>U8</Type>
                <Comment>coded bearer cap</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="8" Month="11" Year="1999"/>
                <Author>AK</Author>
                <Comment>initial</Comment>
            </History>
            <History>
                <Date Day="13" Month="3" Year="2000"/>
                <Author>HM</Author>
                <Comment>Added bcconf2</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter identifies the originator of the bearer capability coding/decoding request.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>req_id</Name>
                <Type>U8</Type>
                <Comment>Request identifier of originator</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="10" Month="11" Year="1999"/>
                <Author>AK</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the type of the recall.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>rcl_type</Name>
                <Type>U8</Type>
                <Comment>recall type</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_rcl_type</Name>
            </ValuesLink>
            <History>
                <Date Day="4" Month="2" Year="2000"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the cause for the ACI-CC synchronization.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>synccs</Name>
                <Type>U16</Type>
                <Comment>Synchronization cause</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_synccs</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="11" Year="2001"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the event occurred in conjunction with multi party which may change the hold and/or multi party auxiliary states in CC.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>mpty_event</Name>
                <Type>U8</Type>
                <Comment>multi party event</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_mpty_event</Name>
            </ValuesLink>
            <History>
                <Date Day="26" Month="11" Year="2001"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the address of the redirecting party. For values of ton, npi, present and screen, see the definition of the calling party address.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>c_redir_num</Name>
                <Type>U8</Type>
                <Comment>number of BCD digits</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the address of the redirecting party. For values of ton, npi, present and screen, see the definition of the calling party address.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>redir_num</Name>
                <Type>U8</Type>
                <Comment>bcd</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates whether support of a Cellular Text Telephone Modem shall be signalled to the network..</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ctm_ena</Name>
                <Type>U8</Type>
                <Comment>CTM support send to NW in BC indicating speech</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_ctm_ena</Name>
            </ValuesLink>
            <History>
                <Date Day="28" Month="11" Year="2002"/>
                <Author>FK</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the type of number of the calling, called, connected or redirecting party.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ton</Name>
                <Type>U8</Type>
                <Comment>type of number</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_ton</Name>
            </ValuesLink>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>added TON_NOT_PRES, fixed typo</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter indicates the type of numbering plan identification of the calling, called, connected or redirecting party.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>npi</Name>
                <Type>U8</Type>
                <Comment>numbering plan identification</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_npi</Name>
            </ValuesLink>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
            <History>
                <Date Day="11" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>added NPI_NOT_PRES</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter is the presentation indicator of the calling or redirecting party.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>present</Name>
                <Type>U8</Type>
                <Comment>presentation indicator</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_present</Name>
            </ValuesLink>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>The parameter is the screening indicator of the calling or redirecting party.</Section>
            </Description>
            <PrimBasicElemDef>
                <Name>screen</Name>
                <Type>U8</Type>
                <Comment>screening indicator</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_screen</Name>
            </ValuesLink>
            <History>
                <Date Day="9" Month="4" Year="2002"/>
                <Author>HM</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section>Supplementary Diagnostic Element, available for some specific causes. Introduced for CQ 23619. </Section>
            </Description>
            <PrimBasicElemDef>
                <Name>ss_diag</Name>
                <Type>U8</Type>
                <Comment>Supplementary Diagnostic Element</Comment>
            </PrimBasicElemDef>
            <ValuesLink>
                <DocName DocType="SAP">mncc</DocName>
                <Name>VAL_ss_diag</Name>
            </ValuesLink>
            <History>
                <Date Day="18" Month="08" Year="2004"/>
                <Author>MDF</Author>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>c_raw_cause</Name>
                <Type>U8</Type>
                <Comment>Number of cause bytes</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="16" Month="12" Year="2005"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
        <PrimBasicElem>
            <Description>
                <Section/>
            </Description>
            <PrimBasicElemDef>
                <Name>raw_cause</Name>
                <Type>U8</Type>
                <Comment>cause as received from network</Comment>
            </PrimBasicElemDef>
            <History>
                <Date Day="16" Month="12" Year="2005"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </PrimBasicElem>
    </PrimBasicElementsSection>
    <ValuesSection>
        <Description>
            <Section>This section contains all sets of values that are defined for the MNCC SAP</Section>
        </Description>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ti</Name>
                <Comment>values for ti</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>TI_RES_1</Alias>
                <Comment>reserved</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>TI_RES_2</Alias>
                <Comment>reserved</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>0</MinValue>
                <MaxValue>6</MaxValue>
                <Comment>ms originated identifier</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>8</MinValue>
                <MaxValue>14</MaxValue>
                <Comment>ms terminated transaction</Comment>
            </ValuesRange>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_progress_desc</Name>
                <Comment>values for progress_desc</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PROG_NO_END_TO_END_PLMN</Alias>
                <Comment>call is not end-to-end PLMN/ISDN, further call progress information may be available in-band</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PROG_DEST_NON_PLMN</Alias>
                <Comment>destination address in non-PLMN/ISDN</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>PROG_ORIGIN_NON_PLMN</Alias>
                <Comment>origination address in non-PLMN/ISDN</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>PROG_RETURN_TO_PLMN</Alias>
                <Comment>call has returned to the PLMN/ISDN</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>PROG_INBAND_AVAIL</Alias>
                <Comment>in-band information or appropriate pattern now available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">32</Value>
                <Alias>PROG_END_TO_END_PLMN</Alias>
                <Comment>call is end-to-end PLMN/ISDN</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">64</Value>
                <Alias>PROG_QUEUEING</Alias>
                <Comment>queueing</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">254</Value>
                <Alias>PROG_UNSPECIFIC</Alias>
                <Comment>unspecific, used when coding standard is not equal to GSM; note that the value chosen here must not collide with any defined value of  the progress description IE of the air interface</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>PROG_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_fac_context</Name>
                <Comment>values for fac_context</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>FAC_IN_ALERT</Alias>
                <Comment>Facility information in ALERT message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>FAC_IN_CALL_PROCEED</Alias>
                <Comment>Facility information in CALL PROCEEDING message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>FAC_IN_DISCONNECT</Alias>
                <Comment>Facility information in DISCONNECT message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>FAC_IN_RELEASE</Alias>
                <Comment>Facility information in RELEASE message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>FAC_IN_CONNECT</Alias>
                <Comment>Facility information in CONNECT message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>FAC_IN_SETUP</Alias>
                <Comment>Facility information in SETUP message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>FAC_IN_FACILITY</Alias>
                <Comment>Facility information in USER INFORMATION message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>FAC_IN_RELEASE_COMP</Alias>
                <Comment>Facility information in RELEASE COMPLETE message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>FAC_IN_RECALL</Alias>
                <Comment>Facility information in RECALL message</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_info_context</Name>
                <Comment>values for info_context</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>USER_IN_ALERT</Alias>
                <Comment>User information in ALERT message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>USER_IN_DISCONNECT</Alias>
                <Comment>User information in DISCONNECT message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>USER_IN_PROGRESS</Alias>
                <Comment>User information in PROGRESS message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>USER_IN_RELEASE</Alias>
                <Comment>User information in RELEASE message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>USER_IN_CONNECT</Alias>
                <Comment>User information in CONNECT message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>USER_IN_SETUP</Alias>
                <Comment>User information in SETUP message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>USER_IN_USER</Alias>
                <Comment>User information in USER INFORMATION message</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_pd</Name>
                <Comment>values for pd</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PD_USER</Alias>
                <Comment>user specific protocol</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PD_HIGH_LAYER</Alias>
                <Comment>OSI high layer protocols</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PD_X244</Alias>
                <Comment>X.244</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>PD_SYS_MANAGE</Alias>
                <Comment>reserved for system management convergence function</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>PD_IA5</Alias>
                <Comment>IA5 characters</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>PD_V120</Alias>
                <Comment>Rec.V.120 rate adaption</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>PD_Q931</Alias>
                <Comment>Q.931 (I.451) user-network call control messages</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>16</MinValue>
                <MaxValue>63</MaxValue>
                <Comment>reserved for other network layer or through layer 3 protocols including Rec.X.25</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>64</MinValue>
                <MaxValue>79</MaxValue>
                <Comment>national use</Comment>
            </ValuesRange>
            <ValuesRange ValueType="DEC">
                <MinValue>80</MinValue>
                <MaxValue>254</MaxValue>
                <Comment>reserved for other network through layer or layer 3 protocols including Rec.X.25</Comment>
            </ValuesRange>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_serv</Name>
                <Comment>values for serv</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SERV_SPEECH</Alias>
                <Comment>speech</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SERV_DATA</Alias>
                <Comment>data</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>SERV_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_cause</Name>
                <Comment>values for cause</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="BIN">0000010100000001</Value>
                <Alias>MNCC_CAUSE_UNASSIGN</Alias>
                <Comment>unassigned (unallocated) number</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100000011</Value>
                <Alias>MNCC_CAUSE_NO_ROUTE</Alias>
                <Comment>no route to destination</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100000110</Value>
                <Alias>MNCC_CAUSE_CHAN_UNACCEPT</Alias>
                <Comment>channel unacceptable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100001000</Value>
                <Alias>MNCC_CAUSE_BARRED</Alias>
                <Comment>operator determined barring</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100010000</Value>
                <Alias>MNCC_CAUSE_CALL_CLEAR</Alias>
                <Comment>normal call clearing</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100010001</Value>
                <Alias>MNCC_CAUSE_USER_BUSY</Alias>
                <Comment>user busy</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100010010</Value>
                <Alias>MNCC_CAUSE_NO_RESPONSE</Alias>
                <Comment>no user responding</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100010011</Value>
                <Alias>MNCC_CAUSE_ALERT_NO_ANSWER</Alias>
                <Comment>user alerting, no answer</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100010101</Value>
                <Alias>MNCC_CAUSE_CALL_REJECT</Alias>
                <Comment>call rejected</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100010110</Value>
                <Alias>MNCC_CAUSE_NUM_CHANGED</Alias>
                <Comment>number changed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100011001</Value>
                <Alias>MNCC_CAUSE_PREEMPTION</Alias>
                <Comment>pre-emption</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100011010</Value>
                <Alias>MNCC_CAUSE_USER_CLEAR</Alias>
                <Comment>non selected user clearing</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100011011</Value>
                <Alias>MNCC_CAUSE_DEST_ORDER</Alias>
                <Comment>destination out of order</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100011100</Value>
                <Alias>MNCC_CAUSE_NUM_FORMAT</Alias>
                <Comment>invalid number format (incomplete number)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100011101</Value>
                <Alias>MNCC_CAUSE_FACILITY_REJECT</Alias>
                <Comment>facility rejected</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100011110</Value>
                <Alias>MNCC_CAUSE_STATUS_ENQUIRY</Alias>
                <Comment>response to status enquiry</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100011111</Value>
                <Alias>MNCC_CAUSE_UNSPECIFIED</Alias>
                <Comment>normal, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100100010</Value>
                <Alias>MNCC_CAUSE_NO_CHAN_AVAIL</Alias>
                <Comment>no circuit / channel available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100100110</Value>
                <Alias>MNCC_CAUSE_NETWORK_ORDER</Alias>
                <Comment>network out of order</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100101001</Value>
                <Alias>MNCC_CAUSE_TEMP_FAIL</Alias>
                <Comment>temporary failure</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100101010</Value>
                <Alias>MNCC_CAUSE_SWITCH_CONGEST</Alias>
                <Comment>switching equipment congestion</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100101011</Value>
                <Alias>MNCC_CAUSE_INFO_DISCARD</Alias>
                <Comment>access information discarded</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100101100</Value>
                <Alias>MNCC_CAUSE_REQ_CHAN_UNAVAIL</Alias>
                <Comment>requested circuit / channel not available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100101111</Value>
                <Alias>MNCC_CAUSE_RESOURCE_UNAVAIL</Alias>
                <Comment>resources unavailable, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100110001</Value>
                <Alias>MNCC_CAUSE_QOS_UNAVAIL</Alias>
                <Comment>quality of service unavailable</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100110010</Value>
                <Alias>MNCC_CAUSE_FACILITY_UNSUBSCRIB</Alias>
                <Comment>requested facility not subscribed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100110111</Value>
                <Alias>MNCC_CAUSE_BARRED_IN_CUG</Alias>
                <Comment>incoming calls barred within the CUG</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100111001</Value>
                <Alias>MNCC_CAUSE_BEARER_CAP_AUTHORIZ</Alias>
                <Comment>bearer capability not authorized</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100111010</Value>
                <Alias>MNCC_CAUSE_BEARER_CAP_UNAVAIL</Alias>
                <Comment>bearer capability not presently available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010100111111</Value>
                <Alias>MNCC_CAUSE_SERVICE_UNAVAIL</Alias>
                <Comment>service or option not available, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101000001</Value>
                <Alias>MNCC_CAUSE_BEARER_NOT_IMPLEM</Alias>
                <Comment>bearer service not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101000100</Value>
                <Alias>MNCC_CAUSE_ACM_MAX</Alias>
                <Comment>ACM equal or greater than ACMmax</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101000101</Value>
                <Alias>MNCC_CAUSE_FACILITY_NOT_IMPLEM</Alias>
                <Comment>requested facility not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101000110</Value>
                <Alias>MNCC_CAUSE_RESTICT_BEARER_CAP</Alias>
                <Comment>only restricted digital information bearer capability is available</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101001111</Value>
                <Alias>MNCC_CAUSE_SERVICE_NOT_IMPLEM</Alias>
                <Comment>service or option not implemented, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101010001</Value>
                <Alias>MNCC_CAUSE_INVALID_TI</Alias>
                <Comment>invalid transaction identifier value</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101010111</Value>
                <Alias>MNCC_CAUSE_USER_NOT_IN_CUG</Alias>
                <Comment>user not member of CUG</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101011000</Value>
                <Alias>MNCC_CAUSE_INCOMPAT_DEST</Alias>
                <Comment>incompatible destination (originated by net)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101011011</Value>
                <Alias>MNCC_CAUSE_INVALID_TRANS_NET</Alias>
                <Comment>invalid transit network selection</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101011111</Value>
                <Alias>MNCC_CAUSE_INCORRECT_MESSAGE</Alias>
                <Comment>semantically incorrect message</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101100000</Value>
                <Alias>MNCC_CAUSE_INVALID_MAND_INFO</Alias>
                <Comment>invalid mandatory information</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101100001</Value>
                <Alias>MNCC_CAUSE_MESSAGE_TYPE_NOT_IMPLEM</Alias>
                <Comment>message type non-existent or not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101100010</Value>
                <Alias>MNCC_CAUSE_MESSAGE_TYPE_INCOMPAT</Alias>
                <Comment>message type not compatible with protocol state</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101100011</Value>
                <Alias>MNCC_CAUSE_INFO_ELEM_NOT_IMPLEM</Alias>
                <Comment>information element non-existent or not implemented</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101100100</Value>
                <Alias>MNCC_CAUSE_COND_INFO_ELEM</Alias>
                <Comment>conditional information element error</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101100101</Value>
                <Alias>MNCC_CAUSE_MESSAGE_INCOMPAT</Alias>
                <Comment>message not compatible with protocol state</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101100110</Value>
                <Alias>MNCC_CAUSE_TIMER</Alias>
                <Comment>recovery on timer expiry</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101101111</Value>
                <Alias>MNCC_CAUSE_PROTOCOL</Alias>
                <Comment>protocol error, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0000010101111111</Value>
                <Alias>MNCC_CAUSE_INTERWORKING</Alias>
                <Comment>interworking, unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100010100011101</Value>
                <Alias>MNCC_CAUSE_MS_FACILITY_REJECT</Alias>
                <Comment>facility rejected (originated by MS)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100010101000001</Value>
                <Alias>MNCC_CAUSE_MS_BEARER_NOT_IMPLEM</Alias>
                <Comment>bearer service not implemented (originated by MS)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100010101010001</Value>
                <Alias>MNCC_CAUSE_MS_INVALID_TI</Alias>
                <Comment>invalid transaction identifier value (originated by MS)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100010101011000</Value>
                <Alias>MNCC_CAUSE_MS_INCOMPAT_DEST</Alias>
                <Comment>incompatible destination (originated by MS)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100010101100000</Value>
                <Alias>MNCC_CAUSE_MS_INVALID_MAND_INFO</Alias>
                <Comment>invalid mandatory information (originated by MS)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100010101100100</Value>
                <Alias>MNCC_CAUSE_MS_COND_INFO_ELEM</Alias>
                <Comment>conditional information element error (originated by MS)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100010101100101</Value>
                <Alias>MNCC_CAUSE_MS_MESSAGE_INCOMPAT</Alias>
                <Comment>message not compatible with protocol state (originated by MS)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">0100010101100110</Value>
                <Alias>MNCC_CAUSE_MS_TIMER</Alias>
                <Comment>recovery on timer expiry (originated by MS)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1000010100000000</Value>
                <Alias>MNCC_CAUSE_MODIFY_SUCCESS</Alias>
                <Comment>in-call modification successfully performed, MODIFY COMPLETE message received</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1000010100000010</Value>
                <Alias>MNCC_CAUSE_HOLD_SUCCESS</Alias>
                <Comment>hold successfully performed, HOLD ACKNOWLEDGE message received</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1000010100000011</Value>
                <Alias>MNCC_CAUSE_RETRIEVE_SUCCESS</Alias>
                <Comment>retrieve successfully performed, RETRIEVE ACKNOWLEDGE message received</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1000010100000100</Value>
                <Alias>MNCC_CAUSE_DTMF_START_SUCCESS</Alias>
                <Comment>start of DTMF successfully performed, START DTMF ACKNOWLEDGE message received</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1000010100000101</Value>
                <Alias>MNCC_CAUSE_DTMF_STOP_SUCCESS</Alias>
                <Comment>stop of DTMF successfully performed, STOP DTMF ACKNOWLEDGE message received</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1000010111111111</Value>
                <Alias>MNCC_CAUSE_NO_NET_CAUSE</Alias>
                <Comment>network initiated without cause</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100010100000000</Value>
                <Alias>MNCC_CAUSE_SUCCESS</Alias>
                <Comment>operation successfully performed (e.g. a call establishment); this cause is used only if no more specific cause applies</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100010100000001</Value>
                <Alias>MNCC_CAUSE_DTMF_NOT_ALLOWED</Alias>
                <Comment>DTMF is currently not allowed (no speech TCH)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100010100000010</Value>
                <Alias>MNCC_CAUSE_DTMF_BUFFER_FULL</Alias>
                <Comment>DTMF storage buffer overflow</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100010100000011</Value>
                <Alias>MNCC_CAUSE_DTMF_ABORTED</Alias>
                <Comment>DTMF was aborted (e.g. due to state change)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100010100000100</Value>
                <Alias>MNCC_CAUSE_MAX_NO_RECALLS_REACHED</Alias>
                <Comment>maximum number of recalls (CCBS) was reached</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100010100000101</Value>
                <Alias>MNCC_CAUSE_MAX_NO_CALLS_REACHED</Alias>
                <Comment>maximum number of calls was reached</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100010100000110</Value>
                <Alias>MNCC_CAUSE_CHANNEL_SYNC</Alias>
                <Comment>channel mode or type information (changed)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100010100000111</Value>
                <Alias>MNCC_CAUSE_REEST_STARTED</Alias>
                <Comment>call re-establishment started</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100010100001000</Value>
                <Alias>MNCC_CAUSE_REEST_FINISHED</Alias>
                <Comment>call re-establishment is finished</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="BIN">1100010111111111</Value>
                <Alias>MNCC_CAUSE_NO_MS_CAUSE</Alias>
                <Comment>MS initiated without cause</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_nd</Name>
                <Comment>values for nd</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>ND_USER_SUSPEND</Alias>
                <Comment>user suspended</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>ND_USER_RESUME</Alias>
                <Comment>user resumed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>ND_BEAR_CHANGE</Alias>
                <Comment>bearer change</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>ND_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_tos</Name>
                <Comment>values for tos</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TOS_NSAP</Alias>
                <Comment>NSAP (X.213/ISO 8348 AD2)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>TOS_USER_SPEC</Alias>
                <Comment>user specified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>TOS_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_odd_even</Name>
                <Comment>values for odd_even</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>OE_EVEN</Alias>
                <Comment>even number of address signals</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>OE_ODD</Alias>
                <Comment>odd number of address signals</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_key</Name>
                <Comment>values for key</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="HEX">30</Value>
                <Alias>DIG_0</Alias>
                <Comment>digit '0'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">31</Value>
                <Alias>DIG_1</Alias>
                <Comment>digit '1'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">32</Value>
                <Alias>DIG_2</Alias>
                <Comment>digit '2'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">33</Value>
                <Alias>DIG_3</Alias>
                <Comment>digit '3'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">34</Value>
                <Alias>DIG_4</Alias>
                <Comment>digit '4'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">35</Value>
                <Alias>DIG_5</Alias>
                <Comment>digit '5'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">36</Value>
                <Alias>DIG_6</Alias>
                <Comment>digit '6'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">37</Value>
                <Alias>DIG_7</Alias>
                <Comment>digit '7'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">38</Value>
                <Alias>DIG_8</Alias>
                <Comment>digit '8'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">39</Value>
                <Alias>DIG_9</Alias>
                <Comment>digit '9'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">41</Value>
                <Alias>DIG_A</Alias>
                <Comment>'A'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">42</Value>
                <Alias>DIG_B</Alias>
                <Comment>'B'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">43</Value>
                <Alias>DIG_C</Alias>
                <Comment>'C'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">44</Value>
                <Alias>DIG_D</Alias>
                <Comment>'D'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">2A</Value>
                <Alias>DIG_STAR</Alias>
                <Comment>'('</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">23</Value>
                <Alias>DIG_HASH</Alias>
                <Comment>'#'</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">7F</Value>
                <Alias>DIG_RES</Alias>
                <Comment>reserved</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ch_mode</Name>
                <Comment>values for ch_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CHM_SIG_ONLY</Alias>
                <Comment>signalling only</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CHM_SPEECH</Alias>
                <Comment>speech full rate or half rate version 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">33</Value>
                <Alias>CHM_SPEECH_V2</Alias>
                <Comment>speech full rate or half rate version 2</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">65</Value>
                <Alias>CHM_SPEECH_V3</Alias>
                <Comment>speech full rate or half rate version 3</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CHM_DATA_9_6</Alias>
                <Comment>data 9.6 kBit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>CHM_DATA_4_8</Alias>
                <Comment>data 4.8 kBit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">19</Value>
                <Alias>CHM_DATA_2_4</Alias>
                <Comment>data 2.4 kBit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>CHM_DATA_14_4</Alias>
                <Comment>data 2.4 kBit/s</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ch_type</Name>
                <Comment>values for ch_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CH_SDCCH</Alias>
                <Comment>SDCCH channel</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CH_TCH_F</Alias>
                <Comment>TCH Fullrate</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CH_TCH_H</Alias>
                <Comment>TCH Halfrate</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_more_data</Name>
                <Comment>values for more_data</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MD_NO_MORE_DATA</Alias>
                <Comment>no more data</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MD_MORE_DATA</Alias>
                <Comment>more data</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>MD_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_prio</Name>
                <Comment>values for prio</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PRIO_NORM_CALL</Alias>
                <Comment>normal call</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PRIO_EMERG_CALL</Alias>
                <Comment>emergency call</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_clir_sup</Name>
                <Comment>values for clir_sup</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CLR_SUP</Alias>
                <Comment>CLIR suppressed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CLR_SUP_NOT</Alias>
                <Comment>CLIR not suppressed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">FF</Value>
                <Alias>CLR_NOT_PRES</Alias>
                <Comment>CLIR not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_sig</Name>
                <Comment>values for sig</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SIG_DIAL_TONE_ON</Alias>
                <Comment>dial tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SIG_RING_BACK_TONE_ON</Alias>
                <Comment>ring back tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SIG_INT_TONE_ON</Alias>
                <Comment>intercept tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SIG_NET_CONG_TONE_ON</Alias>
                <Comment>network congestion tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SIG_BUSY_TONE_ON</Alias>
                <Comment>busy tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SIG_CONF_TONE_ON</Alias>
                <Comment>confirm tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>SIG_ANS_TONE_ON</Alias>
                <Comment>answer tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>SIG_CALL_WAIT_TONE_ON</Alias>
                <Comment>call waiting tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>SIG_OFF_HOOK_WARN_TONE_ON</Alias>
                <Comment>off-hook warning tone on</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">63</Value>
                <Alias>SIG_TONES_OFF</Alias>
                <Comment>tones off</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">79</Value>
                <Alias>SIG_ALERT_OFF</Alias>
                <Comment>alerting off</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>SIG_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_congest_lev</Name>
                <Comment>values for congest_lev</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CL_RECEIVER_READY</Alias>
                <Comment>receiver ready</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">15</Value>
                <Alias>CL_RECEIVER_NOT_READY</Alias>
                <Comment>receiver not ready</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>CL_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ss_version</Name>
                <Comment>values for ss_version</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SS_VERSION_2</Alias>
                <Comment>phase 2 service, ellipsis notation and phase 2 error handling</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SS_VERSION_3</Alias>
                <Comment>SS-Protocol version 3 and phase 2 error handling</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>SS_VER_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ri</Name>
                <Comment>values for ri</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>RI_CIRCULAR</Alias>
                <Comment>circular</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>RI_SEQUENTIAL</Alias>
                <Comment>sequential</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>RI_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_parity</Name>
                <Comment>values for parity</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PARITY_ODD</Alias>
                <Comment>odd parity</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PARITY_EVEN</Alias>
                <Comment>even parity</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>PARITY_NONE</Alias>
                <Comment>no parity</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>PARITY_FORCED_TO_0</Alias>
                <Comment>parity forced to zero</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>PARITY_FORCED_TO_1</Alias>
                <Comment>parity forced to one</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bearer_serv</Name>
                <Comment>values for bearer_serv</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>BEARER_SERV_SYNC</Alias>
                <Comment>synchronous</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>BEARER_SERV_ASYNC</Alias>
                <Comment>asynchronous</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>BEARER_SERV_PAD_ACCESS</Alias>
                <Comment>PAD access (async)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>BEARER_SERV_PACKET_ACCESS</Alias>
                <Comment>packet access (sync)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>BEARER_SERV_FAX</Alias>
                <Comment>fax</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>BEARER_SERV_SPEECH</Alias>
                <Comment>Speech</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>BEARER_SERV_AUX_SPEECH</Alias>
                <Comment>Auxiliary Speech</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>BEARER_SERV_SPEECH_CTM</Alias>
                <Comment>Speech with CTM (TTY) support</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>BEARER_SERV_AUX_SPEECH_CTM</Alias>
                <Comment>Auxiliary Speech CTM (TTY) support</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>BEARER_SERV_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_modem_type</Name>
                <Comment>values for modem_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MT_NONE</Alias>
                <Comment>modem type none</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MT_V21</Alias>
                <Comment>modem type V.21</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MT_V22</Alias>
                <Comment>modem type V.22</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MT_V22_BIS</Alias>
                <Comment>modem type V.22bis</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>MT_V23</Alias>
                <Comment>modem type V.23</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>MT_V26_TER</Alias>
                <Comment>modem type V.26ter</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>MT_V32</Alias>
                <Comment>modem type V.32</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>MT_UNDEF</Alias>
                <Comment>modem type for undefined interface</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>MT_AUTOBAUD</Alias>
                <Comment>modem type autobauding type 1</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>MT_V32_BIS</Alias>
                <Comment>modem type V.32bis</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>MT_V34</Alias>
                <Comment>modem type V.34</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_rate</Name>
                <Comment>values for rate</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>UR_0_3_KBIT</Alias>
                <Comment>rate : 0.3 kbit/s Recommendation X.1 and V.110</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>UR_1_2_KBIT</Alias>
                <Comment>rate : 1.2 kbit/s Recommendation X.1 and V.110</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>UR_2_4_KBIT</Alias>
                <Comment>rate : 2.4 kbit/s Recommendation X.1 and V.110</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>UR_4_8_KBIT</Alias>
                <Comment>rate : 4.8 kbit/s Recommendation X.1 and V.110</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>UR_9_6_KBIT</Alias>
                <Comment>rate : 9.6 kbit/s Recommendation X.1 and V.110</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>UR_12_0_KBIT_TRANS</Alias>
                <Comment>rate : 12.0 kbit/s transparent</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>UR_1_2_KBIT_V23</Alias>
                <Comment>rate : 1.2 kbit/s/75 bit/s Recommendation V.23, X.1,V.110.</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>UR_14_4_KBIT</Alias>
                <Comment>rate : 14.4 kbit/s</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>UR_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_flow_control</Name>
                <Comment>values for flow_control</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>INBAND_FLOW_CONTROL</Alias>
                <Comment>inband flow control (ISO 6429)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">12</Value>
                <Alias>NO_FLOW_CONTROL</Alias>
                <Comment>no flow control (COPnoFLCT)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>OUTBAND_FLOW_CONTROL</Alias>
                <Comment>outband flow control</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_conn_elem</Name>
                <Comment>values for conn_elem</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CONN_ELEM_TRANS</Alias>
                <Comment>transparent</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CONN_ELEM_NON_TRANS</Alias>
                <Comment>non transparent (RLP)</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>CONN_ELEM_TRANS_PREF</Alias>
                <Comment>both, transparent preferred</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>CONN_ELEM_NON_TRANS_PREF</Alias>
                <Comment>both, non transparent (RLP) preferred</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>CONN_ELEM_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_stop_bits</Name>
                <Comment>values for stop_bits</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>STOP_1_BIT</Alias>
                <Comment>one stop bit</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>STOP_2_BIT</Alias>
                <Comment>two stop bits</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_data_bits</Name>
                <Comment>values for data_bits</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DATA_7_BIT</Alias>
                <Comment>seven data bits</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DATA_8_BIT</Alias>
                <Comment>eight data bits</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_diagnostic</Name>
                <Comment>values for diagnostic</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">129</Value>
                <Alias>DIAG_MOC_BAR_CUG</Alias>
                <Comment>Outgoing calls barred within CUG</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">130</Value>
                <Alias>DIAG_NO_CUG_SELECTED</Alias>
                <Comment>No CUG selected</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">131</Value>
                <Alias>DIAG_UNKNOWN_CUG_INDEX</Alias>
                <Comment>Unknown CUG index</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">132</Value>
                <Alias>DIAG_INCOMPAT_CUG_INDEX</Alias>
                <Comment>CUG index incompatible with requested basic service</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">133</Value>
                <Alias>DIAG_CUG_FAIL_UNSPEC</Alias>
                <Comment>CUG call Failure unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">134</Value>
                <Alias>DIAG_CLIR_NOT_SUBSCRIBED</Alias>
                <Comment>CLIR not subscribed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">135</Value>
                <Alias>DIAG_CCBS_POSSIBLE</Alias>
                <Comment>CCBS possible</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">136</Value>
                <Alias>DIAG_CCBS_NOT_POSSIBLE</Alias>
                <Comment>CCBS not possible</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>Values for ss_diag, see specification TS 24.008 section 10.5.4.11 "NOTE 1"</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ss_diag</Name>
                <Comment>Values for ss_diag</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SS_DIAG_MOC_BAR_CUG</Alias>
                <Comment>Outgoing calls barred within CUG</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SS_DIAG_NO_CUG_SELECTED</Alias>
                <Comment>No CUG selected</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SS_DIAG_UNKNOWN_CUG_INDEX</Alias>
                <Comment>Unknown CUG index</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SS_DIAG_INCOMPAT_CUG_INDEX</Alias>
                <Comment>CUG index incompatible with requested basic service</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SS_DIAG_CUG_FAIL_UNSPEC</Alias>
                <Comment>CUG call Failure unspecified</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>SS_DIAG_CLIR_NOT_SUBSCRIBED</Alias>
                <Comment>CLIR not subscribed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>SS_DIAG_CCBS_POSSIBLE</Alias>
                <Comment>CCBS possible</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>SS_DIAG_CCBS_NOT_POSSIBLE</Alias>
                <Comment>CCBS not possible</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>SS_DIAG_NOT_PROVIDED</Alias>
                <Comment>Not Provided</Comment>
            </ValuesItem>
            <History>
                <Date Day="18" Month="08" Year="2004"/>
                <Author/>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_sns_mode</Name>
                <Comment>values for sns_mode</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SNS_MODE_VOICE</Alias>
                <Comment>voice calls</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SNS_MODE_VAF_VOICE</Alias>
                <Comment>voice alternating FAX, voice first</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SNS_MODE_FAX</Alias>
                <Comment>FAX calls</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SNS_MODE_VAD_VOICE</Alias>
                <Comment>voice alternating data, voice first</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>SNS_MODE_DATA</Alias>
                <Comment>data calls</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>SNS_MODE_VAF_FAX</Alias>
                <Comment>voice alternating FAX, FAX first</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>SNS_MODE_VAD_DATA</Alias>
                <Comment>voice alternating data, data first</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>SNS_MODE_VFD</Alias>
                <Comment>voice followed by data</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_dtmf_mod</Name>
                <Comment>values for dtmf_mod</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>DTMF_MOD_AUTO</Alias>
                <Comment>automatic mode with fixed duration</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>DTMF_MOD_MAN_START</Alias>
                <Comment>manual mode start sending DTMF digit</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>DTMF_MOD_MAN_STOP</Alias>
                <Comment>manual mode stop sending DTMF digit</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_bc_mod</Name>
                <Comment>values for bc_mod</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>BC_MOD_CODE</Alias>
                <Comment>code bearer capabilities</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>BC_MOD_DECODE</Alias>
                <Comment>decode bearer capabilities</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_rcl_type</Name>
                <Comment>values for rcl_type</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>RCL_CCBS</Alias>
                <Comment>CCBS</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>RCL_CCBS_1</Alias>
                <Comment>treated as CCBS</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>RCL_CCBS_2</Alias>
                <Comment>treated as CCBS</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>RCL_CCBS_3</Alias>
                <Comment>treated as CCBS</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>RCL_CCBS_4</Alias>
                <Comment>treated as CCBS</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>RCL_CCBS_5</Alias>
                <Comment>treated as CCBS</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>RCL_CCBS_6</Alias>
                <Comment>treated as CCBS</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_synccs</Name>
                <Comment>values for synccs</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SYNCCS_MPTY_EVENT</Alias>
                <Comment>Multi party event</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">FFFF</Value>
                <Alias>SYNCCS_NOT_PRESENT</Alias>
                <Comment>Synchronization cause not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_mpty_event</Name>
                <Comment>values for mpty_event</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>MPTY_BUILD_SENT</Alias>
                <Comment>BuildMPTY Invoke sent</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>MPTY_BUILD_FAIL</Alias>
                <Comment>BuildMPTY Invoke failed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>MPTY_BUILD_SUCCESS</Alias>
                <Comment>BuildMPTY Invoke ok</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>MPTY_SPLIT_SENT</Alias>
                <Comment>SplitMPTY Invoke sent</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>MPTY_SPLIT_FAIL</Alias>
                <Comment>SplitMPTY Invoke failed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">5</Value>
                <Alias>MPTY_SPLIT_SUCCESS</Alias>
                <Comment>SplitMPTY Invoke Return Result ok</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">6</Value>
                <Alias>MPTY_HOLD_SENT</Alias>
                <Comment>HoldMPTY Invoke sent</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">7</Value>
                <Alias>MPTY_HOLD_FAIL</Alias>
                <Comment>HoldMPTY Invoke failed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>MPTY_HOLD_SUCCESS</Alias>
                <Comment>HoldMPTY Invoke ok</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>MPTY_RETRIEVE_SENT</Alias>
                <Comment>RetrieveMPTY Invoke</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">10</Value>
                <Alias>MPTY_RETRIEVE_FAIL</Alias>
                <Comment>RetrieveMPTY Invoke failed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">11</Value>
                <Alias>MPTY_RETRIEVE_SUCCESS</Alias>
                <Comment>RetrieveMPTY Invoke Return Result ok</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="HEX">FF</Value>
                <Alias>MPTY_NOT_PRESENT</Alias>
                <Comment>Parameter not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ctm_ena</Name>
                <Comment>values for ctm_ena</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>CTM_DISABLED</Alias>
                <Comment>CTM not supported</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>CTM_ENABLED</Alias>
                <Comment>CTM supported</Comment>
            </ValuesItem>
            <ValuesRange ValueType="DEC">
                <MinValue>2</MinValue>
                <MaxValue>255</MaxValue>
                <Comment>reserved, to be treated as CTM not supported</Comment>
            </ValuesRange>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_ton</Name>
                <Comment>values for ton</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>TON_UNKNOWN</Alias>
                <Comment>unknown</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>TON_INT_NUMB</Alias>
                <Comment>international number</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>TON_NAT_NUMB</Alias>
                <Comment>national number</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>TON_NET_SPEC_NUMB</Alias>
                <Comment>network specific number</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>TON_DED_ACC_SC</Alias>
                <Comment>dedicated access, short code</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>TON_NOT_PRES</Alias>
                <Comment>type of number not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_npi</Name>
                <Comment>values for npi</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>NPI_UNKNOW</Alias>
                <Comment>unknown</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>NPI_ISDN_TEL_NUMB_PLAN</Alias>
                <Comment>ISDN/telephony numbering plan</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>NPI_DATA_NUMB_PLAN</Alias>
                <Comment>data numbering plan</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">4</Value>
                <Alias>NPI_TELEX_NUMB_PLAN</Alias>
                <Comment>telex numbering plan</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">8</Value>
                <Alias>NPI_NAT_NUMB_PLAN</Alias>
                <Comment>national numbering plan</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">9</Value>
                <Alias>NPI_PRIV_NUMB_PLAN</Alias>
                <Comment>private numbering plan</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>NPI_NOT_PRES</Alias>
                <Comment>numbering plan identification not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_present</Name>
                <Comment>values for present</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>PRES_PRES_ALLOW</Alias>
                <Comment>presentation allowed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>PRES_PRES_REST</Alias>
                <Comment>presentation restricted</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>PRES_NUMB_NOT_AVAIL</Alias>
                <Comment>number not available due to interworking</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>PRES_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
        <Values>
            <Description>
                <Section>This former local values table was generated by the doc2XML converter tool. Please exchange this description by a more meaningful one !!!</Section>
            </Description>
            <ValuesDef>
                <Name>VAL_screen</Name>
                <Comment>values for screen</Comment>
            </ValuesDef>
            <ValuesItem>
                <Value ValueType="DEC">0</Value>
                <Alias>SCREEN_USER_PROV_NOT_SCREEN</Alias>
                <Comment>user provided, not screened</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">1</Value>
                <Alias>SCREEN_USER_PROV_VER_PASS</Alias>
                <Comment>user provided, verified and passed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">2</Value>
                <Alias>SCREEN_USER_PROV_VER_FAIL</Alias>
                <Comment>user provided, verified and failed</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">3</Value>
                <Alias>SCREEN_NET_PROV</Alias>
                <Comment>network provided</Comment>
            </ValuesItem>
            <ValuesItem>
                <Value ValueType="DEC">255</Value>
                <Alias>SCREEN_IND_NOT_PRES</Alias>
                <Comment>not present</Comment>
            </ValuesItem>
            <History>
                <Date Day="26" Month="11" Year="2003"/>
                <Author>doc2XML</Author>
                <Comment>Initial</Comment>
            </History>
        </Values>
    </ValuesSection>
</SAP>
